From e892dea7229d56b75c46a76b9039f9e179584a91 Mon Sep 17 00:00:00 2001
From: Yunhui Cui <B56489@freescale.com>
Date: Mon, 1 Feb 2016 18:48:49 +0800
Subject: [PATCH 100/113] mtd:spi_nor: Disable Micron flash HW protection

For Micron family ,The status register write enable/disable bit,
provides hardware data protection for the device.
When the enable/disable bit is set to 1, the status register
nonvolatile bits become read-only and the WRITE STATUS REGISTER
operation will not execute.

Signed-off-by: Yunhui Cui <B56489@freescale.com>
---
 drivers/mtd/spi-nor/spi-nor.c |    9 +++++++++
 1 file changed, 9 insertions(+)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -39,6 +39,7 @@
 
 #define SPI_NOR_MAX_ID_LEN	6
 #define SPI_NOR_MAX_ADDR_WIDTH	4
+#define SPI_NOR_MICRON_WRITE_ENABLE	0x7f
 
 struct flash_info {
 	char		*name;
@@ -1238,6 +1239,14 @@ int spi_nor_scan(struct spi_nor *nor, co
 	if (ret)
 		return ret;
 
+	if (JEDEC_MFR(info) == SNOR_MFR_MICRON) {
+		ret = read_sr(nor);
+		ret &= SPI_NOR_MICRON_WRITE_ENABLE;
+
+		write_enable(nor);
+		write_sr(nor, ret);
+	}
+
 	if (!mtd->name)
 		mtd->name = dev_name(dev);
 	mtd->priv = nor;
