#!/bin/sh
#
# Copyright (c) 2015 The Linux Foundation. All rights reserved.
# Copyright (c) 2011-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/ipq806x.sh
. /lib/functions/system.sh

board_config_update

board=$(ipq806x_board_name)

case "$board" in
ap148 |\
c2600 |\
d7800 |\
r7500 |\
r7500v2 |\
r7800 |\
vr2600v)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6@eth1" "5:wan" "0@eth0"
	;;
db149)
	ucidef_set_interface_lan "eth1 eth2 eth3"
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6@eth1" "5:wan" "0@eth0"
	;;
ea8500)

	hw_mac_addr=$(mtd_get_mac_ascii devinfo hw_mac_addr)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "0t@eth0" "5:wan" "0t@eth0"
	ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
	ucidef_set_interface_macaddr "wan" "$hw_mac_addr"
	;;
nbg6817)
	hw_mac_addr=$(mtd_get_mac_ascii 0:APPSBLENV ethaddr)
	ucidef_add_switch "switch0" \
		"1:lan" "2:lan" "3:lan" "4:lan" "6@eth1" "5:wan" "0@eth0"
	ucidef_set_interface_macaddr "lan" "$hw_mac_addr"
	ucidef_set_interface_macaddr "wan" "$(macaddr_add $hw_mac_addr 1)"
	;;
*)
	echo "Unsupported hardware. Network interfaces not intialized"
	;;
esac

board_config_flush

exit 0
