From 07b50db6e685172a41b9978aebffb2438166d9b6 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Thu, 19 May 2016 22:07:35 +0200
Subject: [PATCH] MIPS: ralink: fix MT7628 wled_an pinmux gpio
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Cc: john@phrozen.org
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/13307/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ralink/mt7620.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/arch/mips/ralink/mt7620.c
+++ b/arch/mips/ralink/mt7620.c
@@ -196,10 +196,10 @@ static struct rt2880_pmx_func wled_kn_gr
 };
 
 static struct rt2880_pmx_func wled_an_grp_mt7628[] = {
-	FUNC("rsvd", 3, 35, 1),
-	FUNC("rsvd", 2, 35, 1),
-	FUNC("gpio", 1, 35, 1),
-	FUNC("wled_an", 0, 35, 1),
+	FUNC("rsvd", 3, 44, 1),
+	FUNC("rsvd", 2, 44, 1),
+	FUNC("gpio", 1, 44, 1),
+	FUNC("wled_an", 0, 44, 1),
 };
 
 #define MT7628_GPIO_MODE_MASK		0x3
