From ac88474b485e297429614c8544e779d9329d2851 Mon Sep 17 00:00:00 2001
From: Matthias Reichl <hias@horus.com>
Date: Sat, 4 Jun 2016 11:30:48 +0200
Subject: [PATCH] gpio-ir overlay: gpio_pin shouldn't change pull setting

Signed-off-by: Matthias Reichl <hias@horus.com>
---
 arch/arm/boot/dts/overlays/gpio-ir-overlay.dts | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
+++ b/arch/arm/boot/dts/overlays/gpio-ir-overlay.dts
@@ -36,8 +36,7 @@
         __overrides__ {
                 // parameters
                 gpio_pin =      <&gpio_ir>,"gpios:4",
-                                        <&gpio_ir_pins>,"brcm,pins:0",
-                                        <&gpio_ir_pins>,"brcm,pull:0";  // pin number
+                                        <&gpio_ir_pins>,"brcm,pins:0";  // pin number
                 gpio_pull = <&gpio_ir_pins>,"brcm,pull:0";              // pull-up/down state
 
                 rc-map-name = <&gpio_ir>,"linux,rc-map-name";           // default rc map
