#!/bin/sh
#
# Copyright (C) 2012-2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/kirkwood.sh

board_config_update

board=$(kirkwood_board_name)

case "$board" in
"dockstar")
	ucidef_set_led_default "health" "health" "status:green:health" "1"
	ucidef_set_led_default "fault" "fault" "status:orange:fault" "1"
	;;
"linksys-audi")
	ucidef_set_led_default "power" "power" "audi:green:power" "1"
	;;
"linksys-viper")
	ucidef_set_led_default "health" "health" "viper:white:health" "1"
	ucidef_set_led_default "pulse" "pulse" "viper:white:pulse" "1"
	;;
"goflexhome" | \
"goflexnet")
	ucidef_set_led_default "health" "health" "status:green:health" "1"
	ucidef_set_led_default "fault" "fault" "status:orange:fault" "0"
	;;
"ib62x0")
	ucidef_set_led_default "health" "health" "ib62x0:green:os" "1"
	ucidef_set_led_default "fault" "fault" "ib62x0:red:os" "1"
	;;
"pogo_e02")
	ucidef_set_led_default "health" "health" "pogo_e02:green:health" "1"
	ucidef_set_led_default "fault" "fault" "pogo_e02:orange:fault" "1"
	;;
"guruplug-server-plus")
	ucidef_set_led_timer "health" "health" "guruplug:red:health" "200" "800"
	;;
"sheevaplug" | \
"sheevaplug-esata")
	ucidef_set_led_timer "health" "health" "sheevaplug:blue:health" "200" "800"
	;;
*)
	;;
esac

board_config_flush

exit 0
