From 2875141e9d5005e964e31e55b892e2fb1919e58e Mon Sep 17 00:00:00 2001
From: Jools Wills <buzz@exotica.org.uk>
Date: Sun, 26 Jun 2016 16:28:48 +0000
Subject: [PATCH] enable led support for xpad driver - fixes flashing leds on
 controller

---
 arch/arm/configs/bcm2709_defconfig | 1 +
 arch/arm/configs/bcmrpi_defconfig  | 1 +
 2 files changed, 2 insertions(+)

--- a/arch/arm/configs/bcm2709_defconfig
+++ b/arch/arm/configs/bcm2709_defconfig
@@ -559,6 +559,7 @@ CONFIG_JOYSTICK_IFORCE=m
 CONFIG_JOYSTICK_IFORCE_USB=y
 CONFIG_JOYSTICK_XPAD=m
 CONFIG_JOYSTICK_XPAD_FF=y
+CONFIG_JOYSTICK_XPAD_LEDS=y
 CONFIG_JOYSTICK_RPISENSE=m
 CONFIG_INPUT_TOUCHSCREEN=y
 CONFIG_TOUCHSCREEN_ADS7846=m
--- a/arch/arm/configs/bcmrpi_defconfig
+++ b/arch/arm/configs/bcmrpi_defconfig
@@ -552,6 +552,7 @@ CONFIG_JOYSTICK_IFORCE=m
 CONFIG_JOYSTICK_IFORCE_USB=y
 CONFIG_JOYSTICK_XPAD=m
 CONFIG_JOYSTICK_XPAD_FF=y
+CONFIG_JOYSTICK_XPAD_LEDS=y
 CONFIG_JOYSTICK_RPISENSE=m
 CONFIG_INPUT_TOUCHSCREEN=y
 CONFIG_TOUCHSCREEN_ADS7846=m
