From 8527843351169d999995d331bbdad75560ccafb2 Mon Sep 17 00:00:00 2001
From: Michal Suchanek <hramrach@gmail.com>
Date: Wed, 2 Dec 2015 10:38:20 +0000
Subject: [PATCH 093/113] mtd: spi-nor: check return value from read/write

SPI NOR hardware drivers now return useful value from their read/write
functions so check them.

Signed-off-by: Michal Suchanek <hramrach@gmail.com>
Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@freescale.com>
---
 drivers/mtd/spi-nor/spi-nor.c |   50 +++++++++++++++++++++++++++++------------
 1 file changed, 36 insertions(+), 14 deletions(-)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -923,7 +923,10 @@ static int spi_nor_read(struct mtd_info
 	ret = nor->read(nor, from, len, retlen, buf);
 
 	spi_nor_unlock_and_unprep(nor, SPI_NOR_OPS_READ);
-	return ret;
+	if (ret < 0)
+		return ret;
+
+	return 0;
 }
 
 static int sst_write(struct mtd_info *mtd, loff_t to, size_t len,
@@ -949,10 +952,14 @@ static int sst_write(struct mtd_info *mt
 		nor->program_opcode = SPINOR_OP_BP;
 
 		/* write one byte. */
-		nor->write(nor, to, 1, retlen, buf);
+		ret = nor->write(nor, to, 1, retlen, buf);
+		if (ret < 0)
+			goto sst_write_err;
+		WARN(ret != 1, "While writing 1 byte written %i bytes\n",
+		     (int)ret);
 		ret = spi_nor_wait_till_ready(nor);
 		if (ret)
-			goto time_out;
+			goto sst_write_err;
 	}
 	to += actual;
 
@@ -961,10 +968,14 @@ static int sst_write(struct mtd_info *mt
 		nor->program_opcode = SPINOR_OP_AAI_WP;
 
 		/* write two bytes. */
-		nor->write(nor, to, 2, retlen, buf + actual);
+		ret = nor->write(nor, to, 2, retlen, buf + actual);
+		if (ret < 0)
+			goto sst_write_err;
+		WARN(ret != 2, "While writing 2 bytes written %i bytes\n",
+		     (int)ret);
 		ret = spi_nor_wait_till_ready(nor);
 		if (ret)
-			goto time_out;
+			goto sst_write_err;
 		to += 2;
 		nor->sst_write_second = true;
 	}
@@ -973,21 +984,24 @@ static int sst_write(struct mtd_info *mt
 	write_disable(nor);
 	ret = spi_nor_wait_till_ready(nor);
 	if (ret)
-		goto time_out;
+		goto sst_write_err;
 
 	/* Write out trailing byte if it exists. */
 	if (actual != len) {
 		write_enable(nor);
 
 		nor->program_opcode = SPINOR_OP_BP;
-		nor->write(nor, to, 1, retlen, buf + actual);
-
+		ret = nor->write(nor, to, 1, retlen, buf + actual);
+		if (ret < 0)
+			goto sst_write_err;
+		WARN(ret != 1, "While writing 1 byte written %i bytes\n",
+		     (int)ret);
 		ret = spi_nor_wait_till_ready(nor);
 		if (ret)
-			goto time_out;
+			goto sst_write_err;
 		write_disable(nor);
 	}
-time_out:
+sst_write_err:
 	spi_nor_unlock_and_unprep(nor, SPI_NOR_OPS_WRITE);
 	return ret;
 }
@@ -1016,14 +1030,18 @@ static int spi_nor_write(struct mtd_info
 
 	/* do all the bytes fit onto one page? */
 	if (page_offset + len <= nor->page_size) {
-		nor->write(nor, to, len, retlen, buf);
+		ret = nor->write(nor, to, len, retlen, buf);
+		if (ret < 0)
+			goto write_err;
 	} else {
 		/* the size of data remaining on the first page */
 		page_size = nor->page_size - page_offset;
-		nor->write(nor, to, page_size, retlen, buf);
+		ret = nor->write(nor, to, page_size, retlen, buf);
+		if (ret < 0)
+			goto write_err;
 
 		/* write everything in nor->page_size chunks */
-		for (i = page_size; i < len; i += page_size) {
+		for (i = ret; i < len; ) {
 			page_size = len - i;
 			if (page_size > nor->page_size)
 				page_size = nor->page_size;
@@ -1034,7 +1052,11 @@ static int spi_nor_write(struct mtd_info
 
 			write_enable(nor);
 
-			nor->write(nor, to + i, page_size, retlen, buf + i);
+			ret = nor->write(nor, to + i, page_size, retlen,
+					 buf + i);
+			if (ret < 0)
+				goto write_err;
+			i += ret;
 		}
 	}
 
