#!/bin/sh
#
# Copyright (C) 2011-2015 OpenWrt.org
# based on ar71xx
#

. /lib/functions/uci-defaults.sh
. /lib/functions/lantiq.sh

board_config_update

led_wifi="$(lantiq_get_dt_led wifi)"
[ -n "$led_wifi" ] && ucidef_set_led_wlan "wifi" "wifi" "$led_wifi" "phy0tpt"

led_usb="$(lantiq_get_dt_led usb)"
[ -n "$led_usb" ] && ucidef_set_led_usbdev "usb" "usb" "$led_usb" "1-1"

led_usb2="$(lantiq_get_dt_led usb2)"
[ -n "$led_usb2" ] && ucidef_set_led_usbdev "usb2" "usb2" "$led_usb2" "2-1"

led_internet="$(lantiq_get_dt_led internet)"
[ -n "$led_internet" ] && {
	interface="nas0"

	led_dsl="$(lantiq_get_dt_led dsl)"
	[ -n "$led_dsl" ] && {
		interface="pppoe-wan"
		ucidef_set_led_default "dsl" "dsl" "$led_dsl" "0"
	}

	ucidef_set_led_netdev "internet" "internet" "$led_internet" "$interface"
}

board=$(lantiq_board_name)

case "$board" in
ARV4525PW)
	ucidef_set_led_netdev "wifi" "wifi" "arv4525pw:green:wlan" "wlan0"
	;;
ARV7506PW11)
	ucidef_set_led_wlan "wifi" "wifi" "arv7506pw11:green:wlan" "phy0radio"
	;;
ARV7519RW22)
	ucidef_set_led_netdev "lan" "lan" "arv7519rw22:green:lan" "eth0.1"
	;;
BTHOMEHUBV5A)
	ucidef_set_led_default "dimmed" "dimmed" "dimmed" "0"
	;;
FRITZ7320)
	ucidef_set_led_netdev "wifi" "wifi" "fritz7320:green:wlan" "wlan0"
	;;
P2812HNUF*)
	ucidef_set_led_wlan "wifi" "wifi" "p2812hnufx:green:wlan" "phy0radio"
	;;
VGV7510KW22*)
	ucidef_set_led_wlan "wifi" "wifi" "vgv7510kw22:green:wlan" "phy0radio"
	;;
VGV7519*)
	ucidef_set_led_wlan "wifi" "wifi" "vgv7519:green:wireless" "phy0radio"
	;;
WBMR300)
	ucidef_set_led_switch "lan1" "LAN1" "wbmr300:green:lan1" "switch0" "0x08"
	ucidef_set_led_switch "lan2" "LAN2" "wbmr300:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "wan" "WAN" "wbmr300:green:wan" "switch0" "0x10"
	ucidef_set_led_switch "lan3" "LAN3" "wbmr300:green:lan3" "switch0" "0x20"
	ucidef_set_led_default "router" "router" "wbmr300:green:router" "1"
	;;
*)
	;;
esac

board_config_flush

exit 0
