From e2b301610e6201df40deb62942b18c772365eb1c Mon Sep 17 00:00:00 2001
From: Shaohui Xie <Shaohui.Xie@freescale.com>
Date: Thu, 21 Jan 2016 11:29:22 +0800
Subject: [PATCH 13/70] dts: ls1043ardb: add mdio & phy nodes

Signed-off-by: Shaohui Xie <Shaohui.Xie@freescale.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts |   65 +++++++++++++++++++++
 1 file changed, 65 insertions(+)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a-rdb.dts
@@ -115,3 +115,68 @@
 &duart1 {
 	status = "okay";
 };
+
+&fman0 {
+	ethernet@e0000 {
+		phy-handle = <&qsgmii_phy1>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@e2000 {
+		phy-handle = <&qsgmii_phy2>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@e4000 {
+		phy-handle = <&rgmii_phy1>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e6000 {
+		phy-handle = <&rgmii_phy2>;
+		phy-connection-type = "rgmii";
+	};
+
+	ethernet@e8000 {
+		phy-handle = <&qsgmii_phy3>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@ea000 {
+		phy-handle = <&qsgmii_phy4>;
+		phy-connection-type = "qsgmii";
+	};
+
+	ethernet@f0000 { /* 10GEC1 */
+		phy-handle = <&aqr105_phy>;
+		phy-connection-type = "xgmii";
+	};
+
+	mdio@fc000 {
+		rgmii_phy1: ethernet-phy@1 {
+			reg = <0x1>;
+		};
+		rgmii_phy2: ethernet-phy@2 {
+			reg = <0x2>;
+		};
+		qsgmii_phy1: ethernet-phy@3 {
+			reg = <0x4>;
+		};
+		qsgmii_phy2: ethernet-phy@4 {
+			reg = <0x5>;
+		};
+		qsgmii_phy3: ethernet-phy@5 {
+			reg = <0x6>;
+		};
+		qsgmii_phy4: ethernet-phy@6 {
+			reg = <0x7>;
+		};
+	};
+
+	mdio@fd000 {
+		aqr105_phy: ethernet-phy@c {
+			compatible = "ethernet-phy-ieee802.3-c45";
+			reg = <0x1>;
+		};
+	};
+};
