From caddf479c2deacf3d681a84db56ff164d8a5c9f7 Mon Sep 17 00:00:00 2001
From: Madalin Bucur <madalin.bucur@freescale.com>
Date: Wed, 23 Mar 2016 21:25:30 +0200
Subject: [PATCH 25/70] arm64/dts: align to the new clocking model

Signed-off-by: Madalin Bucur <madalin.bucur@freescale.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi |    6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -203,9 +203,9 @@
 			compatible = "fsl,fman", "simple-bus";
 			ranges = <0x0 0x00 0x1a00000 0x100000>;
 			reg = <0x00 0x1a00000 0x0 0x100000>;
-			clock-frequency = <0>;
-			interrupts = <0 44 0x4>,
-				     <0 45 0x4>;
+			interrupts = <0 44 0x4>, <0 45 0x4>;
+			clocks = <&clockgen 3 0>;
+			clock-names = "fmanclk";
 
 			cc {
 				compatible = "fsl,fman-cc";
