From 1892fcf687116720d07135c83d489a23ec56a166 Mon Sep 17 00:00:00 2001
From: James Liao <jamesjj.liao@mediatek.com>
Date: Wed, 30 Dec 2015 14:41:43 +0800
Subject: [PATCH 002/102] soc: mediatek: Separate scpsys driver common code

Separate scpsys driver common code to mtk-scpsys.c, and move MT8173
platform code to mtk-scpsys-mt8173.c.

Signed-off-by: James Liao <jamesjj.liao@mediatek.com>
---
 drivers/soc/mediatek/Kconfig             |   13 +-
 drivers/soc/mediatek/Makefile            |    1 +
 drivers/soc/mediatek/mtk-scpsys-mt8173.c |  179 ++++++++++++++++++
 drivers/soc/mediatek/mtk-scpsys.c        |  301 ++++++++----------------------
 drivers/soc/mediatek/mtk-scpsys.h        |   54 ++++++
 5 files changed, 320 insertions(+), 228 deletions(-)
 create mode 100644 drivers/soc/mediatek/mtk-scpsys-mt8173.c
 create mode 100644 drivers/soc/mediatek/mtk-scpsys.h

--- a/drivers/soc/mediatek/Kconfig
+++ b/drivers/soc/mediatek/Kconfig
@@ -22,11 +22,20 @@ config MTK_PMIC_WRAP
 
 config MTK_SCPSYS
 	bool "MediaTek SCPSYS Support"
-	depends on ARCH_MEDIATEK || COMPILE_TEST
-	default ARM64 && ARCH_MEDIATEK
 	select REGMAP
 	select MTK_INFRACFG
 	select PM_GENERIC_DOMAINS if PM
 	help
 	  Say yes here to add support for the MediaTek SCPSYS power domain
 	  driver.
+
+config MTK_SCPSYS_MT8173
+	bool "MediaTek MT8173 SCPSYS Support"
+	depends on ARCH_MEDIATEK || COMPILE_TEST
+	select MTK_SCPSYS
+	default ARCH_MEDIATEK
+	help
+	  Say yes here to add support for the MT8173 SCPSYS power domain
+	  driver.
+	  The System Control Processor System (SCPSYS) has several power
+	  management related tasks in the system.
--- a/drivers/soc/mediatek/Makefile
+++ b/drivers/soc/mediatek/Makefile
@@ -1,3 +1,4 @@
 obj-$(CONFIG_MTK_INFRACFG) += mtk-infracfg.o
 obj-$(CONFIG_MTK_PMIC_WRAP) += mtk-pmic-wrap.o
 obj-$(CONFIG_MTK_SCPSYS) += mtk-scpsys.o
+obj-$(CONFIG_MTK_SCPSYS_MT8173) += mtk-scpsys-mt8173.o
--- /dev/null
+++ b/drivers/soc/mediatek/mtk-scpsys-mt8173.c
@@ -0,0 +1,179 @@
+/*
+ * Copyright (c) 2015 Pengutronix, Sascha Hauer <kernel@pengutronix.de>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ */
+#include <linux/mfd/syscon.h>
+#include <linux/module.h>
+#include <linux/of_device.h>
+#include <linux/pm_domain.h>
+#include <linux/soc/mediatek/infracfg.h>
+#include <dt-bindings/power/mt8173-power.h>
+
+#include "mtk-scpsys.h"
+
+#define SPM_VDE_PWR_CON			0x0210
+#define SPM_MFG_PWR_CON			0x0214
+#define SPM_VEN_PWR_CON			0x0230
+#define SPM_ISP_PWR_CON			0x0238
+#define SPM_DIS_PWR_CON			0x023c
+#define SPM_VEN2_PWR_CON		0x0298
+#define SPM_AUDIO_PWR_CON		0x029c
+#define SPM_MFG_2D_PWR_CON		0x02c0
+#define SPM_MFG_ASYNC_PWR_CON		0x02c4
+#define SPM_USB_PWR_CON			0x02cc
+
+#define PWR_STATUS_DISP			BIT(3)
+#define PWR_STATUS_MFG			BIT(4)
+#define PWR_STATUS_ISP			BIT(5)
+#define PWR_STATUS_VDEC			BIT(7)
+#define PWR_STATUS_VENC_LT		BIT(20)
+#define PWR_STATUS_VENC			BIT(21)
+#define PWR_STATUS_MFG_2D		BIT(22)
+#define PWR_STATUS_MFG_ASYNC		BIT(23)
+#define PWR_STATUS_AUDIO		BIT(24)
+#define PWR_STATUS_USB			BIT(25)
+
+static const struct scp_domain_data scp_domain_data[] __initconst = {
+	[MT8173_POWER_DOMAIN_VDEC] = {
+		.name = "vdec",
+		.sta_mask = PWR_STATUS_VDEC,
+		.ctl_offs = SPM_VDE_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(12, 12),
+		.clk_id = {CLK_MM},
+	},
+	[MT8173_POWER_DOMAIN_VENC] = {
+		.name = "venc",
+		.sta_mask = PWR_STATUS_VENC,
+		.ctl_offs = SPM_VEN_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(15, 12),
+		.clk_id = {CLK_MM, CLK_VENC},
+	},
+	[MT8173_POWER_DOMAIN_ISP] = {
+		.name = "isp",
+		.sta_mask = PWR_STATUS_ISP,
+		.ctl_offs = SPM_ISP_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(13, 12),
+		.clk_id = {CLK_MM},
+	},
+	[MT8173_POWER_DOMAIN_MM] = {
+		.name = "mm",
+		.sta_mask = PWR_STATUS_DISP,
+		.ctl_offs = SPM_DIS_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(12, 12),
+		.clk_id = {CLK_MM},
+		.bus_prot_mask = MT8173_TOP_AXI_PROT_EN_MM_M0 |
+			MT8173_TOP_AXI_PROT_EN_MM_M1,
+	},
+	[MT8173_POWER_DOMAIN_VENC_LT] = {
+		.name = "venc_lt",
+		.sta_mask = PWR_STATUS_VENC_LT,
+		.ctl_offs = SPM_VEN2_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(15, 12),
+		.clk_id = {CLK_MM, CLK_VENC_LT},
+	},
+	[MT8173_POWER_DOMAIN_AUDIO] = {
+		.name = "audio",
+		.sta_mask = PWR_STATUS_AUDIO,
+		.ctl_offs = SPM_AUDIO_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(15, 12),
+		.clk_id = {CLK_NONE},
+	},
+	[MT8173_POWER_DOMAIN_USB] = {
+		.name = "usb",
+		.sta_mask = PWR_STATUS_USB,
+		.ctl_offs = SPM_USB_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(15, 12),
+		.clk_id = {CLK_NONE},
+		.active_wakeup = true,
+	},
+	[MT8173_POWER_DOMAIN_MFG_ASYNC] = {
+		.name = "mfg_async",
+		.sta_mask = PWR_STATUS_MFG_ASYNC,
+		.ctl_offs = SPM_MFG_ASYNC_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = 0,
+		.clk_id = {CLK_MFG},
+	},
+	[MT8173_POWER_DOMAIN_MFG_2D] = {
+		.name = "mfg_2d",
+		.sta_mask = PWR_STATUS_MFG_2D,
+		.ctl_offs = SPM_MFG_2D_PWR_CON,
+		.sram_pdn_bits = GENMASK(11, 8),
+		.sram_pdn_ack_bits = GENMASK(13, 12),
+		.clk_id = {CLK_NONE},
+	},
+	[MT8173_POWER_DOMAIN_MFG] = {
+		.name = "mfg",
+		.sta_mask = PWR_STATUS_MFG,
+		.ctl_offs = SPM_MFG_PWR_CON,
+		.sram_pdn_bits = GENMASK(13, 8),
+		.sram_pdn_ack_bits = GENMASK(21, 16),
+		.clk_id = {CLK_NONE},
+		.bus_prot_mask = MT8173_TOP_AXI_PROT_EN_MFG_S |
+			MT8173_TOP_AXI_PROT_EN_MFG_M0 |
+			MT8173_TOP_AXI_PROT_EN_MFG_M1 |
+			MT8173_TOP_AXI_PROT_EN_MFG_SNOOP_OUT,
+	},
+};
+
+#define NUM_DOMAINS	ARRAY_SIZE(scp_domain_data)
+
+static int __init scpsys_probe(struct platform_device *pdev)
+{
+	struct scp *scp;
+	struct genpd_onecell_data *pd_data;
+	int ret;
+
+	scp = init_scp(pdev, scp_domain_data, NUM_DOMAINS);
+	if (IS_ERR(scp))
+		return PTR_ERR(scp);
+
+	mtk_register_power_domains(pdev, scp, NUM_DOMAINS);
+
+	pd_data = &scp->pd_data;
+
+	ret = pm_genpd_add_subdomain(pd_data->domains[MT8173_POWER_DOMAIN_MFG_ASYNC],
+		pd_data->domains[MT8173_POWER_DOMAIN_MFG_2D]);
+	if (ret && IS_ENABLED(CONFIG_PM))
+		dev_err(&pdev->dev, "Failed to add subdomain: %d\n", ret);
+
+	ret = pm_genpd_add_subdomain(pd_data->domains[MT8173_POWER_DOMAIN_MFG_2D],
+		pd_data->domains[MT8173_POWER_DOMAIN_MFG]);
+	if (ret && IS_ENABLED(CONFIG_PM))
+		dev_err(&pdev->dev, "Failed to add subdomain: %d\n", ret);
+
+	return 0;
+}
+
+static const struct of_device_id of_scpsys_match_tbl[] = {
+	{
+		.compatible = "mediatek,mt8173-scpsys",
+	}, {
+		/* sentinel */
+	}
+};
+
+static struct platform_driver scpsys_drv = {
+	.driver = {
+		.name = "mtk-scpsys-mt8173",
+		.owner = THIS_MODULE,
+		.of_match_table = of_match_ptr(of_scpsys_match_tbl),
+	},
+};
+
+module_platform_driver_probe(scpsys_drv, scpsys_probe);
--- a/drivers/soc/mediatek/mtk-scpsys.c
+++ b/drivers/soc/mediatek/mtk-scpsys.c
@@ -11,28 +11,14 @@
  * GNU General Public License for more details.
  */
 #include <linux/clk.h>
-#include <linux/delay.h>
 #include <linux/io.h>
-#include <linux/kernel.h>
 #include <linux/mfd/syscon.h>
-#include <linux/module.h>
-#include <linux/of_device.h>
 #include <linux/platform_device.h>
 #include <linux/pm_domain.h>
-#include <linux/regmap.h>
 #include <linux/soc/mediatek/infracfg.h>
-#include <dt-bindings/power/mt8173-power.h>
 
-#define SPM_VDE_PWR_CON			0x0210
-#define SPM_MFG_PWR_CON			0x0214
-#define SPM_VEN_PWR_CON			0x0230
-#define SPM_ISP_PWR_CON			0x0238
-#define SPM_DIS_PWR_CON			0x023c
-#define SPM_VEN2_PWR_CON		0x0298
-#define SPM_AUDIO_PWR_CON		0x029c
-#define SPM_MFG_2D_PWR_CON		0x02c0
-#define SPM_MFG_ASYNC_PWR_CON		0x02c4
-#define SPM_USB_PWR_CON			0x02cc
+#include "mtk-scpsys.h"
+
 #define SPM_PWR_STATUS			0x060c
 #define SPM_PWR_STATUS_2ND		0x0610
 
@@ -42,153 +28,6 @@
 #define PWR_ON_2ND_BIT			BIT(3)
 #define PWR_CLK_DIS_BIT			BIT(4)
 
-#define PWR_STATUS_DISP			BIT(3)
-#define PWR_STATUS_MFG			BIT(4)
-#define PWR_STATUS_ISP			BIT(5)
-#define PWR_STATUS_VDEC			BIT(7)
-#define PWR_STATUS_VENC_LT		BIT(20)
-#define PWR_STATUS_VENC			BIT(21)
-#define PWR_STATUS_MFG_2D		BIT(22)
-#define PWR_STATUS_MFG_ASYNC		BIT(23)
-#define PWR_STATUS_AUDIO		BIT(24)
-#define PWR_STATUS_USB			BIT(25)
-
-enum clk_id {
-	MT8173_CLK_NONE,
-	MT8173_CLK_MM,
-	MT8173_CLK_MFG,
-	MT8173_CLK_VENC,
-	MT8173_CLK_VENC_LT,
-	MT8173_CLK_MAX,
-};
-
-#define MAX_CLKS	2
-
-struct scp_domain_data {
-	const char *name;
-	u32 sta_mask;
-	int ctl_offs;
-	u32 sram_pdn_bits;
-	u32 sram_pdn_ack_bits;
-	u32 bus_prot_mask;
-	enum clk_id clk_id[MAX_CLKS];
-	bool active_wakeup;
-};
-
-static const struct scp_domain_data scp_domain_data[] __initconst = {
-	[MT8173_POWER_DOMAIN_VDEC] = {
-		.name = "vdec",
-		.sta_mask = PWR_STATUS_VDEC,
-		.ctl_offs = SPM_VDE_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(12, 12),
-		.clk_id = {MT8173_CLK_MM},
-	},
-	[MT8173_POWER_DOMAIN_VENC] = {
-		.name = "venc",
-		.sta_mask = PWR_STATUS_VENC,
-		.ctl_offs = SPM_VEN_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(15, 12),
-		.clk_id = {MT8173_CLK_MM, MT8173_CLK_VENC},
-	},
-	[MT8173_POWER_DOMAIN_ISP] = {
-		.name = "isp",
-		.sta_mask = PWR_STATUS_ISP,
-		.ctl_offs = SPM_ISP_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(13, 12),
-		.clk_id = {MT8173_CLK_MM},
-	},
-	[MT8173_POWER_DOMAIN_MM] = {
-		.name = "mm",
-		.sta_mask = PWR_STATUS_DISP,
-		.ctl_offs = SPM_DIS_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(12, 12),
-		.clk_id = {MT8173_CLK_MM},
-		.bus_prot_mask = MT8173_TOP_AXI_PROT_EN_MM_M0 |
-			MT8173_TOP_AXI_PROT_EN_MM_M1,
-	},
-	[MT8173_POWER_DOMAIN_VENC_LT] = {
-		.name = "venc_lt",
-		.sta_mask = PWR_STATUS_VENC_LT,
-		.ctl_offs = SPM_VEN2_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(15, 12),
-		.clk_id = {MT8173_CLK_MM, MT8173_CLK_VENC_LT},
-	},
-	[MT8173_POWER_DOMAIN_AUDIO] = {
-		.name = "audio",
-		.sta_mask = PWR_STATUS_AUDIO,
-		.ctl_offs = SPM_AUDIO_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(15, 12),
-		.clk_id = {MT8173_CLK_NONE},
-	},
-	[MT8173_POWER_DOMAIN_USB] = {
-		.name = "usb",
-		.sta_mask = PWR_STATUS_USB,
-		.ctl_offs = SPM_USB_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(15, 12),
-		.clk_id = {MT8173_CLK_NONE},
-		.active_wakeup = true,
-	},
-	[MT8173_POWER_DOMAIN_MFG_ASYNC] = {
-		.name = "mfg_async",
-		.sta_mask = PWR_STATUS_MFG_ASYNC,
-		.ctl_offs = SPM_MFG_ASYNC_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = 0,
-		.clk_id = {MT8173_CLK_MFG},
-	},
-	[MT8173_POWER_DOMAIN_MFG_2D] = {
-		.name = "mfg_2d",
-		.sta_mask = PWR_STATUS_MFG_2D,
-		.ctl_offs = SPM_MFG_2D_PWR_CON,
-		.sram_pdn_bits = GENMASK(11, 8),
-		.sram_pdn_ack_bits = GENMASK(13, 12),
-		.clk_id = {MT8173_CLK_NONE},
-	},
-	[MT8173_POWER_DOMAIN_MFG] = {
-		.name = "mfg",
-		.sta_mask = PWR_STATUS_MFG,
-		.ctl_offs = SPM_MFG_PWR_CON,
-		.sram_pdn_bits = GENMASK(13, 8),
-		.sram_pdn_ack_bits = GENMASK(21, 16),
-		.clk_id = {MT8173_CLK_NONE},
-		.bus_prot_mask = MT8173_TOP_AXI_PROT_EN_MFG_S |
-			MT8173_TOP_AXI_PROT_EN_MFG_M0 |
-			MT8173_TOP_AXI_PROT_EN_MFG_M1 |
-			MT8173_TOP_AXI_PROT_EN_MFG_SNOOP_OUT,
-	},
-};
-
-#define NUM_DOMAINS	ARRAY_SIZE(scp_domain_data)
-
-struct scp;
-
-struct scp_domain {
-	struct generic_pm_domain genpd;
-	struct scp *scp;
-	struct clk *clk[MAX_CLKS];
-	u32 sta_mask;
-	void __iomem *ctl_addr;
-	u32 sram_pdn_bits;
-	u32 sram_pdn_ack_bits;
-	u32 bus_prot_mask;
-	bool active_wakeup;
-};
-
-struct scp {
-	struct scp_domain domains[NUM_DOMAINS];
-	struct genpd_onecell_data pd_data;
-	struct device *dev;
-	void __iomem *base;
-	struct regmap *infracfg;
-};
-
 static int scpsys_domain_is_on(struct scp_domain *scpd)
 {
 	struct scp *scp = scpd->scp;
@@ -398,63 +237,89 @@ static bool scpsys_active_wakeup(struct
 	return scpd->active_wakeup;
 }
 
-static int __init scpsys_probe(struct platform_device *pdev)
+static void init_clks(struct platform_device *pdev, struct clk *clk[CLK_MAX])
+{
+	enum clk_id clk_ids[] = {
+		CLK_MM,
+		CLK_MFG,
+		CLK_VENC,
+		CLK_VENC_LT
+	};
+
+	static const char * const clk_names[] = {
+		"mm",
+		"mfg",
+		"venc",
+		"venc_lt",
+	};
+
+	int i;
+
+	for (i = 0; i < ARRAY_SIZE(clk_ids); i++)
+		clk[clk_ids[i]] = devm_clk_get(&pdev->dev, clk_names[i]);
+}
+
+struct scp *init_scp(struct platform_device *pdev,
+			const struct scp_domain_data *scp_domain_data, int num)
 {
 	struct genpd_onecell_data *pd_data;
 	struct resource *res;
-	int i, j, ret;
+	int i, j;
 	struct scp *scp;
-	struct clk *clk[MT8173_CLK_MAX];
+	struct clk *clk[CLK_MAX];
 
 	scp = devm_kzalloc(&pdev->dev, sizeof(*scp), GFP_KERNEL);
 	if (!scp)
-		return -ENOMEM;
+		return ERR_PTR(-ENOMEM);
 
 	scp->dev = &pdev->dev;
 
 	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
 	scp->base = devm_ioremap_resource(&pdev->dev, res);
 	if (IS_ERR(scp->base))
-		return PTR_ERR(scp->base);
-
-	pd_data = &scp->pd_data;
-
-	pd_data->domains = devm_kzalloc(&pdev->dev,
-			sizeof(*pd_data->domains) * NUM_DOMAINS, GFP_KERNEL);
-	if (!pd_data->domains)
-		return -ENOMEM;
-
-	clk[MT8173_CLK_MM] = devm_clk_get(&pdev->dev, "mm");
-	if (IS_ERR(clk[MT8173_CLK_MM]))
-		return PTR_ERR(clk[MT8173_CLK_MM]);
-
-	clk[MT8173_CLK_MFG] = devm_clk_get(&pdev->dev, "mfg");
-	if (IS_ERR(clk[MT8173_CLK_MFG]))
-		return PTR_ERR(clk[MT8173_CLK_MFG]);
-
-	clk[MT8173_CLK_VENC] = devm_clk_get(&pdev->dev, "venc");
-	if (IS_ERR(clk[MT8173_CLK_VENC]))
-		return PTR_ERR(clk[MT8173_CLK_VENC]);
-
-	clk[MT8173_CLK_VENC_LT] = devm_clk_get(&pdev->dev, "venc_lt");
-	if (IS_ERR(clk[MT8173_CLK_VENC_LT]))
-		return PTR_ERR(clk[MT8173_CLK_VENC_LT]);
+		return ERR_CAST(scp->base);
 
 	scp->infracfg = syscon_regmap_lookup_by_phandle(pdev->dev.of_node,
 			"infracfg");
 	if (IS_ERR(scp->infracfg)) {
 		dev_err(&pdev->dev, "Cannot find infracfg controller: %ld\n",
 				PTR_ERR(scp->infracfg));
-		return PTR_ERR(scp->infracfg);
+		return ERR_CAST(scp->infracfg);
 	}
 
-	pd_data->num_domains = NUM_DOMAINS;
+	scp->domains = devm_kzalloc(&pdev->dev,
+				sizeof(*scp->domains) * num, GFP_KERNEL);
+	if (!scp->domains)
+		return ERR_PTR(-ENOMEM);
+
+	pd_data = &scp->pd_data;
 
-	for (i = 0; i < NUM_DOMAINS; i++) {
+	pd_data->domains = devm_kzalloc(&pdev->dev,
+			sizeof(*pd_data->domains) * num, GFP_KERNEL);
+	if (!pd_data->domains)
+		return ERR_PTR(-ENOMEM);
+
+	pd_data->num_domains = num;
+
+	init_clks(pdev, clk);
+
+	for (i = 0; i < num; i++) {
 		struct scp_domain *scpd = &scp->domains[i];
 		struct generic_pm_domain *genpd = &scpd->genpd;
 		const struct scp_domain_data *data = &scp_domain_data[i];
 
+		for (j = 0; j < MAX_CLKS && data->clk_id[j]; j++) {
+			struct clk *c = clk[data->clk_id[j]];
+
+			if (IS_ERR(c)) {
+				dev_err(&pdev->dev, "%s: clk unavailable\n",
+					data->name);
+				return ERR_CAST(c);
+			}
+
+			scpd->clk[j] = c;
+		}
+
 		pd_data->domains[i] = genpd;
 		scpd->scp = scp;
 
@@ -464,13 +329,25 @@ static int __init scpsys_probe(struct pl
 		scpd->sram_pdn_ack_bits = data->sram_pdn_ack_bits;
 		scpd->bus_prot_mask = data->bus_prot_mask;
 		scpd->active_wakeup = data->active_wakeup;
-		for (j = 0; j < MAX_CLKS && data->clk_id[j]; j++)
-			scpd->clk[j] = clk[data->clk_id[j]];
 
 		genpd->name = data->name;
 		genpd->power_off = scpsys_power_off;
 		genpd->power_on = scpsys_power_on;
 		genpd->dev_ops.active_wakeup = scpsys_active_wakeup;
+	}
+
+	return scp;
+}
+
+void mtk_register_power_domains(struct platform_device *pdev,
+				struct scp *scp, int num)
+{
+	struct genpd_onecell_data *pd_data;
+	int i, ret;
+
+	for (i = 0; i < num; i++) {
+		struct scp_domain *scpd = &scp->domains[i];
+		struct generic_pm_domain *genpd = &scpd->genpd;
 
 		/*
 		 * Initially turn on all domains to make the domains usable
@@ -489,37 +366,9 @@ static int __init scpsys_probe(struct pl
 	 * valid.
 	 */
 
-	ret = pm_genpd_add_subdomain(pd_data->domains[MT8173_POWER_DOMAIN_MFG_ASYNC],
-		pd_data->domains[MT8173_POWER_DOMAIN_MFG_2D]);
-	if (ret && IS_ENABLED(CONFIG_PM))
-		dev_err(&pdev->dev, "Failed to add subdomain: %d\n", ret);
-
-	ret = pm_genpd_add_subdomain(pd_data->domains[MT8173_POWER_DOMAIN_MFG_2D],
-		pd_data->domains[MT8173_POWER_DOMAIN_MFG]);
-	if (ret && IS_ENABLED(CONFIG_PM))
-		dev_err(&pdev->dev, "Failed to add subdomain: %d\n", ret);
+	pd_data = &scp->pd_data;
 
 	ret = of_genpd_add_provider_onecell(pdev->dev.of_node, pd_data);
 	if (ret)
 		dev_err(&pdev->dev, "Failed to add OF provider: %d\n", ret);
-
-	return 0;
 }
-
-static const struct of_device_id of_scpsys_match_tbl[] = {
-	{
-		.compatible = "mediatek,mt8173-scpsys",
-	}, {
-		/* sentinel */
-	}
-};
-
-static struct platform_driver scpsys_drv = {
-	.driver = {
-		.name = "mtk-scpsys",
-		.owner = THIS_MODULE,
-		.of_match_table = of_match_ptr(of_scpsys_match_tbl),
-	},
-};
-
-module_platform_driver_probe(scpsys_drv, scpsys_probe);
--- /dev/null
+++ b/drivers/soc/mediatek/mtk-scpsys.h
@@ -0,0 +1,54 @@
+#ifndef __DRV_SOC_MTK_H
+#define __DRV_SOC_MTK_H
+
+enum clk_id {
+	CLK_NONE,
+	CLK_MM,
+	CLK_MFG,
+	CLK_VENC,
+	CLK_VENC_LT,
+	CLK_MAX,
+};
+
+#define MAX_CLKS	2
+
+struct scp_domain_data {
+	const char *name;
+	u32 sta_mask;
+	int ctl_offs;
+	u32 sram_pdn_bits;
+	u32 sram_pdn_ack_bits;
+	u32 bus_prot_mask;
+	enum clk_id clk_id[MAX_CLKS];
+	bool active_wakeup;
+};
+
+struct scp;
+
+struct scp_domain {
+	struct generic_pm_domain genpd;
+	struct scp *scp;
+	struct clk *clk[MAX_CLKS];
+	u32 sta_mask;
+	void __iomem *ctl_addr;
+	u32 sram_pdn_bits;
+	u32 sram_pdn_ack_bits;
+	u32 bus_prot_mask;
+	bool active_wakeup;
+};
+
+struct scp {
+	struct scp_domain *domains;
+	struct genpd_onecell_data pd_data;
+	struct device *dev;
+	void __iomem *base;
+	struct regmap *infracfg;
+};
+
+struct scp *init_scp(struct platform_device *pdev,
+			const struct scp_domain_data *scp_domain_data, int num);
+
+void mtk_register_power_domains(struct platform_device *pdev,
+				struct scp *scp, int num);
+
+#endif /* __DRV_SOC_MTK_H */
