From 883112e5caaefcb620248e9f63426e82349033e0 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Fri, 8 Jul 2016 11:25:09 -0700
Subject: [PATCH] drm/vc4: Bind the HVS before we bind the individual CRTCs.

We need to be able to look at the CRTC's registers in the HVS as part
of initialization, while the HVS doesn't need to look at the PV
registers.

Signed-off-by: Eric Anholt <eric@anholt.net>
Reviewed-and-tested-by: Mario Kleiner <mario.kleiner.de@gmail.com>
(cherry picked from commit 7a100969f30b77761901c05a5c810bcaea65df44)
---
 drivers/gpu/drm/vc4/vc4_drv.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/gpu/drm/vc4/vc4_drv.c
+++ b/drivers/gpu/drm/vc4/vc4_drv.c
@@ -295,8 +295,8 @@ static struct platform_driver *const com
 	&vc4_hdmi_driver,
 	&vc4_dpi_driver,
 	&vc4_dsi_driver,
-	&vc4_crtc_driver,
 	&vc4_hvs_driver,
+	&vc4_crtc_driver,
 	&vc4_v3d_driver,
 };
 
