#!/bin/sh

. /lib/functions/system.sh
. /lib/functions/uci-defaults.sh
. /lib/apm821xx.sh

board_config_update

board=$(apm821xx_board_name)

case "$board" in
mbl|\
mr24)
	ucidef_set_interface_lan "eth0"
	;;

mx60|\
wndr4700)
	ucidef_add_switch "switch0" \
		"0@eth0" "4:lan" "3:lan" "2:lan" "1:lan" "5:wan"
	;;

*)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
esac

board_config_flush

exit 0
