From 09f0b50ae838bd6e2bbf0aa22de9f352122297de Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Fri, 22 Apr 2016 11:06:03 +0200
Subject: [PATCH 079/102] net-next: mediatek: add fixed-phy support

The MT7623 SoC has a builtin gigabit switch. If we want to use it, GMAC1
needs to be configured using a fixed link speed and flow control settings.
The easiest way to do this is to used the fixed-phy driver, allowing us to
reuse the existing mdio polling code to setup the MAC.

Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c |    6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -229,6 +229,9 @@ static int mtk_phy_connect(struct mtk_ma
 	u32 val, ge_mode;
 
 	np = of_parse_phandle(mac->of_node, "phy-handle", 0);
+	if (!np && of_phy_is_fixed_link(mac->of_node))
+		if (!of_phy_register_fixed_link(mac->of_node))
+			np = of_node_get(mac->of_node);
 	if (!np)
 		return -ENODEV;
 
@@ -257,6 +260,9 @@ static int mtk_phy_connect(struct mtk_ma
 	mac->phy_dev->autoneg = AUTONEG_ENABLE;
 	mac->phy_dev->speed = 0;
 	mac->phy_dev->duplex = 0;
+	if (of_phy_is_fixed_link(mac->of_node))
+		mac->phy_dev->supported |= SUPPORTED_Pause |
+					   SUPPORTED_Asym_Pause;
 	mac->phy_dev->supported &= PHY_GBIT_FEATURES | SUPPORTED_Pause |
 				   SUPPORTED_Asym_Pause;
 	mac->phy_dev->advertising = mac->phy_dev->supported |
