From f7792176d939e79b4f525114a95d0fd8266bef8e Mon Sep 17 00:00:00 2001
From: Madalin Bucur <madalin.bucur@freescale.com>
Date: Wed, 19 Nov 2014 13:06:54 +0200
Subject: [PATCH 18/70] devres: add devm_alloc_percpu()

Introduce managed counterparts for alloc_percpu() and free_percpu().
Add devm_alloc_percpu() and devm_free_percpu() into the managed
interfaces list.

Signed-off-by: Madalin Bucur <madalin.bucur@freescale.com>

Change-Id: I93546348e7b0e1974fda8b6c7a3b3710ce45b724
Reviewed-on: http://git.am.freescale.net:8181/24140
Reviewed-by: Madalin-Cristian Bucur <madalin.bucur@freescale.com>
Tested-by: Madalin-Cristian Bucur <madalin.bucur@freescale.com>

Conflicts:
	Documentation/driver-model/devres.txt
	drivers/base/devres.c

Conflicts:
	drivers/base/devres.c
---
 Documentation/driver-model/devres.txt |    4 +++
 drivers/base/devres.c                 |   63 +++++++++++++++++++++++++++++++++
 include/linux/device.h                |   19 ++++++++++
 3 files changed, 86 insertions(+)

--- a/Documentation/driver-model/devres.txt
+++ b/Documentation/driver-model/devres.txt
@@ -321,6 +321,10 @@ PHY
   devm_usb_get_phy()
   devm_usb_put_phy()
 
+PER-CPU MEM
+  devm_alloc_percpu()
+  devm_free_percpu()
+
 PINCTRL
   devm_pinctrl_get()
   devm_pinctrl_put()
--- a/drivers/base/devres.c
+++ b/drivers/base/devres.c
@@ -985,3 +985,66 @@ void devm_free_pages(struct device *dev,
 			       &devres));
 }
 EXPORT_SYMBOL_GPL(devm_free_pages);
+
+static void devm_percpu_release(struct device *dev, void *pdata)
+{
+	void __percpu *p;
+
+	p = *(void __percpu **)pdata;
+	free_percpu(p);
+}
+
+static int devm_percpu_match(struct device *dev, void *data, void *p)
+{
+	struct devres *devr = container_of(data, struct devres, data);
+
+	return *(void **)devr->data == p;
+}
+
+/**
+ * __devm_alloc_percpu - Resource-managed alloc_percpu
+ * @dev: Device to allocate per-cpu memory for
+ * @size: Size of per-cpu memory to allocate
+ * @align: Alignement of per-cpu memory to allocate
+ *
+ * Managed alloc_percpu. Per-cpu memory allocated with this function is
+ * automatically freed on driver detach.
+ *
+ * RETURNS:
+ * Pointer to allocated memory on success, NULL on failure.
+ */
+void __percpu *__devm_alloc_percpu(struct device *dev, size_t size,
+		size_t align)
+{
+	void *p;
+	void __percpu *pcpu;
+
+	pcpu = __alloc_percpu(size, align);
+	if (!pcpu)
+		return NULL;
+
+	p = devres_alloc(devm_percpu_release, sizeof(void *), GFP_KERNEL);
+	if (!p)
+		return NULL;
+
+	*(void __percpu **)p = pcpu;
+
+	devres_add(dev, p);
+
+	return pcpu;
+}
+EXPORT_SYMBOL_GPL(__devm_alloc_percpu);
+
+/**
+ * devm_free_percpu - Resource-managed free_percpu
+ * @dev: Device this memory belongs to
+ * @pdata: Per-cpu memory to free
+ *
+ * Free memory allocated with devm_alloc_percpu().
+ */
+void devm_free_percpu(struct device *dev, void __percpu *pdata)
+{
+	WARN_ON(devres_destroy(dev, devm_percpu_release, devm_percpu_match,
+			       (void *)pdata));
+}
+EXPORT_SYMBOL_GPL(devm_free_percpu);
--- a/include/linux/device.h
+++ b/include/linux/device.h
@@ -681,6 +681,25 @@ void __iomem *devm_ioremap_resource(stru
 int devm_add_action(struct device *dev, void (*action)(void *), void *data);
 void devm_remove_action(struct device *dev, void (*action)(void *), void *data);
 
+/**
+ * devm_alloc_percpu - Resource-managed alloc_percpu
+ * @dev: Device to allocate per-cpu memory for
+ * @type: Type to allocate per-cpu memory for
+ *
+ * Managed alloc_percpu. Per-cpu memory allocated with this function is
+ * automatically freed on driver detach.
+ *
+ * RETURNS:
+ * Pointer to allocated memory on success, NULL on failure.
+ */
+#define devm_alloc_percpu(dev, type)      \
+	(typeof(type) __percpu *)__devm_alloc_percpu(dev, sizeof(type), \
+						     __alignof__(type))
+
+void __percpu *__devm_alloc_percpu(struct device *dev, size_t size,
+				   size_t align);
+void devm_free_percpu(struct device *dev, void __percpu *pdata);
+
 struct device_dma_parameters {
 	/*
 	 * a low level driver may set these to teach IOMMU code about
