From 2022e9d50798aa592887ccb5a7d045e537f3855f Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Tue, 7 Jun 2016 15:06:13 -0700
Subject: [PATCH 1/3] bgmac: Bind net_device with backing device structure

In preparation for allowing different helpers to be utilized against
network devices created by the bgmac driver, make sure that we bind the
net_device with core->dev.

Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/bgmac.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -1602,6 +1602,7 @@ static int bgmac_probe(struct bcma_devic
 	bgmac->net_dev = net_dev;
 	bgmac->core = core;
 	bcma_set_drvdata(core, bgmac);
+	SET_NETDEV_DEV(net_dev, &core->dev);
 
 	/* Defaults */
 	memcpy(bgmac->net_dev->dev_addr, mac, ETH_ALEN);
