Adding registration for 3G modem DWM-158 in usb-serial-option

Signed-off-by: Giuseppe Lippolis <giu.lippolis@gmail.com>

--- a/drivers/usb/serial/option.c
+++ b/drivers/usb/serial/option.c
@@ -1989,6 +1989,7 @@ static const struct usb_device_id option
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x7d02, 0xff, 0x00, 0x00) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x7d03, 0xff, 0x02, 0x01) },
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x7d03, 0xff, 0x00, 0x00) },
+	{ USB_DEVICE_INTERFACE_CLASS(0x2001, 0x7d04, 0xff) },			/* D-Link DWM-158 */
 	{ USB_DEVICE_INTERFACE_CLASS(0x2001, 0x7e19, 0xff),			/* D-Link DWM-221 B1 */
 	  .driver_info = (kernel_ulong_t)&net_intf4_blacklist },
 	{ USB_DEVICE_AND_INTERFACE_INFO(0x07d1, 0x3e01, 0xff, 0xff, 0xff) }, /* D-Link DWM-152/C1 */
