From 73bff3c4c33a2bfbddc593fad53c6c58af93bfab Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Mon, 6 May 2013 11:03:41 -0300
Subject: [PATCH] ARM: sunxi: add PLL4 support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This commit adds the PLL4 definition to the sun4i, sun5i and sun7i
device trees. PLL4 is compatible with PLL1.

Signed-off-by: Emilio López <emilio@elopez.com.ar>
---
 arch/arm/boot/dts/sun4i-a10.dtsi  | 7 +++++++
 arch/arm/boot/dts/sun5i-a10s.dtsi | 7 +++++++
 arch/arm/boot/dts/sun5i-a13.dtsi  | 7 +++++++
 arch/arm/boot/dts/sun7i-a20.dtsi  | 7 +++++++
 4 files changed, 28 insertions(+)

diff --git a/arch/arm/boot/dts/sun4i-a10.dtsi b/arch/arm/boot/dts/sun4i-a10.dtsi
index 319cc6b..a6c1cae 100644
--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -66,6 +66,13 @@
 			clocks = <&osc24M>;
 		};
 
+		pll4: pll4@01c20018 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-pll1-clk";
+			reg = <0x01c20018 0x4>;
+			clocks = <&osc24M>;
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
diff --git a/arch/arm/boot/dts/sun5i-a10s.dtsi b/arch/arm/boot/dts/sun5i-a10s.dtsi
index 5247674..c3f4eed 100644
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -63,6 +63,13 @@
 			clocks = <&osc24M>;
 		};
 
+		pll4: pll4@01c20018 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-pll1-clk";
+			reg = <0x01c20018 0x4>;
+			clocks = <&osc24M>;
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index ce8ef2a..8c4a9c3 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -67,6 +67,13 @@
 			clocks = <&osc24M>;
 		};
 
+		pll4: pll4@01c20018 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-pll1-clk";
+			reg = <0x01c20018 0x4>;
+			clocks = <&osc24M>;
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index 282c775..21bf143 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -62,6 +62,13 @@
 			clocks = <&osc24M>;
 		};
 
+		pll4: pll4@01c20018 {
+			#clock-cells = <0>;
+			compatible = "allwinner,sun4i-pll1-clk";
+			reg = <0x01c20018 0x4>;
+			clocks = <&osc24M>;
+		};
+
 		/*
 		 * This is a dummy clock, to be used as placeholder on
 		 * other mux clocks when a specific parent clock is not
-- 
1.8.4

