From 5ace5467690055b1772dcac69dd1377735b8a34b Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 7 Nov 2013 12:01:48 +0100
Subject: [PATCH] ARM: sun5i: a10s: Add support for the High Speed Timers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The Allwinner A10s has support for two high speed timers. Now that we
have a driver to support it, we can enable them in the device tree.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Tested-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Daniel Lezcano <daniel.lezcano@linaro.org>
---
 arch/arm/boot/dts/sun5i-a10s.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a10s.dtsi b/arch/arm/boot/dts/sun5i-a10s.dtsi
index b4764be..924a2c1 100644
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -336,5 +336,12 @@
 			clock-frequency = <100000>;
 			status = "disabled";
 		};
+
+		timer@01c60000 {
+			compatible = "allwinner,sun5i-a13-hstimer";
+			reg = <0x01c60000 0x1000>;
+			interrupts = <82>, <83>;
+			clocks = <&ahb_gates 28>;
+		};
 	};
 };
-- 
1.8.5.1

