--- a/hostapd/Makefile
+++ b/hostapd/Makefile
@@ -105,6 +105,11 @@ OBJS += ../src/common/wpa_common.o
 
 OBJS += ../src/eapol_auth/eapol_auth_sm.o
 
+ifdef CONFIG_UBUS
+CFLAGS += -DUBUS_SUPPORT
+OBJS += ../src/ap/ubus.o
+LIBS += -lubox -lubus
+endif
 
 ifndef CONFIG_NO_DUMP_STATE
 # define HOSTAPD_DUMP_STATE to include SIGUSR1 handler for dumping state to
--- a/src/ap/hostapd.h
+++ b/src/ap/hostapd.h
@@ -11,6 +11,7 @@
 
 #include "common/defs.h"
 #include "ap_config.h"
+#include "ubus.h"
 
 struct wpa_driver_ops;
 struct wpa_ctrl_dst;
@@ -105,6 +106,7 @@ struct hostapd_data {
 	struct hostapd_iface *iface;
 	struct hostapd_config *iconf;
 	struct hostapd_bss_config *conf;
+	struct hostapd_ubus_bss ubus;
 	int interface_added; /* virtual interface added for this BSS */
 	unsigned int started:1;
 
@@ -256,6 +258,8 @@ struct hostapd_iface {
 	struct hostapd_config *conf;
 	char phy[16]; /* Name of the PHY (radio) */
 
+	struct hostapd_ubus_iface ubus;
+
 	enum hostapd_iface_state {
 		HAPD_IFACE_UNINITIALIZED,
 		HAPD_IFACE_DISABLED,
--- /dev/null
+++ b/src/ap/ubus.c
@@ -0,0 +1,373 @@
+/*
+ * hostapd / ubus support
+ * Copyright (c) 2013, Felix Fietkau <nbd@openwrt.org>
+ *
+ * This software may be distributed under the terms of the BSD license.
+ * See README for more details.
+ */
+
+#include "utils/includes.h"
+#include "utils/common.h"
+#include "utils/eloop.h"
+#include "common/ieee802_11_defs.h"
+#include "hostapd.h"
+#include "sta_info.h"
+#include "ubus.h"
+
+static struct ubus_context *ctx;
+static struct blob_buf b;
+static int ctx_ref;
+
+struct ubus_banned_client {
+	struct avl_node avl;
+	u8 addr[ETH_ALEN];
+};
+
+static void ubus_receive(int sock, void *eloop_ctx, void *sock_ctx)
+{
+	struct ubus_context *ctx = eloop_ctx;
+	ubus_handle_event(ctx);
+}
+
+static void ubus_reconnect_timeout(void *eloop_data, void *user_ctx)
+{
+	if (ubus_reconnect(ctx, NULL)) {
+		eloop_register_timeout(1, 0, ubus_reconnect_timeout, ctx, NULL);
+		return;
+	}
+
+	eloop_register_read_sock(ctx->sock.fd, ubus_receive, ctx, NULL);
+}
+
+static void hostapd_ubus_connection_lost(struct ubus_context *ctx)
+{
+	eloop_unregister_read_sock(ctx->sock.fd);
+	eloop_register_timeout(1, 0, ubus_reconnect_timeout, ctx, NULL);
+}
+
+static bool hostapd_ubus_init(void)
+{
+	if (ctx)
+		return true;
+
+	ctx = ubus_connect(NULL);
+	if (!ctx)
+		return false;
+
+	ctx->connection_lost = hostapd_ubus_connection_lost;
+	eloop_register_read_sock(ctx->sock.fd, ubus_receive, ctx, NULL);
+	return true;
+}
+
+static void hostapd_ubus_ref_inc(void)
+{
+	ctx_ref++;
+}
+
+static void hostapd_ubus_ref_dec(void)
+{
+	ctx_ref--;
+	if (!ctx)
+		return;
+
+	if (ctx_ref)
+		return;
+
+	eloop_unregister_read_sock(ctx->sock.fd);
+	ubus_free(ctx);
+	ctx = NULL;
+}
+
+void hostapd_ubus_add_iface(struct hostapd_iface *iface)
+{
+	if (!hostapd_ubus_init())
+		return;
+}
+
+void hostapd_ubus_free_iface(struct hostapd_iface *iface)
+{
+	if (!ctx)
+		return;
+}
+
+static void
+hostapd_bss_del_ban(void *eloop_data, void *user_ctx)
+{
+	struct ubus_banned_client *ban = eloop_data;
+	struct hostapd_data *hapd = user_ctx;
+
+	avl_delete(&hapd->ubus.banned, &ban->avl);
+	free(ban);
+}
+
+static void
+hostapd_bss_ban_client(struct hostapd_data *hapd, u8 *addr, int time)
+{
+	struct ubus_banned_client *ban;
+
+	if (time < 0)
+		time = 0;
+
+	ban = avl_find_element(&hapd->ubus.banned, addr, ban, avl);
+	if (!ban) {
+		if (!time)
+			return;
+
+		ban = os_zalloc(sizeof(*ban));
+		memcpy(ban->addr, addr, sizeof(ban->addr));
+		ban->avl.key = ban->addr;
+		avl_insert(&hapd->ubus.banned, &ban->avl);
+	} else {
+		eloop_cancel_timeout(hostapd_bss_del_ban, ban, hapd);
+		if (!time) {
+			hostapd_bss_del_ban(ban, hapd);
+			return;
+		}
+	}
+
+	eloop_register_timeout(0, time * 1000, hostapd_bss_del_ban, ban, hapd);
+}
+
+static int
+hostapd_bss_get_clients(struct ubus_context *ctx, struct ubus_object *obj,
+			struct ubus_request_data *req, const char *method,
+			struct blob_attr *msg)
+{
+	struct hostapd_data *hapd = container_of(obj, struct hostapd_data, ubus.obj);
+	struct sta_info *sta;
+	void *list, *c;
+	char mac_buf[20];
+	static const struct {
+		const char *name;
+		uint32_t flag;
+	} sta_flags[] = {
+		{ "auth", WLAN_STA_AUTH },
+		{ "assoc", WLAN_STA_ASSOC },
+		{ "authorized", WLAN_STA_AUTHORIZED },
+		{ "preauth", WLAN_STA_PREAUTH },
+		{ "wds", WLAN_STA_WDS },
+		{ "wmm", WLAN_STA_WMM },
+		{ "ht", WLAN_STA_HT },
+		{ "vht", WLAN_STA_VHT },
+		{ "wps", WLAN_STA_WPS },
+		{ "mfp", WLAN_STA_MFP },
+	};
+
+	blob_buf_init(&b, 0);
+	blobmsg_add_u32(&b, "freq", hapd->iface->freq);
+	list = blobmsg_open_table(&b, "clients");
+	for (sta = hapd->sta_list; sta; sta = sta->next) {
+		int i;
+
+		sprintf(mac_buf, MACSTR, MAC2STR(sta->addr));
+		c = blobmsg_open_table(&b, mac_buf);
+		for (i = 0; i < ARRAY_SIZE(sta_flags); i++)
+			blobmsg_add_u8(&b, sta_flags[i].name,
+				       !!(sta->flags & sta_flags[i].flag));
+		blobmsg_add_u32(&b, "aid", sta->aid);
+		blobmsg_close_table(&b, c);
+	}
+	blobmsg_close_array(&b, list);
+	ubus_send_reply(ctx, req, b.head);
+
+	return 0;
+}
+
+enum {
+	DEL_CLIENT_ADDR,
+	DEL_CLIENT_REASON,
+	DEL_CLIENT_DEAUTH,
+	DEL_CLIENT_BAN_TIME,
+	__DEL_CLIENT_MAX
+};
+
+static const struct blobmsg_policy del_policy[__DEL_CLIENT_MAX] = {
+	[DEL_CLIENT_ADDR] = { "addr", BLOBMSG_TYPE_STRING },
+	[DEL_CLIENT_REASON] = { "reason", BLOBMSG_TYPE_INT32 },
+	[DEL_CLIENT_DEAUTH] = { "deauth", BLOBMSG_TYPE_INT8 },
+	[DEL_CLIENT_BAN_TIME] = { "ban_time", BLOBMSG_TYPE_INT32 },
+};
+
+static int
+hostapd_bss_del_client(struct ubus_context *ctx, struct ubus_object *obj,
+			struct ubus_request_data *req, const char *method,
+			struct blob_attr *msg)
+{
+	struct blob_attr *tb[__DEL_CLIENT_MAX];
+	struct hostapd_data *hapd = container_of(obj, struct hostapd_data, ubus.obj);
+	struct sta_info *sta;
+	bool deauth = false;
+	int reason;
+	u8 addr[ETH_ALEN];
+
+	blobmsg_parse(del_policy, __DEL_CLIENT_MAX, tb, blob_data(msg), blob_len(msg));
+
+	if (!tb[DEL_CLIENT_ADDR])
+		return UBUS_STATUS_INVALID_ARGUMENT;
+
+	if (hwaddr_aton(blobmsg_data(tb[DEL_CLIENT_ADDR]), addr))
+		return UBUS_STATUS_INVALID_ARGUMENT;
+
+	if (tb[DEL_CLIENT_REASON])
+		reason = blobmsg_get_u32(tb[DEL_CLIENT_REASON]);
+
+	if (tb[DEL_CLIENT_DEAUTH])
+		deauth = blobmsg_get_bool(tb[DEL_CLIENT_DEAUTH]);
+
+	sta = ap_get_sta(hapd, addr);
+	if (sta) {
+		if (deauth) {
+			hostapd_drv_sta_deauth(hapd, addr, reason);
+			ap_sta_deauthenticate(hapd, sta, reason);
+		} else {
+			hostapd_drv_sta_disassoc(hapd, addr, reason);
+			ap_sta_disassociate(hapd, sta, reason);
+		}
+	}
+
+	if (tb[DEL_CLIENT_BAN_TIME])
+		hostapd_bss_ban_client(hapd, addr, blobmsg_get_u32(tb[DEL_CLIENT_BAN_TIME]));
+
+	return 0;
+}
+
+static void
+blobmsg_add_macaddr(struct blob_buf *buf, const char *name, const u8 *addr)
+{
+	char *s;
+
+	s = blobmsg_alloc_string_buffer(buf, name, 20);
+	sprintf(s, MACSTR, MAC2STR(addr));
+	blobmsg_add_string_buffer(buf);
+}
+
+static int
+hostapd_bss_list_bans(struct ubus_context *ctx, struct ubus_object *obj,
+		      struct ubus_request_data *req, const char *method,
+		      struct blob_attr *msg)
+{
+	struct hostapd_data *hapd = container_of(obj, struct hostapd_data, ubus.obj);
+	struct ubus_banned_client *ban;
+	void *c;
+
+	blob_buf_init(&b, 0);
+	c = blobmsg_open_array(&b, "clients");
+	avl_for_each_element(&hapd->ubus.banned, ban, avl)
+		blobmsg_add_macaddr(&b, NULL, ban->addr);
+	blobmsg_close_array(&b, c);
+	ubus_send_reply(ctx, req, b.head);
+
+	return 0;
+}
+
+static const struct ubus_method bss_methods[] = {
+	UBUS_METHOD_NOARG("get_clients", hostapd_bss_get_clients),
+	UBUS_METHOD("del_client", hostapd_bss_del_client, del_policy),
+	UBUS_METHOD_NOARG("list_bans", hostapd_bss_list_bans),
+};
+
+static struct ubus_object_type bss_object_type =
+	UBUS_OBJECT_TYPE("hostapd_bss", bss_methods);
+
+static int avl_compare_macaddr(const void *k1, const void *k2, void *ptr)
+{
+	return memcmp(k1, k2, ETH_ALEN);
+}
+
+void hostapd_ubus_add_bss(struct hostapd_data *hapd)
+{
+	struct ubus_object *obj = &hapd->ubus.obj;
+	char *name;
+	int ret;
+
+	if (!hostapd_ubus_init())
+		return;
+
+	if (asprintf(&name, "hostapd.%s", hapd->conf->iface) < 0)
+		return;
+
+	avl_init(&hapd->ubus.banned, avl_compare_macaddr, false, NULL);
+	obj->name = name;
+	obj->type = &bss_object_type;
+	obj->methods = bss_object_type.methods;
+	obj->n_methods = bss_object_type.n_methods;
+	ret = ubus_add_object(ctx, obj);
+	hostapd_ubus_ref_inc();
+}
+
+void hostapd_ubus_free_bss(struct hostapd_data *hapd)
+{
+	struct ubus_object *obj = &hapd->ubus.obj;
+	char *name = (char *) obj->name;
+
+	if (!ctx)
+		return;
+
+	if (obj->id) {
+		ubus_remove_object(ctx, obj);
+		hostapd_ubus_ref_dec();
+	}
+
+	free(name);
+}
+
+struct ubus_event_req {
+	struct ubus_notify_request nreq;
+	bool deny;
+};
+
+static void
+ubus_event_cb(struct ubus_notify_request *req, int idx, int ret)
+{
+	struct ubus_event_req *ureq = container_of(req, struct ubus_event_req, nreq);
+
+	if (ret)
+		ureq->deny = true;
+}
+
+int hostapd_ubus_handle_event(struct hostapd_data *hapd, struct hostapd_ubus_request *req)
+{
+	struct ubus_banned_client *ban;
+	const char *types[HOSTAPD_UBUS_TYPE_MAX] = {
+		[HOSTAPD_UBUS_PROBE_REQ] = "probe",
+		[HOSTAPD_UBUS_AUTH_REQ] = "auth",
+		[HOSTAPD_UBUS_ASSOC_REQ] = "assoc",
+	};
+	const char *type = "mgmt";
+	struct ubus_event_req ureq = {};
+	const u8 *addr;
+
+	if (req->mgmt_frame)
+		addr = req->mgmt_frame->sa;
+	else
+		addr = req->addr;
+
+	ban = avl_find_element(&hapd->ubus.banned, addr, ban, avl);
+	if (ban)
+		return -2;
+
+	if (!hapd->ubus.obj.has_subscribers)
+		return 0;
+
+	if (req->type < ARRAY_SIZE(types))
+		type = types[req->type];
+
+	blob_buf_init(&b, 0);
+	blobmsg_add_macaddr(&b, "address", addr);
+	if (req->mgmt_frame)
+		blobmsg_add_macaddr(&b, "target", req->mgmt_frame->da);
+	if (req->frame_info)
+		blobmsg_add_u32(&b, "signal", req->frame_info->ssi_signal);
+	blobmsg_add_u32(&b, "freq", hapd->iface->freq);
+
+	if (ubus_notify_async(ctx, &hapd->ubus.obj, type, b.head, &ureq.nreq))
+		return 0;
+
+	ureq.nreq.status_cb = ubus_event_cb;
+	ubus_complete_request(ctx, &ureq.nreq.req, 100);
+
+	if (ureq.deny)
+		return -1;
+
+	return 0;
+}
--- /dev/null
+++ b/src/ap/ubus.h
@@ -0,0 +1,78 @@
+/*
+ * hostapd / ubus support
+ * Copyright (c) 2013, Felix Fietkau <nbd@openwrt.org>
+ *
+ * This software may be distributed under the terms of the BSD license.
+ * See README for more details.
+ */
+#ifndef __HOSTAPD_UBUS_H
+#define __HOSTAPD_UBUS_H
+
+enum hostapd_ubus_event_type {
+	HOSTAPD_UBUS_PROBE_REQ,
+	HOSTAPD_UBUS_AUTH_REQ,
+	HOSTAPD_UBUS_ASSOC_REQ,
+	HOSTAPD_UBUS_TYPE_MAX
+};
+
+struct hostapd_ubus_request {
+	enum hostapd_ubus_event_type type;
+	const struct ieee80211_mgmt *mgmt_frame;
+	const struct hostapd_frame_info *frame_info;
+	const u8 *addr;
+};
+
+struct hostapd_iface;
+struct hostapd_data;
+
+#ifdef UBUS_SUPPORT
+
+#include <libubox/avl.h>
+#include <libubus.h>
+
+struct hostapd_ubus_iface {
+	struct ubus_object obj;
+};
+
+struct hostapd_ubus_bss {
+	struct ubus_object obj;
+	struct avl_tree banned;
+};
+
+void hostapd_ubus_add_iface(struct hostapd_iface *iface);
+void hostapd_ubus_free_iface(struct hostapd_iface *iface);
+void hostapd_ubus_add_bss(struct hostapd_data *hapd);
+void hostapd_ubus_free_bss(struct hostapd_data *hapd);
+
+int hostapd_ubus_handle_event(struct hostapd_data *hapd, struct hostapd_ubus_request *req);
+
+#else
+
+struct hostapd_ubus_iface {};
+
+struct hostapd_ubus_bss {};
+
+static inline void hostapd_ubus_add_iface(struct hostapd_iface *iface)
+{
+}
+
+static inline void hostapd_ubus_free_iface(struct hostapd_iface *iface)
+{
+}
+
+static inline void hostapd_ubus_add_bss(struct hostapd_data *hapd)
+{
+}
+
+static inline void hostapd_ubus_free_bss(struct hostapd_data *hapd)
+{
+}
+
+static inline int hostapd_ubus_handle_event(struct hostapd_data *hapd, struct hostapd_ubus_request *req)
+{
+	return 0;
+}
+
+#endif
+
+#endif
--- a/src/ap/hostapd.c
+++ b/src/ap/hostapd.c
@@ -265,6 +265,7 @@ static void hostapd_free_hapd_data(struc
 	hapd->started = 0;
 
 	wpa_printf(MSG_DEBUG, "%s(%s)", __func__, hapd->conf->iface);
+	hostapd_ubus_free_bss(hapd);
 	iapp_deinit(hapd->iapp);
 	hapd->iapp = NULL;
 	accounting_deinit(hapd);
@@ -834,6 +835,8 @@ static int hostapd_setup_bss(struct host
 	if (hapd->driver && hapd->driver->set_operstate)
 		hapd->driver->set_operstate(hapd->drv_priv, 1);
 
+	hostapd_ubus_add_bss(hapd);
+
 	return 0;
 }
 
@@ -1108,6 +1111,7 @@ int hostapd_setup_interface_complete(str
 	if (err)
 		goto error;
 
+	hostapd_ubus_add_iface(iface);
 	wpa_printf(MSG_DEBUG, "Completing interface initialization");
 	if (iface->conf->channel) {
 #ifdef NEED_AP_MLME
@@ -1216,6 +1220,7 @@ int hostapd_setup_interface_complete(str
 
 error:
 	wpa_printf(MSG_ERROR, "Interface initialization failed");
+	hostapd_ubus_free_iface(iface);
 	hostapd_set_state(iface, HAPD_IFACE_DISABLED);
 	if (iface->interfaces && iface->interfaces->terminate_on_error)
 		eloop_terminate();
@@ -1537,6 +1542,7 @@ void hostapd_interface_deinit_free(struc
 		   (unsigned int) iface->conf->num_bss);
 	driver = iface->bss[0]->driver;
 	drv_priv = iface->bss[0]->drv_priv;
+	hostapd_ubus_free_iface(iface);
 	hostapd_interface_deinit(iface);
 	wpa_printf(MSG_DEBUG, "%s: driver=%p drv_priv=%p -> hapd_deinit",
 		   __func__, driver, drv_priv);
--- a/src/ap/ieee802_11.c
+++ b/src/ap/ieee802_11.c
@@ -535,7 +535,8 @@ static void handle_auth_sae(struct hosta
 
 
 static void handle_auth(struct hostapd_data *hapd,
-			const struct ieee80211_mgmt *mgmt, size_t len)
+			const struct ieee80211_mgmt *mgmt, size_t len,
+			struct hostapd_frame_info *fi)
 {
 	u16 auth_alg, auth_transaction, status_code;
 	u16 resp = WLAN_STATUS_SUCCESS;
@@ -550,6 +551,11 @@ static void handle_auth(struct hostapd_d
 	size_t resp_ies_len = 0;
 	char *identity = NULL;
 	char *radius_cui = NULL;
+	struct hostapd_ubus_request req = {
+		.type = HOSTAPD_UBUS_AUTH_REQ,
+		.mgmt_frame = mgmt,
+		.frame_info = fi,
+	};
 
 	if (len < IEEE80211_HDRLEN + sizeof(mgmt->u.auth)) {
 		wpa_printf(MSG_INFO, "handle_auth - too short payload (len=%lu)",
@@ -633,6 +639,14 @@ static void handle_auth(struct hostapd_d
 		resp = WLAN_STATUS_UNSPECIFIED_FAILURE;
 		goto fail;
 	}
+
+	if (hostapd_ubus_handle_event(hapd, &req)) {
+		wpa_printf(MSG_DEBUG, "Station " MACSTR " rejected by ubus handler.\n",
+		       MAC2STR(mgmt->sa));
+		resp = WLAN_STATUS_UNSPECIFIED_FAILURE;
+		goto fail;
+	}
+
 	if (res == HOSTAPD_ACL_PENDING) {
 		wpa_printf(MSG_DEBUG, "Authentication frame from " MACSTR
 			   " waiting for an external authentication",
@@ -1245,13 +1259,18 @@ static void send_assoc_resp(struct hosta
 
 static void handle_assoc(struct hostapd_data *hapd,
 			 const struct ieee80211_mgmt *mgmt, size_t len,
-			 int reassoc)
+			 int reassoc, struct hostapd_frame_info *fi)
 {
 	u16 capab_info, listen_interval;
 	u16 resp = WLAN_STATUS_SUCCESS;
 	const u8 *pos;
 	int left, i;
 	struct sta_info *sta;
+	struct hostapd_ubus_request req = {
+		.type = HOSTAPD_UBUS_ASSOC_REQ,
+		.mgmt_frame = mgmt,
+		.frame_info = fi,
+	};
 
 	if (len < IEEE80211_HDRLEN + (reassoc ? sizeof(mgmt->u.reassoc_req) :
 				      sizeof(mgmt->u.assoc_req))) {
@@ -1350,6 +1369,13 @@ static void handle_assoc(struct hostapd_
 		goto fail;
 	}
 
+	if (hostapd_ubus_handle_event(hapd, &req)) {
+		wpa_printf(MSG_DEBUG, "Station " MACSTR " assoc rejected by ubus handler.\n",
+		       MAC2STR(mgmt->sa));
+		resp = WLAN_STATUS_UNSPECIFIED_FAILURE;
+		goto fail;
+	}
+
 	sta->capability = capab_info;
 	sta->listen_interval = listen_interval;
 
@@ -1759,7 +1785,7 @@ void ieee802_11_mgmt(struct hostapd_data
 
 
 	if (stype == WLAN_FC_STYPE_PROBE_REQ) {
-		handle_probe_req(hapd, mgmt, len, fi->ssi_signal);
+		handle_probe_req(hapd, mgmt, len, fi);
 		return;
 	}
 
@@ -1774,15 +1800,15 @@ void ieee802_11_mgmt(struct hostapd_data
 	switch (stype) {
 	case WLAN_FC_STYPE_AUTH:
 		wpa_printf(MSG_DEBUG, "mgmt::auth");
-		handle_auth(hapd, mgmt, len);
+		handle_auth(hapd, mgmt, len, fi);
 		break;
 	case WLAN_FC_STYPE_ASSOC_REQ:
 		wpa_printf(MSG_DEBUG, "mgmt::assoc_req");
-		handle_assoc(hapd, mgmt, len, 0);
+		handle_assoc(hapd, mgmt, len, 0, fi);
 		break;
 	case WLAN_FC_STYPE_REASSOC_REQ:
 		wpa_printf(MSG_DEBUG, "mgmt::reassoc_req");
-		handle_assoc(hapd, mgmt, len, 1);
+		handle_assoc(hapd, mgmt, len, 1, fi);
 		break;
 	case WLAN_FC_STYPE_DISASSOC:
 		wpa_printf(MSG_DEBUG, "mgmt::disassoc");
--- a/src/ap/beacon.c
+++ b/src/ap/beacon.c
@@ -398,7 +398,7 @@ static enum ssid_match_result ssid_match
 
 void handle_probe_req(struct hostapd_data *hapd,
 		      const struct ieee80211_mgmt *mgmt, size_t len,
-		      int ssi_signal)
+		      struct hostapd_frame_info *fi)
 {
 	u8 *resp;
 	struct ieee802_11_elems elems;
@@ -406,8 +406,14 @@ void handle_probe_req(struct hostapd_dat
 	size_t ie_len;
 	struct sta_info *sta = NULL;
 	size_t i, resp_len;
+	int ssi_signal = fi->ssi_signal;
 	int noack;
 	enum ssid_match_result res;
+	struct hostapd_ubus_request req = {
+		.type = HOSTAPD_UBUS_PROBE_REQ,
+		.mgmt_frame = mgmt,
+		.frame_info = fi,
+	};
 
 	ie = mgmt->u.probe_req.variable;
 	if (len < IEEE80211_HDRLEN + sizeof(mgmt->u.probe_req))
@@ -546,6 +552,12 @@ void handle_probe_req(struct hostapd_dat
 	}
 #endif /* CONFIG_P2P */
 
+	if (hostapd_ubus_handle_event(hapd, &req)) {
+		wpa_printf(MSG_DEBUG, "Probe request for " MACSTR " rejected by ubus handler.\n",
+		       MAC2STR(mgmt->sa));
+		return;
+	}
+
 	/* TODO: verify that supp_rates contains at least one matching rate
 	 * with AP configuration */
 
--- a/src/ap/beacon.h
+++ b/src/ap/beacon.h
@@ -20,7 +20,7 @@ struct ieee80211_mgmt;
 
 void handle_probe_req(struct hostapd_data *hapd,
 		      const struct ieee80211_mgmt *mgmt, size_t len,
-		      int ssi_signal);
+		      struct hostapd_frame_info *fi);
 void ieee802_11_set_beacon(struct hostapd_data *hapd);
 void ieee802_11_set_beacons(struct hostapd_iface *iface);
 void ieee802_11_update_beacons(struct hostapd_iface *iface);
