From f3443f6d43a69a520ae1e636d69a71c4a6bee21e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Sun, 8 Sep 2013 18:12:28 -0300
Subject: [PATCH] ARM: sunxi: dt: unify APB1 clock
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

With the new factors infrastructure in place, we can unify apb1 and
apb1_mux as a single clock now.

Signed-off-by: Emilio López <emilio@elopez.com.ar>
---
 arch/arm/boot/dts/sun4i-a10.dtsi  | 9 +--------
 arch/arm/boot/dts/sun5i-a10s.dtsi | 9 +--------
 arch/arm/boot/dts/sun5i-a13.dtsi  | 9 +--------
 arch/arm/boot/dts/sun7i-a20.dtsi  | 9 +--------
 4 files changed, 4 insertions(+), 32 deletions(-)

diff --git a/arch/arm/boot/dts/sun4i-a10.dtsi b/arch/arm/boot/dts/sun4i-a10.dtsi
index 2828427e..4dccdb0 100644
--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -158,18 +158,11 @@
 				"apb0_ir1", "apb0_keypad";
 		};
 
-		apb1_mux: apb1_mux@01c20058 {
-			#clock-cells = <0>;
-			compatible = "allwinner,sun4i-apb1-mux-clk";
-			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
-		};
-
 		apb1: apb1@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&apb1_mux>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1_gates: apb1_gates@01c2006c {
diff --git a/arch/arm/boot/dts/sun5i-a10s.dtsi b/arch/arm/boot/dts/sun5i-a10s.dtsi
index 60bd3f7..9cb1b14 100644
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -150,18 +150,11 @@
 				"apb0_ir", "apb0_keypad";
 		};
 
-		apb1_mux: apb1_mux@01c20058 {
-			#clock-cells = <0>;
-			compatible = "allwinner,sun4i-apb1-mux-clk";
-			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
-		};
-
 		apb1: apb1@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&apb1_mux>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1_gates: apb1_gates@01c2006c {
diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index 3e616a0..6b74dd0 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -148,18 +148,11 @@
 			clock-output-names = "apb0_codec", "apb0_pio", "apb0_ir";
 		};
 
-		apb1_mux: apb1_mux@01c20058 {
-			#clock-cells = <0>;
-			compatible = "allwinner,sun4i-apb1-mux-clk";
-			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
-		};
-
 		apb1: apb1@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&apb1_mux>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1_gates: apb1_gates@01c2006c {
diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index 0bf5d07..55d3e14 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -148,18 +148,11 @@
 				"apb0_iis2", "apb0_keypad";
 		};
 
-		apb1_mux: apb1_mux@01c20058 {
-			#clock-cells = <0>;
-			compatible = "allwinner,sun4i-apb1-mux-clk";
-			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
-		};
-
 		apb1: apb1@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&apb1_mux>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1_gates: apb1_gates@01c2006c {
-- 
1.8.5.1

