From 29f3723bf62d46c238dcc5436787a8ad6b25a385 Mon Sep 17 00:00:00 2001
From: Lars Poeschel <poeschel@lemonage.de>
Date: Wed, 7 Aug 2013 13:06:32 +0200
Subject: [PATCH 02/14] ARM: dts: AM33xx: Correct gpio #interrupt-cells
 property

Following commit ff5c9059 and therefore other omap platforms using
the gpio-omap driver correct the #interrupt-cells property on am33xx
too. The omap gpio binding documentaion also states that
the #interrupt-cells property should be 2.

Signed-off-by: Lars Poeschel <poeschel@lemonage.de>
Reviewed-by: Javier Martinez Canillas <javier@dowhile0.org>
Acked-by: Mark Rutland <mark.rutland@arm.com>
Signed-off-by: Benoit Cousson <bcousson@baylibre.com>
---
 arch/arm/boot/dts/am33xx.dtsi | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -106,7 +106,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 			reg = <0x44e07000 0x1000>;
 			interrupts = <96>;
 		};
@@ -117,7 +117,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 			reg = <0x4804c000 0x1000>;
 			interrupts = <98>;
 		};
@@ -128,7 +128,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 			reg = <0x481ac000 0x1000>;
 			interrupts = <32>;
 		};
@@ -139,7 +139,7 @@
 			gpio-controller;
 			#gpio-cells = <2>;
 			interrupt-controller;
-			#interrupt-cells = <1>;
+			#interrupt-cells = <2>;
 			reg = <0x481ae000 0x1000>;
 			interrupts = <62>;
 		};
