--- /dev/null
+++ b/arch/arm/boot/dts/kirkwood-pogo_e02.dts
@@ -0,0 +1,117 @@
+/dts-v1/;
+
+/include/ "kirkwood.dtsi"
+/include/ "kirkwood-6281.dtsi"
+
+/ {
+	model = "Cloud Engines Pogoplug E02";
+	compatible = "cloudengines,pogoe02", "marvell,kirkwood-88f6281", "marvell,kirkwood";
+
+	memory {
+		device_type = "memory";
+		reg = <0x00000000 0x10000000>;
+	};
+
+	chosen {
+		bootargs = "console=ttyS0,115200n8 earlyprintk";
+	};
+
+	ocp@f1000000 {
+		pinctrl: pinctrl@10000 {
+
+			pinctrl-0 = < &pmx_usb_power_enable &pmx_led_orange
+				      &pmx_led_green >;
+			pinctrl-names = "default";
+
+			pmx_usb_power_enable: pmx-usb-power-enable {
+				marvell,pins = "mpp29";
+				marvell,function = "gpio";
+			};
+			pmx_led_green: pmx-led_green {
+				marvell,pins = "mpp48";
+				marvell,function = "gpio";
+			};
+			pmx_led_orange: pmx-led_orange {
+				marvell,pins = "mpp49";
+				marvell,function = "gpio";
+			};
+		};
+
+		serial@12000 {
+			status = "okay";
+		};
+
+		nand@3000000 {
+			status = "okay";
+
+			partition@0 {
+				label = "u-boot";
+				reg = <0x0000000 0x100000>;
+			};
+
+			partition@100000 {
+				label = "uImage";
+				reg = <0x0100000 0x400000>;
+			};
+
+			partition@500000 {
+				label = "rootfs";
+				reg = <0x0500000 0x2000000>;
+			};
+
+			partition@2500000 {
+				label = "data";
+				reg = <0x2500000 0x5b00000>;
+			};
+		};
+	};
+
+	gpio-leds {
+		compatible = "gpio-leds";
+
+		health {
+			label = "status:green:health";
+			gpios = <&gpio1 16 1>;
+			linux,default-trigger = "default-on";
+		};
+		fault {
+			label = "status:orange:fault";
+			gpios = <&gpio1 17 1>;
+		};
+	};
+
+	regulators {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		usb_power: regulator@1 {
+			compatible = "regulator-fixed";
+			reg = <1>;
+			regulator-name = "USB Power";
+			regulator-min-microvolt = <5000000>;
+			regulator-max-microvolt = <5000000>;
+			enable-active-high;
+			regulator-always-on;
+			regulator-boot-on;
+			gpio = <&gpio0 29 0>;
+		};
+	};
+};
+
+&mdio {
+	status = "okay";
+
+	ethphy0: ethernet-phy@0 {
+		device_type = "ethernet-phy";
+		reg = <0>;
+	};
+};
+
+&eth0 {
+	status = "okay";
+
+	ethernet0-port@0 {
+		phy-handle = <&ethphy0>;
+	};
+};
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -86,6 +86,7 @@ dtb-$(CONFIG_ARCH_KIRKWOOD) += kirkwood-
 	kirkwood-ns2max.dtb \
 	kirkwood-ns2mini.dtb \
 	kirkwood-nsa310.dtb \
+	kirkwood-pogo_e02.dtb \
 	kirkwood-topkick.dtb \
 	kirkwood-ts219-6281.dtb \
 	kirkwood-ts219-6282.dtb \
