From 855094d7e46eb14c597ca09631cf95a92909982d Mon Sep 17 00:00:00 2001
From: Ilia Mirkin <imirkin@alum.mit.edu>
Date: Fri, 6 Dec 2013 18:56:53 -0500
Subject: [PATCH] MIPS: BCM47XX: Fix some very confused types and data
 corruption

Fix nvram_read_alpha2 copying too many bytes over the ssb_sprom
structure. Also fix the arguments of the read_macaddr, although the code
was technically not wrong before due to an extra dereference.

Signed-off-by: Ilia Mirkin <imirkin@alum.mit.edu>
Acked-by: Hauke Mehrtens <hauke@hauke-m.de>
Acked-by: John Crispin <blogic@openwrt.org>
Patchwork: http://patchwork.linux-mips.org/patch/6211/
---
 arch/mips/bcm47xx/sprom.c |   18 +++++++++---------
 1 file changed, 9 insertions(+), 9 deletions(-)

--- a/arch/mips/bcm47xx/sprom.c
+++ b/arch/mips/bcm47xx/sprom.c
@@ -135,7 +135,7 @@ static void nvram_read_leddc(const char
 }
 
 static void nvram_read_macaddr(const char *prefix, const char *name,
-			       u8 (*val)[6], bool fallback)
+			       u8 val[6], bool fallback)
 {
 	char buf[100];
 	int err;
@@ -144,11 +144,11 @@ static void nvram_read_macaddr(const cha
 	if (err < 0)
 		return;
 
-	bcm47xx_nvram_parse_macaddr(buf, *val);
+	bcm47xx_nvram_parse_macaddr(buf, val);
 }
 
 static void nvram_read_alpha2(const char *prefix, const char *name,
-			     char (*val)[2], bool fallback)
+			     char val[2], bool fallback)
 {
 	char buf[10];
 	int err;
@@ -162,7 +162,7 @@ static void nvram_read_alpha2(const char
 		pr_warn("alpha2 is too long %s\n", buf);
 		return;
 	}
-	memcpy(val, buf, sizeof(val));
+	memcpy(val, buf, 2);
 }
 
 static void bcm47xx_fill_sprom_r1234589(struct ssb_sprom *sprom,
@@ -180,7 +180,7 @@ static void bcm47xx_fill_sprom_r1234589(
 		      fallback);
 	nvram_read_s8(prefix, NULL, "ag1", &sprom->antenna_gain.a1, 0,
 		      fallback);
-	nvram_read_alpha2(prefix, "ccode", &sprom->alpha2, fallback);
+	nvram_read_alpha2(prefix, "ccode", sprom->alpha2, fallback);
 }
 
 static void bcm47xx_fill_sprom_r12389(struct ssb_sprom *sprom,
@@ -633,20 +633,20 @@ static void bcm47xx_fill_sprom_path_r45(
 static void bcm47xx_fill_sprom_ethernet(struct ssb_sprom *sprom,
 					const char *prefix, bool fallback)
 {
-	nvram_read_macaddr(prefix, "et0macaddr", &sprom->et0mac, fallback);
+	nvram_read_macaddr(prefix, "et0macaddr", sprom->et0mac, fallback);
 	nvram_read_u8(prefix, NULL, "et0mdcport", &sprom->et0mdcport, 0,
 		      fallback);
 	nvram_read_u8(prefix, NULL, "et0phyaddr", &sprom->et0phyaddr, 0,
 		      fallback);
 
-	nvram_read_macaddr(prefix, "et1macaddr", &sprom->et1mac, fallback);
+	nvram_read_macaddr(prefix, "et1macaddr", sprom->et1mac, fallback);
 	nvram_read_u8(prefix, NULL, "et1mdcport", &sprom->et1mdcport, 0,
 		      fallback);
 	nvram_read_u8(prefix, NULL, "et1phyaddr", &sprom->et1phyaddr, 0,
 		      fallback);
 
-	nvram_read_macaddr(prefix, "macaddr", &sprom->il0mac, fallback);
-	nvram_read_macaddr(prefix, "il0macaddr", &sprom->il0mac, fallback);
+	nvram_read_macaddr(prefix, "macaddr", sprom->il0mac, fallback);
+	nvram_read_macaddr(prefix, "il0macaddr", sprom->il0mac, fallback);
 }
 
 static void bcm47xx_fill_board_data(struct ssb_sprom *sprom, const char *prefix,
