From 43c2d3189567342f68ec192f2eeab6ae4c4d1ddf Mon Sep 17 00:00:00 2001
From: arokux <arokux@gmail.com>
Date: Thu, 19 Sep 2013 21:59:32 +0200
Subject: [PATCH] clk: sunxi: Add support for USB clocks

---
 drivers/clk/sunxi/clk-sunxi.c | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/drivers/clk/sunxi/clk-sunxi.c b/drivers/clk/sunxi/clk-sunxi.c
index 96c01b2..cbe1516 100644
--- a/drivers/clk/sunxi/clk-sunxi.c
+++ b/drivers/clk/sunxi/clk-sunxi.c
@@ -619,6 +619,10 @@ struct gates_data {
 	.mask = {0x7F77FFF, 0x14FB3F},
 };
 
+static const struct gates_data sun47i_usb_gates_data __initconst = {
+	.mask = {0x1C0},
+};
+
 static const struct gates_data sun5i_a10s_ahb_gates_data __initconst = {
 	.mask = {0x147667e7, 0x185915},
 };
@@ -867,6 +871,7 @@ static void __init sunxi_divs_clk_setup(struct device_node *node,
 static const struct of_device_id clk_gates_match[] __initconst = {
 	{.compatible = "allwinner,sun4i-axi-gates-clk", .data = &sun4i_axi_gates_data,},
 	{.compatible = "allwinner,sun4i-ahb-gates-clk", .data = &sun4i_ahb_gates_data,},
+	{.compatible = "allwinner,sun47i-usb-gates-clk", .data = &sun47i_usb_gates_data,},
 	{.compatible = "allwinner,sun5i-a10s-ahb-gates-clk", .data = &sun5i_a10s_ahb_gates_data,},
 	{.compatible = "allwinner,sun5i-a13-ahb-gates-clk", .data = &sun5i_a13_ahb_gates_data,},
 	{.compatible = "allwinner,sun6i-a31-ahb1-gates-clk", .data = &sun6i_a31_ahb1_gates_data,},
-- 
1.8.4

