From 2be714d9730da5723de68b4f9bfd5941ccd5bc4c Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sat, 29 Jun 2013 19:21:22 +0200
Subject: [PATCH 14/34] MTD: lantiq: handle NO_XIP on cfi0001 flash

---
 drivers/mtd/maps/lantiq-flash.c |    6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

--- a/drivers/mtd/maps/lantiq-flash.c
+++ b/drivers/mtd/maps/lantiq-flash.c
@@ -134,7 +134,11 @@ ltq_mtd_probe(struct platform_device *pd
 	}
 
 	ltq_mtd->map = kzalloc(sizeof(struct map_info), GFP_KERNEL);
-	ltq_mtd->map->phys = ltq_mtd->res->start;
+	if (of_find_property(pdev->dev.of_node, "lantiq,noxip", NULL))
+		ltq_mtd->map->phys = NO_XIP;
+	else
+		ltq_mtd->map->phys = ltq_mtd->res->start;
+	ltq_mtd->res->start;
 	ltq_mtd->map->size = resource_size(ltq_mtd->res);
 	ltq_mtd->map->virt = devm_ioremap_resource(&pdev->dev, ltq_mtd->res);
 	if (IS_ERR(ltq_mtd->map->virt)) {
