From 9249f2f6a309e3f45c35d16decdcc5b2cadcadb8 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Fri, 26 Apr 2013 12:06:03 +0200
Subject: [PATCH 38/53] MIPS: BCM63XX: allow setting affinity for IPIC

Signed-off-by: Jonas Gorski <jogo@openwrt.org>
---
 arch/mips/bcm63xx/irq.c | 43 +++++++++++++++++++++++++++++++++++++------
 1 file changed, 37 insertions(+), 6 deletions(-)

--- a/arch/mips/bcm63xx/irq.c
+++ b/arch/mips/bcm63xx/irq.c
@@ -32,7 +32,7 @@ static unsigned int ext_irq_count;
 static unsigned int ext_irq_start, ext_irq_end;
 static unsigned int ext_irq_cfg_reg1, ext_irq_cfg_reg2;
 static void (*internal_irq_mask)(struct irq_data *d);
-static void (*internal_irq_unmask)(struct irq_data *d);
+static void (*internal_irq_unmask)(struct irq_data *d, const struct cpumask *m);
 
 
 static inline u32 get_ext_irq_perf_reg(int irq)
@@ -51,6 +51,20 @@ static inline void handle_internal(int i
 		do_IRQ(intbit + IRQ_INTERNAL_BASE);
 }
 
+static inline int enable_irq_for_cpu(int cpu, struct irq_data *d,
+				     const struct cpumask *m)
+{
+	bool enable = cpu_online(cpu);
+#ifdef CONFIG_SMP
+
+	if (m)
+		enable &= cpu_isset(cpu, *m);
+	else if (irqd_affinity_was_set(d))
+		enable &= cpu_isset(cpu, *d->affinity);
+#endif
+	return enable;
+}
+
 /*
  * dispatch internal devices IRQ (uart, enet, watchdog, ...). do not
  * prioritize any interrupt relatively to another. the static counter
@@ -117,7 +131,8 @@ static void __internal_irq_mask_##width(
 	spin_unlock_irqrestore(&ipic_lock, flags);			\
 }									\
 									\
-static void __internal_irq_unmask_##width(struct irq_data *d)		\
+static void __internal_irq_unmask_##width(struct irq_data *d,		\
+					  const struct cpumask *m)	\
 { 									\
 	u32 val;							\
 	unsigned irq = d->irq - IRQ_INTERNAL_BASE;			\
@@ -132,7 +147,7 @@ static void __internal_irq_unmask_##widt
 			break;						\
 									\
 		val = bcm_readl(irq_mask_addr[cpu] + reg * sizeof(u32));\
-		if (cpu_online(cpu))					\
+		if (enable_irq_for_cpu(cpu, d, m))			\
 			val |= (1 << bit); 				\
 		else							\
 			val &= ~(1 << bit);				\
@@ -189,7 +204,7 @@ static void bcm63xx_internal_irq_mask(st
 
 static void bcm63xx_internal_irq_unmask(struct irq_data *d)
 {
-	internal_irq_unmask(d);
+	internal_irq_unmask(d, NULL);
 }
 
 /*
@@ -237,7 +252,8 @@ static void bcm63xx_external_irq_unmask(
 	spin_unlock_irqrestore(&epic_lock, flags);
 
 	if (is_ext_irq_cascaded)
-		internal_irq_unmask(irq_get_irq_data(irq + ext_irq_start));
+		internal_irq_unmask(irq_get_irq_data(irq + ext_irq_start),
+				    NULL);
 }
 
 static void bcm63xx_external_irq_clear(struct irq_data *d)
@@ -356,6 +372,18 @@ static int bcm63xx_external_irq_set_type
 	return IRQ_SET_MASK_OK_NOCOPY;
 }
 
+#ifdef CONFIG_SMP
+static int bcm63xx_internal_set_affinity(struct irq_data *data,
+					 const struct cpumask *dest,
+					 bool force)
+{
+	if (!irqd_irq_disabled(data))
+		internal_irq_unmask(data, dest);
+
+	return 0;
+}
+#endif
+
 static struct irq_chip bcm63xx_internal_irq_chip = {
 	.name		= "bcm63xx_ipic",
 	.irq_mask	= bcm63xx_internal_irq_mask,
@@ -523,7 +551,10 @@ void __init arch_init_irq(void)
 
 	setup_irq(MIPS_CPU_IRQ_BASE + 2, &cpu_ip2_cascade_action);
 #ifdef CONFIG_SMP
-	if (is_ext_irq_cascaded)
+	if (is_ext_irq_cascaded) {
 		setup_irq(MIPS_CPU_IRQ_BASE + 3, &cpu_ip3_cascade_action);
+		bcm63xx_internal_irq_chip.irq_set_affinity =
+			bcm63xx_internal_set_affinity;
+	}
 #endif
 }
