Index: linux-2.6.23/drivers/mtd/Kconfig
===================================================================
--- linux-2.6.23.orig/drivers/mtd/Kconfig
+++ linux-2.6.23/drivers/mtd/Kconfig
@@ -160,6 +160,22 @@ config MTD_AFS_PARTS
 	  for your particular device. It won't happen automatically. The
 	  'armflash' map driver (CONFIG_MTD_ARMFLASH) does this, for example.
 
+config MTD_MYLOADER_PARTS
+	tristate "MyLoader partition parsing"
+	depends on MIPS_ADM5120 && MTD_PARTITIONS
+	---help---
+	  MyLoader is a bootloader which allows the user to define partitions
+	  in flash devices, by putting a table in the second erase block
+	  on the device, similar to a partition table. This table gives the 
+	  offsets and lengths of the user defined partitions.
+
+	  If you need code which can detect and parse these tables, and
+	  register MTD 'partitions' corresponding to each image detected,
+	  enable this option.
+
+	  You will still need the parsing functions to be called by the driver
+	  for your particular device. It won't happen automatically.
+
 comment "User Modules And Translation Layers"
 
 config MTD_CHAR
Index: linux-2.6.23/drivers/mtd/Makefile
===================================================================
--- linux-2.6.23.orig/drivers/mtd/Makefile
+++ linux-2.6.23/drivers/mtd/Makefile
@@ -11,6 +11,7 @@ obj-$(CONFIG_MTD_CONCAT)	+= mtdconcat.o
 obj-$(CONFIG_MTD_REDBOOT_PARTS) += redboot.o
 obj-$(CONFIG_MTD_CMDLINE_PARTS) += cmdlinepart.o
 obj-$(CONFIG_MTD_AFS_PARTS)	+= afs.o
+obj-$(CONFIG_MTD_MYLOADER_PARTS) += myloader.o
 
 # 'Users' - code which presents functionality to userspace.
 obj-$(CONFIG_MTD_CHAR)		+= mtdchar.o
