Index: linux-2.6.23-rc7/include/net/xfrmudp.h
===================================================================
--- /dev/null	1970-01-01 00:00:00.000000000 +0000
+++ linux-2.6.23-rc7/include/net/xfrmudp.h	2007-10-02 00:58:05.000000000 +0800
@@ -0,0 +1,10 @@
+/*
+ * pointer to function for type that xfrm4_input wants, to permit
+ * decoupling of XFRM from udp.c
+ */
+#define HAVE_XFRM4_UDP_REGISTER
+
+typedef int (*xfrm4_rcv_encap_t)(struct sk_buff *skb, __u16 encap_type);
+extern int udp4_register_esp_rcvencap(xfrm4_rcv_encap_t func
+				      , xfrm4_rcv_encap_t *oldfunc);
+extern int udp4_unregister_esp_rcvencap(xfrm4_rcv_encap_t func);
Index: linux-2.6.23-rc7/net/ipv4/Kconfig
===================================================================
--- linux-2.6.23-rc7.orig/net/ipv4/Kconfig	2007-10-02 00:58:02.000000000 +0800
+++ linux-2.6.23-rc7/net/ipv4/Kconfig	2007-10-02 00:58:05.000000000 +0800
@@ -224,6 +224,12 @@
 	  Network), but can be distributed all over the Internet. If you want
 	  to do that, say Y here and to "IP multicast routing" below.
 
+config IPSEC_NAT_TRAVERSAL
+	bool "IPSEC NAT-Traversal (KLIPS compatible)"
+	depends on INET
+	---help---
+          Includes support for RFC3947/RFC3948 NAT-Traversal of ESP over UDP.
+
 config IP_MROUTE
 	bool "IP: multicast routing"
 	depends on IP_MULTICAST
Index: linux-2.6.23-rc7/net/ipv4/xfrm4_input.c
===================================================================
--- linux-2.6.23-rc7.orig/net/ipv4/xfrm4_input.c	2007-10-02 00:58:02.000000000 +0800
+++ linux-2.6.23-rc7/net/ipv4/xfrm4_input.c	2007-10-02 00:58:33.000000000 +0800
@@ -15,6 +15,7 @@
 #include <linux/netfilter_ipv4.h>
 #include <net/ip.h>
 #include <net/xfrm.h>
+#include <net/xfrmudp.h>
 
 static int xfrm4_parse_spi(struct sk_buff *skb, u8 nexthdr, __be32 *spi, __be32 *seq)
 {
@@ -161,6 +162,29 @@
 	return 0;
 }
 
+#ifdef CONFIG_IPSEC_NAT_TRAVERSAL
+static xfrm4_rcv_encap_t xfrm4_rcv_encap_func = NULL;
+
+int udp4_register_esp_rcvencap(xfrm4_rcv_encap_t func,
+			       xfrm4_rcv_encap_t *oldfunc)
+{
+	if(oldfunc != NULL)
+		*oldfunc = xfrm4_rcv_encap_func;
+
+	xfrm4_rcv_encap_func = func;
+	return 0;
+}
+
+int udp4_unregister_esp_rcvencap(xfrm4_rcv_encap_t func)
+{
+	if(xfrm4_rcv_encap_func != func)
+		return -1;
+
+	xfrm4_rcv_encap_func = NULL;
+	return 0;
+}
+#endif /* CONFIG_IPSEC_NAT_TRAVERSAL */
+
 /* If it's a keepalive packet, then just eat it.
  * If it's an encapsulated packet, then pass it to the
  * IPsec xfrm input.
@@ -251,7 +275,13 @@
 	iph->protocol = IPPROTO_ESP;
 
 	/* process ESP */
+#ifdef CONFIG_IPSEC_NAT_TRAVERSAL
+	if(xfrm4_rcv_encap_func == NULL)
+		goto drop;
+	ret = (*xfrm4_rcv_encap_func)(skb, up->encap_type);
+#else
 	ret = xfrm4_rcv_encap(skb, encap_type);
+#endif
 	return ret;
 
 drop:
@@ -265,3 +295,8 @@
 }
 
 EXPORT_SYMBOL(xfrm4_rcv);
+
+#ifdef CONFIG_IPSEC_NAT_TRAVERSAL
+EXPORT_SYMBOL(udp4_register_esp_rcvencap);
+EXPORT_SYMBOL(udp4_unregister_esp_rcvencap);
+#endif
