diff -urN linux-2.6.19/arch/mips/Kconfig linux-2.6.19.new/arch/mips/Kconfig
--- linux-2.6.19/arch/mips/Kconfig	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/Kconfig	2006-12-16 18:46:31.000000000 +0100
@@ -4,6 +4,10 @@
 	# Horrible source of confusion.  Die, die, die ...
 	select EMBEDDED
 
+config CFE
+       bool
+       # Common Firmware Environment
+
 mainmenu "Linux/MIPS Kernel Configuration"
 
 menu "Machine selection"
@@ -15,6 +15,18 @@
 	prompt "System type"
 	default SGI_IP22
 
+config BCM963XX 
+	bool "Support for Broadcom BCM963xx SoC"
+	select SYS_SUPPORTS_32BIT_KERNEL
+	select SYS_SUPPORTS_BIG_ENDIAN
+	select SYS_HAS_CPU_MIPS32_R1
+	select HW_HAS_PCI
+	select DMA_NONCOHERENT
+	select IRQ_CPU
+	select CFE
+	help
+	 This is a fmaily of boards based on the Broadcom MIPS32
+
 config MACH_ALCHEMY
 	bool "Alchemy processor based machines"
 
diff -urN linux-2.6.19/arch/mips/Makefile linux-2.6.19.new/arch/mips/Makefile
--- linux-2.6.19/arch/mips/Makefile	2006-12-16 17:36:29.000000000 +0100
+++ linux-2.6.19.new/arch/mips/Makefile	2006-12-16 18:46:31.000000000 +0100
@@ -158,6 +158,19 @@
 #
 
 #
+# Broadcom BCM963xx SoC
+#
+core-$(CONFIG_BCM963XX)	+= arch/mips/bcm963xx/
+cflags-$(CONFIG_BCM963XX)     	+= -Iinclude/asm-mips/mach-bcm963xx
+load-$(CONFIG_BCM963XX)	+= 0xffffffff80010000
+
+
+#
+# Common Firmware Environment
+#
+core-$(CONFIG_CFE)             += arch/mips/cfe/
+
+#
 # Acer PICA 61, Mips Magnum 4000 and Olivetti M700.
 #
 core-$(CONFIG_MACH_JAZZ)	+= arch/mips/jazz/
diff -urN linux-2.6.19/arch/mips/kernel/cpu-probe.c linux-2.6.19.new/arch/mips/kernel/cpu-probe.c
--- linux-2.6.19/arch/mips/kernel/cpu-probe.c	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/kernel/cpu-probe.c	2006-12-16 18:46:31.000000000 +0100
@@ -590,6 +590,28 @@
 		return;
 }
 
+static inline void cpu_probe_broadcom(struct cpuinfo_mips *c)
+{
+       decode_configs(c);
+       switch (c->processor_id & 0xff00) {
+       case PRID_IMP_BCM6338:
+               c->cputype = CPU_BCM6338;
+               break;
+       case PRID_IMP_BCM6345:
+               c->cputype = CPU_BCM6345;
+               break;
+       case PRID_IMP_BCM6348:
+               c->cputype = CPU_BCM6348;
+               break;
+	case PRID_IMP_BCM6358:
+		c->cputype = CPU_BCM6358;
+		break;
+       default:
+               c->cputype = CPU_UNKNOWN;
+               break;
+       }
+}
+
 static inline void cpu_probe_mips(struct cpuinfo_mips *c)
 {
 	decode_configs(c);
@@ -724,6 +743,9 @@
 	case PRID_COMP_LEGACY:
 		cpu_probe_legacy(c);
 		break;
+        case PRID_COMP_BROADCOM:
+                cpu_probe_broadcom(c);
+                break;
 	case PRID_COMP_MIPS:
 		cpu_probe_mips(c);
 		break;
diff -urN linux-2.6.19/arch/mips/kernel/proc.c linux-2.6.19.new/arch/mips/kernel/proc.c
--- linux-2.6.19/arch/mips/kernel/proc.c	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/kernel/proc.c	2006-12-16 18:46:31.000000000 +0100
@@ -84,6 +84,10 @@
 	[CPU_VR4181A]	= "NEC VR4181A",
 	[CPU_SR71000]	= "Sandcraft SR71000",
 	[CPU_PR4450]	= "Philips PR4450",
+	[CPU_BCM6338]   = "BCM6338",
+	[CPU_BCM6345]   = "BCM6345",
+	[CPU_BCM6348]   = "BCM6348",
+	[CPU_BCM6358]	= "BCM6358",
 };
 
 
diff -urN linux-2.6.19/arch/mips/mm/c-r4k.c linux-2.6.19.new/arch/mips/mm/c-r4k.c
--- linux-2.6.19/arch/mips/mm/c-r4k.c	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/mm/c-r4k.c	2006-12-16 18:46:31.000000000 +0100
@@ -852,6 +852,13 @@
 		if (!(config & MIPS_CONF_M))
 			panic("Don't know how to probe P-caches on this cpu.");
 
+		if (c->cputype == CPU_BCM6338 || c->cputype == CPU_BCM6345 || c->cputype == CPU_BCM6348 || c->cputype == CPU_BCM6358)
+		{
+			printk("bcm963xx: enabling icache and dcache...\n");
+			/* Enable caches */
+			write_c0_diag(read_c0_diag() | 0xC0000000);
+		}
+
 		/*
 		 * So we seem to be a MIPS32 or MIPS64 CPU
 		 * So let's probe the I-cache ...
diff -urN linux-2.6.19/arch/mips/mm/tlbex.c linux-2.6.19.new/arch/mips/mm/tlbex.c
--- linux-2.6.19/arch/mips/mm/tlbex.c	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/mm/tlbex.c	2006-12-16 18:46:31.000000000 +0100
@@ -892,6 +892,10 @@
 	case CPU_4KSC:
 	case CPU_20KC:
 	case CPU_25KF:
+	case CPU_BCM6338:
+	case CPU_BCM6345:
+	case CPU_BCM6348:
+	case CPU_BCM6358:
 		tlbw(p);
 		break;
 
diff -urN linux-2.6.19/arch/mips/pci/Makefile linux-2.6.19.new/arch/mips/pci/Makefile
--- linux-2.6.19/arch/mips/pci/Makefile	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/arch/mips/pci/Makefile	2006-12-16 18:48:18.000000000 +0100
@@ -16,6 +16,7 @@
 obj-$(CONFIG_PCI_VR41XX)	+= ops-vr41xx.o pci-vr41xx.o
 obj-$(CONFIG_NEC_CMBVR4133)	+= fixup-vr4133.o
 obj-$(CONFIG_MARKEINS)		+= ops-emma2rh.o pci-emma2rh.o fixup-emma2rh.o
+obj-$(CONFIG_BCM963XX)		+= fixup-bcm96348.o pci-bcm96348.o ops-bcm96348.o
 
 #
 # These are still pretty much in the old state, watch, go blind.
diff -urN linux-2.6.19/include/asm-mips/bootinfo.h linux-2.6.19.new/include/asm-mips/bootinfo.h
--- linux-2.6.19/include/asm-mips/bootinfo.h	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/include/asm-mips/bootinfo.h	2006-12-16 18:46:31.000000000 +0100
@@ -213,6 +213,15 @@
 #define MACH_GROUP_NEC_EMMA2RH 25	/* NEC EMMA2RH (was 23)		*/
 #define  MACH_NEC_MARKEINS	0	/* NEC EMMA2RH Mark-eins	*/
 
+/*
+ * Valid machtype for group BRCM
+ */
+#define MACH_GROUP_BRCM        23      /* Broadcom boards              */
+#define MACH_BCM96338          0
+#define MACH_BCM96345          1
+#define MACH_BCM96348          2
+#define MACH_BCM96358		3
+
 #define CL_SIZE			COMMAND_LINE_SIZE
 
 const char *get_system_type(void);
diff -urN linux-2.6.19/include/asm-mips/cpu.h linux-2.6.19.new/include/asm-mips/cpu.h
--- linux-2.6.19/include/asm-mips/cpu.h	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/include/asm-mips/cpu.h	2006-12-16 18:46:31.000000000 +0100
@@ -103,6 +103,14 @@
 
 #define PRID_IMP_SR71000        0x0400
 
+/* These are the PRID's for when 23:16 == PRID_COMP_BROADCOM
+ */
+
+#define PRID_IMP_BCM6338       	0x9000
+#define PRID_IMP_BCM6345       	0x8000
+#define PRID_IMP_BCM6348       	0x9100
+#define PRID_IMP_BCM6358		0xA000
+
 /*
  * Definitions for 7:0 on legacy processors
  */
@@ -200,7 +207,11 @@
 #define CPU_SB1A		62
 #define CPU_74K			63
 #define CPU_R14000		64
-#define CPU_LAST		64
+#define CPU_BCM6338             65
+#define CPU_BCM6345             66
+#define CPU_BCM6348             67
+#define CPU_BCM6358		 68	
+#define CPU_LAST		68
 
 /*
  * ISA Level encodings
diff -urN linux-2.6.19/include/asm-mips/module.h linux-2.6.19.new/include/asm-mips/module.h
--- linux-2.6.19/include/asm-mips/module.h	2006-11-29 22:57:37.000000000 +0100
+++ linux-2.6.19.new/include/asm-mips/module.h	2006-12-16 19:03:22.000000000 +0100
@@ -112,6 +112,14 @@
 #define MODULE_PROC_FAMILY "RM9000 "
 #elif defined CONFIG_CPU_SB1
 #define MODULE_PROC_FAMILY "SB1 "
+#elif defined CONFIG_CPU_BCM6338
+#define MODULE_PROC_FAMILY "BCM6338 "
+#elif defined CONFIG_CPU_BCM6345
+#define MODULE_PROC_FAMILY "BCM6345 "
+#elif defined CONFIG_CPU_BCM6348
+#define MODULE_PROC_FAMILY "BCM6348 "
+#elif defined CONFIG_CPU_BCM6358
+#define MODULE_PROC_FAMILY "BCM6358 "
 #else
 #error MODULE_PROC_FAMILY undefined for your processor configuration
 #endif
