diff -urN linux-2.6.22-rc5/arch/arm/boot/compressed/head-at91rm9200.S linux-2.6.22-rc5.new/arch/arm/boot/compressed/head-at91rm9200.S
--- linux-2.6.22-rc5/arch/arm/boot/compressed/head-at91rm9200.S	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/boot/compressed/head-at91rm9200.S	2007-07-29 05:23:04.000000000 +0200
@@ -73,6 +73,12 @@
 		cmp	r7, r3
 		beq	99f
 
+		@ Promwad Chub : 1181
+		mov	r3,	#(MACH_TYPE_CHUB & 0xff)
+		orr	r3, r3, #(MACH_TYPE_CHUB & 0xff00)
+		cmp	r7, r3
+		beq	99f
+
 		@ Unknown board, use the AT91RM9200DK board
 		@ mov	r7, #MACH_TYPE_AT91RM9200
 		mov	r7,	#(MACH_TYPE_AT91RM9200DK & 0xff)
diff -urN linux-2.6.22-rc5/arch/arm/configs/at91sam9260ek_defconfig linux-2.6.22-rc5.new/arch/arm/configs/at91sam9260ek_defconfig
--- linux-2.6.22-rc5/arch/arm/configs/at91sam9260ek_defconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/configs/at91sam9260ek_defconfig	2007-07-29 05:23:04.000000000 +0200
@@ -1,18 +1,24 @@
 #
 # Automatically generated make config: don't edit
-# Linux kernel version: 2.6.19-rc6
-# Fri Nov 17 18:42:21 2006
+# Linux kernel version: 2.6.21
+# Mon May  7 11:42:02 2007
 #
 CONFIG_ARM=y
+CONFIG_SYS_SUPPORTS_APM_EMULATION=y
+CONFIG_GENERIC_GPIO=y
 # CONFIG_GENERIC_TIME is not set
 CONFIG_MMU=y
+# CONFIG_NO_IOPORT is not set
 CONFIG_GENERIC_HARDIRQS=y
 CONFIG_TRACE_IRQFLAGS_SUPPORT=y
 CONFIG_HARDIRQS_SW_RESEND=y
 CONFIG_GENERIC_IRQ_PROBE=y
 CONFIG_RWSEM_GENERIC_SPINLOCK=y
+# CONFIG_ARCH_HAS_ILOG2_U32 is not set
+# CONFIG_ARCH_HAS_ILOG2_U64 is not set
 CONFIG_GENERIC_HWEIGHT=y
 CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_ZONE_DMA=y
 CONFIG_VECTORS_BASE=0xffff0000
 CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
 
@@ -31,13 +37,16 @@
 # CONFIG_SWAP is not set
 CONFIG_SYSVIPC=y
 # CONFIG_IPC_NS is not set
+CONFIG_SYSVIPC_SYSCTL=y
 # CONFIG_POSIX_MQUEUE is not set
 # CONFIG_BSD_PROCESS_ACCT is not set
 # CONFIG_TASKSTATS is not set
 # CONFIG_UTS_NS is not set
 # CONFIG_AUDIT is not set
 # CONFIG_IKCONFIG is not set
+CONFIG_SYSFS_DEPRECATED=y
 # CONFIG_RELAY is not set
+CONFIG_BLK_DEV_INITRD=y
 CONFIG_INITRAMFS_SOURCE=""
 CONFIG_CC_OPTIMIZE_FOR_SIZE=y
 CONFIG_SYSCTL=y
@@ -76,7 +85,9 @@
 # Block layer
 #
 CONFIG_BLOCK=y
+# CONFIG_LBD is not set
 # CONFIG_BLK_DEV_IO_TRACE is not set
+# CONFIG_LSF is not set
 
 #
 # IO Schedulers
@@ -110,10 +121,12 @@
 # CONFIG_ARCH_IMX is not set
 # CONFIG_ARCH_IOP32X is not set
 # CONFIG_ARCH_IOP33X is not set
+# CONFIG_ARCH_IOP13XX is not set
 # CONFIG_ARCH_IXP4XX is not set
 # CONFIG_ARCH_IXP2000 is not set
 # CONFIG_ARCH_IXP23XX is not set
 # CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_NS9XXX is not set
 # CONFIG_ARCH_PNX4008 is not set
 # CONFIG_ARCH_PXA is not set
 # CONFIG_ARCH_RPC is not set
@@ -129,21 +142,29 @@
 # CONFIG_ARCH_AT91RM9200 is not set
 CONFIG_ARCH_AT91SAM9260=y
 # CONFIG_ARCH_AT91SAM9261 is not set
+# CONFIG_ARCH_AT91SAM9263 is not set
+
+#
+# AT91SAM9260 Variants
+#
+# CONFIG_ARCH_AT91SAM9260_SAM9XE is not set
 
 #
-# AT91SAM9260 Board Type
+# AT91SAM9260 / AT91SAM9XE Board Type
 #
 CONFIG_MACH_AT91SAM9260EK=y
 
 #
 # AT91 Board Options
 #
+# CONFIG_MTD_AT91_DATAFLASH_CARD is not set
 # CONFIG_MTD_NAND_AT91_BUSWIDTH_16 is not set
 
 #
 # AT91 Feature Selections
 #
 # CONFIG_AT91_PROGRAMMABLE_CLOCKS is not set
+# CONFIG_ATMEL_TCLIB is not set
 
 #
 # Processor Type
@@ -166,6 +187,7 @@
 # CONFIG_CPU_DCACHE_DISABLE is not set
 # CONFIG_CPU_DCACHE_WRITETHROUGH is not set
 # CONFIG_CPU_CACHE_ROUND_ROBIN is not set
+# CONFIG_OUTER_CACHE is not set
 
 #
 # Bus support
@@ -193,6 +215,7 @@
 # CONFIG_SPARSEMEM_STATIC is not set
 CONFIG_SPLIT_PTLOCK_CPUS=4096
 # CONFIG_RESOURCES_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=1
 # CONFIG_LEDS is not set
 CONFIG_ALIGNMENT_TRAP=y
 
@@ -203,6 +226,7 @@
 CONFIG_ZBOOT_ROM_BSS=0x0
 CONFIG_CMDLINE="mem=64M console=ttyS0,115200 initrd=0x21100000,3145728 root=/dev/ram0 rw"
 # CONFIG_XIP_KERNEL is not set
+# CONFIG_KEXEC is not set
 
 #
 # Floating point emulation
@@ -228,7 +252,6 @@
 # Power management options
 #
 # CONFIG_PM is not set
-# CONFIG_APM is not set
 
 #
 # Networking
@@ -242,9 +265,6 @@
 CONFIG_PACKET=y
 # CONFIG_PACKET_MMAP is not set
 CONFIG_UNIX=y
-CONFIG_XFRM=y
-# CONFIG_XFRM_USER is not set
-# CONFIG_XFRM_SUB_POLICY is not set
 # CONFIG_NET_KEY is not set
 CONFIG_INET=y
 # CONFIG_IP_MULTICAST is not set
@@ -263,14 +283,15 @@
 # CONFIG_INET_IPCOMP is not set
 # CONFIG_INET_XFRM_TUNNEL is not set
 # CONFIG_INET_TUNNEL is not set
-CONFIG_INET_XFRM_MODE_TRANSPORT=y
-CONFIG_INET_XFRM_MODE_TUNNEL=y
-CONFIG_INET_XFRM_MODE_BEET=y
+# CONFIG_INET_XFRM_MODE_TRANSPORT is not set
+# CONFIG_INET_XFRM_MODE_TUNNEL is not set
+# CONFIG_INET_XFRM_MODE_BEET is not set
 CONFIG_INET_DIAG=y
 CONFIG_INET_TCP_DIAG=y
 # CONFIG_TCP_CONG_ADVANCED is not set
 CONFIG_TCP_CONG_CUBIC=y
 CONFIG_DEFAULT_TCP_CONG="cubic"
+# CONFIG_TCP_MD5SIG is not set
 # CONFIG_IPV6 is not set
 # CONFIG_INET6_XFRM_TUNNEL is not set
 # CONFIG_INET6_TUNNEL is not set
@@ -328,6 +349,7 @@
 CONFIG_PREVENT_FIRMWARE_BUILD=y
 # CONFIG_FW_LOADER is not set
 # CONFIG_DEBUG_DRIVER is not set
+# CONFIG_DEBUG_DEVRES is not set
 # CONFIG_SYS_HYPERVISOR is not set
 
 #
@@ -348,6 +370,7 @@
 #
 # Plug and Play support
 #
+# CONFIG_PNPACPI is not set
 
 #
 # Block devices
@@ -360,7 +383,6 @@
 CONFIG_BLK_DEV_RAM_COUNT=16
 CONFIG_BLK_DEV_RAM_SIZE=8192
 CONFIG_BLK_DEV_RAM_BLOCKSIZE=1024
-CONFIG_BLK_DEV_INITRD=y
 # CONFIG_CDROM_PKTCDVD is not set
 # CONFIG_ATA_OVER_ETH is not set
 
@@ -369,6 +391,7 @@
 #
 # CONFIG_RAID_ATTRS is not set
 CONFIG_SCSI=y
+# CONFIG_SCSI_TGT is not set
 # CONFIG_SCSI_NETLINK is not set
 CONFIG_SCSI_PROC_FS=y
 
@@ -388,6 +411,7 @@
 CONFIG_SCSI_MULTI_LUN=y
 # CONFIG_SCSI_CONSTANTS is not set
 # CONFIG_SCSI_LOGGING is not set
+# CONFIG_SCSI_SCAN_ASYNC is not set
 
 #
 # SCSI Transports
@@ -405,6 +429,11 @@
 # CONFIG_SCSI_DEBUG is not set
 
 #
+# Serial ATA (prod) and Parallel ATA (experimental) drivers
+#
+# CONFIG_ATA is not set
+
+#
 # Multi-device support (RAID and LVM)
 #
 # CONFIG_MD is not set
@@ -425,7 +454,51 @@
 #
 # Network device support
 #
-# CONFIG_NETDEVICES is not set
+CONFIG_NETDEVICES=y
+# CONFIG_DUMMY is not set
+# CONFIG_BONDING is not set
+# CONFIG_EQUALIZER is not set
+# CONFIG_TUN is not set
+
+#
+# PHY device support
+#
+# CONFIG_PHYLIB is not set
+
+#
+# Ethernet (10 or 100Mbit)
+#
+CONFIG_NET_ETHERNET=y
+CONFIG_MII=y
+CONFIG_MACB=y
+# CONFIG_SMC91X is not set
+# CONFIG_DM9000 is not set
+
+#
+# Ethernet (1000 Mbit)
+#
+
+#
+# Ethernet (10000 Mbit)
+#
+
+#
+# Token Ring devices
+#
+
+#
+# Wireless LAN (non-hamradio)
+#
+# CONFIG_NET_RADIO is not set
+
+#
+# Wan interfaces
+#
+# CONFIG_WAN is not set
+# CONFIG_PPP is not set
+# CONFIG_SLIP is not set
+# CONFIG_SHAPER is not set
+# CONFIG_NETCONSOLE is not set
 # CONFIG_NETPOLL is not set
 # CONFIG_NET_POLL_CONTROLLER is not set
 
@@ -517,10 +590,6 @@
 # CONFIG_NVRAM is not set
 # CONFIG_DTLK is not set
 # CONFIG_R3964 is not set
-
-#
-# Ftape, the floppy tape device driver
-#
 # CONFIG_RAW_DRIVER is not set
 
 #
@@ -553,7 +622,11 @@
 #
 # Misc devices
 #
-# CONFIG_TIFM_CORE is not set
+
+#
+# Multifunction device drivers
+#
+# CONFIG_MFD_SM501 is not set
 
 #
 # LED devices
@@ -582,7 +655,7 @@
 #
 # Graphics support
 #
-# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 # CONFIG_FB is not set
 
 #
@@ -590,7 +663,6 @@
 #
 # CONFIG_VGA_CONSOLE is not set
 CONFIG_DUMMY_CONSOLE=y
-# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 
 #
 # Sound
@@ -598,6 +670,12 @@
 # CONFIG_SOUND is not set
 
 #
+# HID Devices
+#
+CONFIG_HID=y
+# CONFIG_HID_DEBUG is not set
+
+#
 # USB support
 #
 CONFIG_USB_ARCH_HAS_HCD=y
@@ -610,7 +688,6 @@
 # Miscellaneous USB options
 #
 CONFIG_USB_DEVICEFS=y
-# CONFIG_USB_BANDWIDTH is not set
 # CONFIG_USB_DYNAMIC_MINORS is not set
 # CONFIG_USB_OTG is not set
 
@@ -619,7 +696,8 @@
 #
 # CONFIG_USB_ISP116X_HCD is not set
 CONFIG_USB_OHCI_HCD=y
-# CONFIG_USB_OHCI_BIG_ENDIAN is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_DESC is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_MMIO is not set
 CONFIG_USB_OHCI_LITTLE_ENDIAN=y
 # CONFIG_USB_SL811_HCD is not set
 
@@ -671,6 +749,7 @@
 # CONFIG_USB_ATI_REMOTE2 is not set
 # CONFIG_USB_KEYSPAN_REMOTE is not set
 # CONFIG_USB_APPLETOUCH is not set
+# CONFIG_USB_GTCO is not set
 
 #
 # USB Imaging devices
@@ -708,6 +787,7 @@
 # CONFIG_USB_RIO500 is not set
 # CONFIG_USB_LEGOTOWER is not set
 # CONFIG_USB_LCD is not set
+# CONFIG_USB_BERRY_CHARGE is not set
 # CONFIG_USB_LED is not set
 # CONFIG_USB_CYPRESS_CY7C63 is not set
 # CONFIG_USB_CYTHERM is not set
@@ -717,6 +797,7 @@
 # CONFIG_USB_APPLEDISPLAY is not set
 # CONFIG_USB_LD is not set
 # CONFIG_USB_TRANCEVIBRATOR is not set
+# CONFIG_USB_IOWARRIOR is not set
 # CONFIG_USB_TEST is not set
 
 #
@@ -889,6 +970,11 @@
 # CONFIG_NLS_UTF8 is not set
 
 #
+# Distributed Lock Manager
+#
+# CONFIG_DLM is not set
+
+#
 # Profiling support
 #
 # CONFIG_PROFILING is not set
@@ -900,28 +986,30 @@
 CONFIG_ENABLE_MUST_CHECK=y
 # CONFIG_MAGIC_SYSRQ is not set
 # CONFIG_UNUSED_SYMBOLS is not set
+# CONFIG_DEBUG_FS is not set
+# CONFIG_HEADERS_CHECK is not set
 CONFIG_DEBUG_KERNEL=y
+# CONFIG_DEBUG_SHIRQ is not set
 CONFIG_LOG_BUF_SHIFT=14
 CONFIG_DETECT_SOFTLOCKUP=y
 # CONFIG_SCHEDSTATS is not set
+# CONFIG_TIMER_STATS is not set
 # CONFIG_DEBUG_SLAB is not set
 # CONFIG_DEBUG_RT_MUTEXES is not set
 # CONFIG_RT_MUTEX_TESTER is not set
 # CONFIG_DEBUG_SPINLOCK is not set
 # CONFIG_DEBUG_MUTEXES is not set
-# CONFIG_DEBUG_RWSEMS is not set
 # CONFIG_DEBUG_SPINLOCK_SLEEP is not set
 # CONFIG_DEBUG_LOCKING_API_SELFTESTS is not set
 # CONFIG_DEBUG_KOBJECT is not set
 CONFIG_DEBUG_BUGVERBOSE=y
 # CONFIG_DEBUG_INFO is not set
-# CONFIG_DEBUG_FS is not set
 # CONFIG_DEBUG_VM is not set
 # CONFIG_DEBUG_LIST is not set
 CONFIG_FRAME_POINTER=y
 CONFIG_FORCED_INLINING=y
-# CONFIG_HEADERS_CHECK is not set
 # CONFIG_RCU_TORTURE_TEST is not set
+# CONFIG_FAULT_INJECTION is not set
 CONFIG_DEBUG_USER=y
 # CONFIG_DEBUG_ERRORS is not set
 CONFIG_DEBUG_LL=y
@@ -941,9 +1029,12 @@
 #
 # Library routines
 #
+CONFIG_BITREVERSE=y
 # CONFIG_CRC_CCITT is not set
 # CONFIG_CRC16 is not set
 CONFIG_CRC32=y
 # CONFIG_LIBCRC32C is not set
 CONFIG_ZLIB_INFLATE=y
 CONFIG_PLIST=y
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_IOPORT=y
diff -urN linux-2.6.22-rc5/arch/arm/configs/at91sam9261ek_defconfig linux-2.6.22-rc5.new/arch/arm/configs/at91sam9261ek_defconfig
--- linux-2.6.22-rc5/arch/arm/configs/at91sam9261ek_defconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/configs/at91sam9261ek_defconfig	2007-07-29 05:23:04.000000000 +0200
@@ -1,18 +1,24 @@
 #
 # Automatically generated make config: don't edit
-# Linux kernel version: 2.6.19-rc6
-# Fri Nov 17 18:00:38 2006
+# Linux kernel version: 2.6.21
+# Mon May  7 11:42:30 2007
 #
 CONFIG_ARM=y
+CONFIG_SYS_SUPPORTS_APM_EMULATION=y
+CONFIG_GENERIC_GPIO=y
 # CONFIG_GENERIC_TIME is not set
 CONFIG_MMU=y
+# CONFIG_NO_IOPORT is not set
 CONFIG_GENERIC_HARDIRQS=y
 CONFIG_TRACE_IRQFLAGS_SUPPORT=y
 CONFIG_HARDIRQS_SW_RESEND=y
 CONFIG_GENERIC_IRQ_PROBE=y
 CONFIG_RWSEM_GENERIC_SPINLOCK=y
+# CONFIG_ARCH_HAS_ILOG2_U32 is not set
+# CONFIG_ARCH_HAS_ILOG2_U64 is not set
 CONFIG_GENERIC_HWEIGHT=y
 CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_ZONE_DMA=y
 CONFIG_VECTORS_BASE=0xffff0000
 CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
 
@@ -31,13 +37,16 @@
 # CONFIG_SWAP is not set
 CONFIG_SYSVIPC=y
 # CONFIG_IPC_NS is not set
+CONFIG_SYSVIPC_SYSCTL=y
 # CONFIG_POSIX_MQUEUE is not set
 # CONFIG_BSD_PROCESS_ACCT is not set
 # CONFIG_TASKSTATS is not set
 # CONFIG_UTS_NS is not set
 # CONFIG_AUDIT is not set
 # CONFIG_IKCONFIG is not set
+CONFIG_SYSFS_DEPRECATED=y
 # CONFIG_RELAY is not set
+CONFIG_BLK_DEV_INITRD=y
 CONFIG_INITRAMFS_SOURCE=""
 CONFIG_CC_OPTIMIZE_FOR_SIZE=y
 CONFIG_SYSCTL=y
@@ -76,7 +85,9 @@
 # Block layer
 #
 CONFIG_BLOCK=y
+# CONFIG_LBD is not set
 # CONFIG_BLK_DEV_IO_TRACE is not set
+# CONFIG_LSF is not set
 
 #
 # IO Schedulers
@@ -110,10 +121,12 @@
 # CONFIG_ARCH_IMX is not set
 # CONFIG_ARCH_IOP32X is not set
 # CONFIG_ARCH_IOP33X is not set
+# CONFIG_ARCH_IOP13XX is not set
 # CONFIG_ARCH_IXP4XX is not set
 # CONFIG_ARCH_IXP2000 is not set
 # CONFIG_ARCH_IXP23XX is not set
 # CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_NS9XXX is not set
 # CONFIG_ARCH_PNX4008 is not set
 # CONFIG_ARCH_PXA is not set
 # CONFIG_ARCH_RPC is not set
@@ -129,6 +142,7 @@
 # CONFIG_ARCH_AT91RM9200 is not set
 # CONFIG_ARCH_AT91SAM9260 is not set
 CONFIG_ARCH_AT91SAM9261=y
+# CONFIG_ARCH_AT91SAM9263 is not set
 
 #
 # AT91SAM9261 Board Type
@@ -138,12 +152,14 @@
 #
 # AT91 Board Options
 #
+# CONFIG_MTD_AT91_DATAFLASH_CARD is not set
 # CONFIG_MTD_NAND_AT91_BUSWIDTH_16 is not set
 
 #
 # AT91 Feature Selections
 #
 # CONFIG_AT91_PROGRAMMABLE_CLOCKS is not set
+# CONFIG_ATMEL_TCLIB is not set
 
 #
 # Processor Type
@@ -166,6 +182,7 @@
 # CONFIG_CPU_DCACHE_DISABLE is not set
 # CONFIG_CPU_DCACHE_WRITETHROUGH is not set
 # CONFIG_CPU_CACHE_ROUND_ROBIN is not set
+# CONFIG_OUTER_CACHE is not set
 
 #
 # Bus support
@@ -193,6 +210,7 @@
 # CONFIG_SPARSEMEM_STATIC is not set
 CONFIG_SPLIT_PTLOCK_CPUS=4096
 # CONFIG_RESOURCES_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=1
 # CONFIG_LEDS is not set
 CONFIG_ALIGNMENT_TRAP=y
 
@@ -203,6 +221,7 @@
 CONFIG_ZBOOT_ROM_BSS=0x0
 CONFIG_CMDLINE="mem=64M console=ttyS0,115200 initrd=0x21100000,3145728 root=/dev/ram0 rw"
 # CONFIG_XIP_KERNEL is not set
+# CONFIG_KEXEC is not set
 
 #
 # Floating point emulation
@@ -228,7 +247,6 @@
 # Power management options
 #
 # CONFIG_PM is not set
-# CONFIG_APM is not set
 
 #
 # Networking
@@ -245,6 +263,7 @@
 CONFIG_XFRM=y
 # CONFIG_XFRM_USER is not set
 # CONFIG_XFRM_SUB_POLICY is not set
+# CONFIG_XFRM_MIGRATE is not set
 # CONFIG_NET_KEY is not set
 CONFIG_INET=y
 # CONFIG_IP_MULTICAST is not set
@@ -271,6 +290,7 @@
 # CONFIG_TCP_CONG_ADVANCED is not set
 CONFIG_TCP_CONG_CUBIC=y
 CONFIG_DEFAULT_TCP_CONG="cubic"
+# CONFIG_TCP_MD5SIG is not set
 # CONFIG_IPV6 is not set
 # CONFIG_INET6_XFRM_TUNNEL is not set
 # CONFIG_INET6_TUNNEL is not set
@@ -328,6 +348,7 @@
 CONFIG_PREVENT_FIRMWARE_BUILD=y
 # CONFIG_FW_LOADER is not set
 # CONFIG_DEBUG_DRIVER is not set
+# CONFIG_DEBUG_DEVRES is not set
 # CONFIG_SYS_HYPERVISOR is not set
 
 #
@@ -350,6 +371,7 @@
 # User Modules And Translation Layers
 #
 # CONFIG_MTD_CHAR is not set
+CONFIG_MTD_BLKDEVS=y
 CONFIG_MTD_BLOCK=y
 # CONFIG_FTL is not set
 # CONFIG_NFTL is not set
@@ -386,6 +408,8 @@
 #
 # Self-contained MTD device drivers
 #
+# CONFIG_MTD_DATAFLASH is not set
+# CONFIG_MTD_M25P80 is not set
 # CONFIG_MTD_SLRAM is not set
 # CONFIG_MTD_PHRAM is not set
 # CONFIG_MTD_MTDRAM is not set
@@ -422,6 +446,7 @@
 #
 # Plug and Play support
 #
+# CONFIG_PNPACPI is not set
 
 #
 # Block devices
@@ -434,7 +459,6 @@
 CONFIG_BLK_DEV_RAM_COUNT=16
 CONFIG_BLK_DEV_RAM_SIZE=8192
 CONFIG_BLK_DEV_RAM_BLOCKSIZE=1024
-CONFIG_BLK_DEV_INITRD=y
 # CONFIG_CDROM_PKTCDVD is not set
 # CONFIG_ATA_OVER_ETH is not set
 
@@ -443,6 +467,7 @@
 #
 # CONFIG_RAID_ATTRS is not set
 CONFIG_SCSI=y
+# CONFIG_SCSI_TGT is not set
 # CONFIG_SCSI_NETLINK is not set
 CONFIG_SCSI_PROC_FS=y
 
@@ -462,6 +487,7 @@
 CONFIG_SCSI_MULTI_LUN=y
 # CONFIG_SCSI_CONSTANTS is not set
 # CONFIG_SCSI_LOGGING is not set
+# CONFIG_SCSI_SCAN_ASYNC is not set
 
 #
 # SCSI Transports
@@ -479,6 +505,11 @@
 # CONFIG_SCSI_DEBUG is not set
 
 #
+# Serial ATA (prod) and Parallel ATA (experimental) drivers
+#
+# CONFIG_ATA is not set
+
+#
 # Multi-device support (RAID and LVM)
 #
 # CONFIG_MD is not set
@@ -575,7 +606,16 @@
 # CONFIG_INPUT_KEYBOARD is not set
 # CONFIG_INPUT_MOUSE is not set
 # CONFIG_INPUT_JOYSTICK is not set
-# CONFIG_INPUT_TOUCHSCREEN is not set
+CONFIG_INPUT_TOUCHSCREEN=y
+CONFIG_TOUCHSCREEN_ADS7846=y
+# CONFIG_TOUCHSCREEN_GUNZE is not set
+# CONFIG_TOUCHSCREEN_ELO is not set
+# CONFIG_TOUCHSCREEN_MTOUCH is not set
+# CONFIG_TOUCHSCREEN_MK712 is not set
+# CONFIG_TOUCHSCREEN_PENMOUNT is not set
+# CONFIG_TOUCHSCREEN_TOUCHRIGHT is not set
+# CONFIG_TOUCHSCREEN_TOUCHWIN is not set
+# CONFIG_TOUCHSCREEN_UCB1400 is not set
 # CONFIG_INPUT_MISC is not set
 
 #
@@ -634,10 +674,6 @@
 # CONFIG_NVRAM is not set
 # CONFIG_DTLK is not set
 # CONFIG_R3964 is not set
-
-#
-# Ftape, the floppy tape device driver
-#
 # CONFIG_RAW_DRIVER is not set
 
 #
@@ -662,6 +698,7 @@
 # I2C Hardware Bus support
 #
 CONFIG_I2C_AT91=y
+CONFIG_I2C_AT91_CLOCKRATE=100000
 # CONFIG_I2C_OCORES is not set
 # CONFIG_I2C_PARPORT_LIGHT is not set
 # CONFIG_I2C_STUB is not set
@@ -686,8 +723,20 @@
 #
 # SPI support
 #
-# CONFIG_SPI is not set
-# CONFIG_SPI_MASTER is not set
+CONFIG_SPI=y
+# CONFIG_SPI_DEBUG is not set
+CONFIG_SPI_MASTER=y
+
+#
+# SPI Master Controller Drivers
+#
+CONFIG_SPI_ATMEL=y
+# CONFIG_SPI_BITBANG is not set
+
+#
+# SPI Protocol Masters
+#
+# CONFIG_SPI_AT25 is not set
 
 #
 # Dallas's 1-wire bus
@@ -703,7 +752,11 @@
 #
 # Misc devices
 #
-# CONFIG_TIFM_CORE is not set
+
+#
+# Multifunction device drivers
+#
+# CONFIG_MFD_SM501 is not set
 
 #
 # LED devices
@@ -732,7 +785,7 @@
 #
 # Graphics support
 #
-# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 # CONFIG_FB is not set
 
 #
@@ -740,7 +793,6 @@
 #
 # CONFIG_VGA_CONSOLE is not set
 CONFIG_DUMMY_CONSOLE=y
-# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 
 #
 # Sound
@@ -748,6 +800,12 @@
 # CONFIG_SOUND is not set
 
 #
+# HID Devices
+#
+CONFIG_HID=y
+# CONFIG_HID_DEBUG is not set
+
+#
 # USB support
 #
 CONFIG_USB_ARCH_HAS_HCD=y
@@ -760,7 +818,6 @@
 # Miscellaneous USB options
 #
 CONFIG_USB_DEVICEFS=y
-# CONFIG_USB_BANDWIDTH is not set
 # CONFIG_USB_DYNAMIC_MINORS is not set
 # CONFIG_USB_OTG is not set
 
@@ -769,7 +826,8 @@
 #
 # CONFIG_USB_ISP116X_HCD is not set
 CONFIG_USB_OHCI_HCD=y
-# CONFIG_USB_OHCI_BIG_ENDIAN is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_DESC is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_MMIO is not set
 CONFIG_USB_OHCI_LITTLE_ENDIAN=y
 # CONFIG_USB_SL811_HCD is not set
 
@@ -821,6 +879,7 @@
 # CONFIG_USB_ATI_REMOTE2 is not set
 # CONFIG_USB_KEYSPAN_REMOTE is not set
 # CONFIG_USB_APPLETOUCH is not set
+# CONFIG_USB_GTCO is not set
 
 #
 # USB Imaging devices
@@ -858,6 +917,7 @@
 # CONFIG_USB_RIO500 is not set
 # CONFIG_USB_LEGOTOWER is not set
 # CONFIG_USB_LCD is not set
+# CONFIG_USB_BERRY_CHARGE is not set
 # CONFIG_USB_LED is not set
 # CONFIG_USB_CYPRESS_CY7C63 is not set
 # CONFIG_USB_CYTHERM is not set
@@ -867,6 +927,7 @@
 # CONFIG_USB_APPLEDISPLAY is not set
 # CONFIG_USB_LD is not set
 # CONFIG_USB_TRANCEVIBRATOR is not set
+# CONFIG_USB_IOWARRIOR is not set
 # CONFIG_USB_TEST is not set
 
 #
@@ -903,7 +964,6 @@
 # CONFIG_MMC_DEBUG is not set
 CONFIG_MMC_BLOCK=y
 CONFIG_MMC_AT91=m
-# CONFIG_MMC_TIFM_SD is not set
 
 #
 # Real Time Clock
@@ -973,7 +1033,6 @@
 # CONFIG_BEFS_FS is not set
 # CONFIG_BFS_FS is not set
 # CONFIG_EFS_FS is not set
-# CONFIG_JFFS_FS is not set
 # CONFIG_JFFS2_FS is not set
 CONFIG_CRAMFS=y
 # CONFIG_VXFS_FS is not set
@@ -1045,6 +1104,11 @@
 # CONFIG_NLS_UTF8 is not set
 
 #
+# Distributed Lock Manager
+#
+# CONFIG_DLM is not set
+
+#
 # Profiling support
 #
 # CONFIG_PROFILING is not set
@@ -1056,28 +1120,30 @@
 CONFIG_ENABLE_MUST_CHECK=y
 # CONFIG_MAGIC_SYSRQ is not set
 # CONFIG_UNUSED_SYMBOLS is not set
+# CONFIG_DEBUG_FS is not set
+# CONFIG_HEADERS_CHECK is not set
 CONFIG_DEBUG_KERNEL=y
+# CONFIG_DEBUG_SHIRQ is not set
 CONFIG_LOG_BUF_SHIFT=14
 CONFIG_DETECT_SOFTLOCKUP=y
 # CONFIG_SCHEDSTATS is not set
+# CONFIG_TIMER_STATS is not set
 # CONFIG_DEBUG_SLAB is not set
 # CONFIG_DEBUG_RT_MUTEXES is not set
 # CONFIG_RT_MUTEX_TESTER is not set
 # CONFIG_DEBUG_SPINLOCK is not set
 # CONFIG_DEBUG_MUTEXES is not set
-# CONFIG_DEBUG_RWSEMS is not set
 # CONFIG_DEBUG_SPINLOCK_SLEEP is not set
 # CONFIG_DEBUG_LOCKING_API_SELFTESTS is not set
 # CONFIG_DEBUG_KOBJECT is not set
 CONFIG_DEBUG_BUGVERBOSE=y
 # CONFIG_DEBUG_INFO is not set
-# CONFIG_DEBUG_FS is not set
 # CONFIG_DEBUG_VM is not set
 # CONFIG_DEBUG_LIST is not set
 CONFIG_FRAME_POINTER=y
 CONFIG_FORCED_INLINING=y
-# CONFIG_HEADERS_CHECK is not set
 # CONFIG_RCU_TORTURE_TEST is not set
+# CONFIG_FAULT_INJECTION is not set
 CONFIG_DEBUG_USER=y
 # CONFIG_DEBUG_ERRORS is not set
 CONFIG_DEBUG_LL=y
@@ -1097,9 +1163,12 @@
 #
 # Library routines
 #
+CONFIG_BITREVERSE=y
 # CONFIG_CRC_CCITT is not set
 # CONFIG_CRC16 is not set
 CONFIG_CRC32=y
 # CONFIG_LIBCRC32C is not set
 CONFIG_ZLIB_INFLATE=y
 CONFIG_PLIST=y
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_IOPORT=y
diff -urN linux-2.6.22-rc5/arch/arm/configs/at91sam9263ek_defconfig linux-2.6.22-rc5.new/arch/arm/configs/at91sam9263ek_defconfig
--- linux-2.6.22-rc5/arch/arm/configs/at91sam9263ek_defconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/configs/at91sam9263ek_defconfig	2007-07-29 05:23:04.000000000 +0200
@@ -1,11 +1,14 @@
 #
 # Automatically generated make config: don't edit
-# Linux kernel version: 2.6.20-rc1
-# Mon Jan  8 16:06:54 2007
+# Linux kernel version: 2.6.21
+# Mon May  7 11:42:49 2007
 #
 CONFIG_ARM=y
+CONFIG_SYS_SUPPORTS_APM_EMULATION=y
+CONFIG_GENERIC_GPIO=y
 # CONFIG_GENERIC_TIME is not set
 CONFIG_MMU=y
+# CONFIG_NO_IOPORT is not set
 CONFIG_GENERIC_HARDIRQS=y
 CONFIG_TRACE_IRQFLAGS_SUPPORT=y
 CONFIG_HARDIRQS_SW_RESEND=y
@@ -15,6 +18,7 @@
 # CONFIG_ARCH_HAS_ILOG2_U64 is not set
 CONFIG_GENERIC_HWEIGHT=y
 CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_ZONE_DMA=y
 CONFIG_VECTORS_BASE=0xffff0000
 CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
 
@@ -33,6 +37,7 @@
 # CONFIG_SWAP is not set
 CONFIG_SYSVIPC=y
 # CONFIG_IPC_NS is not set
+CONFIG_SYSVIPC_SYSCTL=y
 # CONFIG_POSIX_MQUEUE is not set
 # CONFIG_BSD_PROCESS_ACCT is not set
 # CONFIG_TASKSTATS is not set
@@ -41,6 +46,7 @@
 # CONFIG_IKCONFIG is not set
 CONFIG_SYSFS_DEPRECATED=y
 # CONFIG_RELAY is not set
+CONFIG_BLK_DEV_INITRD=y
 CONFIG_INITRAMFS_SOURCE=""
 CONFIG_CC_OPTIMIZE_FOR_SIZE=y
 CONFIG_SYSCTL=y
@@ -120,6 +126,7 @@
 # CONFIG_ARCH_IXP2000 is not set
 # CONFIG_ARCH_IXP23XX is not set
 # CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_NS9XXX is not set
 # CONFIG_ARCH_PNX4008 is not set
 # CONFIG_ARCH_PXA is not set
 # CONFIG_ARCH_RPC is not set
@@ -152,6 +159,7 @@
 # AT91 Feature Selections
 #
 # CONFIG_AT91_PROGRAMMABLE_CLOCKS is not set
+# CONFIG_ATMEL_TCLIB is not set
 
 #
 # Processor Type
@@ -174,6 +182,7 @@
 # CONFIG_CPU_DCACHE_DISABLE is not set
 # CONFIG_CPU_DCACHE_WRITETHROUGH is not set
 # CONFIG_CPU_CACHE_ROUND_ROBIN is not set
+# CONFIG_OUTER_CACHE is not set
 
 #
 # Bus support
@@ -201,6 +210,7 @@
 # CONFIG_SPARSEMEM_STATIC is not set
 CONFIG_SPLIT_PTLOCK_CPUS=4096
 # CONFIG_RESOURCES_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=1
 # CONFIG_LEDS is not set
 CONFIG_ALIGNMENT_TRAP=y
 
@@ -211,6 +221,7 @@
 CONFIG_ZBOOT_ROM_BSS=0x0
 CONFIG_CMDLINE="mem=64M console=ttyS0,115200 initrd=0x21100000,3145728 root=/dev/ram0 rw"
 # CONFIG_XIP_KERNEL is not set
+# CONFIG_KEXEC is not set
 
 #
 # Floating point emulation
@@ -236,7 +247,6 @@
 # Power management options
 #
 # CONFIG_PM is not set
-# CONFIG_APM is not set
 
 #
 # Networking
@@ -333,6 +343,7 @@
 CONFIG_PREVENT_FIRMWARE_BUILD=y
 # CONFIG_FW_LOADER is not set
 # CONFIG_DEBUG_DRIVER is not set
+# CONFIG_DEBUG_DEVRES is not set
 # CONFIG_SYS_HYPERVISOR is not set
 
 #
@@ -430,6 +441,7 @@
 #
 # Plug and Play support
 #
+# CONFIG_PNPACPI is not set
 
 #
 # Block devices
@@ -443,7 +455,6 @@
 CONFIG_BLK_DEV_RAM_COUNT=16
 CONFIG_BLK_DEV_RAM_SIZE=8192
 CONFIG_BLK_DEV_RAM_BLOCKSIZE=1024
-CONFIG_BLK_DEV_INITRD=y
 # CONFIG_CDROM_PKTCDVD is not set
 # CONFIG_ATA_OVER_ETH is not set
 
@@ -531,6 +542,7 @@
 #
 CONFIG_NET_ETHERNET=y
 CONFIG_MII=y
+CONFIG_MACB=y
 # CONFIG_SMC91X is not set
 # CONFIG_DM9000 is not set
 
@@ -685,6 +697,7 @@
 # I2C Hardware Bus support
 #
 CONFIG_I2C_AT91=y
+CONFIG_I2C_AT91_CLOCKRATE=100000
 # CONFIG_I2C_OCORES is not set
 # CONFIG_I2C_PARPORT_LIGHT is not set
 # CONFIG_I2C_STUB is not set
@@ -722,6 +735,7 @@
 #
 # SPI Protocol Masters
 #
+# CONFIG_SPI_AT25 is not set
 
 #
 # Dallas's 1-wire bus
@@ -737,7 +751,11 @@
 #
 # Misc devices
 #
-# CONFIG_TIFM_CORE is not set
+
+#
+# Multifunction device drivers
+#
+# CONFIG_MFD_SM501 is not set
 
 #
 # LED devices
@@ -766,15 +784,23 @@
 #
 # Graphics support
 #
-# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 CONFIG_FB=y
+# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_FB_DDC is not set
 # CONFIG_FB_CFB_FILLRECT is not set
 # CONFIG_FB_CFB_COPYAREA is not set
 # CONFIG_FB_CFB_IMAGEBLIT is not set
+# CONFIG_FB_SVGALIB is not set
 # CONFIG_FB_MACMODES is not set
 # CONFIG_FB_BACKLIGHT is not set
 # CONFIG_FB_MODE_HELPERS is not set
 # CONFIG_FB_TILEBLITTING is not set
+
+#
+# Frame buffer hardware drivers
+#
+# CONFIG_FB_S1D15605 is not set
 # CONFIG_FB_S1D13XXX is not set
 # CONFIG_FB_VIRTUAL is not set
 
@@ -789,7 +815,6 @@
 # Logo configuration
 #
 # CONFIG_LOGO is not set
-# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
 
 #
 # Sound
@@ -800,6 +825,7 @@
 # HID Devices
 #
 CONFIG_HID=y
+# CONFIG_HID_DEBUG is not set
 
 #
 # USB support
@@ -814,9 +840,7 @@
 # Miscellaneous USB options
 #
 CONFIG_USB_DEVICEFS=y
-# CONFIG_USB_BANDWIDTH is not set
 # CONFIG_USB_DYNAMIC_MINORS is not set
-# CONFIG_USB_MULTITHREAD_PROBE is not set
 # CONFIG_USB_OTG is not set
 
 #
@@ -824,7 +848,8 @@
 #
 # CONFIG_USB_ISP116X_HCD is not set
 CONFIG_USB_OHCI_HCD=y
-# CONFIG_USB_OHCI_BIG_ENDIAN is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_DESC is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_MMIO is not set
 CONFIG_USB_OHCI_LITTLE_ENDIAN=y
 # CONFIG_USB_SL811_HCD is not set
 
@@ -877,6 +902,7 @@
 # CONFIG_USB_ATI_REMOTE2 is not set
 # CONFIG_USB_KEYSPAN_REMOTE is not set
 # CONFIG_USB_APPLETOUCH is not set
+# CONFIG_USB_GTCO is not set
 
 #
 # USB Imaging devices
@@ -914,6 +940,7 @@
 # CONFIG_USB_RIO500 is not set
 # CONFIG_USB_LEGOTOWER is not set
 # CONFIG_USB_LCD is not set
+# CONFIG_USB_BERRY_CHARGE is not set
 # CONFIG_USB_LED is not set
 # CONFIG_USB_CYPRESS_CY7C63 is not set
 # CONFIG_USB_CYTHERM is not set
@@ -923,6 +950,7 @@
 # CONFIG_USB_APPLEDISPLAY is not set
 # CONFIG_USB_LD is not set
 # CONFIG_USB_TRANCEVIBRATOR is not set
+# CONFIG_USB_IOWARRIOR is not set
 # CONFIG_USB_TEST is not set
 
 #
@@ -959,7 +987,6 @@
 # CONFIG_MMC_DEBUG is not set
 CONFIG_MMC_BLOCK=y
 CONFIG_MMC_AT91=m
-# CONFIG_MMC_TIFM_SD is not set
 
 #
 # Real Time Clock
@@ -1136,15 +1163,16 @@
 # CONFIG_DEBUG_FS is not set
 # CONFIG_HEADERS_CHECK is not set
 CONFIG_DEBUG_KERNEL=y
+# CONFIG_DEBUG_SHIRQ is not set
 CONFIG_LOG_BUF_SHIFT=14
 CONFIG_DETECT_SOFTLOCKUP=y
 # CONFIG_SCHEDSTATS is not set
+# CONFIG_TIMER_STATS is not set
 # CONFIG_DEBUG_SLAB is not set
 # CONFIG_DEBUG_RT_MUTEXES is not set
 # CONFIG_RT_MUTEX_TESTER is not set
 # CONFIG_DEBUG_SPINLOCK is not set
 # CONFIG_DEBUG_MUTEXES is not set
-# CONFIG_DEBUG_RWSEMS is not set
 # CONFIG_DEBUG_SPINLOCK_SLEEP is not set
 # CONFIG_DEBUG_LOCKING_API_SELFTESTS is not set
 # CONFIG_DEBUG_KOBJECT is not set
@@ -1155,6 +1183,7 @@
 CONFIG_FRAME_POINTER=y
 CONFIG_FORCED_INLINING=y
 # CONFIG_RCU_TORTURE_TEST is not set
+# CONFIG_FAULT_INJECTION is not set
 CONFIG_DEBUG_USER=y
 # CONFIG_DEBUG_ERRORS is not set
 CONFIG_DEBUG_LL=y
@@ -1180,5 +1209,7 @@
 CONFIG_CRC32=y
 # CONFIG_LIBCRC32C is not set
 CONFIG_ZLIB_INFLATE=y
+CONFIG_ZLIB_DEFLATE=y
 CONFIG_PLIST=y
-CONFIG_IOMAP_COPY=y
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_IOPORT=y
diff -urN linux-2.6.22-rc5/arch/arm/configs/cam60_defconfig linux-2.6.22-rc5.new/arch/arm/configs/cam60_defconfig
--- linux-2.6.22-rc5/arch/arm/configs/cam60_defconfig	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/configs/cam60_defconfig	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,954 @@
+#
+# Automatically generated make config: don't edit
+# Linux kernel version: 2.6.20
+# Tue May  1 21:06:33 2007
+#
+CONFIG_ARM=y
+# CONFIG_GENERIC_TIME is not set
+CONFIG_MMU=y
+CONFIG_GENERIC_HARDIRQS=y
+CONFIG_TRACE_IRQFLAGS_SUPPORT=y
+CONFIG_HARDIRQS_SW_RESEND=y
+CONFIG_GENERIC_IRQ_PROBE=y
+CONFIG_RWSEM_GENERIC_SPINLOCK=y
+# CONFIG_ARCH_HAS_ILOG2_U32 is not set
+# CONFIG_ARCH_HAS_ILOG2_U64 is not set
+CONFIG_GENERIC_HWEIGHT=y
+CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_VECTORS_BASE=0xffff0000
+CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
+
+#
+# Code maturity level options
+#
+CONFIG_EXPERIMENTAL=y
+CONFIG_BROKEN_ON_SMP=y
+CONFIG_INIT_ENV_ARG_LIMIT=32
+
+#
+# General setup
+#
+CONFIG_LOCALVERSION=""
+# CONFIG_LOCALVERSION_AUTO is not set
+# CONFIG_SWAP is not set
+CONFIG_SYSVIPC=y
+# CONFIG_IPC_NS is not set
+# CONFIG_POSIX_MQUEUE is not set
+# CONFIG_BSD_PROCESS_ACCT is not set
+# CONFIG_TASKSTATS is not set
+# CONFIG_UTS_NS is not set
+# CONFIG_AUDIT is not set
+CONFIG_IKCONFIG=y
+CONFIG_IKCONFIG_PROC=y
+CONFIG_SYSFS_DEPRECATED=y
+# CONFIG_RELAY is not set
+CONFIG_INITRAMFS_SOURCE=""
+CONFIG_CC_OPTIMIZE_FOR_SIZE=y
+CONFIG_SYSCTL=y
+# CONFIG_EMBEDDED is not set
+CONFIG_UID16=y
+CONFIG_SYSCTL_SYSCALL=y
+CONFIG_KALLSYMS=y
+# CONFIG_KALLSYMS_ALL is not set
+# CONFIG_KALLSYMS_EXTRA_PASS is not set
+CONFIG_HOTPLUG=y
+CONFIG_PRINTK=y
+CONFIG_BUG=y
+CONFIG_ELF_CORE=y
+CONFIG_BASE_FULL=y
+CONFIG_FUTEX=y
+CONFIG_EPOLL=y
+CONFIG_SHMEM=y
+CONFIG_SLAB=y
+CONFIG_VM_EVENT_COUNTERS=y
+CONFIG_RT_MUTEXES=y
+# CONFIG_TINY_SHMEM is not set
+CONFIG_BASE_SMALL=0
+# CONFIG_SLOB is not set
+
+#
+# Loadable module support
+#
+CONFIG_MODULES=y
+CONFIG_MODULE_UNLOAD=y
+CONFIG_MODULE_FORCE_UNLOAD=y
+# CONFIG_MODVERSIONS is not set
+# CONFIG_MODULE_SRCVERSION_ALL is not set
+# CONFIG_KMOD is not set
+
+#
+# Block layer
+#
+CONFIG_BLOCK=y
+# CONFIG_LBD is not set
+# CONFIG_BLK_DEV_IO_TRACE is not set
+# CONFIG_LSF is not set
+
+#
+# IO Schedulers
+#
+CONFIG_IOSCHED_NOOP=y
+CONFIG_IOSCHED_AS=y
+# CONFIG_IOSCHED_DEADLINE is not set
+# CONFIG_IOSCHED_CFQ is not set
+CONFIG_DEFAULT_AS=y
+# CONFIG_DEFAULT_DEADLINE is not set
+# CONFIG_DEFAULT_CFQ is not set
+# CONFIG_DEFAULT_NOOP is not set
+CONFIG_DEFAULT_IOSCHED="anticipatory"
+
+#
+# System Type
+#
+# CONFIG_ARCH_AAEC2000 is not set
+# CONFIG_ARCH_INTEGRATOR is not set
+# CONFIG_ARCH_REALVIEW is not set
+# CONFIG_ARCH_VERSATILE is not set
+CONFIG_ARCH_AT91=y
+# CONFIG_ARCH_CLPS7500 is not set
+# CONFIG_ARCH_CLPS711X is not set
+# CONFIG_ARCH_CO285 is not set
+# CONFIG_ARCH_EBSA110 is not set
+# CONFIG_ARCH_EP93XX is not set
+# CONFIG_ARCH_FOOTBRIDGE is not set
+# CONFIG_ARCH_NETX is not set
+# CONFIG_ARCH_H720X is not set
+# CONFIG_ARCH_IMX is not set
+# CONFIG_ARCH_IOP32X is not set
+# CONFIG_ARCH_IOP33X is not set
+# CONFIG_ARCH_IOP13XX is not set
+# CONFIG_ARCH_IXP4XX is not set
+# CONFIG_ARCH_IXP2000 is not set
+# CONFIG_ARCH_IXP23XX is not set
+# CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_PNX4008 is not set
+# CONFIG_ARCH_PXA is not set
+# CONFIG_ARCH_RPC is not set
+# CONFIG_ARCH_SA1100 is not set
+# CONFIG_ARCH_S3C2410 is not set
+# CONFIG_ARCH_SHARK is not set
+# CONFIG_ARCH_LH7A40X is not set
+# CONFIG_ARCH_OMAP is not set
+
+#
+# Atmel AT91 System-on-Chip
+#
+# CONFIG_ARCH_AT91RM9200 is not set
+CONFIG_ARCH_AT91SAM9260=y
+# CONFIG_ARCH_AT91SAM9261 is not set
+# CONFIG_ARCH_AT91SAM9263 is not set
+
+#
+# AT91SAM9260 Board Type
+#
+# CONFIG_MACH_AT91SAM9260EK is not set
+CONFIG_MACH_CAM60=y
+
+#
+# AT91 Board Options
+#
+
+#
+# AT91 Feature Selections
+#
+# CONFIG_AT91_PROGRAMMABLE_CLOCKS is not set
+
+#
+# Processor Type
+#
+CONFIG_CPU_32=y
+CONFIG_CPU_ARM926T=y
+CONFIG_CPU_32v5=y
+CONFIG_CPU_ABRT_EV5TJ=y
+CONFIG_CPU_CACHE_VIVT=y
+CONFIG_CPU_COPY_V4WB=y
+CONFIG_CPU_TLB_V4WBI=y
+CONFIG_CPU_CP15=y
+CONFIG_CPU_CP15_MMU=y
+
+#
+# Processor Features
+#
+# CONFIG_ARM_THUMB is not set
+# CONFIG_CPU_ICACHE_DISABLE is not set
+# CONFIG_CPU_DCACHE_DISABLE is not set
+# CONFIG_CPU_DCACHE_WRITETHROUGH is not set
+# CONFIG_CPU_CACHE_ROUND_ROBIN is not set
+
+#
+# Bus support
+#
+
+#
+# PCCARD (PCMCIA/CardBus) support
+#
+# CONFIG_PCCARD is not set
+
+#
+# Kernel Features
+#
+# CONFIG_PREEMPT is not set
+# CONFIG_NO_IDLE_HZ is not set
+CONFIG_HZ=100
+# CONFIG_AEABI is not set
+# CONFIG_ARCH_DISCONTIGMEM_ENABLE is not set
+CONFIG_SELECT_MEMORY_MODEL=y
+CONFIG_FLATMEM_MANUAL=y
+# CONFIG_DISCONTIGMEM_MANUAL is not set
+# CONFIG_SPARSEMEM_MANUAL is not set
+CONFIG_FLATMEM=y
+CONFIG_FLAT_NODE_MEM_MAP=y
+# CONFIG_SPARSEMEM_STATIC is not set
+CONFIG_SPLIT_PTLOCK_CPUS=4096
+# CONFIG_RESOURCES_64BIT is not set
+# CONFIG_LEDS is not set
+CONFIG_ALIGNMENT_TRAP=y
+
+#
+# Boot options
+#
+CONFIG_ZBOOT_ROM_TEXT=0x22000000
+CONFIG_ZBOOT_ROM_BSS=0x20004000
+# CONFIG_ZBOOT_ROM is not set
+CONFIG_CMDLINE="console=ttyS0,115200 noinitrd root=/dev/mtdblock3 rootfstype=jffs2 mem=64M"
+# CONFIG_XIP_KERNEL is not set
+
+#
+# Floating point emulation
+#
+
+#
+# At least one emulation must be selected
+#
+CONFIG_FPE_NWFPE=y
+# CONFIG_FPE_NWFPE_XP is not set
+# CONFIG_FPE_FASTFPE is not set
+# CONFIG_VFP is not set
+
+#
+# Userspace binary formats
+#
+CONFIG_BINFMT_ELF=y
+# CONFIG_BINFMT_AOUT is not set
+# CONFIG_BINFMT_MISC is not set
+# CONFIG_ARTHUR is not set
+
+#
+# Power management options
+#
+# CONFIG_PM is not set
+# CONFIG_APM is not set
+
+#
+# Networking
+#
+CONFIG_NET=y
+
+#
+# Networking options
+#
+# CONFIG_NETDEBUG is not set
+CONFIG_PACKET=y
+# CONFIG_PACKET_MMAP is not set
+CONFIG_UNIX=y
+CONFIG_XFRM=y
+# CONFIG_XFRM_USER is not set
+# CONFIG_XFRM_SUB_POLICY is not set
+# CONFIG_NET_KEY is not set
+CONFIG_INET=y
+# CONFIG_IP_MULTICAST is not set
+# CONFIG_IP_ADVANCED_ROUTER is not set
+CONFIG_IP_FIB_HASH=y
+CONFIG_IP_PNP=y
+# CONFIG_IP_PNP_DHCP is not set
+CONFIG_IP_PNP_BOOTP=y
+# CONFIG_IP_PNP_RARP is not set
+# CONFIG_NET_IPIP is not set
+# CONFIG_NET_IPGRE is not set
+# CONFIG_ARPD is not set
+# CONFIG_SYN_COOKIES is not set
+# CONFIG_INET_AH is not set
+# CONFIG_INET_ESP is not set
+# CONFIG_INET_IPCOMP is not set
+# CONFIG_INET_XFRM_TUNNEL is not set
+# CONFIG_INET_TUNNEL is not set
+CONFIG_INET_XFRM_MODE_TRANSPORT=y
+CONFIG_INET_XFRM_MODE_TUNNEL=y
+CONFIG_INET_XFRM_MODE_BEET=y
+CONFIG_INET_DIAG=y
+CONFIG_INET_TCP_DIAG=y
+# CONFIG_TCP_CONG_ADVANCED is not set
+CONFIG_TCP_CONG_CUBIC=y
+CONFIG_DEFAULT_TCP_CONG="cubic"
+# CONFIG_TCP_MD5SIG is not set
+# CONFIG_IPV6 is not set
+# CONFIG_INET6_XFRM_TUNNEL is not set
+# CONFIG_INET6_TUNNEL is not set
+# CONFIG_NETWORK_SECMARK is not set
+# CONFIG_NETFILTER is not set
+
+#
+# DCCP Configuration (EXPERIMENTAL)
+#
+# CONFIG_IP_DCCP is not set
+
+#
+# SCTP Configuration (EXPERIMENTAL)
+#
+# CONFIG_IP_SCTP is not set
+
+#
+# TIPC Configuration (EXPERIMENTAL)
+#
+# CONFIG_TIPC is not set
+# CONFIG_ATM is not set
+# CONFIG_BRIDGE is not set
+# CONFIG_VLAN_8021Q is not set
+# CONFIG_DECNET is not set
+# CONFIG_LLC2 is not set
+# CONFIG_IPX is not set
+# CONFIG_ATALK is not set
+# CONFIG_X25 is not set
+# CONFIG_LAPB is not set
+# CONFIG_ECONET is not set
+# CONFIG_WAN_ROUTER is not set
+
+#
+# QoS and/or fair queueing
+#
+# CONFIG_NET_SCHED is not set
+
+#
+# Network testing
+#
+# CONFIG_NET_PKTGEN is not set
+# CONFIG_HAMRADIO is not set
+# CONFIG_IRDA is not set
+# CONFIG_BT is not set
+# CONFIG_IEEE80211 is not set
+
+#
+# Device Drivers
+#
+
+#
+# Generic Driver Options
+#
+CONFIG_STANDALONE=y
+CONFIG_PREVENT_FIRMWARE_BUILD=y
+# CONFIG_FW_LOADER is not set
+# CONFIG_DEBUG_DRIVER is not set
+# CONFIG_SYS_HYPERVISOR is not set
+
+#
+# Connector - unified userspace <-> kernelspace linker
+#
+# CONFIG_CONNECTOR is not set
+
+#
+# Memory Technology Devices (MTD)
+#
+CONFIG_MTD=y
+# CONFIG_MTD_DEBUG is not set
+CONFIG_MTD_CONCAT=y
+CONFIG_MTD_PARTITIONS=y
+# CONFIG_MTD_REDBOOT_PARTS is not set
+CONFIG_MTD_CMDLINE_PARTS=y
+# CONFIG_MTD_AFS_PARTS is not set
+
+#
+# User Modules And Translation Layers
+#
+CONFIG_MTD_CHAR=y
+CONFIG_MTD_BLKDEVS=y
+CONFIG_MTD_BLOCK=y
+# CONFIG_FTL is not set
+# CONFIG_NFTL is not set
+# CONFIG_INFTL is not set
+# CONFIG_RFD_FTL is not set
+# CONFIG_SSFDC is not set
+
+#
+# RAM/ROM/Flash chip drivers
+#
+CONFIG_MTD_CFI=y
+# CONFIG_MTD_JEDECPROBE is not set
+CONFIG_MTD_GEN_PROBE=y
+# CONFIG_MTD_CFI_ADV_OPTIONS is not set
+CONFIG_MTD_MAP_BANK_WIDTH_1=y
+CONFIG_MTD_MAP_BANK_WIDTH_2=y
+CONFIG_MTD_MAP_BANK_WIDTH_4=y
+# CONFIG_MTD_MAP_BANK_WIDTH_8 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_16 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_32 is not set
+CONFIG_MTD_CFI_I1=y
+CONFIG_MTD_CFI_I2=y
+# CONFIG_MTD_CFI_I4 is not set
+# CONFIG_MTD_CFI_I8 is not set
+# CONFIG_MTD_CFI_INTELEXT is not set
+# CONFIG_MTD_CFI_AMDSTD is not set
+# CONFIG_MTD_CFI_STAA is not set
+# CONFIG_MTD_RAM is not set
+# CONFIG_MTD_ROM is not set
+# CONFIG_MTD_ABSENT is not set
+# CONFIG_MTD_OBSOLETE_CHIPS is not set
+
+#
+# Mapping drivers for chip access
+#
+CONFIG_MTD_COMPLEX_MAPPINGS=y
+# CONFIG_MTD_PHYSMAP is not set
+# CONFIG_MTD_ARM_INTEGRATOR is not set
+# CONFIG_MTD_PLATRAM is not set
+
+#
+# Self-contained MTD device drivers
+#
+CONFIG_MTD_DATAFLASH=y
+# CONFIG_MTD_M25P80 is not set
+# CONFIG_MTD_SLRAM is not set
+# CONFIG_MTD_PHRAM is not set
+# CONFIG_MTD_MTDRAM is not set
+# CONFIG_MTD_BLOCK2MTD is not set
+
+#
+# Disk-On-Chip Device Drivers
+#
+# CONFIG_MTD_DOC2000 is not set
+# CONFIG_MTD_DOC2001 is not set
+# CONFIG_MTD_DOC2001PLUS is not set
+
+#
+# NAND Flash Device Drivers
+#
+# CONFIG_MTD_NAND is not set
+
+#
+# OneNAND Flash Device Drivers
+#
+# CONFIG_MTD_ONENAND is not set
+
+#
+# Parallel port support
+#
+# CONFIG_PARPORT is not set
+
+#
+# Plug and Play support
+#
+
+#
+# Block devices
+#
+# CONFIG_BLK_DEV_COW_COMMON is not set
+# CONFIG_BLK_DEV_LOOP is not set
+# CONFIG_BLK_DEV_NBD is not set
+CONFIG_BLK_DEV_RAM=y
+CONFIG_BLK_DEV_RAM_COUNT=16
+CONFIG_BLK_DEV_RAM_SIZE=8192
+CONFIG_BLK_DEV_RAM_BLOCKSIZE=1024
+CONFIG_BLK_DEV_INITRD=y
+# CONFIG_CDROM_PKTCDVD is not set
+# CONFIG_ATA_OVER_ETH is not set
+
+#
+# SCSI device support
+#
+# CONFIG_RAID_ATTRS is not set
+# CONFIG_SCSI is not set
+# CONFIG_SCSI_NETLINK is not set
+
+#
+# Serial ATA (prod) and Parallel ATA (experimental) drivers
+#
+# CONFIG_ATA is not set
+
+#
+# Multi-device support (RAID and LVM)
+#
+# CONFIG_MD is not set
+
+#
+# Fusion MPT device support
+#
+# CONFIG_FUSION is not set
+
+#
+# IEEE 1394 (FireWire) support
+#
+
+#
+# I2O device support
+#
+
+#
+# Network device support
+#
+CONFIG_NETDEVICES=y
+# CONFIG_DUMMY is not set
+# CONFIG_BONDING is not set
+# CONFIG_EQUALIZER is not set
+# CONFIG_TUN is not set
+
+#
+# PHY device support
+#
+# CONFIG_PHYLIB is not set
+
+#
+# Ethernet (10 or 100Mbit)
+#
+CONFIG_NET_ETHERNET=y
+CONFIG_MII=y
+CONFIG_MACB=y
+# CONFIG_SMC91X is not set
+# CONFIG_DM9000 is not set
+
+#
+# Ethernet (1000 Mbit)
+#
+
+#
+# Ethernet (10000 Mbit)
+#
+
+#
+# Token Ring devices
+#
+
+#
+# Wireless LAN (non-hamradio)
+#
+# CONFIG_NET_RADIO is not set
+
+#
+# Wan interfaces
+#
+# CONFIG_WAN is not set
+# CONFIG_PPP is not set
+# CONFIG_SLIP is not set
+# CONFIG_SHAPER is not set
+# CONFIG_NETCONSOLE is not set
+# CONFIG_NETPOLL is not set
+# CONFIG_NET_POLL_CONTROLLER is not set
+
+#
+# ISDN subsystem
+#
+# CONFIG_ISDN is not set
+
+#
+# Input device support
+#
+CONFIG_INPUT=y
+# CONFIG_INPUT_FF_MEMLESS is not set
+
+#
+# Userland interfaces
+#
+CONFIG_INPUT_MOUSEDEV=y
+# CONFIG_INPUT_MOUSEDEV_PSAUX is not set
+CONFIG_INPUT_MOUSEDEV_SCREEN_X=1024
+CONFIG_INPUT_MOUSEDEV_SCREEN_Y=768
+# CONFIG_INPUT_JOYDEV is not set
+# CONFIG_INPUT_TSDEV is not set
+# CONFIG_INPUT_EVDEV is not set
+# CONFIG_INPUT_EVBUG is not set
+
+#
+# Input Device Drivers
+#
+# CONFIG_INPUT_KEYBOARD is not set
+# CONFIG_INPUT_MOUSE is not set
+# CONFIG_INPUT_JOYSTICK is not set
+# CONFIG_INPUT_TOUCHSCREEN is not set
+# CONFIG_INPUT_MISC is not set
+
+#
+# Hardware I/O ports
+#
+# CONFIG_SERIO is not set
+# CONFIG_GAMEPORT is not set
+
+#
+# Character devices
+#
+CONFIG_VT=y
+CONFIG_VT_CONSOLE=y
+CONFIG_HW_CONSOLE=y
+# CONFIG_VT_HW_CONSOLE_BINDING is not set
+# CONFIG_SERIAL_NONSTANDARD is not set
+
+#
+# Serial drivers
+#
+# CONFIG_SERIAL_8250 is not set
+
+#
+# Non-8250 serial port support
+#
+CONFIG_SERIAL_ATMEL=y
+CONFIG_SERIAL_ATMEL_CONSOLE=y
+# CONFIG_SERIAL_ATMEL_TTYAT is not set
+CONFIG_SERIAL_CORE=y
+CONFIG_SERIAL_CORE_CONSOLE=y
+CONFIG_UNIX98_PTYS=y
+CONFIG_LEGACY_PTYS=y
+CONFIG_LEGACY_PTY_COUNT=256
+
+#
+# IPMI
+#
+# CONFIG_IPMI_HANDLER is not set
+
+#
+# Watchdog Cards
+#
+# CONFIG_WATCHDOG is not set
+# CONFIG_HW_RANDOM is not set
+# CONFIG_NVRAM is not set
+# CONFIG_DTLK is not set
+# CONFIG_R3964 is not set
+# CONFIG_RAW_DRIVER is not set
+
+#
+# TPM devices
+#
+# CONFIG_TCG_TPM is not set
+
+#
+# I2C support
+#
+# CONFIG_I2C is not set
+
+#
+# SPI support
+#
+CONFIG_SPI=y
+# CONFIG_SPI_DEBUG is not set
+CONFIG_SPI_MASTER=y
+
+#
+# SPI Master Controller Drivers
+#
+CONFIG_SPI_ATMEL=y
+# CONFIG_SPI_BITBANG is not set
+
+#
+# SPI Protocol Masters
+#
+
+#
+# Dallas's 1-wire bus
+#
+# CONFIG_W1 is not set
+
+#
+# Hardware Monitoring support
+#
+# CONFIG_HWMON is not set
+# CONFIG_HWMON_VID is not set
+
+#
+# Misc devices
+#
+# CONFIG_TIFM_CORE is not set
+
+#
+# LED devices
+#
+# CONFIG_NEW_LEDS is not set
+
+#
+# LED drivers
+#
+
+#
+# LED Triggers
+#
+
+#
+# Multimedia devices
+#
+# CONFIG_VIDEO_DEV is not set
+
+#
+# Digital Video Broadcasting Devices
+#
+# CONFIG_DVB is not set
+
+#
+# Graphics support
+#
+# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_FB is not set
+
+#
+# Console display driver support
+#
+# CONFIG_VGA_CONSOLE is not set
+CONFIG_DUMMY_CONSOLE=y
+# CONFIG_BACKLIGHT_LCD_SUPPORT is not set
+
+#
+# Sound
+#
+# CONFIG_SOUND is not set
+
+#
+# HID Devices
+#
+# CONFIG_HID is not set
+
+#
+# USB support
+#
+CONFIG_USB_ARCH_HAS_HCD=y
+CONFIG_USB_ARCH_HAS_OHCI=y
+# CONFIG_USB_ARCH_HAS_EHCI is not set
+# CONFIG_USB is not set
+
+#
+# NOTE: USB_STORAGE enables SCSI, and 'SCSI disk support'
+#
+
+#
+# USB Gadget Support
+#
+# CONFIG_USB_GADGET is not set
+
+#
+# MMC/SD Card support
+#
+# CONFIG_MMC is not set
+
+#
+# Real Time Clock
+#
+CONFIG_RTC_LIB=y
+# CONFIG_RTC_CLASS is not set
+
+#
+# File systems
+#
+CONFIG_EXT2_FS=y
+# CONFIG_EXT2_FS_XATTR is not set
+# CONFIG_EXT2_FS_XIP is not set
+CONFIG_EXT3_FS=y
+CONFIG_EXT3_FS_XATTR=y
+# CONFIG_EXT3_FS_POSIX_ACL is not set
+# CONFIG_EXT3_FS_SECURITY is not set
+# CONFIG_EXT4DEV_FS is not set
+CONFIG_JBD=y
+# CONFIG_JBD_DEBUG is not set
+CONFIG_FS_MBCACHE=y
+# CONFIG_REISERFS_FS is not set
+# CONFIG_JFS_FS is not set
+# CONFIG_FS_POSIX_ACL is not set
+# CONFIG_XFS_FS is not set
+# CONFIG_GFS2_FS is not set
+# CONFIG_OCFS2_FS is not set
+# CONFIG_MINIX_FS is not set
+# CONFIG_ROMFS_FS is not set
+CONFIG_INOTIFY=y
+CONFIG_INOTIFY_USER=y
+# CONFIG_QUOTA is not set
+CONFIG_DNOTIFY=y
+# CONFIG_AUTOFS_FS is not set
+CONFIG_AUTOFS4_FS=y
+# CONFIG_FUSE_FS is not set
+
+#
+# CD-ROM/DVD Filesystems
+#
+# CONFIG_ISO9660_FS is not set
+# CONFIG_UDF_FS is not set
+
+#
+# DOS/FAT/NT Filesystems
+#
+CONFIG_FAT_FS=y
+# CONFIG_MSDOS_FS is not set
+CONFIG_VFAT_FS=y
+CONFIG_FAT_DEFAULT_CODEPAGE=437
+CONFIG_FAT_DEFAULT_IOCHARSET="iso8859-1"
+# CONFIG_NTFS_FS is not set
+
+#
+# Pseudo filesystems
+#
+CONFIG_PROC_FS=y
+CONFIG_PROC_SYSCTL=y
+CONFIG_SYSFS=y
+CONFIG_TMPFS=y
+# CONFIG_TMPFS_POSIX_ACL is not set
+# CONFIG_HUGETLB_PAGE is not set
+CONFIG_RAMFS=y
+# CONFIG_CONFIGFS_FS is not set
+
+#
+# Miscellaneous filesystems
+#
+# CONFIG_ADFS_FS is not set
+# CONFIG_AFFS_FS is not set
+# CONFIG_HFS_FS is not set
+# CONFIG_HFSPLUS_FS is not set
+# CONFIG_BEFS_FS is not set
+# CONFIG_BFS_FS is not set
+# CONFIG_EFS_FS is not set
+CONFIG_JFFS2_FS=y
+CONFIG_JFFS2_FS_DEBUG=0
+CONFIG_JFFS2_FS_WRITEBUFFER=y
+# CONFIG_JFFS2_SUMMARY is not set
+# CONFIG_JFFS2_FS_XATTR is not set
+# CONFIG_JFFS2_COMPRESSION_OPTIONS is not set
+CONFIG_JFFS2_ZLIB=y
+CONFIG_JFFS2_RTIME=y
+# CONFIG_JFFS2_RUBIN is not set
+CONFIG_CRAMFS=y
+# CONFIG_VXFS_FS is not set
+# CONFIG_HPFS_FS is not set
+# CONFIG_QNX4FS_FS is not set
+# CONFIG_SYSV_FS is not set
+# CONFIG_UFS_FS is not set
+
+#
+# Network File Systems
+#
+CONFIG_NFS_FS=y
+CONFIG_NFS_V3=y
+# CONFIG_NFS_V3_ACL is not set
+# CONFIG_NFS_V4 is not set
+# CONFIG_NFS_DIRECTIO is not set
+# CONFIG_NFSD is not set
+CONFIG_ROOT_NFS=y
+CONFIG_LOCKD=y
+CONFIG_LOCKD_V4=y
+CONFIG_NFS_COMMON=y
+CONFIG_SUNRPC=y
+# CONFIG_RPCSEC_GSS_KRB5 is not set
+# CONFIG_RPCSEC_GSS_SPKM3 is not set
+# CONFIG_SMB_FS is not set
+# CONFIG_CIFS is not set
+# CONFIG_NCP_FS is not set
+# CONFIG_CODA_FS is not set
+# CONFIG_AFS_FS is not set
+# CONFIG_9P_FS is not set
+
+#
+# Partition Types
+#
+# CONFIG_PARTITION_ADVANCED is not set
+CONFIG_MSDOS_PARTITION=y
+
+#
+# Native Language Support
+#
+CONFIG_NLS=y
+CONFIG_NLS_DEFAULT="iso8859-1"
+CONFIG_NLS_CODEPAGE_437=y
+# CONFIG_NLS_CODEPAGE_737 is not set
+# CONFIG_NLS_CODEPAGE_775 is not set
+CONFIG_NLS_CODEPAGE_850=y
+# CONFIG_NLS_CODEPAGE_852 is not set
+# CONFIG_NLS_CODEPAGE_855 is not set
+# CONFIG_NLS_CODEPAGE_857 is not set
+# CONFIG_NLS_CODEPAGE_860 is not set
+# CONFIG_NLS_CODEPAGE_861 is not set
+# CONFIG_NLS_CODEPAGE_862 is not set
+# CONFIG_NLS_CODEPAGE_863 is not set
+# CONFIG_NLS_CODEPAGE_864 is not set
+# CONFIG_NLS_CODEPAGE_865 is not set
+# CONFIG_NLS_CODEPAGE_866 is not set
+# CONFIG_NLS_CODEPAGE_869 is not set
+# CONFIG_NLS_CODEPAGE_936 is not set
+# CONFIG_NLS_CODEPAGE_950 is not set
+# CONFIG_NLS_CODEPAGE_932 is not set
+# CONFIG_NLS_CODEPAGE_949 is not set
+# CONFIG_NLS_CODEPAGE_874 is not set
+# CONFIG_NLS_ISO8859_8 is not set
+# CONFIG_NLS_CODEPAGE_1250 is not set
+# CONFIG_NLS_CODEPAGE_1251 is not set
+# CONFIG_NLS_ASCII is not set
+CONFIG_NLS_ISO8859_1=y
+# CONFIG_NLS_ISO8859_2 is not set
+# CONFIG_NLS_ISO8859_3 is not set
+# CONFIG_NLS_ISO8859_4 is not set
+# CONFIG_NLS_ISO8859_5 is not set
+# CONFIG_NLS_ISO8859_6 is not set
+# CONFIG_NLS_ISO8859_7 is not set
+# CONFIG_NLS_ISO8859_9 is not set
+# CONFIG_NLS_ISO8859_13 is not set
+# CONFIG_NLS_ISO8859_14 is not set
+# CONFIG_NLS_ISO8859_15 is not set
+# CONFIG_NLS_KOI8_R is not set
+# CONFIG_NLS_KOI8_U is not set
+# CONFIG_NLS_UTF8 is not set
+
+#
+# Distributed Lock Manager
+#
+# CONFIG_DLM is not set
+
+#
+# Profiling support
+#
+# CONFIG_PROFILING is not set
+
+#
+# Kernel hacking
+#
+# CONFIG_PRINTK_TIME is not set
+CONFIG_ENABLE_MUST_CHECK=y
+# CONFIG_MAGIC_SYSRQ is not set
+# CONFIG_UNUSED_SYMBOLS is not set
+# CONFIG_DEBUG_FS is not set
+# CONFIG_HEADERS_CHECK is not set
+CONFIG_DEBUG_KERNEL=y
+CONFIG_LOG_BUF_SHIFT=14
+CONFIG_DETECT_SOFTLOCKUP=y
+# CONFIG_SCHEDSTATS is not set
+# CONFIG_DEBUG_SLAB is not set
+# CONFIG_DEBUG_RT_MUTEXES is not set
+# CONFIG_RT_MUTEX_TESTER is not set
+# CONFIG_DEBUG_SPINLOCK is not set
+# CONFIG_DEBUG_MUTEXES is not set
+# CONFIG_DEBUG_RWSEMS is not set
+# CONFIG_DEBUG_SPINLOCK_SLEEP is not set
+# CONFIG_DEBUG_LOCKING_API_SELFTESTS is not set
+# CONFIG_DEBUG_KOBJECT is not set
+CONFIG_DEBUG_BUGVERBOSE=y
+# CONFIG_DEBUG_INFO is not set
+# CONFIG_DEBUG_VM is not set
+# CONFIG_DEBUG_LIST is not set
+CONFIG_FRAME_POINTER=y
+CONFIG_FORCED_INLINING=y
+# CONFIG_RCU_TORTURE_TEST is not set
+CONFIG_DEBUG_USER=y
+# CONFIG_DEBUG_ERRORS is not set
+CONFIG_DEBUG_LL=y
+# CONFIG_DEBUG_ICEDCC is not set
+
+#
+# Security options
+#
+# CONFIG_KEYS is not set
+# CONFIG_SECURITY is not set
+
+#
+# Cryptographic options
+#
+# CONFIG_CRYPTO is not set
+
+#
+# Library routines
+#
+CONFIG_BITREVERSE=y
+# CONFIG_CRC_CCITT is not set
+# CONFIG_CRC16 is not set
+CONFIG_CRC32=y
+# CONFIG_LIBCRC32C is not set
+CONFIG_ZLIB_INFLATE=y
+CONFIG_ZLIB_DEFLATE=y
+CONFIG_PLIST=y
+CONFIG_IOMAP_COPY=y
diff -urN linux-2.6.22-rc5/arch/arm/configs/kb9202_defconfig linux-2.6.22-rc5.new/arch/arm/configs/kb9202_defconfig
--- linux-2.6.22-rc5/arch/arm/configs/kb9202_defconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/configs/kb9202_defconfig	2007-07-29 05:23:04.000000000 +0200
@@ -1,19 +1,31 @@
 #
 # Automatically generated make config: don't edit
-# Linux kernel version: 2.6.13-rc2
-# Sun Aug 14 19:26:59 2005
+# Linux kernel version: 2.6.21
+# Mon May  7 11:43:14 2007
 #
 CONFIG_ARM=y
+CONFIG_SYS_SUPPORTS_APM_EMULATION=y
+CONFIG_GENERIC_GPIO=y
+# CONFIG_GENERIC_TIME is not set
 CONFIG_MMU=y
-CONFIG_UID16=y
+# CONFIG_NO_IOPORT is not set
+CONFIG_GENERIC_HARDIRQS=y
+CONFIG_TRACE_IRQFLAGS_SUPPORT=y
+CONFIG_HARDIRQS_SW_RESEND=y
+CONFIG_GENERIC_IRQ_PROBE=y
 CONFIG_RWSEM_GENERIC_SPINLOCK=y
+# CONFIG_ARCH_HAS_ILOG2_U32 is not set
+# CONFIG_ARCH_HAS_ILOG2_U64 is not set
+CONFIG_GENERIC_HWEIGHT=y
 CONFIG_GENERIC_CALIBRATE_DELAY=y
+CONFIG_ZONE_DMA=y
+CONFIG_VECTORS_BASE=0xffff0000
+CONFIG_DEFCONFIG_LIST="/lib/modules/$UNAME_RELEASE/.config"
 
 #
 # Code maturity level options
 #
-# CONFIG_EXPERIMENTAL is not set
-CONFIG_CLEAN_COMPILE=y
+CONFIG_EXPERIMENTAL=y
 CONFIG_BROKEN_ON_SMP=y
 CONFIG_INIT_ENV_ARG_LIMIT=32
 
@@ -21,54 +33,103 @@
 # General setup
 #
 CONFIG_LOCALVERSION=""
-# CONFIG_SWAP is not set
-# CONFIG_SYSVIPC is not set
-# CONFIG_BSD_PROCESS_ACCT is not set
+CONFIG_LOCALVERSION_AUTO=y
+CONFIG_SWAP=y
+CONFIG_SYSVIPC=y
+# CONFIG_IPC_NS is not set
+CONFIG_SYSVIPC_SYSCTL=y
+CONFIG_POSIX_MQUEUE=y
+CONFIG_BSD_PROCESS_ACCT=y
+# CONFIG_BSD_PROCESS_ACCT_V3 is not set
+# CONFIG_TASKSTATS is not set
+# CONFIG_UTS_NS is not set
+CONFIG_AUDIT=y
+CONFIG_IKCONFIG=y
+CONFIG_IKCONFIG_PROC=y
+CONFIG_SYSFS_DEPRECATED=y
+# CONFIG_RELAY is not set
+CONFIG_BLK_DEV_INITRD=y
+CONFIG_INITRAMFS_SOURCE=""
+# CONFIG_CC_OPTIMIZE_FOR_SIZE is not set
 CONFIG_SYSCTL=y
-# CONFIG_AUDIT is not set
-CONFIG_HOTPLUG=y
-# CONFIG_KOBJECT_UEVENT is not set
-# CONFIG_IKCONFIG is not set
 # CONFIG_EMBEDDED is not set
+CONFIG_UID16=y
+CONFIG_SYSCTL_SYSCALL=y
 CONFIG_KALLSYMS=y
 # CONFIG_KALLSYMS_ALL is not set
-# CONFIG_KALLSYMS_EXTRA_PASS is not set
+CONFIG_KALLSYMS_EXTRA_PASS=y
+CONFIG_HOTPLUG=y
 CONFIG_PRINTK=y
 CONFIG_BUG=y
+CONFIG_ELF_CORE=y
 CONFIG_BASE_FULL=y
 CONFIG_FUTEX=y
 CONFIG_EPOLL=y
-CONFIG_CC_OPTIMIZE_FOR_SIZE=y
 CONFIG_SHMEM=y
-CONFIG_CC_ALIGN_FUNCTIONS=0
-CONFIG_CC_ALIGN_LABELS=0
-CONFIG_CC_ALIGN_LOOPS=0
-CONFIG_CC_ALIGN_JUMPS=0
+CONFIG_SLAB=y
+CONFIG_VM_EVENT_COUNTERS=y
+CONFIG_RT_MUTEXES=y
 # CONFIG_TINY_SHMEM is not set
 CONFIG_BASE_SMALL=0
+# CONFIG_SLOB is not set
 
 #
 # Loadable module support
 #
 CONFIG_MODULES=y
 CONFIG_MODULE_UNLOAD=y
-CONFIG_OBSOLETE_MODPARM=y
-# CONFIG_MODULE_SRCVERSION_ALL is not set
+# CONFIG_MODULE_FORCE_UNLOAD is not set
+CONFIG_MODVERSIONS=y
+CONFIG_MODULE_SRCVERSION_ALL=y
 CONFIG_KMOD=y
 
 #
+# Block layer
+#
+CONFIG_BLOCK=y
+CONFIG_LBD=y
+# CONFIG_BLK_DEV_IO_TRACE is not set
+# CONFIG_LSF is not set
+
+#
+# IO Schedulers
+#
+CONFIG_IOSCHED_NOOP=y
+CONFIG_IOSCHED_AS=y
+CONFIG_IOSCHED_DEADLINE=y
+CONFIG_IOSCHED_CFQ=y
+# CONFIG_DEFAULT_AS is not set
+# CONFIG_DEFAULT_DEADLINE is not set
+CONFIG_DEFAULT_CFQ=y
+# CONFIG_DEFAULT_NOOP is not set
+CONFIG_DEFAULT_IOSCHED="cfq"
+
+#
 # System Type
 #
+# CONFIG_ARCH_AAEC2000 is not set
+# CONFIG_ARCH_INTEGRATOR is not set
+# CONFIG_ARCH_REALVIEW is not set
+# CONFIG_ARCH_VERSATILE is not set
+CONFIG_ARCH_AT91=y
 # CONFIG_ARCH_CLPS7500 is not set
 # CONFIG_ARCH_CLPS711X is not set
 # CONFIG_ARCH_CO285 is not set
 # CONFIG_ARCH_EBSA110 is not set
+# CONFIG_ARCH_EP93XX is not set
 # CONFIG_ARCH_FOOTBRIDGE is not set
-# CONFIG_ARCH_INTEGRATOR is not set
-# CONFIG_ARCH_IOP3XX is not set
+# CONFIG_ARCH_NETX is not set
+# CONFIG_ARCH_H720X is not set
+# CONFIG_ARCH_IMX is not set
+# CONFIG_ARCH_IOP32X is not set
+# CONFIG_ARCH_IOP33X is not set
+# CONFIG_ARCH_IOP13XX is not set
 # CONFIG_ARCH_IXP4XX is not set
 # CONFIG_ARCH_IXP2000 is not set
+# CONFIG_ARCH_IXP23XX is not set
 # CONFIG_ARCH_L7200 is not set
+# CONFIG_ARCH_NS9XXX is not set
+# CONFIG_ARCH_PNX4008 is not set
 # CONFIG_ARCH_PXA is not set
 # CONFIG_ARCH_RPC is not set
 # CONFIG_ARCH_SA1100 is not set
@@ -76,34 +137,52 @@
 # CONFIG_ARCH_SHARK is not set
 # CONFIG_ARCH_LH7A40X is not set
 # CONFIG_ARCH_OMAP is not set
-# CONFIG_ARCH_VERSATILE is not set
-# CONFIG_ARCH_IMX is not set
-# CONFIG_ARCH_H720X is not set
-# CONFIG_ARCH_AAEC2000 is not set
-CONFIG_ARCH_AT91=y
+
+#
+# Atmel AT91 System-on-Chip
+#
 CONFIG_ARCH_AT91RM9200=y
+# CONFIG_ARCH_AT91SAM9260 is not set
+# CONFIG_ARCH_AT91SAM9261 is not set
+# CONFIG_ARCH_AT91SAM9263 is not set
 
 #
-# AT91RM9200 Implementations
+# AT91RM9200 Board Type
 #
+# CONFIG_MACH_ONEARM is not set
 # CONFIG_ARCH_AT91RM9200DK is not set
 # CONFIG_MACH_AT91RM9200EK is not set
 # CONFIG_MACH_CSB337 is not set
 # CONFIG_MACH_CSB637 is not set
 # CONFIG_MACH_CARMEVA is not set
+# CONFIG_MACH_ATEB9200 is not set
 CONFIG_MACH_KB9200=y
+# CONFIG_MACH_KAFA is not set
+# CONFIG_MACH_CHUB is not set
+
+#
+# AT91 Board Options
+#
+
+#
+# AT91 Feature Selections
+#
+# CONFIG_AT91_PROGRAMMABLE_CLOCKS is not set
+# CONFIG_ATMEL_TCLIB is not set
 
 #
 # Processor Type
 #
 CONFIG_CPU_32=y
 CONFIG_CPU_ARM920T=y
-CONFIG_CPU_32v4=y
+CONFIG_CPU_32v4T=y
 CONFIG_CPU_ABRT_EV4T=y
 CONFIG_CPU_CACHE_V4WT=y
 CONFIG_CPU_CACHE_VIVT=y
 CONFIG_CPU_COPY_V4WB=y
 CONFIG_CPU_TLB_V4WBI=y
+CONFIG_CPU_CP15=y
+CONFIG_CPU_CP15_MMU=y
 
 #
 # Processor Features
@@ -112,24 +191,44 @@
 # CONFIG_CPU_ICACHE_DISABLE is not set
 # CONFIG_CPU_DCACHE_DISABLE is not set
 # CONFIG_CPU_DCACHE_WRITETHROUGH is not set
+# CONFIG_OUTER_CACHE is not set
 
 #
 # Bus support
 #
-CONFIG_ISA_DMA_API=y
 
 #
 # PCCARD (PCMCIA/CardBus) support
 #
-# CONFIG_PCCARD is not set
+CONFIG_PCCARD=m
+# CONFIG_PCMCIA_DEBUG is not set
+CONFIG_PCMCIA=m
+CONFIG_PCMCIA_LOAD_CIS=y
+CONFIG_PCMCIA_IOCTL=y
+
+#
+# PC-card bridges
+#
+# CONFIG_AT91_CF is not set
 
 #
 # Kernel Features
 #
+# CONFIG_PREEMPT is not set
 # CONFIG_NO_IDLE_HZ is not set
+CONFIG_HZ=100
+# CONFIG_AEABI is not set
 # CONFIG_ARCH_DISCONTIGMEM_ENABLE is not set
+CONFIG_SELECT_MEMORY_MODEL=y
+CONFIG_FLATMEM_MANUAL=y
+# CONFIG_DISCONTIGMEM_MANUAL is not set
+# CONFIG_SPARSEMEM_MANUAL is not set
 CONFIG_FLATMEM=y
 CONFIG_FLAT_NODE_MEM_MAP=y
+# CONFIG_SPARSEMEM_STATIC is not set
+CONFIG_SPLIT_PTLOCK_CPUS=4096
+# CONFIG_RESOURCES_64BIT is not set
+CONFIG_ZONE_DMA_FLAG=1
 # CONFIG_LEDS is not set
 CONFIG_ALIGNMENT_TRAP=y
 
@@ -138,8 +237,10 @@
 #
 CONFIG_ZBOOT_ROM_TEXT=0x10000000
 CONFIG_ZBOOT_ROM_BSS=0x20040000
-CONFIG_ZBOOT_ROM=y
-CONFIG_CMDLINE="console=ttyS0,115200 root=/dev/ram rw initrd=0x20210000,654933"
+# CONFIG_ZBOOT_ROM is not set
+CONFIG_CMDLINE="noinitrd root=/dev/mtdblock0 rootfstype=jffs2 mem=64M"
+# CONFIG_XIP_KERNEL is not set
+# CONFIG_KEXEC is not set
 
 #
 # Floating point emulation
@@ -150,6 +251,7 @@
 #
 CONFIG_FPE_NWFPE=y
 # CONFIG_FPE_NWFPE_XP is not set
+# CONFIG_FPE_FASTFPE is not set
 
 #
 # Userspace binary formats
@@ -165,6 +267,96 @@
 # CONFIG_PM is not set
 
 #
+# Networking
+#
+CONFIG_NET=y
+
+#
+# Networking options
+#
+# CONFIG_NETDEBUG is not set
+CONFIG_PACKET=y
+# CONFIG_PACKET_MMAP is not set
+CONFIG_UNIX=y
+# CONFIG_NET_KEY is not set
+CONFIG_INET=y
+CONFIG_IP_MULTICAST=y
+# CONFIG_IP_ADVANCED_ROUTER is not set
+CONFIG_IP_FIB_HASH=y
+CONFIG_IP_PNP=y
+# CONFIG_IP_PNP_DHCP is not set
+# CONFIG_IP_PNP_BOOTP is not set
+# CONFIG_IP_PNP_RARP is not set
+# CONFIG_NET_IPIP is not set
+# CONFIG_NET_IPGRE is not set
+# CONFIG_IP_MROUTE is not set
+# CONFIG_ARPD is not set
+# CONFIG_SYN_COOKIES is not set
+# CONFIG_INET_AH is not set
+# CONFIG_INET_ESP is not set
+# CONFIG_INET_IPCOMP is not set
+# CONFIG_INET_XFRM_TUNNEL is not set
+# CONFIG_INET_TUNNEL is not set
+# CONFIG_INET_XFRM_MODE_TRANSPORT is not set
+# CONFIG_INET_XFRM_MODE_TUNNEL is not set
+# CONFIG_INET_XFRM_MODE_BEET is not set
+# CONFIG_INET_DIAG is not set
+# CONFIG_TCP_CONG_ADVANCED is not set
+CONFIG_TCP_CONG_CUBIC=y
+CONFIG_DEFAULT_TCP_CONG="cubic"
+# CONFIG_TCP_MD5SIG is not set
+# CONFIG_IPV6 is not set
+# CONFIG_INET6_XFRM_TUNNEL is not set
+# CONFIG_INET6_TUNNEL is not set
+# CONFIG_NETWORK_SECMARK is not set
+# CONFIG_NETFILTER is not set
+
+#
+# DCCP Configuration (EXPERIMENTAL)
+#
+# CONFIG_IP_DCCP is not set
+
+#
+# SCTP Configuration (EXPERIMENTAL)
+#
+CONFIG_IP_SCTP=m
+# CONFIG_SCTP_DBG_MSG is not set
+# CONFIG_SCTP_DBG_OBJCNT is not set
+# CONFIG_SCTP_HMAC_NONE is not set
+# CONFIG_SCTP_HMAC_SHA1 is not set
+CONFIG_SCTP_HMAC_MD5=y
+
+#
+# TIPC Configuration (EXPERIMENTAL)
+#
+# CONFIG_TIPC is not set
+# CONFIG_ATM is not set
+# CONFIG_BRIDGE is not set
+# CONFIG_VLAN_8021Q is not set
+# CONFIG_DECNET is not set
+# CONFIG_LLC2 is not set
+# CONFIG_IPX is not set
+# CONFIG_ATALK is not set
+# CONFIG_X25 is not set
+# CONFIG_LAPB is not set
+# CONFIG_ECONET is not set
+# CONFIG_WAN_ROUTER is not set
+
+#
+# QoS and/or fair queueing
+#
+# CONFIG_NET_SCHED is not set
+
+#
+# Network testing
+#
+# CONFIG_NET_PKTGEN is not set
+# CONFIG_HAMRADIO is not set
+# CONFIG_IRDA is not set
+# CONFIG_BT is not set
+# CONFIG_IEEE80211 is not set
+
+#
 # Device Drivers
 #
 
@@ -173,13 +365,95 @@
 #
 CONFIG_STANDALONE=y
 CONFIG_PREVENT_FIRMWARE_BUILD=y
-# CONFIG_FW_LOADER is not set
-CONFIG_DEBUG_DRIVER=y
+CONFIG_FW_LOADER=y
+# CONFIG_DEBUG_DRIVER is not set
+# CONFIG_DEBUG_DEVRES is not set
+# CONFIG_SYS_HYPERVISOR is not set
+
+#
+# Connector - unified userspace <-> kernelspace linker
+#
+# CONFIG_CONNECTOR is not set
 
 #
 # Memory Technology Devices (MTD)
 #
-# CONFIG_MTD is not set
+CONFIG_MTD=y
+# CONFIG_MTD_DEBUG is not set
+CONFIG_MTD_CONCAT=y
+CONFIG_MTD_PARTITIONS=y
+# CONFIG_MTD_REDBOOT_PARTS is not set
+CONFIG_MTD_CMDLINE_PARTS=y
+# CONFIG_MTD_AFS_PARTS is not set
+
+#
+# User Modules And Translation Layers
+#
+CONFIG_MTD_CHAR=y
+CONFIG_MTD_BLKDEVS=y
+CONFIG_MTD_BLOCK=y
+# CONFIG_FTL is not set
+# CONFIG_NFTL is not set
+# CONFIG_INFTL is not set
+# CONFIG_RFD_FTL is not set
+# CONFIG_SSFDC is not set
+
+#
+# RAM/ROM/Flash chip drivers
+#
+# CONFIG_MTD_CFI is not set
+# CONFIG_MTD_JEDECPROBE is not set
+CONFIG_MTD_MAP_BANK_WIDTH_1=y
+CONFIG_MTD_MAP_BANK_WIDTH_2=y
+CONFIG_MTD_MAP_BANK_WIDTH_4=y
+# CONFIG_MTD_MAP_BANK_WIDTH_8 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_16 is not set
+# CONFIG_MTD_MAP_BANK_WIDTH_32 is not set
+CONFIG_MTD_CFI_I1=y
+CONFIG_MTD_CFI_I2=y
+# CONFIG_MTD_CFI_I4 is not set
+# CONFIG_MTD_CFI_I8 is not set
+# CONFIG_MTD_RAM is not set
+# CONFIG_MTD_ROM is not set
+# CONFIG_MTD_ABSENT is not set
+# CONFIG_MTD_OBSOLETE_CHIPS is not set
+
+#
+# Mapping drivers for chip access
+#
+CONFIG_MTD_COMPLEX_MAPPINGS=y
+# CONFIG_MTD_PLATRAM is not set
+
+#
+# Self-contained MTD device drivers
+#
+# CONFIG_MTD_SLRAM is not set
+# CONFIG_MTD_PHRAM is not set
+# CONFIG_MTD_MTDRAM is not set
+# CONFIG_MTD_BLOCK2MTD is not set
+
+#
+# Disk-On-Chip Device Drivers
+#
+# CONFIG_MTD_DOC2000 is not set
+# CONFIG_MTD_DOC2001 is not set
+# CONFIG_MTD_DOC2001PLUS is not set
+
+#
+# NAND Flash Device Drivers
+#
+CONFIG_MTD_NAND=y
+# CONFIG_MTD_NAND_VERIFY_WRITE is not set
+# CONFIG_MTD_NAND_ECC_SMC is not set
+CONFIG_MTD_NAND_IDS=y
+# CONFIG_MTD_NAND_DISKONCHIP is not set
+CONFIG_MTD_NAND_AT91=y
+# CONFIG_MTD_NAND_NANDSIM is not set
+
+#
+# OneNAND Flash Device Drivers
+#
+# CONFIG_MTD_ONENAND is not set
 
 #
 # Parallel port support
@@ -189,6 +463,7 @@
 #
 # Plug and Play support
 #
+# CONFIG_PNPACPI is not set
 
 #
 # Block devices
@@ -196,28 +471,27 @@
 # CONFIG_BLK_DEV_COW_COMMON is not set
 CONFIG_BLK_DEV_LOOP=y
 # CONFIG_BLK_DEV_CRYPTOLOOP is not set
-CONFIG_BLK_DEV_NBD=y
+# CONFIG_BLK_DEV_NBD is not set
 # CONFIG_BLK_DEV_UB is not set
 CONFIG_BLK_DEV_RAM=y
 CONFIG_BLK_DEV_RAM_COUNT=16
-CONFIG_BLK_DEV_RAM_SIZE=4096
-CONFIG_BLK_DEV_INITRD=y
-CONFIG_INITRAMFS_SOURCE=""
+CONFIG_BLK_DEV_RAM_SIZE=16384
+CONFIG_BLK_DEV_RAM_BLOCKSIZE=1024
 # CONFIG_CDROM_PKTCDVD is not set
+# CONFIG_ATA_OVER_ETH is not set
 
 #
-# IO Schedulers
+# ATA/ATAPI/MFM/RLL support
 #
-CONFIG_IOSCHED_NOOP=y
-CONFIG_IOSCHED_AS=y
-CONFIG_IOSCHED_DEADLINE=y
-CONFIG_IOSCHED_CFQ=y
-# CONFIG_ATA_OVER_ETH is not set
+# CONFIG_IDE is not set
 
 #
 # SCSI device support
 #
+# CONFIG_RAID_ATTRS is not set
 CONFIG_SCSI=y
+# CONFIG_SCSI_TGT is not set
+# CONFIG_SCSI_NETLINK is not set
 CONFIG_SCSI_PROC_FS=y
 
 #
@@ -233,97 +507,61 @@
 #
 # Some SCSI devices (e.g. CD jukebox) support multiple LUNs
 #
-# CONFIG_SCSI_MULTI_LUN is not set
-# CONFIG_SCSI_CONSTANTS is not set
-# CONFIG_SCSI_LOGGING is not set
+CONFIG_SCSI_MULTI_LUN=y
+CONFIG_SCSI_CONSTANTS=y
+CONFIG_SCSI_LOGGING=y
+# CONFIG_SCSI_SCAN_ASYNC is not set
 
 #
-# SCSI Transport Attributes
+# SCSI Transports
 #
-# CONFIG_SCSI_SPI_ATTRS is not set
+CONFIG_SCSI_SPI_ATTRS=m
 # CONFIG_SCSI_FC_ATTRS is not set
 # CONFIG_SCSI_ISCSI_ATTRS is not set
+# CONFIG_SCSI_SAS_ATTRS is not set
+# CONFIG_SCSI_SAS_LIBSAS is not set
 
 #
 # SCSI low-level drivers
 #
-# CONFIG_SCSI_SATA is not set
+# CONFIG_ISCSI_TCP is not set
 # CONFIG_SCSI_DEBUG is not set
 
 #
-# Multi-device support (RAID and LVM)
-#
-# CONFIG_MD is not set
-
-#
-# Fusion MPT device support
+# PCMCIA SCSI adapter support
 #
-# CONFIG_FUSION is not set
+# CONFIG_PCMCIA_AHA152X is not set
+# CONFIG_PCMCIA_FDOMAIN is not set
+# CONFIG_PCMCIA_NINJA_SCSI is not set
+# CONFIG_PCMCIA_QLOGIC is not set
+# CONFIG_PCMCIA_SYM53C500 is not set
 
 #
-# IEEE 1394 (FireWire) support
+# Serial ATA (prod) and Parallel ATA (experimental) drivers
 #
+# CONFIG_ATA is not set
 
 #
-# I2O device support
+# Multi-device support (RAID and LVM)
 #
+# CONFIG_MD is not set
 
 #
-# Networking support
+# Fusion MPT device support
 #
-CONFIG_NET=y
+# CONFIG_FUSION is not set
 
 #
-# Networking options
+# IEEE 1394 (FireWire) support
 #
-CONFIG_PACKET=y
-# CONFIG_PACKET_MMAP is not set
-CONFIG_UNIX=y
-# CONFIG_NET_KEY is not set
-CONFIG_INET=y
-CONFIG_IP_MULTICAST=y
-# CONFIG_IP_ADVANCED_ROUTER is not set
-CONFIG_IP_FIB_HASH=y
-CONFIG_IP_PNP=y
-CONFIG_IP_PNP_DHCP=y
-# CONFIG_IP_PNP_BOOTP is not set
-# CONFIG_IP_PNP_RARP is not set
-# CONFIG_NET_IPIP is not set
-# CONFIG_NET_IPGRE is not set
-# CONFIG_IP_MROUTE is not set
-# CONFIG_SYN_COOKIES is not set
-# CONFIG_INET_AH is not set
-# CONFIG_INET_ESP is not set
-# CONFIG_INET_IPCOMP is not set
-# CONFIG_INET_TUNNEL is not set
-# CONFIG_IP_TCPDIAG is not set
-# CONFIG_IP_TCPDIAG_IPV6 is not set
-# CONFIG_TCP_CONG_ADVANCED is not set
-CONFIG_TCP_CONG_BIC=y
-# CONFIG_IPV6 is not set
-# CONFIG_NETFILTER is not set
-# CONFIG_BRIDGE is not set
-# CONFIG_VLAN_8021Q is not set
-# CONFIG_DECNET is not set
-# CONFIG_LLC2 is not set
-# CONFIG_IPX is not set
-# CONFIG_ATALK is not set
 
 #
-# QoS and/or fair queueing
+# I2O device support
 #
-# CONFIG_NET_SCHED is not set
-# CONFIG_NET_CLS_ROUTE is not set
 
 #
-# Network testing
+# Network device support
 #
-# CONFIG_NET_PKTGEN is not set
-# CONFIG_NETPOLL is not set
-# CONFIG_NET_POLL_CONTROLLER is not set
-# CONFIG_HAMRADIO is not set
-# CONFIG_IRDA is not set
-# CONFIG_BT is not set
 CONFIG_NETDEVICES=y
 # CONFIG_DUMMY is not set
 # CONFIG_BONDING is not set
@@ -331,6 +569,11 @@
 # CONFIG_TUN is not set
 
 #
+# PHY device support
+#
+# CONFIG_PHYLIB is not set
+
+#
 # Ethernet (10 or 100Mbit)
 #
 CONFIG_NET_ETHERNET=y
@@ -357,11 +600,20 @@
 # CONFIG_NET_RADIO is not set
 
 #
+# PCMCIA network device support
+#
+# CONFIG_NET_PCMCIA is not set
+
+#
 # Wan interfaces
 #
 # CONFIG_WAN is not set
 # CONFIG_PPP is not set
 # CONFIG_SLIP is not set
+# CONFIG_SHAPER is not set
+# CONFIG_NETCONSOLE is not set
+# CONFIG_NETPOLL is not set
+# CONFIG_NET_POLL_CONTROLLER is not set
 
 #
 # ISDN subsystem
@@ -372,6 +624,7 @@
 # Input device support
 #
 CONFIG_INPUT=y
+# CONFIG_INPUT_FF_MEMLESS is not set
 
 #
 # Userland interfaces
@@ -397,9 +650,7 @@
 #
 # Hardware I/O ports
 #
-CONFIG_SERIO=y
-# CONFIG_SERIO_SERPORT is not set
-# CONFIG_SERIO_RAW is not set
+# CONFIG_SERIO is not set
 # CONFIG_GAMEPORT is not set
 
 #
@@ -408,6 +659,7 @@
 CONFIG_VT=y
 CONFIG_VT_CONSOLE=y
 CONFIG_HW_CONSOLE=y
+# CONFIG_VT_HW_CONSOLE_BINDING is not set
 # CONFIG_SERIAL_NONSTANDARD is not set
 
 #
@@ -420,11 +672,11 @@
 #
 CONFIG_SERIAL_ATMEL=y
 CONFIG_SERIAL_ATMEL_CONSOLE=y
+# CONFIG_SERIAL_ATMEL_TTYAT is not set
 CONFIG_SERIAL_CORE=y
 CONFIG_SERIAL_CORE_CONSOLE=y
 CONFIG_UNIX98_PTYS=y
-CONFIG_LEGACY_PTYS=y
-CONFIG_LEGACY_PTY_COUNT=256
+# CONFIG_LEGACY_PTYS is not set
 
 #
 # IPMI
@@ -435,21 +687,23 @@
 # Watchdog Cards
 #
 # CONFIG_WATCHDOG is not set
+# CONFIG_HW_RANDOM is not set
 # CONFIG_NVRAM is not set
-# CONFIG_RTC is not set
-# CONFIG_AT91RM9200_RTC is not set
 # CONFIG_DTLK is not set
 # CONFIG_R3964 is not set
 
 #
-# Ftape, the floppy tape device driver
+# PCMCIA character devices
 #
+# CONFIG_SYNCLINK_CS is not set
+# CONFIG_CARDMAN_4000 is not set
+# CONFIG_CARDMAN_4040 is not set
 # CONFIG_RAW_DRIVER is not set
 
 #
 # TPM devices
 #
-# CONFIG_AT91_SPI is not set
+# CONFIG_TCG_TPM is not set
 
 #
 # I2C support
@@ -457,10 +711,50 @@
 # CONFIG_I2C is not set
 
 #
+# SPI support
+#
+# CONFIG_SPI is not set
+# CONFIG_SPI_MASTER is not set
+
+#
+# Dallas's 1-wire bus
+#
+# CONFIG_W1 is not set
+
+#
+# Hardware Monitoring support
+#
+CONFIG_HWMON=y
+# CONFIG_HWMON_VID is not set
+# CONFIG_SENSORS_ABITUGURU is not set
+# CONFIG_SENSORS_F71805F is not set
+# CONFIG_SENSORS_PC87427 is not set
+# CONFIG_SENSORS_VT1211 is not set
+CONFIG_HWMON_DEBUG_CHIP=y
+
+#
 # Misc devices
 #
 
 #
+# Multifunction device drivers
+#
+# CONFIG_MFD_SM501 is not set
+
+#
+# LED devices
+#
+# CONFIG_NEW_LEDS is not set
+
+#
+# LED drivers
+#
+
+#
+# LED Triggers
+#
+
+#
 # Multimedia devices
 #
 # CONFIG_VIDEO_DEV is not set
@@ -469,17 +763,57 @@
 # Digital Video Broadcasting Devices
 #
 # CONFIG_DVB is not set
+# CONFIG_USB_DABUSB is not set
 
 #
 # Graphics support
 #
-# CONFIG_FB is not set
+CONFIG_BACKLIGHT_LCD_SUPPORT=y
+CONFIG_BACKLIGHT_CLASS_DEVICE=y
+# CONFIG_LCD_CLASS_DEVICE is not set
+CONFIG_BACKLIGHT_KB920x=y
+CONFIG_FB=y
+# CONFIG_FIRMWARE_EDID is not set
+# CONFIG_FB_DDC is not set
+CONFIG_FB_CFB_FILLRECT=y
+CONFIG_FB_CFB_COPYAREA=y
+CONFIG_FB_CFB_IMAGEBLIT=y
+# CONFIG_FB_SVGALIB is not set
+# CONFIG_FB_MACMODES is not set
+# CONFIG_FB_BACKLIGHT is not set
+CONFIG_FB_MODE_HELPERS=y
+CONFIG_FB_TILEBLITTING=y
+
+#
+# Frame buffer hardware drivers
+#
+CONFIG_FB_S1D15605=y
+# CONFIG_FB_S1D13XXX is not set
+# CONFIG_FB_VIRTUAL is not set
 
 #
 # Console display driver support
 #
 # CONFIG_VGA_CONSOLE is not set
 CONFIG_DUMMY_CONSOLE=y
+CONFIG_FRAMEBUFFER_CONSOLE=y
+# CONFIG_FRAMEBUFFER_CONSOLE_ROTATION is not set
+CONFIG_FONTS=y
+# CONFIG_FONT_8x8 is not set
+# CONFIG_FONT_8x16 is not set
+# CONFIG_FONT_6x11 is not set
+# CONFIG_FONT_7x14 is not set
+# CONFIG_FONT_PEARL_8x8 is not set
+# CONFIG_FONT_ACORN_8x8 is not set
+CONFIG_FONT_MINI_4x6=y
+# CONFIG_FONT_SUN8x16 is not set
+# CONFIG_FONT_SUN12x22 is not set
+# CONFIG_FONT_10x18 is not set
+
+#
+# Logo configuration
+#
+# CONFIG_LOGO is not set
 
 #
 # Sound
@@ -487,82 +821,98 @@
 # CONFIG_SOUND is not set
 
 #
+# HID Devices
+#
+CONFIG_HID=y
+# CONFIG_HID_DEBUG is not set
+
+#
 # USB support
 #
 CONFIG_USB_ARCH_HAS_HCD=y
 CONFIG_USB_ARCH_HAS_OHCI=y
+# CONFIG_USB_ARCH_HAS_EHCI is not set
 CONFIG_USB=y
-CONFIG_USB_DEBUG=y
+# CONFIG_USB_DEBUG is not set
 
 #
 # Miscellaneous USB options
 #
 CONFIG_USB_DEVICEFS=y
+# CONFIG_USB_DYNAMIC_MINORS is not set
+# CONFIG_USB_OTG is not set
 
 #
 # USB Host Controller Drivers
 #
 # CONFIG_USB_ISP116X_HCD is not set
 CONFIG_USB_OHCI_HCD=y
-# CONFIG_USB_OHCI_BIG_ENDIAN is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_DESC is not set
+# CONFIG_USB_OHCI_BIG_ENDIAN_MMIO is not set
 CONFIG_USB_OHCI_LITTLE_ENDIAN=y
 # CONFIG_USB_SL811_HCD is not set
 
 #
 # USB Device Class drivers
 #
-# CONFIG_USB_BLUETOOTH_TTY is not set
 # CONFIG_USB_ACM is not set
 # CONFIG_USB_PRINTER is not set
 
 #
-# NOTE: USB_STORAGE enables SCSI, and 'SCSI disk support' may also be needed; see USB_STORAGE Help for more information
+# NOTE: USB_STORAGE enables SCSI, and 'SCSI disk support'
+#
+
+#
+# may also be needed; see USB_STORAGE Help for more information
 #
 CONFIG_USB_STORAGE=y
-CONFIG_USB_STORAGE_DEBUG=y
+# CONFIG_USB_STORAGE_DEBUG is not set
+# CONFIG_USB_STORAGE_DATAFAB is not set
 # CONFIG_USB_STORAGE_FREECOM is not set
 # CONFIG_USB_STORAGE_DPCM is not set
+# CONFIG_USB_STORAGE_USBAT is not set
+# CONFIG_USB_STORAGE_SDDR09 is not set
+# CONFIG_USB_STORAGE_SDDR55 is not set
+# CONFIG_USB_STORAGE_JUMPSHOT is not set
+# CONFIG_USB_STORAGE_ALAUDA is not set
+# CONFIG_USB_STORAGE_KARMA is not set
+CONFIG_USB_LIBUSUAL=y
 
 #
 # USB Input Devices
 #
-# CONFIG_USB_HID is not set
-
-#
-# USB HID Boot Protocol drivers
-#
-# CONFIG_USB_KBD is not set
-# CONFIG_USB_MOUSE is not set
+CONFIG_USB_HID=y
+# CONFIG_USB_HIDINPUT_POWERBOOK is not set
+# CONFIG_HID_FF is not set
+# CONFIG_USB_HIDDEV is not set
 # CONFIG_USB_AIPTEK is not set
 # CONFIG_USB_WACOM is not set
 # CONFIG_USB_ACECAD is not set
 # CONFIG_USB_KBTAB is not set
 # CONFIG_USB_POWERMATE is not set
-# CONFIG_USB_MTOUCH is not set
-# CONFIG_USB_ITMTOUCH is not set
-# CONFIG_USB_EGALAX is not set
+# CONFIG_USB_TOUCHSCREEN is not set
+# CONFIG_USB_YEALINK is not set
 # CONFIG_USB_XPAD is not set
 # CONFIG_USB_ATI_REMOTE is not set
+# CONFIG_USB_ATI_REMOTE2 is not set
+# CONFIG_USB_KEYSPAN_REMOTE is not set
+# CONFIG_USB_APPLETOUCH is not set
+# CONFIG_USB_GTCO is not set
 
 #
 # USB Imaging devices
 #
+# CONFIG_USB_MDC800 is not set
 # CONFIG_USB_MICROTEK is not set
 
 #
-# USB Multimedia devices
-#
-# CONFIG_USB_DABUSB is not set
-
-#
-# Video4Linux support is needed for USB Multimedia device support
-#
-
-#
 # USB Network Adapters
 #
+# CONFIG_USB_CATC is not set
 # CONFIG_USB_KAWETH is not set
 # CONFIG_USB_PEGASUS is not set
+# CONFIG_USB_RTL8150 is not set
+# CONFIG_USB_USBNET_MII is not set
 # CONFIG_USB_USBNET is not set
 # CONFIG_USB_MON is not set
 
@@ -580,12 +930,23 @@
 #
 # CONFIG_USB_EMI62 is not set
 # CONFIG_USB_EMI26 is not set
+# CONFIG_USB_ADUTUX is not set
+# CONFIG_USB_AUERSWALD is not set
+# CONFIG_USB_RIO500 is not set
+# CONFIG_USB_LEGOTOWER is not set
 # CONFIG_USB_LCD is not set
+# CONFIG_USB_BERRY_CHARGE is not set
 # CONFIG_USB_LED is not set
+# CONFIG_USB_CYPRESS_CY7C63 is not set
 # CONFIG_USB_CYTHERM is not set
-# CONFIG_USB_PHIDGETKIT is not set
-# CONFIG_USB_PHIDGETSERVO is not set
+# CONFIG_USB_PHIDGET is not set
 # CONFIG_USB_IDMOUSE is not set
+# CONFIG_USB_FTDI_ELAN is not set
+# CONFIG_USB_APPLEDISPLAY is not set
+# CONFIG_USB_LD is not set
+# CONFIG_USB_TRANCEVIBRATOR is not set
+# CONFIG_USB_IOWARRIOR is not set
+# CONFIG_USB_TEST is not set
 
 #
 # USB DSL modem support
@@ -599,36 +960,51 @@
 #
 # MMC/SD Card support
 #
-# CONFIG_MMC is not set
+CONFIG_MMC=y
+# CONFIG_MMC_DEBUG is not set
+CONFIG_MMC_BLOCK=y
+CONFIG_MMC_AT91=y
+
+#
+# Real Time Clock
+#
+CONFIG_RTC_LIB=y
+# CONFIG_RTC_CLASS is not set
 
 #
 # File systems
 #
 CONFIG_EXT2_FS=y
 CONFIG_EXT2_FS_XATTR=y
-# CONFIG_EXT2_FS_POSIX_ACL is not set
-# CONFIG_EXT2_FS_SECURITY is not set
+CONFIG_EXT2_FS_POSIX_ACL=y
+CONFIG_EXT2_FS_SECURITY=y
 # CONFIG_EXT2_FS_XIP is not set
 CONFIG_EXT3_FS=y
 CONFIG_EXT3_FS_XATTR=y
-# CONFIG_EXT3_FS_POSIX_ACL is not set
-# CONFIG_EXT3_FS_SECURITY is not set
+CONFIG_EXT3_FS_POSIX_ACL=y
+CONFIG_EXT3_FS_SECURITY=y
+# CONFIG_EXT4DEV_FS is not set
 CONFIG_JBD=y
 # CONFIG_JBD_DEBUG is not set
 CONFIG_FS_MBCACHE=y
 # CONFIG_REISERFS_FS is not set
 # CONFIG_JFS_FS is not set
-
-#
-# XFS support
-#
+CONFIG_FS_POSIX_ACL=y
 # CONFIG_XFS_FS is not set
+# CONFIG_GFS2_FS is not set
+# CONFIG_OCFS2_FS is not set
 # CONFIG_MINIX_FS is not set
 # CONFIG_ROMFS_FS is not set
-# CONFIG_QUOTA is not set
+CONFIG_INOTIFY=y
+CONFIG_INOTIFY_USER=y
+CONFIG_QUOTA=y
+# CONFIG_QFMT_V1 is not set
+CONFIG_QFMT_V2=y
+CONFIG_QUOTACTL=y
 CONFIG_DNOTIFY=y
-CONFIG_AUTOFS_FS=y
+# CONFIG_AUTOFS_FS is not set
 CONFIG_AUTOFS4_FS=y
+# CONFIG_FUSE_FS is not set
 
 #
 # CD-ROM/DVD Filesystems
@@ -643,25 +1019,40 @@
 CONFIG_MSDOS_FS=y
 CONFIG_VFAT_FS=y
 CONFIG_FAT_DEFAULT_CODEPAGE=437
-CONFIG_FAT_DEFAULT_IOCHARSET="iso8859-1"
+CONFIG_FAT_DEFAULT_IOCHARSET="ascii"
 # CONFIG_NTFS_FS is not set
 
 #
 # Pseudo filesystems
 #
 CONFIG_PROC_FS=y
+CONFIG_PROC_SYSCTL=y
 CONFIG_SYSFS=y
-CONFIG_DEVPTS_FS_XATTR=y
-# CONFIG_DEVPTS_FS_SECURITY is not set
 CONFIG_TMPFS=y
-# CONFIG_TMPFS_XATTR is not set
+# CONFIG_TMPFS_POSIX_ACL is not set
 # CONFIG_HUGETLB_PAGE is not set
 CONFIG_RAMFS=y
+CONFIG_CONFIGFS_FS=y
 
 #
 # Miscellaneous filesystems
 #
+# CONFIG_ADFS_FS is not set
+# CONFIG_AFFS_FS is not set
+# CONFIG_HFS_FS is not set
 # CONFIG_HFSPLUS_FS is not set
+# CONFIG_BEFS_FS is not set
+# CONFIG_BFS_FS is not set
+# CONFIG_EFS_FS is not set
+CONFIG_JFFS2_FS=y
+CONFIG_JFFS2_FS_DEBUG=0
+CONFIG_JFFS2_FS_WRITEBUFFER=y
+# CONFIG_JFFS2_SUMMARY is not set
+# CONFIG_JFFS2_FS_XATTR is not set
+# CONFIG_JFFS2_COMPRESSION_OPTIONS is not set
+CONFIG_JFFS2_ZLIB=y
+CONFIG_JFFS2_RTIME=y
+# CONFIG_JFFS2_RUBIN is not set
 # CONFIG_CRAMFS is not set
 # CONFIG_VXFS_FS is not set
 # CONFIG_HPFS_FS is not set
@@ -675,16 +1066,23 @@
 CONFIG_NFS_FS=y
 CONFIG_NFS_V3=y
 # CONFIG_NFS_V3_ACL is not set
+CONFIG_NFS_V4=y
+# CONFIG_NFS_DIRECTIO is not set
 # CONFIG_NFSD is not set
 CONFIG_ROOT_NFS=y
 CONFIG_LOCKD=y
 CONFIG_LOCKD_V4=y
 CONFIG_NFS_COMMON=y
 CONFIG_SUNRPC=y
+CONFIG_SUNRPC_GSS=y
+CONFIG_RPCSEC_GSS_KRB5=y
+# CONFIG_RPCSEC_GSS_SPKM3 is not set
 # CONFIG_SMB_FS is not set
 # CONFIG_CIFS is not set
 # CONFIG_NCP_FS is not set
 # CONFIG_CODA_FS is not set
+# CONFIG_AFS_FS is not set
+# CONFIG_9P_FS is not set
 
 #
 # Partition Types
@@ -734,26 +1132,51 @@
 # CONFIG_NLS_ISO8859_15 is not set
 # CONFIG_NLS_KOI8_R is not set
 # CONFIG_NLS_KOI8_U is not set
-# CONFIG_NLS_UTF8 is not set
+CONFIG_NLS_UTF8=y
+
+#
+# Distributed Lock Manager
+#
+# CONFIG_DLM is not set
+
+#
+# Profiling support
+#
+# CONFIG_PROFILING is not set
 
 #
 # Kernel hacking
 #
 # CONFIG_PRINTK_TIME is not set
+CONFIG_ENABLE_MUST_CHECK=y
+CONFIG_MAGIC_SYSRQ=y
+# CONFIG_UNUSED_SYMBOLS is not set
+# CONFIG_DEBUG_FS is not set
+# CONFIG_HEADERS_CHECK is not set
 CONFIG_DEBUG_KERNEL=y
-# CONFIG_MAGIC_SYSRQ is not set
-CONFIG_LOG_BUF_SHIFT=14
+# CONFIG_DEBUG_SHIRQ is not set
+CONFIG_LOG_BUF_SHIFT=17
+CONFIG_DETECT_SOFTLOCKUP=y
 # CONFIG_SCHEDSTATS is not set
+# CONFIG_TIMER_STATS is not set
 # CONFIG_DEBUG_SLAB is not set
-# CONFIG_DEBUG_SPINLOCK is not set
-# CONFIG_DEBUG_SPINLOCK_SLEEP is not set
+# CONFIG_DEBUG_RT_MUTEXES is not set
+# CONFIG_RT_MUTEX_TESTER is not set
+CONFIG_DEBUG_SPINLOCK=y
+# CONFIG_DEBUG_MUTEXES is not set
+CONFIG_DEBUG_SPINLOCK_SLEEP=y
+# CONFIG_DEBUG_LOCKING_API_SELFTESTS is not set
 # CONFIG_DEBUG_KOBJECT is not set
 CONFIG_DEBUG_BUGVERBOSE=y
 # CONFIG_DEBUG_INFO is not set
-# CONFIG_DEBUG_FS is not set
+# CONFIG_DEBUG_VM is not set
+# CONFIG_DEBUG_LIST is not set
 CONFIG_FRAME_POINTER=y
-CONFIG_DEBUG_USER=y
-CONFIG_DEBUG_ERRORS=y
+CONFIG_FORCED_INLINING=y
+# CONFIG_RCU_TORTURE_TEST is not set
+# CONFIG_FAULT_INJECTION is not set
+# CONFIG_DEBUG_USER is not set
+# CONFIG_DEBUG_ERRORS is not set
 CONFIG_DEBUG_LL=y
 # CONFIG_DEBUG_ICEDCC is not set
 
@@ -766,7 +1189,43 @@
 #
 # Cryptographic options
 #
-# CONFIG_CRYPTO is not set
+CONFIG_CRYPTO=y
+CONFIG_CRYPTO_ALGAPI=y
+CONFIG_CRYPTO_BLKCIPHER=y
+CONFIG_CRYPTO_HASH=m
+CONFIG_CRYPTO_MANAGER=y
+CONFIG_CRYPTO_HMAC=m
+# CONFIG_CRYPTO_XCBC is not set
+# CONFIG_CRYPTO_NULL is not set
+# CONFIG_CRYPTO_MD4 is not set
+CONFIG_CRYPTO_MD5=y
+# CONFIG_CRYPTO_SHA1 is not set
+# CONFIG_CRYPTO_SHA256 is not set
+# CONFIG_CRYPTO_SHA512 is not set
+# CONFIG_CRYPTO_WP512 is not set
+# CONFIG_CRYPTO_TGR192 is not set
+# CONFIG_CRYPTO_GF128MUL is not set
+# CONFIG_CRYPTO_ECB is not set
+CONFIG_CRYPTO_CBC=y
+CONFIG_CRYPTO_PCBC=m
+# CONFIG_CRYPTO_LRW is not set
+CONFIG_CRYPTO_DES=y
+# CONFIG_CRYPTO_FCRYPT is not set
+# CONFIG_CRYPTO_BLOWFISH is not set
+# CONFIG_CRYPTO_TWOFISH is not set
+# CONFIG_CRYPTO_SERPENT is not set
+# CONFIG_CRYPTO_AES is not set
+# CONFIG_CRYPTO_CAST5 is not set
+# CONFIG_CRYPTO_CAST6 is not set
+# CONFIG_CRYPTO_TEA is not set
+# CONFIG_CRYPTO_ARC4 is not set
+# CONFIG_CRYPTO_KHAZAD is not set
+# CONFIG_CRYPTO_ANUBIS is not set
+# CONFIG_CRYPTO_DEFLATE is not set
+# CONFIG_CRYPTO_MICHAEL_MIC is not set
+# CONFIG_CRYPTO_CRC32C is not set
+# CONFIG_CRYPTO_CAMELLIA is not set
+# CONFIG_CRYPTO_TEST is not set
 
 #
 # Hardware crypto devices
@@ -775,6 +1234,14 @@
 #
 # Library routines
 #
+CONFIG_BITREVERSE=y
 # CONFIG_CRC_CCITT is not set
+# CONFIG_CRC16 is not set
 CONFIG_CRC32=y
 # CONFIG_LIBCRC32C is not set
+CONFIG_AUDIT_GENERIC=y
+CONFIG_ZLIB_INFLATE=y
+CONFIG_ZLIB_DEFLATE=y
+CONFIG_PLIST=y
+CONFIG_HAS_IOMEM=y
+CONFIG_HAS_IOPORT=y
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91rm9200.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91rm9200.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91rm9200.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91rm9200.c	2007-07-29 05:23:04.000000000 +0200
@@ -267,6 +267,33 @@
 
 
 /* --------------------------------------------------------------------
+ *  Timer/Counter library initialization
+ * -------------------------------------------------------------------- */
+#ifdef CONFIG_ATMEL_TCLIB
+
+#include "tclib.h"
+
+static struct atmel_tcblock at91rm9200_tcblocks[] = {
+	[0] = {
+		.physaddr	= AT91RM9200_BASE_TCB0,
+		.irq		= { AT91RM9200_ID_TC0, AT91RM9200_ID_TC1, AT91RM9200_ID_TC2 },
+		.clk		= { &tc0_clk, &tc1_clk, &tc2_clk },
+	},
+	[1] = {
+		.physaddr	= AT91RM9200_BASE_TCB1,
+		.irq		= { AT91RM9200_ID_TC3, AT91RM9200_ID_TC4, AT91RM9200_ID_TC5 },
+		.clk		= { &tc3_clk, &tc4_clk, &tc5_clk },
+	},
+};
+
+#define at91rm9200_tc_init()	atmel_tc_init(at91rm9200_tcblocks, ARRAY_SIZE(at91rm9200_tcblocks))
+
+#else
+#define at91rm9200_tc_init()	do {} while(0)
+#endif
+
+
+/* --------------------------------------------------------------------
  *  AT91RM9200 processor initialization
  * -------------------------------------------------------------------- */
 void __init at91rm9200_initialize(unsigned long main_clock, unsigned short banks)
@@ -288,6 +315,9 @@
 
 	/* Initialize GPIO subsystem */
 	at91_gpio_init(at91rm9200_gpio, banks);
+
+	/* Initialize the Timer/Counter blocks */
+	at91rm9200_tc_init();
 }
 
 
@@ -301,28 +331,28 @@
 static unsigned int at91rm9200_default_irq_priority[NR_AIC_IRQS] __initdata = {
 	7,	/* Advanced Interrupt Controller (FIQ) */
 	7,	/* System Peripherals */
-	0,	/* Parallel IO Controller A */
-	0,	/* Parallel IO Controller B */
-	0,	/* Parallel IO Controller C */
-	0,	/* Parallel IO Controller D */
-	6,	/* USART 0 */
-	6,	/* USART 1 */
-	6,	/* USART 2 */
-	6,	/* USART 3 */
+	1,	/* Parallel IO Controller A */
+	1,	/* Parallel IO Controller B */
+	1,	/* Parallel IO Controller C */
+	1,	/* Parallel IO Controller D */
+	5,	/* USART 0 */
+	5,	/* USART 1 */
+	5,	/* USART 2 */
+	5,	/* USART 3 */
 	0,	/* Multimedia Card Interface */
-	4,	/* USB Device Port */
-	0,	/* Two-Wire Interface */
-	6,	/* Serial Peripheral Interface */
-	5,	/* Serial Synchronous Controller 0 */
-	5,	/* Serial Synchronous Controller 1 */
-	5,	/* Serial Synchronous Controller 2 */
+	2,	/* USB Device Port */
+	6,	/* Two-Wire Interface */
+	5,	/* Serial Peripheral Interface */
+	4,	/* Serial Synchronous Controller 0 */
+	4,	/* Serial Synchronous Controller 1 */
+	4,	/* Serial Synchronous Controller 2 */
 	0,	/* Timer Counter 0 */
 	0,	/* Timer Counter 1 */
 	0,	/* Timer Counter 2 */
 	0,	/* Timer Counter 3 */
 	0,	/* Timer Counter 4 */
 	0,	/* Timer Counter 5 */
-	3,	/* USB Host port */
+	2,	/* USB Host port */
 	3,	/* Ethernet MAC */
 	0,	/* Advanced Interrupt Controller (IRQ0) */
 	0,	/* Advanced Interrupt Controller (IRQ1) */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91rm9200_devices.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91rm9200_devices.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91rm9200_devices.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91rm9200_devices.c	2007-07-29 05:23:04.000000000 +0200
@@ -477,7 +477,18 @@
  *  SPI
  * -------------------------------------------------------------------- */
 
-#if defined(CONFIG_SPI_AT91) || defined(CONFIG_SPI_AT91_MODULE) || defined(CONFIG_AT91_SPI) || defined(CONFIG_AT91_SPI_MODULE)
+#if defined(CONFIG_AT91_SPI) || defined(CONFIG_AT91_SPI_MODULE)		/* legacy SPI driver */
+#define SPI_DEVNAME	"at91_spi"
+
+#elif defined(CONFIG_SPI_AT91) || defined(CONFIG_SPI_AT91_MODULE)	/* SPI bitbanging driver */
+#define SPI_DEVNAME	"at91_spi"
+
+#elif defined(CONFIG_SPI_ATMEL) || defined(CONFIG_SPI_ATMEL_MODULE)	/* new SPI driver */
+#define SPI_DEVNAME	"atmel_spi"
+
+#endif
+
+#ifdef SPI_DEVNAME
 static u64 spi_dmamask = 0xffffffffUL;
 
 static struct resource spi_resources[] = {
@@ -494,7 +505,7 @@
 };
 
 static struct platform_device at91rm9200_spi_device = {
-	.name		= "at91_spi",
+	.name		= SPI_DEVNAME,
 	.id		= 0,
 	.dev		= {
 				.dma_mask		= &spi_dmamask,
@@ -603,6 +614,32 @@
 #endif
 
 
+#if defined(CONFIG_NEW_LEDS)
+
+static struct platform_device at91_leds = {
+	.name		= "at91_leds",
+	.id		= -1,
+};
+
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr)
+{
+	if (!nr)
+		return;
+
+	at91_leds.dev.platform_data = leds;
+
+	for ( ; nr; nr--, leds++) {
+		leds->index = nr;	/* first record stores number of leds */
+		at91_set_gpio_output(leds->gpio, (leds->flags & 1) == 0);
+	}
+
+	platform_device_register(&at91_leds);
+}
+#else
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr) {}
+#endif
+
+
 /* --------------------------------------------------------------------
  *  UART
  * -------------------------------------------------------------------- */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9260.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9260.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9260.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9260.c	2007-07-29 05:23:04.000000000 +0200
@@ -269,6 +269,33 @@
 
 
 /* --------------------------------------------------------------------
+ *  Timer/Counter library initialization
+ * -------------------------------------------------------------------- */
+#ifdef CONFIG_ATMEL_TCLIB
+
+#include "tclib.h"
+
+static struct atmel_tcblock at91sam9260_tcblocks[] = {
+	[0] = {
+		.physaddr	= AT91SAM9260_BASE_TCB0,
+		.irq		= { AT91SAM9260_ID_TC0, AT91SAM9260_ID_TC1, AT91SAM9260_ID_TC2 },
+		.clk		= { &tc0_clk, &tc1_clk, &tc2_clk },
+	},
+	[1] = {
+		.physaddr	= AT91SAM9260_BASE_TCB1,
+		.irq		= { AT91SAM9260_ID_TC3, AT91SAM9260_ID_TC4, AT91SAM9260_ID_TC5 },
+		.clk		= { &tc3_clk, &tc4_clk, &tc5_clk },
+	},
+};
+
+#define at91sam9260_tc_init()	atmel_tc_init(at91sam9260_tcblocks, ARRAY_SIZE(at91sam9260_tcblocks))
+
+#else
+#define at91sam9260_tc_init()	do {} while(0)
+#endif
+
+
+/* --------------------------------------------------------------------
  *  AT91SAM9260 processor initialization
  * -------------------------------------------------------------------- */
 
@@ -315,6 +342,9 @@
 
 	/* Register GPIO subsystem */
 	at91_gpio_init(at91sam9260_gpio, 3);
+
+	/* Initialize the Timer/Counter blocks */
+	at91sam9260_tc_init();
 }
 
 /* --------------------------------------------------------------------
@@ -327,30 +357,30 @@
 static unsigned int at91sam9260_default_irq_priority[NR_AIC_IRQS] __initdata = {
 	7,	/* Advanced Interrupt Controller */
 	7,	/* System Peripherals */
-	0,	/* Parallel IO Controller A */
-	0,	/* Parallel IO Controller B */
-	0,	/* Parallel IO Controller C */
+	1,	/* Parallel IO Controller A */
+	1,	/* Parallel IO Controller B */
+	1,	/* Parallel IO Controller C */
 	0,	/* Analog-to-Digital Converter */
-	6,	/* USART 0 */
-	6,	/* USART 1 */
-	6,	/* USART 2 */
+	5,	/* USART 0 */
+	5,	/* USART 1 */
+	5,	/* USART 2 */
 	0,	/* Multimedia Card Interface */
-	4,	/* USB Device Port */
-	0,	/* Two-Wire Interface */
-	6,	/* Serial Peripheral Interface 0 */
-	6,	/* Serial Peripheral Interface 1 */
+	2,	/* USB Device Port */
+	6,	/* Two-Wire Interface */
+	5,	/* Serial Peripheral Interface 0 */
+	5,	/* Serial Peripheral Interface 1 */
 	5,	/* Serial Synchronous Controller */
 	0,
 	0,
 	0,	/* Timer Counter 0 */
 	0,	/* Timer Counter 1 */
 	0,	/* Timer Counter 2 */
-	3,	/* USB Host port */
+	2,	/* USB Host port */
 	3,	/* Ethernet */
 	0,	/* Image Sensor Interface */
-	6,	/* USART 3 */
-	6,	/* USART 4 */
-	6,	/* USART 5 */
+	5,	/* USART 3 */
+	5,	/* USART 4 */
+	5,	/* USART 5 */
 	0,	/* Timer Counter 3 */
 	0,	/* Timer Counter 4 */
 	0,	/* Timer Counter 5 */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9260_devices.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9260_devices.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9260_devices.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9260_devices.c	2007-07-29 05:23:04.000000000 +0200
@@ -524,6 +524,32 @@
 #endif
 
 
+#if defined(CONFIG_NEW_LEDS)
+
+static struct platform_device at91_leds = {
+	.name		= "at91_leds",
+	.id		= -1,
+};
+
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr)
+{
+	if (!nr)
+		return;
+
+	at91_leds.dev.platform_data = leds;
+
+	for ( ; nr; nr--, leds++) {
+		leds->index = nr;	/* first record stores number of leds */
+		at91_set_gpio_output(leds->gpio, (leds->flags & 1) == 0);
+	}
+
+	platform_device_register(&at91_leds);
+}
+#else
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr) {}
+#endif
+
+
 /* --------------------------------------------------------------------
  *  UART
  * -------------------------------------------------------------------- */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9261.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9261.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9261.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9261.c	2007-07-29 05:23:04.000000000 +0200
@@ -247,6 +247,28 @@
 
 
 /* --------------------------------------------------------------------
+ *  Timer/Counter library initialization
+ * -------------------------------------------------------------------- */
+#ifdef CONFIG_ATMEL_TCLIB
+
+#include "tclib.h"
+
+static struct atmel_tcblock at91sam9261_tcblocks[] = {
+	[0] = {
+		.physaddr	= AT91SAM9261_BASE_TCB0,
+		.irq		= { AT91SAM9261_ID_TC0, AT91SAM9261_ID_TC1, AT91SAM9261_ID_TC2 },
+		.clk		= { &tc0_clk, &tc1_clk, &tc2_clk },
+	}
+};
+
+#define at91sam9261_tc_init()	atmel_tc_init(at91sam9261_tcblocks, ARRAY_SIZE(at91sam9261_tcblocks))
+
+#else
+#define at91sam9261_tc_init()	do {} while(0)
+#endif
+
+
+/* --------------------------------------------------------------------
  *  AT91SAM9261 processor initialization
  * -------------------------------------------------------------------- */
 
@@ -267,6 +289,9 @@
 
 	/* Register GPIO subsystem */
 	at91_gpio_init(at91sam9261_gpio, 3);
+
+	/* Initialize the Timer/Counter blocks */
+	at91sam9261_tc_init();
 }
 
 /* --------------------------------------------------------------------
@@ -279,25 +304,25 @@
 static unsigned int at91sam9261_default_irq_priority[NR_AIC_IRQS] __initdata = {
 	7,	/* Advanced Interrupt Controller */
 	7,	/* System Peripherals */
-	0,	/* Parallel IO Controller A */
-	0,	/* Parallel IO Controller B */
-	0,	/* Parallel IO Controller C */
-	0,
-	6,	/* USART 0 */
-	6,	/* USART 1 */
-	6,	/* USART 2 */
+	1,	/* Parallel IO Controller A */
+	1,	/* Parallel IO Controller B */
+	1,	/* Parallel IO Controller C */
+	0,
+	5,	/* USART 0 */
+	5,	/* USART 1 */
+	5,	/* USART 2 */
 	0,	/* Multimedia Card Interface */
-	4,	/* USB Device Port */
-	0,	/* Two-Wire Interface */
-	6,	/* Serial Peripheral Interface 0 */
-	6,	/* Serial Peripheral Interface 1 */
-	5,	/* Serial Synchronous Controller 0 */
-	5,	/* Serial Synchronous Controller 1 */
-	5,	/* Serial Synchronous Controller 2 */
+	2,	/* USB Device Port */
+	6,	/* Two-Wire Interface */
+	5,	/* Serial Peripheral Interface 0 */
+	5,	/* Serial Peripheral Interface 1 */
+	4,	/* Serial Synchronous Controller 0 */
+	4,	/* Serial Synchronous Controller 1 */
+	4,	/* Serial Synchronous Controller 2 */
 	0,	/* Timer Counter 0 */
 	0,	/* Timer Counter 1 */
 	0,	/* Timer Counter 2 */
-	3,	/* USB Host port */
+	2,	/* USB Host port */
 	3,	/* LCD Controller */
 	0,
 	0,
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9261_devices.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9261_devices.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9261_devices.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9261_devices.c	2007-07-29 05:23:04.000000000 +0200
@@ -14,6 +14,9 @@
 #include <asm/mach/map.h>
 
 #include <linux/platform_device.h>
+#include <linux/fb.h>
+
+#include <video/atmel_lcdc.h>
 
 #include <asm/arch/board.h>
 #include <asm/arch/gpio.h>
@@ -522,6 +525,32 @@
 #endif
 
 
+#if defined(CONFIG_NEW_LEDS)
+
+static struct platform_device at91_leds = {
+	.name		= "at91_leds",
+	.id		= -1,
+};
+
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr)
+{
+	if (!nr)
+		return;
+
+	at91_leds.dev.platform_data = leds;
+
+	for ( ; nr; nr--, leds++) {
+		leds->index = nr;	/* first record stores number of leds */
+		at91_set_gpio_output(leds->gpio, (leds->flags & 1) == 0);
+	}
+
+	platform_device_register(&at91_leds);
+}
+#else
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr) {}
+#endif
+
+
 /* --------------------------------------------------------------------
  *  UART
  * -------------------------------------------------------------------- */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9263.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9263.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9263.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9263.c	2007-07-29 05:23:04.000000000 +0200
@@ -273,6 +273,28 @@
 
 
 /* --------------------------------------------------------------------
+ *  Timer/Counter library initialization
+ * -------------------------------------------------------------------- */
+#ifdef CONFIG_ATMEL_TCLIB
+
+#include "tclib.h"
+
+static struct atmel_tcblock at91sam9263_tcblocks[] = {
+	[0] = {
+		.physaddr	= AT91SAM9263_BASE_TCB0,
+		.irq		= { AT91SAM9263_ID_TCB, AT91SAM9263_ID_TCB, AT91SAM9263_ID_TCB },
+		.clk		= { &tcb_clk, &tcb_clk, &tcb_clk },
+	}
+};
+
+#define at91sam9263_tc_init()	atmel_tc_init(at91sam9263_tcblocks, ARRAY_SIZE(at91sam9263_tcblocks))
+
+#else
+#define at91sam9263_tc_init()	do {} while(0)
+#endif
+
+
+/* --------------------------------------------------------------------
  *  AT91SAM9263 processor initialization
  * -------------------------------------------------------------------- */
 
@@ -292,6 +314,9 @@
 
 	/* Register GPIO subsystem */
 	at91_gpio_init(at91sam9263_gpio, 5);
+
+	/* Initialize the Timer/Counter blocks */
+	at91sam9263_tc_init();
 }
 
 /* --------------------------------------------------------------------
@@ -304,34 +329,34 @@
 static unsigned int at91sam9263_default_irq_priority[NR_AIC_IRQS] __initdata = {
 	7,	/* Advanced Interrupt Controller (FIQ) */
 	7,	/* System Peripherals */
-	0,	/* Parallel IO Controller A */
-	0,	/* Parallel IO Controller B */
-	0,	/* Parallel IO Controller C, D and E */
+	1,	/* Parallel IO Controller A */
+	1,	/* Parallel IO Controller B */
+	1,	/* Parallel IO Controller C, D and E */
 	0,
 	0,
-	6,	/* USART 0 */
-	6,	/* USART 1 */
-	6,	/* USART 2 */
+	5,	/* USART 0 */
+	5,	/* USART 1 */
+	5,	/* USART 2 */
 	0,	/* Multimedia Card Interface 0 */
 	0,	/* Multimedia Card Interface 1 */
-	4,	/* CAN */
-	0,	/* Two-Wire Interface */
-	6,	/* Serial Peripheral Interface 0 */
-	6,	/* Serial Peripheral Interface 1 */
-	5,	/* Serial Synchronous Controller 0 */
-	5,	/* Serial Synchronous Controller 1 */
-	6,	/* AC97 Controller */
+	3,	/* CAN */
+	6,	/* Two-Wire Interface */
+	5,	/* Serial Peripheral Interface 0 */
+	5,	/* Serial Peripheral Interface 1 */
+	4,	/* Serial Synchronous Controller 0 */
+	4,	/* Serial Synchronous Controller 1 */
+	5,	/* AC97 Controller */
 	0,	/* Timer Counter 0, 1 and 2 */
 	0,	/* Pulse Width Modulation Controller */
 	3,	/* Ethernet */
 	0,
 	0,	/* 2D Graphic Engine */
-	3,	/* USB Device Port */
+	2,	/* USB Device Port */
 	0,	/* Image Sensor Interface */
 	3,	/* LDC Controller */
 	0,	/* DMA Controller */
 	0,
-	3,	/* USB Host port */
+	2,	/* USB Host port */
 	0,	/* Advanced Interrupt Controller (IRQ0) */
 	0,	/* Advanced Interrupt Controller (IRQ1) */
 };
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9263_devices.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9263_devices.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9263_devices.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9263_devices.c	2007-07-29 05:23:04.000000000 +0200
@@ -13,6 +13,9 @@
 #include <asm/mach/map.h>
 
 #include <linux/platform_device.h>
+#include <linux/fb.h>
+
+#include <video/atmel_lcdc.h>
 
 #include <asm/arch/board.h>
 #include <asm/arch/gpio.h>
@@ -625,6 +628,56 @@
 
 
 /* --------------------------------------------------------------------
+ *  Image Sensor Interface
+ * -------------------------------------------------------------------- */
+
+#if defined(CONFIG_VIDEO_AT91_ISI) || defined(CONFIG_VIDEO_AT91_ISI_MODULE)
+
+struct resource isi_resources[] = {
+	[0] = {
+		.start	= AT91SAM9263_BASE_ISI,
+		.end	= AT91SAM9263_BASE_ISI + SZ_16K - 1,
+		.flags	= IORESOURCE_MEM,
+	},
+	[1] = {
+		.start	= AT91SAM9263_ID_ISI,
+		.end	= AT91SAM9263_ID_ISI,
+		.flags	= IORESOURCE_IRQ,
+	},
+};
+
+static struct platform_device at91sam9263_isi_device = {
+	.name		= "at91_isi",
+	.id		= -1,
+	.resource	= isi_resources,
+	.num_resources	= ARRAY_SIZE(isi_resources),
+};
+
+void __init at91_add_device_isi(void)
+{
+	at91_set_A_periph(AT91_PIN_PE0, 0);	/* ISI_D0 */
+	at91_set_A_periph(AT91_PIN_PE1, 0);	/* ISI_D1 */
+	at91_set_A_periph(AT91_PIN_PE2, 0);	/* ISI_D2 */
+	at91_set_A_periph(AT91_PIN_PE3, 0);	/* ISI_D3 */
+	at91_set_A_periph(AT91_PIN_PE4, 0);	/* ISI_D4 */
+	at91_set_A_periph(AT91_PIN_PE5, 0);	/* ISI_D5 */
+	at91_set_A_periph(AT91_PIN_PE6, 0);	/* ISI_D6 */
+	at91_set_A_periph(AT91_PIN_PE7, 0);	/* ISI_D7 */
+	at91_set_A_periph(AT91_PIN_PE8, 0);	/* ISI_PCK */
+	at91_set_A_periph(AT91_PIN_PE9, 0);	/* ISI_HSYNC */
+	at91_set_A_periph(AT91_PIN_PE10, 0);	/* ISI_VSYNC */
+	at91_set_B_periph(AT91_PIN_PE11, 0);	/* ISI_MCK (PCK3) */
+	at91_set_B_periph(AT91_PIN_PE12, 0);	/* ISI_PD8 */
+	at91_set_B_periph(AT91_PIN_PE13, 0);	/* ISI_PD9 */
+	at91_set_B_periph(AT91_PIN_PE14, 0);	/* ISI_PD10 */
+	at91_set_B_periph(AT91_PIN_PE15, 0);	/* ISI_PD11 */
+}
+#else
+void __init at91_add_device_isi(void) {}
+#endif
+
+
+/* --------------------------------------------------------------------
  *  LCD Controller
  * -------------------------------------------------------------------- */
 
@@ -715,6 +768,32 @@
 #endif
 
 
+#if defined(CONFIG_NEW_LEDS)
+
+static struct platform_device at91_leds = {
+	.name		= "at91_leds",
+	.id		= -1,
+};
+
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr)
+{
+	if (!nr)
+		return;
+
+	at91_leds.dev.platform_data = leds;
+
+	for ( ; nr; nr--, leds++) {
+		leds->index = nr;	/* first record stores number of leds */
+		at91_set_gpio_output(leds->gpio, (leds->flags & 1) == 0);
+	}
+
+	platform_device_register(&at91_leds);
+}
+#else
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr) {}
+#endif
+
+
 /* --------------------------------------------------------------------
  *  UART
  * -------------------------------------------------------------------- */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9rl.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9rl.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9rl.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9rl.c	2007-07-29 05:23:04.000000000 +0200
@@ -246,6 +246,28 @@
 
 
 /* --------------------------------------------------------------------
+ *  Timer/Counter library initialization
+ * -------------------------------------------------------------------- */
+#ifdef CONFIG_ATMEL_TCLIB
+
+#include "tclib.h"
+
+static struct atmel_tcblock at91sam9rl_tcblocks[] = {
+	[0] = {
+		.physaddr	= AT91SAM9RL_BASE_TCB0,
+		.irq		= { AT91SAM9RL_ID_TC0, AT91SAM9RL_ID_TC1, AT91SAM9RL_ID_TC2 },
+		.clk		= { &tc0_clk, &tc1_clk, &tc2_clk },
+	}
+};
+
+#define at91sam9rl_tc_init()	atmel_tc_init(at91sam9rl_tcblocks, ARRAY_SIZE(at91sam9rl_tcblocks))
+
+#else
+#define at91sam9rl_tc_init()	do {} while(0)
+#endif
+
+
+/* --------------------------------------------------------------------
  *  AT91SAM9RL processor initialization
  * -------------------------------------------------------------------- */
 
@@ -284,6 +306,9 @@
 
 	/* Register GPIO subsystem */
 	at91_gpio_init(at91sam9rl_gpio, 4);
+	
+	/* Initialize the Timer/Counter blocks */
+	at91sam9rl_tc_init();
 }
 
 /* --------------------------------------------------------------------
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9rl_devices.c linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9rl_devices.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/at91sam9rl_devices.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/at91sam9rl_devices.c	2007-07-29 05:23:04.000000000 +0200
@@ -370,6 +370,32 @@
 #endif
 
 
+#if defined(CONFIG_NEW_LEDS)
+
+static struct platform_device at91_leds = {
+	.name		= "at91_leds",
+	.id		= -1,
+};
+
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr)
+{
+	if (!nr)
+		return;
+
+	at91_leds.dev.platform_data = leds;
+
+	for ( ; nr; nr--, leds++) {
+		leds->index = nr;	/* first record stores number of leds */
+		at91_set_gpio_output(leds->gpio, (leds->flags & 1) == 0);
+	}
+
+	platform_device_register(&at91_leds);
+}
+#else
+void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr) {}
+#endif
+
+
 /* --------------------------------------------------------------------
  *  UART
  * -------------------------------------------------------------------- */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-cam60.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-cam60.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-cam60.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-cam60.c	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,148 @@
+/*
+ * KwikByte CAM60
+ *
+ * based on board-sam9260ek.c
+ *   Copyright (C) 2005 SAN People
+ *   Copyright (C) 2006 Atmel
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#include <linux/types.h>
+#include <linux/init.h>
+#include <linux/mm.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/spi/spi.h>
+#include <linux/spi/flash.h>
+
+#include <asm/hardware.h>
+#include <asm/setup.h>
+#include <asm/mach-types.h>
+#include <asm/irq.h>
+
+#include <asm/mach/arch.h>
+#include <asm/mach/map.h>
+#include <asm/mach/irq.h>
+
+#include <asm/arch/board.h>
+#include <asm/arch/gpio.h>
+#include <asm/arch/at91sam926x_mc.h>
+
+#include "generic.h"
+
+
+/*
+ * Serial port configuration.
+ *    0 .. 5 = USART0 .. USART5
+ *    6      = DBGU
+ */
+static struct at91_uart_config __initdata cam60_uart_config = {
+	.console_tty	= 0,				/* ttyS0 */
+	.nr_tty		= 1,
+	.tty_map	= { 6, -1, -1, -1, -1, -1, -1 }	/* ttyS0, ..., ttyS6 */
+};
+
+static void __init cam60_map_io(void)
+{
+	/* Initialize processor: 10 MHz crystal */
+	at91sam9260_initialize(10000000);
+
+	/* Setup the serial ports and console */
+	at91_init_serial(&cam60_uart_config);
+}
+
+static void __init cam60_init_irq(void)
+{
+	at91sam9260_init_interrupts(NULL);
+}
+
+
+/*
+ * SPI devices.
+ */
+#if defined(CONFIG_MTD_DATAFLASH)
+static struct mtd_partition __initdata cam60_spi_partitions[] = {
+	{
+		.name	= "BOOT1",
+		.offset	= 0,
+		.size	= 4 * 1056,
+	},
+	{
+		.name	= "BOOT2",
+		.offset	= MTDPART_OFS_NXTBLK,
+		.size	= 256 * 1056,
+	},
+	{
+		.name	= "kernel",
+		.offset	= MTDPART_OFS_NXTBLK,
+		.size	= 2222 * 1056,
+	},
+	{
+		.name	= "file system",
+		.offset	= MTDPART_OFS_NXTBLK,
+		.size	= MTDPART_SIZ_FULL,
+	},
+};
+
+static struct flash_platform_data __initdata cam60_spi_flash_platform_data = {
+	.name		= "spi_flash",
+	.parts		= cam60_spi_partitions,
+	.nr_parts	= ARRAY_SIZE(cam60_spi_partitions)
+};
+#endif
+
+static struct spi_board_info cam60_spi_devices[] = {
+#if defined(CONFIG_MTD_DATAFLASH)
+	{	/* DataFlash chip */
+		.modalias	= "mtd_dataflash",
+		.chip_select	= 0,
+		.max_speed_hz	= 15 * 1000 * 1000,
+		.bus_num	= 0,
+		.platform_data	= &cam60_spi_flash_platform_data
+	},
+#endif
+};
+
+
+/*
+ * MACB Ethernet device
+ */
+static struct __initdata at91_eth_data cam60_macb_data = {
+	.phy_irq_pin	= AT91_PIN_PB5,
+	.is_rmii	= 0,
+};
+
+
+static void __init cam60_board_init(void)
+{
+	/* Serial */
+	at91_add_device_serial();
+	/* SPI */
+	at91_add_device_spi(cam60_spi_devices, ARRAY_SIZE(cam60_spi_devices));
+	/* Ethernet */
+	at91_add_device_eth(&cam60_macb_data);
+}
+
+MACHINE_START(CAM60, "KwikByte CAM60")
+	/* Maintainer: KwikByte */
+	.phys_io	= AT91_BASE_SYS,
+	.io_pg_offst	= (AT91_VA_BASE_SYS >> 18) & 0xfffc,
+	.boot_params	= AT91_SDRAM_BASE + 0x100,
+	.timer		= &at91sam926x_timer,
+	.map_io		= cam60_map_io,
+	.init_irq	= cam60_init_irq,
+	.init_machine	= cam60_board_init,
+MACHINE_END
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-chub.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-chub.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-chub.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-chub.c	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,132 @@
+/*
+ * linux/arch/arm/mach-at91/board-chub.c
+ *
+ *  Copyright (C) 2005 SAN People, adapted for Promwad Chub board
+ *  by Kuten Ivan
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#include <linux/types.h>
+#include <linux/init.h>
+#include <linux/mm.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <asm/hardware.h>
+#include <asm/setup.h>
+#include <asm/mach-types.h>
+#include <asm/irq.h>
+
+#include <asm/mach/arch.h>
+#include <asm/mach/map.h>
+#include <asm/mach/irq.h>
+
+#include <asm/arch/board.h>
+#include <asm/arch/gpio.h>
+
+#include "generic.h"
+
+/*
+ * Serial port configuration.
+ *    0 .. 3 = USART0 .. USART3
+ *    4      = DBGU
+ */
+static struct at91_uart_config __initdata chub_uart_config = {
+	.console_tty	= 0,				/* ttyS0 */
+	.nr_tty		= 5,
+	.tty_map	= { 4, 0, 1, 2, 3 }		/* ttyS0, ..., ttyS4 */
+};
+
+static void __init chub_init_irq(void)
+{
+	at91rm9200_init_interrupts(NULL);
+}
+
+static void __init chub_map_io(void)
+{
+	/* Initialize clocks: 18.432 MHz crystal */
+	at91rm9200_initialize(18432000, AT91RM9200_PQFP);
+
+	/* Setup the serial ports and console */
+	at91_init_serial(&chub_uart_config);
+}
+
+static struct at91_eth_data __initdata chub_eth_data = {
+	.phy_irq_pin	= AT91_PIN_PB29,
+	.is_rmii	= 0,
+};
+
+static struct mtd_partition __initdata chub_nand_partition[] = {
+	{
+		.name	= "NAND Partition 1",
+		.offset = 0,
+		.size	= MTDPART_SIZ_FULL,
+	},
+};
+
+static struct mtd_partition * __init nand_partitions(int size, int *num_partitions)
+{
+	*num_partitions = ARRAY_SIZE(chub_nand_partition);
+	return chub_nand_partition;
+}
+
+static struct at91_nand_data __initdata chub_nand_data = {
+	.ale		= 22,
+	.cle		= 21,
+	.enable_pin	= AT91_PIN_PA27,
+	.partition_info	= nand_partitions,
+};
+
+static struct spi_board_info chub_spi_devices[] = {
+	{	/* DataFlash chip */
+		.modalias	= "mtd_dataflash",
+		.chip_select	= 0,
+		.max_speed_hz	= 15 * 1000 * 1000,
+	},
+};
+
+static void __init chub_board_init(void)
+{
+	/* Serial */
+	at91_add_device_serial();
+	/* I2C */
+	at91_add_device_i2c();
+	/* Ethernet */
+	at91_add_device_eth(&chub_eth_data);
+	/* SPI */
+	at91_add_device_spi(chub_spi_devices, ARRAY_SIZE(chub_spi_devices));
+	/* NAND Flash */
+	at91_add_device_nand(&chub_nand_data);
+	/* Disable write protect for NAND */
+	at91_set_gpio_output(AT91_PIN_PB7, 1);
+	/* Power enable for 3x RS-232 and 1x RS-485 */
+	at91_set_gpio_output(AT91_PIN_PB9, 1);
+	/* Disable write protect for FRAM */
+	at91_set_gpio_output(AT91_PIN_PA21, 1);
+	/* Disable write protect for Dataflash */
+	at91_set_gpio_output(AT91_PIN_PA19, 1);
+}
+
+MACHINE_START(CHUB, "Promwad Chub")
+	/* Maintainer: Ivan Kuten AT Promwad DOT com */
+	.phys_io	= AT91_BASE_SYS,
+	.io_pg_offst	= (AT91_VA_BASE_SYS >> 18) & 0xfffc,
+	.boot_params	= AT91_SDRAM_BASE + 0x100,
+	.timer		= &at91rm9200_timer,
+	.map_io		= chub_map_io,
+	.init_irq	= chub_init_irq,
+	.init_machine	= chub_board_init,
+MACHINE_END
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-csb337.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-csb337.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-csb337.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-csb337.c	2007-07-29 05:23:04.000000000 +0200
@@ -24,6 +24,7 @@
 #include <linux/module.h>
 #include <linux/platform_device.h>
 #include <linux/spi/spi.h>
+#include <linux/interrupt.h>
 #include <linux/mtd/physmap.h>
 
 #include <asm/hardware.h>
@@ -59,6 +60,7 @@
 
 	/* Setup the LEDs */
 	at91_init_leds(AT91_PIN_PB0, AT91_PIN_PB1);
+	at91_set_gpio_output(AT91_PIN_PB2, 1);		/* third (unused) LED */
 
 	/* Setup the serial ports and console */
 	at91_init_serial(&csb337_uart_config);
@@ -149,6 +151,55 @@
 	.num_resources	= ARRAY_SIZE(csb_flash_resources),
 };
 
+static struct at91_gpio_led csb337_leds[] = {
+	{
+		.name		= "led0",
+		.gpio		= AT91_PIN_PB0,
+		.trigger	= "heartbeat",
+	},
+	{
+		.name		= "led1",
+		.gpio		= AT91_PIN_PB1,
+		.trigger	= "timer",
+	},
+	{
+		.name		= "led2",
+		.gpio		= AT91_PIN_PB2,
+	}
+};
+
+#if defined(CONFIG_CSB300_WAKE_SW0) || defined(CONFIG_CSB300_WAKE_SW1)
+static irqreturn_t switch_irq_handler(int irq, void *context)
+{
+	return IRQ_HANDLED;
+}
+
+static inline void __init switch_irq_setup(int irq, char *name, unsigned long mode)
+{
+	int res;
+
+	res = request_irq(irq, switch_irq_handler, IRQF_SAMPLE_RANDOM | mode, name, NULL);
+	if (res == 0)
+		enable_irq_wake(irq);
+}
+
+static void __init csb300_switches(void)
+{
+#ifdef CONFIG_CSB300_WAKE_SW0
+	at91_set_A_periph(AT91_PIN_PB29, 1);		/* IRQ0 */
+	switch_irq_setup(AT91RM9200_ID_IRQ0, "csb300_sw0", IRQF_TRIGGER_FALLING);
+#endif
+#ifdef CONFIG_CSB300_WAKE_SW1
+	at91_set_gpio_input(AT91_PIN_PB28, 1);
+	at91_set_deglitch(AT91_PIN_PB28, 1);
+	switch_irq_setup(AT91_PIN_PB28, "csb300_sw1", IRQF_TRIGGER_RISING | IRQF_TRIGGER_FALLING);
+#endif
+	/* there's also SW2 at PA21, GPIO or TIOA2 */
+}
+#else
+static void __init csb300_switches(void) {}
+#endif
+
 static void __init csb337_board_init(void)
 {
 	/* Serial */
@@ -168,8 +219,12 @@
 	at91_add_device_spi(csb337_spi_devices, ARRAY_SIZE(csb337_spi_devices));
 	/* MMC */
 	at91_add_device_mmc(0, &csb337_mmc_data);
+	/* LEDS */
+	at91_gpio_leds(csb337_leds, ARRAY_SIZE(csb337_leds));
 	/* NOR flash */
 	platform_device_register(&csb_flash);
+	/* Switches on CSB300 */
+	csb300_switches();
 }
 
 MACHINE_START(CSB337, "Cogent CSB337")
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-dk.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-dk.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-dk.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-dk.c	2007-07-29 05:23:04.000000000 +0200
@@ -73,6 +73,185 @@
 	at91rm9200_init_interrupts(NULL);
 }
 
+#if defined(CONFIG_FB_S1D13XXX) || defined(CONFIG_FB_S1D13XXX_MODULE)
+#include <video/s1d13xxxfb.h>
+#include <asm/arch/ics1523.h>
+
+/* EPSON S1D13806 FB */
+#define AT91_FB_REG_BASE	0x30000000L
+#define AT91_FB_REG_SIZE	0x200
+#define AT91_FB_VMEM_BASE	0x30200000L
+#define AT91_FB_VMEM_SIZE	0x140000L
+
+static void __init dk_init_video(void)
+{
+	/* NWAIT Signal */
+	at91_set_A_periph(AT91_PIN_PC6, 0);
+
+	/* Initialization of the Static Memory Controller for Chip Select 2 */
+	at91_sys_write(AT91_SMC_CSR(2), AT91_SMC_DBW_16			/* 16 bit */
+				| AT91_SMC_WSEN | AT91_SMC_NWS_(4)	/* wait states */
+				| AT91_SMC_TDF_(1)			/* float time */
+	);
+
+	at91_ics1523_init();
+}
+
+/* CRT:    (active)   640x480 60Hz (PCLK=CLKI=25.175MHz)
+   Memory: Embedded SDRAM (MCLK=CLKI3=50.000MHz) (BUSCLK=60.000MHz) */
+static const struct s1d13xxxfb_regval dk_s1dfb_initregs[] = {
+	{S1DREG_MISC,			0x00},	/* Enable Memory/Register select bit */
+	{S1DREG_COM_DISP_MODE,		0x00},	/* disable display output */
+	{S1DREG_GPIO_CNF0,		0x00},
+	{S1DREG_GPIO_CNF1,		0x00},
+	{S1DREG_GPIO_CTL0,		0x08},
+	{S1DREG_GPIO_CTL1,		0x00},
+	{S1DREG_CLK_CNF,		0x01},	/* no divide, MCLK source is CLKI3 0x02*/
+	{S1DREG_LCD_CLK_CNF,		0x00},
+	{S1DREG_CRT_CLK_CNF,		0x00},
+	{S1DREG_MPLUG_CLK_CNF,		0x00},
+	{S1DREG_CPU2MEM_WST_SEL,	0x01},	/* 2*period(MCLK) - 4ns > period(BCLK) */
+	{S1DREG_SDRAM_REF_RATE,		0x03},	/* 32768 <= MCLK <= 50000 (MHz) */
+	{S1DREG_SDRAM_TC0,		0x00},	/* MCLK source freq (MHz): */
+	{S1DREG_SDRAM_TC1,		0x01},	/* 42 <= MCLK <= 50 */
+	{S1DREG_MEM_CNF,		0x80},	/* SDRAM Initialization - needed before mem access */
+	{S1DREG_PANEL_TYPE,		0x25},	/* std TFT 16bit, 8bit SCP format 2, single passive LCD */
+	{S1DREG_MOD_RATE,		0x00},	/* toggle every FPFRAME */
+	{S1DREG_LCD_DISP_HWIDTH,	0x4F},	/* 680 pix */
+	{S1DREG_LCD_NDISP_HPER,		0x12},	/* 152 pix */
+	{S1DREG_TFT_FPLINE_START,	0x01},	/* 13 pix */
+	{S1DREG_TFT_FPLINE_PWIDTH,	0x0B},	/* 96 pix */
+	{S1DREG_LCD_DISP_VHEIGHT0,	0xDF},
+	{S1DREG_LCD_DISP_VHEIGHT1,	0x01},	/* 480 lines */
+	{S1DREG_LCD_NDISP_VPER,		0x2C},	/* 44 lines */
+	{S1DREG_TFT_FPFRAME_START,	0x0A},	/* 10 lines */
+	{S1DREG_TFT_FPFRAME_PWIDTH,	0x01},	/* 2 lines */
+	{S1DREG_LCD_DISP_MODE,		0x05},  /* 16 bpp */
+	{S1DREG_LCD_MISC,		0x00},	/* dithering enabled, dual panel buffer enabled */
+	{S1DREG_LCD_DISP_START0,	0x00},
+	{S1DREG_LCD_DISP_START1,	0xC8},
+	{S1DREG_LCD_DISP_START2,	0x00},
+	{S1DREG_LCD_MEM_OFF0,		0x80},
+	{S1DREG_LCD_MEM_OFF1,		0x02},
+	{S1DREG_LCD_PIX_PAN,		0x00},
+	{S1DREG_LCD_DISP_FIFO_HTC,	0x3B},
+	{S1DREG_LCD_DISP_FIFO_LTC,	0x3C},
+	{S1DREG_CRT_DISP_HWIDTH,	0x4F},	/* 680 pix */
+	{S1DREG_CRT_NDISP_HPER,		0x13},	/* 160 pix */
+	{S1DREG_CRT_HRTC_START,		0x01},	/* 13 pix */
+	{S1DREG_CRT_HRTC_PWIDTH,	0x0B},	/* 96 pix */
+	{S1DREG_CRT_DISP_VHEIGHT0,	0xDF},
+	{S1DREG_CRT_DISP_VHEIGHT1,	0x01},	/* 480 lines */
+	{S1DREG_CRT_NDISP_VPER,		0x2B},	/* 44 lines */
+	{S1DREG_CRT_VRTC_START,		0x09},	/* 10 lines */
+	{S1DREG_CRT_VRTC_PWIDTH,	0x01},	/* 2 lines */
+	{S1DREG_TV_OUT_CTL,		0x10},
+	{S1DREG_CRT_DISP_MODE,		0x05},	/* 16 bpp */
+	{S1DREG_CRT_DISP_START0,	0x00},
+	{S1DREG_CRT_DISP_START1,	0x00},
+	{S1DREG_CRT_DISP_START2,	0x00},
+	{S1DREG_CRT_MEM_OFF0,		0x80},
+	{S1DREG_CRT_MEM_OFF1,		0x02},
+	{S1DREG_CRT_PIX_PAN,		0x00},
+	{S1DREG_CRT_DISP_FIFO_HTC,	0x3B},
+	{S1DREG_CRT_DISP_FIFO_LTC,	0x3C},
+	{S1DREG_LCD_CUR_CTL,		0x00},	/* inactive */
+	{S1DREG_LCD_CUR_START,		0x01},
+	{S1DREG_LCD_CUR_XPOS0,		0x00},
+	{S1DREG_LCD_CUR_XPOS1,		0x00},
+	{S1DREG_LCD_CUR_YPOS0,		0x00},
+	{S1DREG_LCD_CUR_YPOS1,		0x00},
+	{S1DREG_LCD_CUR_BCTL0,		0x00},
+	{S1DREG_LCD_CUR_GCTL0,		0x00},
+	{S1DREG_LCD_CUR_RCTL0,		0x00},
+	{S1DREG_LCD_CUR_BCTL1,		0x1F},
+	{S1DREG_LCD_CUR_GCTL1,		0x3F},
+	{S1DREG_LCD_CUR_RCTL1,		0x1F},
+	{S1DREG_LCD_CUR_FIFO_HTC,	0x00},
+	{S1DREG_CRT_CUR_CTL,		0x00},	/* inactive */
+	{S1DREG_CRT_CUR_START,		0x01},
+	{S1DREG_CRT_CUR_XPOS0,		0x00},
+	{S1DREG_CRT_CUR_XPOS1,		0x00},
+	{S1DREG_CRT_CUR_YPOS0,		0x00},
+	{S1DREG_CRT_CUR_YPOS1,		0x00},
+	{S1DREG_CRT_CUR_BCTL0,		0x00},
+	{S1DREG_CRT_CUR_GCTL0,		0x00},
+	{S1DREG_CRT_CUR_RCTL0,		0x00},
+	{S1DREG_CRT_CUR_BCTL1,		0x1F},
+	{S1DREG_CRT_CUR_GCTL1,		0x3F},
+	{S1DREG_CRT_CUR_RCTL1,		0x1F},
+	{S1DREG_CRT_CUR_FIFO_HTC,	0x00},
+	{S1DREG_BBLT_CTL0,		0x00},
+	{S1DREG_BBLT_CTL0,		0x00},
+	{S1DREG_BBLT_CC_EXP,		0x00},
+	{S1DREG_BBLT_OP,		0x00},
+	{S1DREG_BBLT_SRC_START0,	0x00},
+	{S1DREG_BBLT_SRC_START1,	0x00},
+	{S1DREG_BBLT_SRC_START2,	0x00},
+	{S1DREG_BBLT_DST_START0,	0x00},
+	{S1DREG_BBLT_DST_START1,	0x00},
+	{S1DREG_BBLT_DST_START2,	0x00},
+	{S1DREG_BBLT_MEM_OFF0,		0x00},
+	{S1DREG_BBLT_MEM_OFF1,		0x00},
+	{S1DREG_BBLT_WIDTH0,		0x00},
+	{S1DREG_BBLT_WIDTH1,		0x00},
+	{S1DREG_BBLT_HEIGHT0,		0x00},
+	{S1DREG_BBLT_HEIGHT1,		0x00},
+	{S1DREG_BBLT_BGC0,		0x00},
+	{S1DREG_BBLT_BGC1,		0x00},
+	{S1DREG_BBLT_FGC0,		0x00},
+	{S1DREG_BBLT_FGC1,		0x00},
+	{S1DREG_LKUP_MODE,		0x00},	/* LCD LUT r | LCD and CRT/TV LUT w */
+	{S1DREG_LKUP_ADDR,		0x00},
+	{S1DREG_PS_CNF,			0x00},	/* Power Save disable */
+	{S1DREG_PS_STATUS,		0x02},	/* LCD Panel down, mem up */
+	{S1DREG_CPU2MEM_WDOGT,		0x00},
+	{S1DREG_COM_DISP_MODE,		0x02},	/* enable CRT display output */
+};
+
+static struct s1d13xxxfb_pdata dk_s1dfb_pdata = {
+	.initregs		= dk_s1dfb_initregs,
+	.initregssize		= ARRAY_SIZE(dk_s1dfb_initregs),
+	.platform_init_video	= dk_init_video,
+};
+
+static u64 s1dfb_dmamask = 0xffffffffUL;
+
+static struct resource dk_s1dfb_resource[] = {
+	[0] = {	/* video mem */
+		.name   = "s1d13806 memory",
+		.start  = AT91_FB_VMEM_BASE,
+		.end    = AT91_FB_VMEM_BASE + AT91_FB_VMEM_SIZE -1,
+		.flags  = IORESOURCE_MEM,
+	},
+	[1] = {	/* video registers */
+		.name   = "s1d13806 registers",
+		.start  = AT91_FB_REG_BASE,
+		.end    = AT91_FB_REG_BASE + AT91_FB_REG_SIZE -1,
+		.flags  = IORESOURCE_MEM,
+	},
+};
+
+static struct platform_device dk_s1dfb_device = {
+	.name		= "s1d13806fb",
+	.id		= -1,
+	.dev		= {
+			.dma_mask		= &s1dfb_dmamask,
+			.coherent_dma_mask	= 0xffffffff,
+			.platform_data		= &dk_s1dfb_pdata,
+	},
+	.resource	= dk_s1dfb_resource,
+	.num_resources	= ARRAY_SIZE(dk_s1dfb_resource),
+};
+
+static void __init dk_add_device_video(void)
+{
+	platform_device_register(&dk_s1dfb_device);
+}
+#else
+static void __init dk_add_device_video(void) {}
+#endif
+
 static struct at91_eth_data __initdata dk_eth_data = {
 	.phy_irq_pin	= AT91_PIN_PC4,
 	.is_rmii	= 1,
@@ -151,7 +330,7 @@
 #define DK_FLASH_SIZE	0x200000
 
 static struct physmap_flash_data dk_flash_data = {
-	.width	= 2,
+	.width		= 2,
 };
 
 static struct resource dk_flash_resource = {
@@ -170,6 +349,13 @@
 	.num_resources	= 1,
 };
 
+static struct at91_gpio_led dk_leds[] = {
+	{
+		.name		= "led0",
+		.gpio		= AT91_PIN_PB2,
+		.trigger	= "timer",
+	}
+};
 
 static void __init dk_board_init(void)
 {
@@ -200,8 +386,10 @@
 	at91_add_device_nand(&dk_nand_data);
 	/* NOR Flash */
 	platform_device_register(&dk_flash);
+	/* LEDs */
+	at91_gpio_leds(dk_leds, ARRAY_SIZE(dk_leds));
 	/* VGA */
-//	dk_add_device_video();
+	dk_add_device_video();
 }
 
 MACHINE_START(AT91RM9200DK, "Atmel AT91RM9200-DK")
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-ek.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-ek.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-ek.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-ek.c	2007-07-29 05:23:04.000000000 +0200
@@ -73,6 +73,187 @@
 	at91rm9200_init_interrupts(NULL);
 }
 
+#if defined(CONFIG_FB_S1D13XXX) || defined(CONFIG_FB_S1D13XXX_MODULE)
+#include <video/s1d13xxxfb.h>
+#include <asm/arch/ics1523.h>
+
+/* EPSON S1D13806 FB */
+#define AT91_FB_REG_BASE	0x40000000L
+#define	AT91_FB_REG_SIZE	0x200
+#define AT91_FB_VMEM_BASE	0x40200000L
+#define AT91_FB_VMEM_SIZE	0x140000L
+
+static void __init ek_init_video(void)
+{
+	/* NWAIT Signal */
+	at91_set_A_periph(AT91_PIN_PC6, 0);
+
+	/* Initialization of the Static Memory Controller for Chip Select 3 */
+	at91_sys_write(AT91_SMC_CSR(3), AT91_SMC_DBW_16			/* 16 bit */
+				| AT91_SMC_WSEN | AT91_SMC_NWS_(5)	/* wait states */
+				| AT91_SMC_TDF_(1)			/* float time */
+	);
+
+	at91_ics1523_init();
+}
+
+/* CRT:    (active)   640x480 60Hz (PCLK=CLKI=25.175MHz)
+   Memory: Embedded SDRAM (MCLK=CLKI3=50.000MHz) (BUSCLK=60.000MHz) */
+static const struct s1d13xxxfb_regval ek_s1dfb_initregs[] = {
+	{S1DREG_MISC,			0x00},	/* Enable Memory/Register select bit */
+	{S1DREG_COM_DISP_MODE,		0x00},	/* disable display output */
+	{S1DREG_GPIO_CNF0,		0xFF},	// 0x00
+	{S1DREG_GPIO_CNF1,		0x1F},	// 0x08
+	{S1DREG_GPIO_CTL0,		0x00},
+	{S1DREG_GPIO_CTL1,		0x00},
+	{S1DREG_CLK_CNF,		0x01},	/* no divide, MCLK source is CLKI3 0x02*/
+	{S1DREG_LCD_CLK_CNF,		0x00},
+	{S1DREG_CRT_CLK_CNF,		0x00},
+	{S1DREG_MPLUG_CLK_CNF,		0x00},
+	{S1DREG_CPU2MEM_WST_SEL,	0x01},	/* 2*period(MCLK) - 4ns > period(BCLK) */
+	{S1DREG_SDRAM_REF_RATE,		0x03},	/* 32768 <= MCLK <= 50000 (MHz) */
+	{S1DREG_SDRAM_TC0,		0x00},	/* MCLK source freq (MHz): */
+	{S1DREG_SDRAM_TC1,		0x01},	/* 42 <= MCLK <= 50 */
+	{S1DREG_MEM_CNF,		0x80},	/* SDRAM Initialization - needed before mem access */
+	{S1DREG_PANEL_TYPE,		0x25},	/* std TFT 16bit, 8bit SCP format 2, single passive LCD */
+	{S1DREG_MOD_RATE,		0x00},	/* toggle every FPFRAME */
+	{S1DREG_LCD_DISP_HWIDTH,	0x4F},	/* 680 pix */
+	{S1DREG_LCD_NDISP_HPER,		0x12},	/* 152 pix */
+	{S1DREG_TFT_FPLINE_START,	0x01},	/* 13 pix */
+	{S1DREG_TFT_FPLINE_PWIDTH,	0x0B},	/* 96 pix */
+	{S1DREG_LCD_DISP_VHEIGHT0,	0xDF},
+	{S1DREG_LCD_DISP_VHEIGHT1,	0x01},	/* 480 lines */
+	{S1DREG_LCD_NDISP_VPER,		0x2C},	/* 44 lines */
+	{S1DREG_TFT_FPFRAME_START,	0x0A},	/* 10 lines */
+	{S1DREG_TFT_FPFRAME_PWIDTH,	0x01},	/* 2 lines */
+	{S1DREG_LCD_DISP_MODE,		0x05},  /* 16 bpp */
+	{S1DREG_LCD_MISC,		0x00},	/* dithering enabled, dual panel buffer enabled */
+	{S1DREG_LCD_DISP_START0,	0x00},
+	{S1DREG_LCD_DISP_START1,	0xC8},
+	{S1DREG_LCD_DISP_START2,	0x00},
+	{S1DREG_LCD_MEM_OFF0,		0x80},
+	{S1DREG_LCD_MEM_OFF1,		0x02},
+	{S1DREG_LCD_PIX_PAN,		0x00},
+	{S1DREG_LCD_DISP_FIFO_HTC,	0x3B},
+	{S1DREG_LCD_DISP_FIFO_LTC,	0x3C},
+	{S1DREG_CRT_DISP_HWIDTH,	0x4F},	/* 680 pix */
+	{S1DREG_CRT_NDISP_HPER,		0x13},	/* 160 pix */
+	{S1DREG_CRT_HRTC_START,		0x01},	/* 13 pix */
+	{S1DREG_CRT_HRTC_PWIDTH,	0x0B},	/* 96 pix */
+	{S1DREG_CRT_DISP_VHEIGHT0,	0xDF},
+	{S1DREG_CRT_DISP_VHEIGHT1,	0x01},	/* 480 lines */
+	{S1DREG_CRT_NDISP_VPER,		0x2B},	/* 44 lines */
+	{S1DREG_CRT_VRTC_START,		0x09},	/* 10 lines */
+	{S1DREG_CRT_VRTC_PWIDTH,	0x01},	/* 2 lines */
+	{S1DREG_TV_OUT_CTL,		0x10},
+	{0x005E,			0x9F},
+	{0x005F,			0x00},
+	{S1DREG_CRT_DISP_MODE,		0x05},	/* 16 bpp */
+	{S1DREG_CRT_DISP_START0,	0x00},
+	{S1DREG_CRT_DISP_START1,	0x00},
+	{S1DREG_CRT_DISP_START2,	0x00},
+	{S1DREG_CRT_MEM_OFF0,		0x80},
+	{S1DREG_CRT_MEM_OFF1,		0x02},
+	{S1DREG_CRT_PIX_PAN,		0x00},
+	{S1DREG_CRT_DISP_FIFO_HTC,	0x3B},
+	{S1DREG_CRT_DISP_FIFO_LTC,	0x3C},
+	{S1DREG_LCD_CUR_CTL,		0x00},	/* inactive */
+	{S1DREG_LCD_CUR_START,		0x01},
+	{S1DREG_LCD_CUR_XPOS0,		0x00},
+	{S1DREG_LCD_CUR_XPOS1,		0x00},
+	{S1DREG_LCD_CUR_YPOS0,		0x00},
+	{S1DREG_LCD_CUR_YPOS1,		0x00},
+	{S1DREG_LCD_CUR_BCTL0,		0x00},
+	{S1DREG_LCD_CUR_GCTL0,		0x00},
+	{S1DREG_LCD_CUR_RCTL0,		0x00},
+	{S1DREG_LCD_CUR_BCTL1,		0x1F},
+	{S1DREG_LCD_CUR_GCTL1,		0x3F},
+	{S1DREG_LCD_CUR_RCTL1,		0x1F},
+	{S1DREG_LCD_CUR_FIFO_HTC,	0x00},
+	{S1DREG_CRT_CUR_CTL,		0x00},	/* inactive */
+	{S1DREG_CRT_CUR_START,		0x01},
+	{S1DREG_CRT_CUR_XPOS0,		0x00},
+	{S1DREG_CRT_CUR_XPOS1,		0x00},
+	{S1DREG_CRT_CUR_YPOS0,		0x00},
+	{S1DREG_CRT_CUR_YPOS1,		0x00},
+	{S1DREG_CRT_CUR_BCTL0,		0x00},
+	{S1DREG_CRT_CUR_GCTL0,		0x00},
+	{S1DREG_CRT_CUR_RCTL0,		0x00},
+	{S1DREG_CRT_CUR_BCTL1,		0x1F},
+	{S1DREG_CRT_CUR_GCTL1,		0x3F},
+	{S1DREG_CRT_CUR_RCTL1,		0x1F},
+	{S1DREG_CRT_CUR_FIFO_HTC,	0x00},
+	{S1DREG_BBLT_CTL0,		0x00},
+	{S1DREG_BBLT_CTL0,		0x00},
+	{S1DREG_BBLT_CC_EXP,		0x00},
+	{S1DREG_BBLT_OP,		0x00},
+	{S1DREG_BBLT_SRC_START0,	0x00},
+	{S1DREG_BBLT_SRC_START1,	0x00},
+	{S1DREG_BBLT_SRC_START2,	0x00},
+	{S1DREG_BBLT_DST_START0,	0x00},
+	{S1DREG_BBLT_DST_START1,	0x00},
+	{S1DREG_BBLT_DST_START2,	0x00},
+	{S1DREG_BBLT_MEM_OFF0,		0x00},
+	{S1DREG_BBLT_MEM_OFF1,		0x00},
+	{S1DREG_BBLT_WIDTH0,		0x00},
+	{S1DREG_BBLT_WIDTH1,		0x00},
+	{S1DREG_BBLT_HEIGHT0,		0x00},
+	{S1DREG_BBLT_HEIGHT1,		0x00},
+	{S1DREG_BBLT_BGC0,		0x00},
+	{S1DREG_BBLT_BGC1,		0x00},
+	{S1DREG_BBLT_FGC0,		0x00},
+	{S1DREG_BBLT_FGC1,		0x00},
+	{S1DREG_LKUP_MODE,		0x00},	/* LCD LUT r | LCD and CRT/TV LUT w */
+	{S1DREG_LKUP_ADDR,		0x00},
+	{S1DREG_PS_CNF,			0x10},	/* Power Save disable */
+	{S1DREG_PS_STATUS,		0x02},	/* LCD Panel down, mem up */
+	{S1DREG_CPU2MEM_WDOGT,		0x00},
+	{S1DREG_COM_DISP_MODE,		0x02},	/* enable CRT display output */
+};
+
+static struct s1d13xxxfb_pdata ek_s1dfb_pdata = {
+	.initregs		= ek_s1dfb_initregs,
+	.initregssize		= ARRAY_SIZE(ek_s1dfb_initregs),
+	.platform_init_video	= ek_init_video,
+};
+
+static u64 s1dfb_dmamask = 0xffffffffUL;
+
+static struct resource ek_s1dfb_resource[] = {
+	[0] = {	/* video mem */
+		.name   = "s1d13806 memory",
+		.start  = AT91_FB_VMEM_BASE,
+		.end    = AT91_FB_VMEM_BASE + AT91_FB_VMEM_SIZE -1,
+		.flags  = IORESOURCE_MEM,
+	},
+	[1] = {	/* video registers */
+		.name   = "s1d13806 registers",
+		.start  = AT91_FB_REG_BASE,
+		.end    = AT91_FB_REG_BASE + AT91_FB_REG_SIZE -1,
+		.flags  = IORESOURCE_MEM,
+	},
+};
+
+static struct platform_device ek_s1dfb_device = {
+	.name		= "s1d13806fb",
+	.id		= -1,
+	.dev		= {
+			.dma_mask		= &s1dfb_dmamask,
+			.coherent_dma_mask	= 0xffffffff,
+			.platform_data		= &ek_s1dfb_pdata,
+	},
+	.resource	= ek_s1dfb_resource,
+	.num_resources	= ARRAY_SIZE(ek_s1dfb_resource),
+};
+
+static void __init ek_add_device_video(void)
+{
+	platform_device_register(&ek_s1dfb_device);
+}
+#else
+static void __init ek_add_device_video(void) {}
+#endif
+
 static struct at91_eth_data __initdata ek_eth_data = {
 	.phy_irq_pin	= AT91_PIN_PC4,
 	.is_rmii	= 1,
@@ -113,7 +294,7 @@
 #define EK_FLASH_SIZE	0x200000
 
 static struct physmap_flash_data ek_flash_data = {
-	.width	= 2,
+	.width		= 2,
 };
 
 static struct resource ek_flash_resource = {
@@ -132,6 +313,18 @@
 	.num_resources	= 1,
 };
 
+static struct at91_gpio_led ek_leds[] = {
+	{
+		.name		= "led0",
+		.gpio		= AT91_PIN_PB1,
+		.trigger	= "heartbeat",
+	},
+	{
+		.name		= "led1",
+		.gpio		= AT91_PIN_PB2,
+		.trigger	= "timer",
+	}
+};
 
 static void __init ek_board_init(void)
 {
@@ -158,8 +351,10 @@
 #endif
 	/* NOR Flash */
 	platform_device_register(&ek_flash);
+	/* LEDs */
+	at91_gpio_leds(ek_leds, ARRAY_SIZE(ek_leds));
 	/* VGA */
-//	ek_add_device_video();
+	ek_add_device_video();
 }
 
 MACHINE_START(AT91RM9200EK, "Atmel AT91RM9200-EK")
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-kb9202.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-kb9202.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-kb9202.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-kb9202.c	2007-07-29 05:23:04.000000000 +0200
@@ -37,6 +37,8 @@
 #include <asm/arch/board.h>
 #include <asm/arch/gpio.h>
 
+#include <asm/arch/at91rm9200_mc.h>
+
 #include "generic.h"
 
 
@@ -111,6 +113,48 @@
 	.partition_info	= nand_partitions,
 };
 
+
+#if defined(CONFIG_FB_S1D15605)
+#warning "Rather pass reset pin via platform_data"
+static struct resource kb9202_lcd_resources[] = {
+	[0] = {
+		.start	= AT91_CHIPSELECT_2,
+		.end	= AT91_CHIPSELECT_2 + 0x200FF,
+		.flags	= IORESOURCE_MEM
+	},
+	[1] = {	/* reset pin */
+		.start	= AT91_PIN_PC22,
+		.end	= AT91_PIN_PC22,
+		.flags	= IORESOURCE_MEM
+	},
+};
+
+static struct platform_device kb9202_lcd_device = {
+	.name		= "s1d15605fb",
+	.id		= 0,
+	.num_resources	= ARRAY_SIZE(kb9202_lcd_resources),
+	.resource	= kb9202_lcd_resources,
+};
+
+static void __init kb9202_add_device_lcd(void)
+{
+ 	/* In case the boot loader did not set the chip select mode and timing */
+	at91_sys_write(AT91_SMC_CSR(2),
+		AT91_SMC_WSEN | AT91_SMC_NWS_(18) | AT91_SMC_TDF_(1) | AT91_SMC_DBW_8 |
+		AT91_SMC_RWSETUP_(1) | AT91_SMC_RWHOLD_(1));
+
+	/* Backlight pin = output, off */
+	at91_set_gpio_output(AT91_PIN_PC23, 0);
+
+	/* Reset pin = output, in reset */
+	at91_set_gpio_output(AT91_PIN_PC22, 0);
+
+	platform_device_register(&kb9202_lcd_device);
+}
+#else
+static void __init kb9202_add_device_lcd(void) {}
+#endif
+
 static void __init kb9202_board_init(void)
 {
 	/* Serial */
@@ -129,6 +173,8 @@
 	at91_add_device_spi(NULL, 0);
 	/* NAND */
 	at91_add_device_nand(&kb9202_nand_data);
+	/* LCD	*/
+	kb9202_add_device_lcd();
 }
 
 MACHINE_START(KB9200, "KB920x")
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-sam9261ek.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-sam9261ek.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-sam9261ek.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-sam9261ek.c	2007-07-29 05:23:04.000000000 +0200
@@ -27,6 +27,9 @@
 #include <linux/spi/spi.h>
 #include <linux/spi/ads7846.h>
 #include <linux/dm9000.h>
+#include <linux/fb.h>
+
+#include <video/atmel_lcdc.h>
 
 #include <asm/hardware.h>
 #include <asm/setup.h>
@@ -251,6 +254,7 @@
 		.bus_num	= 0,
 		.platform_data	= &ads_info,
 		.irq		= AT91SAM9261_ID_IRQ0,
+		.controller_data = AT91_PIN_PA28,	/* CS pin */
 	},
 #endif
 #if defined(CONFIG_MTD_AT91_DATAFLASH_CARD)
@@ -271,6 +275,65 @@
 };
 
 
+/*
+ * LCD Controller
+ */
+#if defined(CONFIG_FB_ATMEL) || defined(CONFIG_FB_ATMEL_MODULE)
+static struct fb_videomode at91_tft_vga_modes[] = {
+	{
+	        .name           = "TX09D50VM1CCA @ 60",
+		.refresh	= 60,
+		.xres		= 240,		.yres		= 320,
+		.pixclock	= KHZ2PICOS(4965),
+
+		.left_margin	= 1,		.right_margin	= 33,
+		.upper_margin	= 1,		.lower_margin	= 0,
+		.hsync_len	= 5,		.vsync_len	= 1,
+
+		.sync		= FB_SYNC_HOR_HIGH_ACT | FB_SYNC_VERT_HIGH_ACT,
+		.vmode		= FB_VMODE_NONINTERLACED,
+	},
+};
+
+static struct fb_monspecs at91fb_default_monspecs = {
+	.manufacturer	= "HIT",
+	.monitor        = "TX09D50VM1CCA",
+
+	.modedb		= at91_tft_vga_modes,
+	.modedb_len	= ARRAY_SIZE(at91_tft_vga_modes),
+	.hfmin		= 15000,
+	.hfmax		= 64000,
+	.vfmin		= 50,
+	.vfmax		= 150,
+};
+
+#define AT91SAM9261_DEFAULT_LCDCON2 	(ATMEL_LCDC_MEMOR_LITTLE \
+					| ATMEL_LCDC_DISTYPE_TFT    \
+					| ATMEL_LCDC_CLKMOD_ALWAYSACTIVE)
+
+static void at91_lcdc_power_control(int on)
+{
+	if (on)
+		at91_set_gpio_value(AT91_PIN_PA12, 0);	/* power up */
+	else
+		at91_set_gpio_value(AT91_PIN_PA12, 1);	/* power down */
+}
+
+/* Driver datas */
+static struct atmel_lcdfb_info __initdata ek_lcdc_data = {
+	.default_bpp			= 16,
+	.default_dmacon			= ATMEL_LCDC_DMAEN,
+	.default_lcdcon2		= AT91SAM9261_DEFAULT_LCDCON2,
+	.default_monspecs		= &at91fb_default_monspecs,
+	.atmel_lcdfb_power_control	= at91_lcdc_power_control,
+	.guard_time			= 1,
+};
+
+#else
+static struct atmel_lcdfb_info __initdata ek_lcdc_data;
+#endif
+
+
 static void __init ek_board_init(void)
 {
 	/* Serial */
@@ -296,6 +359,8 @@
 	/* MMC */
 	at91_add_device_mmc(0, &ek_mmc_data);
 #endif
+	/* LCD Controller */
+	at91_add_device_lcdc(&ek_lcdc_data);
 }
 
 MACHINE_START(AT91SAM9261EK, "Atmel AT91SAM9261-EK")
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/board-sam9263ek.c linux-2.6.22-rc5.new/arch/arm/mach-at91/board-sam9263ek.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/board-sam9263ek.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/board-sam9263ek.c	2007-07-29 05:23:04.000000000 +0200
@@ -26,6 +26,9 @@
 #include <linux/platform_device.h>
 #include <linux/spi/spi.h>
 #include <linux/spi/ads7846.h>
+#include <linux/fb.h>
+
+#include <video/atmel_lcdc.h>
 
 #include <asm/hardware.h>
 #include <asm/setup.h>
@@ -202,6 +205,65 @@
 
 
 /*
+ * LCD Controller
+ */
+#if defined(CONFIG_FB_ATMEL) || defined(CONFIG_FB_ATMEL_MODULE)
+static struct fb_videomode at91_tft_vga_modes[] = {
+	{
+	        .name           = "TX09D50VM1CCA @ 60",
+		.refresh	= 60,
+		.xres		= 240,		.yres		= 320,
+		.pixclock	= KHZ2PICOS(4965),
+
+		.left_margin	= 1,		.right_margin	= 33,
+		.upper_margin	= 1,		.lower_margin	= 0,
+		.hsync_len	= 5,		.vsync_len	= 1,
+
+		.sync		= FB_SYNC_HOR_HIGH_ACT | FB_SYNC_VERT_HIGH_ACT,
+		.vmode		= FB_VMODE_NONINTERLACED,
+	},
+};
+
+static struct fb_monspecs at91fb_default_monspecs = {
+	.manufacturer	= "HIT",
+	.monitor        = "TX09D70VM1CCA",
+
+	.modedb		= at91_tft_vga_modes,
+	.modedb_len	= ARRAY_SIZE(at91_tft_vga_modes),
+	.hfmin		= 15000,
+	.hfmax		= 64000,
+	.vfmin		= 50,
+	.vfmax		= 150,
+};
+
+#define AT91SAM9263_DEFAULT_LCDCON2 	(ATMEL_LCDC_MEMOR_LITTLE \
+					| ATMEL_LCDC_DISTYPE_TFT    \
+					| ATMEL_LCDC_CLKMOD_ALWAYSACTIVE)
+
+static void at91_lcdc_power_control(int on)
+{
+	if (on)
+		at91_set_gpio_value(AT91_PIN_PD12, 0);	/* power up */
+	else
+		at91_set_gpio_value(AT91_PIN_PD12, 1);	/* power down */
+}
+
+/* Driver datas */
+static struct atmel_lcdfb_info __initdata ek_lcdc_data = {
+	.default_bpp			= 16,
+	.default_dmacon			= ATMEL_LCDC_DMAEN,
+	.default_lcdcon2		= AT91SAM9263_DEFAULT_LCDCON2,
+	.default_monspecs		= &at91fb_default_monspecs,
+	.atmel_lcdfb_power_control	= at91_lcdc_power_control,
+	.guard_time			= 1,
+};
+
+#else
+static struct atmel_lcdfb_info __initdata ek_lcdc_data;
+#endif
+
+
+/*
  * AC97
  */
 static struct atmel_ac97_data ek_ac97_data = {
@@ -230,6 +292,8 @@
 	at91_add_device_nand(&ek_nand_data);
 	/* I2C */
 	at91_add_device_i2c();
+	/* LCD Controller */
+	at91_add_device_lcdc(&ek_lcdc_data);
 	/* AC97 */
 	at91_add_device_ac97(&ek_ac97_data);
 }
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/clock.c linux-2.6.22-rc5.new/arch/arm/mach-at91/clock.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/clock.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/clock.c	2007-07-29 05:23:04.000000000 +0200
@@ -32,6 +32,7 @@
 #include <asm/arch/cpu.h>
 
 #include "clock.h"
+#include "generic.h"
 
 
 /*
@@ -254,6 +255,23 @@
 
 /*------------------------------------------------------------------------*/
 
+#ifdef CONFIG_PM
+
+int clk_must_disable(struct clk *clk)
+{
+	if (!at91_suspend_entering_slow_clock())
+		return 0;
+
+	while (clk->parent)
+		clk = clk->parent;
+	return clk != &clk32k;
+}
+EXPORT_SYMBOL(clk_must_disable);
+
+#endif
+
+/*------------------------------------------------------------------------*/
+
 #ifdef CONFIG_AT91_PROGRAMMABLE_CLOCKS
 
 /*
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/generic.h linux-2.6.22-rc5.new/arch/arm/mach-at91/generic.h
--- linux-2.6.22-rc5/arch/arm/mach-at91/generic.h	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/generic.h	2007-07-29 05:23:04.000000000 +0200
@@ -36,6 +36,7 @@
  /* Power Management */
 extern void at91_irq_suspend(void);
 extern void at91_irq_resume(void);
+extern int at91_suspend_entering_slow_clock(void);
 
  /* GPIO */
 #define AT91RM9200_PQFP		3	/* AT91RM9200 PQFP package has 3 banks */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/ics1523.c linux-2.6.22-rc5.new/arch/arm/mach-at91/ics1523.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/ics1523.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/ics1523.c	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,207 @@
+/*
+ * arch/arm/mach-at91rm9200/ics1523.c
+ *
+ *  Copyright (C) 2003 ATMEL Rousset
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#include <asm/hardware.h>
+#include <asm/io.h>
+
+#include <linux/clk.h>
+#include <linux/delay.h>
+#include <linux/err.h>
+#include <linux/init.h>
+
+#include <asm/arch/ics1523.h>
+#include <asm/arch/at91_twi.h>
+#include <asm/arch/gpio.h>
+
+/* TWI Errors */
+#define	AT91_TWI_ERROR	(AT91_TWI_NACK | AT91_TWI_UNRE | AT91_TWI_OVRE)
+
+
+static void __iomem *twi_base;
+
+#define at91_twi_read(reg)		__raw_readl(twi_base + (reg))
+#define at91_twi_write(reg, val)	__raw_writel((val), twi_base + (reg))
+
+
+/* -----------------------------------------------------------------------------
+ * Initialization of TWI CLOCK
+ * ----------------------------------------------------------------------------- */
+
+static void at91_ics1523_SetTwiClock(unsigned int mck_khz)
+{
+	int sclock;
+
+	/* Here, CKDIV = 1 and CHDIV = CLDIV  ==> CLDIV = CHDIV = 1/4*((Fmclk/FTWI) -6) */
+	sclock = (10*mck_khz / ICS_TRANSFER_RATE);
+	if (sclock % 10 >= 5)
+		sclock = (sclock /10) - 5;
+	else
+		sclock = (sclock /10)- 6;
+	sclock = (sclock + (4 - sclock %4)) >> 2;	/* div 4 */
+
+	at91_twi_write(AT91_TWI_CWGR, 0x00010000 | sclock | (sclock << 8));
+}
+
+/* -----------------------------------------------------------------------------
+ * Read a byte with TWI Interface from the Clock Generator ICS1523
+ * ----------------------------------------------------------------------------- */
+
+static int at91_ics1523_ReadByte(unsigned char reg_address, unsigned char *data_in)
+{
+	int Status, nb_trial;
+
+	at91_twi_write(AT91_TWI_MMR, AT91_TWI_MREAD | AT91_TWI_IADRSZ_1 | ((ICS_ADDR << 16) & AT91_TWI_DADR));
+	at91_twi_write(AT91_TWI_IADR, reg_address);
+	at91_twi_write(AT91_TWI_CR, AT91_TWI_START | AT91_TWI_STOP);
+
+	/* Program temporizing period (300us) */
+	udelay(300);
+
+	/* Wait TXcomplete ... */
+	nb_trial = 0;
+	Status = at91_twi_read(AT91_TWI_SR);
+	while (!(Status & AT91_TWI_TXCOMP) && (nb_trial < 10)) {
+		nb_trial++;
+		Status = at91_twi_read(AT91_TWI_SR);
+	}
+
+	if (Status & AT91_TWI_TXCOMP) {
+		*data_in = (unsigned char) at91_twi_read(AT91_TWI_RHR);
+		return ICS1523_ACCESS_OK;
+	}
+	else
+		return ICS1523_ACCESS_ERROR;
+}
+
+/* -----------------------------------------------------------------------------
+ * Write a byte with TWI Interface to the Clock Generator ICS1523
+ * ----------------------------------------------------------------------------- */
+
+static int at91_ics1523_WriteByte(unsigned char reg_address, unsigned char data_out)
+{
+	int Status, nb_trial;
+
+	at91_twi_write(AT91_TWI_MMR, AT91_TWI_IADRSZ_1 | ((ICS_ADDR << 16) & AT91_TWI_DADR));
+	at91_twi_write(AT91_TWI_IADR, reg_address);
+	at91_twi_write(AT91_TWI_THR, data_out);
+	at91_twi_write(AT91_TWI_CR, AT91_TWI_START | AT91_TWI_STOP);
+
+	/* Program temporizing period (300us) */
+	udelay(300);
+
+	nb_trial = 0;
+	Status = at91_twi_read(AT91_TWI_SR);
+	while (!(Status & AT91_TWI_TXCOMP) && (nb_trial < 10)) {
+		nb_trial++;
+		if (Status & AT91_TWI_ERROR) {
+			/* If Underrun OR NACK - Start again */
+			at91_twi_write(AT91_TWI_CR, AT91_TWI_START | AT91_TWI_STOP);
+
+			/*  Program temporizing period (300us) */
+			udelay(300);
+		}
+		Status = at91_twi_read(AT91_TWI_SR);
+	};
+
+	if (Status & AT91_TWI_TXCOMP)
+		return ICS1523_ACCESS_OK;
+	else
+		return ICS1523_ACCESS_ERROR;
+}
+
+/* -----------------------------------------------------------------------------
+ * Initialization of the Clock Generator ICS1523
+ * ----------------------------------------------------------------------------- */
+
+int at91_ics1523_init(void)
+{
+	int		nb_trial;
+	int		ack = ICS1523_ACCESS_OK;
+	unsigned int	status = 0xffffffff;
+	struct clk	*twi_clk;
+
+	/* Map in TWI peripheral */
+	twi_base = ioremap(AT91RM9200_BASE_TWI, SZ_16K);
+	if (!twi_base)
+		return -ENOMEM;
+
+	/* pins used for TWI interface */
+	at91_set_A_periph(AT91_PIN_PA25, 0);            /* TWD */
+	at91_set_multi_drive(AT91_PIN_PA25, 1);
+	at91_set_A_periph(AT91_PIN_PA26, 0);            /* TWCK */
+	at91_set_multi_drive(AT91_PIN_PA26, 1);
+
+	/* Enable the TWI clock */
+	twi_clk = clk_get(NULL, "twi_clk");
+	if (IS_ERR(twi_clk))
+		return ICS1523_ACCESS_ERROR;
+	clk_enable(twi_clk);
+
+	/* Disable interrupts */
+	at91_twi_write(AT91_TWI_IDR, -1);
+
+	/* Reset peripheral */
+	at91_twi_write(AT91_TWI_CR, AT91_TWI_SWRST);
+
+	/* Set Master mode */
+	at91_twi_write(AT91_TWI_CR, AT91_TWI_MSEN);
+
+	/* Set TWI Clock Waveform Generator Register */
+	at91_ics1523_SetTwiClock(60000);     /* MCK in KHz = 60000 KHz */
+
+	/* ICS1523 Initialisation */
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_ICR, (unsigned char) 0);
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_OE, (unsigned char) (ICS_OEF | ICS_OET2 | ICS_OETCK));
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_OD, (unsigned char) (ICS_INSEL | 0x7F));
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_DPAO, (unsigned char) 0);
+
+	nb_trial = 0;
+	do {
+		nb_trial++;
+		ack |= at91_ics1523_WriteByte ((unsigned char) ICS_ICR, (unsigned char) (ICS_ENDLS | ICS_ENPLS | ICS_PDEN /*| ICS_FUNCSEL*/));
+		ack |= at91_ics1523_WriteByte ((unsigned char) ICS_LCR, (unsigned char) (ICS_PSD | ICS_PFD));
+		ack |= at91_ics1523_WriteByte ((unsigned char) ICS_FD0, (unsigned char) 0x39) ; /* 0x7A */
+		ack |= at91_ics1523_WriteByte ((unsigned char) ICS_FD1, (unsigned char) 0x00);
+		ack |= at91_ics1523_WriteByte ((unsigned char) ICS_SWRST, (unsigned char) (ICS_PLLR));
+
+		/* Program 1ms temporizing period */
+		mdelay(1);
+
+		at91_ics1523_ReadByte ((unsigned char) ICS_SR, (char *)&status);
+	} while (!((unsigned int) status & (unsigned int) ICS_PLLLOCK) && (nb_trial < 10));
+
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_DPAC, (unsigned char) 0x03) ; /* 0x01 */
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_SWRST, (unsigned char) (ICS_DPAR));
+
+	/* Program 1ms temporizing period */
+	mdelay(1);
+
+	ack |= at91_ics1523_WriteByte ((unsigned char) ICS_DPAO, (unsigned char) 0x00);
+
+	/* Program 1ms temporizing period */
+	mdelay(1);
+	
+	/* All done - cleanup */
+	iounmap(twi_base);
+	clk_disable(twi_clk);
+	clk_put(twi_clk);
+
+	return ack;
+}
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/Kconfig linux-2.6.22-rc5.new/arch/arm/mach-at91/Kconfig
--- linux-2.6.22-rc5/arch/arm/mach-at91/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/Kconfig	2007-07-29 05:23:04.000000000 +0200
@@ -97,6 +97,12 @@
 	help
 	  Select this if you are using Sperry-Sun's KAFA board.
 
+config MACH_CHUB
+	bool "Promwad Chub board"
+	depends on ARCH_AT91RM9200
+	help
+	  Select this if you are using Promwad's Chub board.
+
 endif
 
 # ----------------------------------------------------------
@@ -121,6 +127,13 @@
 	  Select this if you are using Atmel's AT91SAM9260-EK or AT91SAM9XE Evaluation Kit
 	  <http://www.atmel.com/dyn/products/tools_card.asp?tool_id=3933>
 
+config MACH_CAM60
+	bool "KwikByte CAM60 board"
+	depends on ARCH_AT91SAM9260
+	help
+	  Select this if you are using KwikByte's CAM60 board based on the Atmel AT91SAM9260.
+	  <http://www.kwikbyte.com>
+
 endif
 
 # ----------------------------------------------------------
@@ -184,6 +197,20 @@
 	  On AT91SAM926x boards both types of NAND flash can be present
 	  (8 and 16 bit data bus width).
 
+config CSB300_WAKE_SW0
+	bool "CSB300 SW0 irq0 wakeup"
+	depends on MACH_CSB337 && PM
+	help
+	  If you have a CSB300 connected to your CSB337, this lets
+	  SW0 serve as a wakeup button.  It uses IRQ0.
+
+config CSB300_WAKE_SW1
+	bool "CSB300 SW1 gpio wakeup"
+	depends on MACH_CSB337 && PM
+	help
+	  If you have a CSB300 connected to your CSB337, this lets
+	  SW1 serve as a wakeup button.  It uses GPIO.
+
 # ----------------------------------------------------------
 
 comment "AT91 Feature Selections"
@@ -194,6 +221,20 @@
 	  Select this if you need to program one or more of the PCK0..PCK3
 	  programmable clock outputs.
 
+config ATMEL_TCLIB
+	bool "Timer/Counter Library"
+	help
+	  Select this if you want a library to allocate the Timer/Counter
+	  blocks found on many Atmel processors.  This facilitates using
+	  these modules despite processor differences.
+
+config AT91_SLOW_CLOCK
+	bool "Suspend-to-RAM uses slow clock mode (EXPERIMENTAL)"
+	depends on PM && EXPERIMENTAL
+	help
+	  Select this if you wish to put the CPU into slow clock mode
+	  while in the "Suspend to RAM" state, to save more power.
+
 endmenu
 
 endif
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/Makefile linux-2.6.22-rc5.new/arch/arm/mach-at91/Makefile
--- linux-2.6.22-rc5/arch/arm/mach-at91/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/Makefile	2007-07-29 05:23:04.000000000 +0200
@@ -8,6 +8,8 @@
 obj-		:=
 
 obj-$(CONFIG_PM)		+= pm.o
+obj-$(CONFIG_AT91_SLOW_CLOCK)	+= pm_slowclock.o
+obj-$(CONFIG_ATMEL_TCLIB)	+= tclib.o
 
 # CPU-specific support
 obj-$(CONFIG_ARCH_AT91RM9200)	+= at91rm9200.o at91rm9200_time.o at91rm9200_devices.o
@@ -26,10 +28,12 @@
 obj-$(CONFIG_MACH_KB9200)	+= board-kb9202.o
 obj-$(CONFIG_MACH_ATEB9200)	+= board-eb9200.o
 obj-$(CONFIG_MACH_KAFA)		+= board-kafa.o
+obj-$(CONFIG_MACH_CHUB)		+= board-chub.o
 obj-$(CONFIG_MACH_PICOTUX2XX)	+= board-picotux200.o
 
 # AT91SAM9260 board-specific support
 obj-$(CONFIG_MACH_AT91SAM9260EK) += board-sam9260ek.o
+obj-$(CONFIG_MACH_CAM60)	+= board-cam60.o
 
 # AT91SAM9261 board-specific support
 obj-$(CONFIG_MACH_AT91SAM9261EK) += board-sam9261ek.o
@@ -51,7 +55,7 @@
 obj-$(CONFIG_LEDS) += $(led-y)
 
 # VGA support
-#obj-$(CONFIG_FB_S1D13XXX)	+= ics1523.o
+obj-$(CONFIG_FB_S1D13XXX)	+= ics1523.o
 
 
 ifeq ($(CONFIG_PM_DEBUG),y)
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/pm.c linux-2.6.22-rc5.new/arch/arm/mach-at91/pm.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/pm.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/pm.c	2007-07-29 05:23:04.000000000 +0200
@@ -63,6 +63,7 @@
  * Verify that all the clocks are correct before entering
  * slow-clock mode.
  */
+#warning "SAM9260 only has 3 programmable clocks."
 static int at91_pm_verify_clocks(void)
 {
 	unsigned long scsr;
@@ -103,20 +104,15 @@
 }
 
 /*
- * Call this from platform driver suspend() to see how deeply to suspend.
+ * This is called from clk_must_disable(), to see how deeply to suspend.
  * For example, some controllers (like OHCI) need one of the PLL clocks
  * in order to act as a wakeup source, and those are not available when
  * going into slow clock mode.
- *
- * REVISIT: generalize as clk_will_be_available(clk)?  Other platforms have
- * the very same problem (but not using at91 main_clk), and it'd be better
- * to add one generic API rather than lots of platform-specific ones.
  */
 int at91_suspend_entering_slow_clock(void)
 {
 	return (target_state == PM_SUSPEND_MEM);
 }
-EXPORT_SYMBOL(at91_suspend_entering_slow_clock);
 
 
 static void (*slow_clock)(void);
@@ -205,16 +201,23 @@
 	.enter		= at91_pm_enter,
 };
 
+#ifdef CONFIG_AT91_SLOW_CLOCK
+extern void at91rm9200_slow_clock(void);
+extern u32 at91rm9200_slow_clock_sz;
+#endif
+
 static int __init at91_pm_init(void)
 {
-	printk("AT91: Power Management\n");
-
-#ifdef CONFIG_AT91_PM_SLOW_CLOCK
-	/* REVISIT allocations of SRAM should be dynamically managed.
+#ifdef CONFIG_AT91_SLOW_CLOCK
+	/*
+	 * REVISIT allocations of SRAM should be dynamically managed.
 	 * FIQ handlers and other components will want SRAM/TCM too...
 	 */
-	slow_clock = (void *) (AT91_VA_BASE_SRAM + (3 * SZ_4K));
+	slow_clock = (void *) (AT91_IO_VIRT_BASE - AT91RM9200_SRAM_SIZE + (3 * SZ_4K));
 	memcpy(slow_clock, at91rm9200_slow_clock, at91rm9200_slow_clock_sz);
+	printk("AT91: Power Management (with slow clock mode)\n");
+#else
+	printk("AT91: Power Management\n");
 #endif
 
 	/* Disable SDRAM low-power mode.  Cannot be used with self-refresh. */
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/pm.c.orig linux-2.6.22-rc5.new/arch/arm/mach-at91/pm.c.orig
--- linux-2.6.22-rc5/arch/arm/mach-at91/pm.c.orig	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/pm.c.orig	2007-06-17 04:09:12.000000000 +0200
@@ -0,0 +1,227 @@
+/*
+ * arch/arm/mach-at91/pm.c
+ * AT91 Power Management
+ *
+ * Copyright (C) 2005 David Brownell
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ */
+
+#include <linux/pm.h>
+#include <linux/sched.h>
+#include <linux/proc_fs.h>
+#include <linux/pm.h>
+#include <linux/interrupt.h>
+#include <linux/sysfs.h>
+#include <linux/module.h>
+#include <linux/platform_device.h>
+
+#include <asm/io.h>
+#include <asm/irq.h>
+#include <asm/atomic.h>
+#include <asm/mach/time.h>
+#include <asm/mach/irq.h>
+#include <asm/mach-types.h>
+
+#include <asm/arch/at91_pmc.h>
+#include <asm/arch/at91rm9200_mc.h>
+#include <asm/arch/gpio.h>
+#include <asm/arch/cpu.h>
+
+#include "generic.h"
+
+
+static int at91_pm_valid_state(suspend_state_t state)
+{
+	switch (state) {
+		case PM_SUSPEND_ON:
+		case PM_SUSPEND_STANDBY:
+		case PM_SUSPEND_MEM:
+			return 1;
+
+		default:
+			return 0;
+	}
+}
+
+
+static suspend_state_t target_state;
+
+/*
+ * Called after processes are frozen, but before we shutdown devices.
+ */
+static int at91_pm_prepare(suspend_state_t state)
+{
+	target_state = state;
+	return 0;
+}
+
+/*
+ * Verify that all the clocks are correct before entering
+ * slow-clock mode.
+ */
+static int at91_pm_verify_clocks(void)
+{
+	unsigned long scsr;
+	int i;
+
+	scsr = at91_sys_read(AT91_PMC_SCSR);
+
+	/* USB must not be using PLLB */
+	if (cpu_is_at91rm9200()) {
+		if ((scsr & (AT91RM9200_PMC_UHP | AT91RM9200_PMC_UDP)) != 0) {
+			pr_debug("AT91: PM - Suspend-to-RAM with USB still active\n");
+			return 0;
+		}
+	} else if (cpu_is_at91sam9260() || cpu_is_at91sam9261() || cpu_is_at91sam9263()) {
+		if ((scsr & (AT91SAM926x_PMC_UHP | AT91SAM926x_PMC_UDP)) != 0) {
+			pr_debug("AT91: PM - Suspend-to-RAM with USB still active\n");
+			return 0;
+		}
+	}
+
+#ifdef CONFIG_AT91_PROGRAMMABLE_CLOCKS
+	/* PCK0..PCK3 must be disabled, or configured to use clk32k */
+	for (i = 0; i < 4; i++) {
+		u32 css;
+
+		if ((scsr & (AT91_PMC_PCK0 << i)) == 0)
+			continue;
+
+		css = at91_sys_read(AT91_PMC_PCKR(i)) & AT91_PMC_CSS;
+		if (css != AT91_PMC_CSS_SLOW) {
+			pr_debug("AT91: PM - Suspend-to-RAM with PCK%d src %d\n", i, css);
+			return 0;
+		}
+	}
+#endif
+
+	return 1;
+}
+
+/*
+ * Call this from platform driver suspend() to see how deeply to suspend.
+ * For example, some controllers (like OHCI) need one of the PLL clocks
+ * in order to act as a wakeup source, and those are not available when
+ * going into slow clock mode.
+ *
+ * REVISIT: generalize as clk_will_be_available(clk)?  Other platforms have
+ * the very same problem (but not using at91 main_clk), and it'd be better
+ * to add one generic API rather than lots of platform-specific ones.
+ */
+int at91_suspend_entering_slow_clock(void)
+{
+	return (target_state == PM_SUSPEND_MEM);
+}
+EXPORT_SYMBOL(at91_suspend_entering_slow_clock);
+
+
+static void (*slow_clock)(void);
+
+
+static int at91_pm_enter(suspend_state_t state)
+{
+	at91_gpio_suspend();
+	at91_irq_suspend();
+
+	pr_debug("AT91: PM - wake mask %08x, pm state %d\n",
+			/* remember all the always-wake irqs */
+			(at91_sys_read(AT91_PMC_PCSR)
+					| (1 << AT91_ID_FIQ)
+					| (1 << AT91_ID_SYS)
+					| (at91_extern_irq))
+				& at91_sys_read(AT91_AIC_IMR),
+			state);
+
+	switch (state) {
+		/*
+		 * Suspend-to-RAM is like STANDBY plus slow clock mode, so
+		 * drivers must suspend more deeply:  only the master clock
+		 * controller may be using the main oscillator.
+		 */
+		case PM_SUSPEND_MEM:
+			/*
+			 * Ensure that clocks are in a valid state.
+			 */
+			if (!at91_pm_verify_clocks())
+				goto error;
+
+			/*
+			 * Enter slow clock mode by switching over to clk32k and
+			 * turning off the main oscillator; reverse on wakeup.
+			 */
+			if (slow_clock) {
+				slow_clock();
+				break;
+			} else {
+				/* DEVELOPMENT ONLY */
+				pr_info("AT91: PM - no slow clock mode yet ...\n");
+				/* FALLTHROUGH leaving master clock alone */
+			}
+
+		/*
+		 * STANDBY mode has *all* drivers suspended; ignores irqs not
+		 * marked as 'wakeup' event sources; and reduces DRAM power.
+		 * But otherwise it's identical to PM_SUSPEND_ON:  cpu idle, and
+		 * nothing fancy done with main or cpu clocks.
+		 */
+		case PM_SUSPEND_STANDBY:
+			/*
+			 * NOTE: the Wait-for-Interrupt instruction needs to be
+			 * in icache so the SDRAM stays in self-refresh mode until
+			 * the wakeup IRQ occurs.
+			 */
+			asm("b 1f; .align 5; 1:");
+			asm("mcr p15, 0, r0, c7, c10, 4");	/* drain write buffer */
+			at91_sys_write(AT91_SDRAMC_SRR, 1);	/* self-refresh mode */
+			/* fall though to next state */
+
+		case PM_SUSPEND_ON:
+			asm("mcr p15, 0, r0, c7, c0, 4");	/* wait for interrupt */
+			break;
+
+		default:
+			pr_debug("AT91: PM - bogus suspend state %d\n", state);
+			goto error;
+	}
+
+	pr_debug("AT91: PM - wakeup %08x\n",
+			at91_sys_read(AT91_AIC_IPR) & at91_sys_read(AT91_AIC_IMR));
+
+error:
+	target_state = PM_SUSPEND_ON;
+	at91_irq_resume();
+	at91_gpio_resume();
+	return 0;
+}
+
+
+static struct pm_ops at91_pm_ops ={
+	.valid		= at91_pm_valid_state,
+	.prepare	= at91_pm_prepare,
+	.enter		= at91_pm_enter,
+};
+
+static int __init at91_pm_init(void)
+{
+	printk("AT91: Power Management\n");
+
+#ifdef CONFIG_AT91_PM_SLOW_CLOCK
+	/* REVISIT allocations of SRAM should be dynamically managed.
+	 * FIQ handlers and other components will want SRAM/TCM too...
+	 */
+	slow_clock = (void *) (AT91_VA_BASE_SRAM + (3 * SZ_4K));
+	memcpy(slow_clock, at91rm9200_slow_clock, at91rm9200_slow_clock_sz);
+#endif
+
+	/* Disable SDRAM low-power mode.  Cannot be used with self-refresh. */
+	at91_sys_write(AT91_SDRAMC_LPR, 0);
+
+	pm_set_ops(&at91_pm_ops);
+
+	return 0;
+}
+arch_initcall(at91_pm_init);
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/pm_slowclock.S linux-2.6.22-rc5.new/arch/arm/mach-at91/pm_slowclock.S
--- linux-2.6.22-rc5/arch/arm/mach-at91/pm_slowclock.S	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/pm_slowclock.S	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,172 @@
+/*
+ * arch/arm/mach-at91/pm_slow_clock.S
+ *
+ *  Copyright (C) 2006 Savin Zlobec
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ *
+ */
+
+#include <linux/linkage.h>
+#include <asm/hardware.h>
+#include <asm/arch/at91_pmc.h>
+#include <asm/arch/at91rm9200_mc.h>
+
+#define MCKRDY_TIMEOUT		1000
+#define MOSCRDY_TIMEOUT 	1000
+#define PLLALOCK_TIMEOUT	1000
+
+	.macro wait_mckrdy
+	mov	r2, #MCKRDY_TIMEOUT
+1:	sub	r2, r2, #1
+	cmp	r2, #0
+	beq	2f
+	ldr	r3, [r1, #AT91_PMC_SR]
+	tst	r3, #AT91_PMC_MCKRDY
+	beq	1b
+2:
+	.endm
+
+	.macro wait_moscrdy
+	mov	r2, #MOSCRDY_TIMEOUT
+1:	sub	r2, r2, #1
+	cmp	r2, #0
+	beq	2f
+	ldr	r3, [r1, #AT91_PMC_SR]
+	tst	r3, #AT91_PMC_MOSCS
+	beq	1b
+2:
+	.endm
+
+	.macro wait_pllalock
+	mov	r2, #PLLALOCK_TIMEOUT
+1:	sub	r2, r2, #1
+	cmp	r2, #0
+	beq	2f
+	ldr	r3, [r1, #AT91_PMC_SR]
+	tst	r3, #AT91_PMC_LOCKA
+	beq	1b
+2:
+	.endm
+
+	.macro wait_plladis
+	mov	r2, #PLLALOCK_TIMEOUT
+1:	sub	r2, r2, #1
+	cmp	r2, #0
+	beq	2f
+	ldr	r3, [r1, #AT91_PMC_SR]
+	tst	r3, #AT91_PMC_LOCKA
+	bne	1b
+2:
+	.endm
+
+	.text
+
+ENTRY(at91rm9200_slow_clock)
+
+	ldr	r1, .at91_va_base_sys
+
+	/* Put SDRAM in self refresh mode */
+
+	b	1f
+	.align	5
+1:	mcr	p15, 0, r0, c7, c10, 4
+	mov	r2, #1
+	str	r2, [r1, #AT91_SDRAMC_SRR]
+
+	/* Save Master clock setting */
+
+	ldr	r2, [r1, #AT91_PMC_MCKR]
+	str	r2, .saved_mckr
+
+	/*
+	 * Set the Master clock source to slow clock
+	 *
+	 * First set the CSS field, wait for MCKRDY
+	 * and than set the PRES and MDIV fields.
+	 *
+	 * See eratta #2[78] for details.
+	 */
+
+	bic	r2, r2, #3
+	str	r2, [r1, #AT91_PMC_MCKR]
+
+	wait_mckrdy
+
+	mov	r2, #0
+	str	r2, [r1, #AT91_PMC_MCKR]
+
+	/* Save PLLA setting and disable it */
+
+	ldr	r2, [r1, #AT91_CKGR_PLLAR]
+	str	r2, .saved_pllar
+
+	mov	r2, #0
+	str	r2, [r1, #AT91_CKGR_PLLAR]
+
+	wait_plladis
+
+	/* Turn off the main oscillator */
+
+	ldr	r2, [r1, #AT91_CKGR_MOR]
+	bic	r2, r2, #AT91_PMC_MOSCEN
+	str	r2, [r1, #AT91_CKGR_MOR]
+
+	/* Wait for interrupt */
+
+	mcr	p15, 0, r0, c7, c0, 4
+
+	/* Turn on the main oscillator */
+
+	ldr	r2, [r1, #AT91_CKGR_MOR]
+	orr	r2, r2, #AT91_PMC_MOSCEN
+	str	r2, [r1, #AT91_CKGR_MOR]
+
+	wait_moscrdy
+
+	/* Restore PLLA setting */
+
+	ldr	r2, .saved_pllar
+	str	r2, [r1, #AT91_CKGR_PLLAR]
+
+	wait_pllalock
+
+	/*
+	 * Restore master clock setting
+	 *
+	 * First set PRES if it was not 0,
+	 * than set CSS and MDIV fields.
+	 * After every change wait for
+	 * MCKRDY.
+	 *
+	 * See eratta #2[78] for details.
+	 */
+
+	ldr	r2, .saved_mckr
+	tst	r2, #0x1C
+	beq	2f
+	and	r2, r2, #0x1C
+	str	r2, [r1, #AT91_PMC_MCKR]
+
+	wait_mckrdy
+
+2:	ldr	r2, .saved_mckr
+	str	r2, [r1, #AT91_PMC_MCKR]
+
+	wait_mckrdy
+
+	mov	pc, lr
+
+.saved_mckr:
+	.word 0
+
+.saved_pllar:
+	.word 0
+
+.at91_va_base_sys:
+	.word AT91_VA_BASE_SYS
+
+ENTRY(at91rm9200_slow_clock_sz)
+	.word .-at91rm9200_slow_clock
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/tclib.c linux-2.6.22-rc5.new/arch/arm/mach-at91/tclib.c
--- linux-2.6.22-rc5/arch/arm/mach-at91/tclib.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/tclib.c	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,17 @@
+#include <linux/clk.h>
+#include <linux/kernel.h>
+#include <linux/module.h>
+
+#include "tclib.h"
+
+static struct atmel_tcblock *blocks;
+static int nblocks;
+
+/*
+ * Called from the processor-specific init to register the TC Blocks.
+ */
+void __init atmel_tc_init(struct atmel_tcblock *tcblocks, int n)
+{
+	blocks = tcblocks;
+	nblocks = n;
+}
diff -urN linux-2.6.22-rc5/arch/arm/mach-at91/tclib.h linux-2.6.22-rc5.new/arch/arm/mach-at91/tclib.h
--- linux-2.6.22-rc5/arch/arm/mach-at91/tclib.h	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/arch/arm/mach-at91/tclib.h	2007-07-29 05:23:04.000000000 +0200
@@ -0,0 +1,11 @@
+
+#define TC_PER_TCB	3
+
+struct atmel_tcblock {
+	u32 		physaddr;
+	void __iomem	*ioaddr;
+	struct clk	*clk[TC_PER_TCB];
+	int		irq[TC_PER_TCB];
+};
+
+extern void __init atmel_tc_init(struct atmel_tcblock *tcblocks, int n);
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/at91_mci.h linux-2.6-stable/include/asm-arm/arch-at91/at91_mci.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/at91_mci.h	Thu Apr 26 05:08:32 2007
+++ linux-2.6-stable/include/asm-arm/arch-at91/at91_mci.h	Tue May  8 12:13:31 2007
@@ -26,6 +26,9 @@
 #define AT91_MCI_MR		0x04		/* Mode Register */
 #define		AT91_MCI_CLKDIV		(0xff  <<  0)	/* Clock Divider */
 #define		AT91_MCI_PWSDIV		(7     <<  8)	/* Power Saving Divider */
+#define		AT91_MCI_RDPROOF	(1     << 11)	/* Read Proof Enable [SAM926[03] only] */
+#define		AT91_MCI_WRPROOF	(1     << 12)	/* Write Proof Enable [SAM926[03] only] */
+#define		AT91_MCI_PDCFBYTE	(1     << 13)	/* PDC Force Byte Transfer [SAM926[03] only] */
 #define		AT91_MCI_PDCPADV	(1     << 14)	/* PDC Padding Value */
 #define		AT91_MCI_PDCMODE	(1     << 15)	/* PDC-orientated Mode */
 #define		AT91_MCI_BLKLEN		(0xfff << 18)	/* Data Block Length */
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/at91_pmc.h linux-2.6-stable/include/asm-arm/arch-at91/at91_pmc.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/at91_pmc.h	Thu Apr 26 05:08:32 2007
+++ linux-2.6-stable/include/asm-arm/arch-at91/at91_pmc.h	Fri May 11 16:45:00 2007
@@ -37,7 +37,9 @@
 #define	AT91_PMC_PCDR		(AT91_PMC + 0x14)	/* Peripheral Clock Disable Register */
 #define	AT91_PMC_PCSR		(AT91_PMC + 0x18)	/* Peripheral Clock Status Register */
 
-#define	AT91_CKGR_MOR		(AT91_PMC + 0x20)	/* Main Oscillator Register */
+#define AT91_CKGR_UCKR		(AT91_PMC + 0x1C)	/* UTMI Clock Register [SAM9RL only] */
+
+#define	AT91_CKGR_MOR		(AT91_PMC + 0x20)	/* Main Oscillator Register [not on SAM9RL] */
 #define		AT91_PMC_MOSCEN		(1    << 0)		/* Main Oscillator Enable */
 #define		AT91_PMC_OSCBYPASS	(1    << 1)		/* Oscillator Bypass [AT91SAM926x only] */
 #define		AT91_PMC_OSCOUNT	(0xff << 8)		/* Main Oscillator Start-up Time */
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/at91sam9260_matrix.h linux-2.6-stable/include/asm-arm/arch-at91/at91sam9260_matrix.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/at91sam9260_matrix.h	Thu Apr 26 05:08:32 2007
+++ linux-2.6-stable/include/asm-arm/arch-at91/at91sam9260_matrix.h	Fri May 11 16:20:33 2007
@@ -67,7 +67,7 @@
 #define		AT91_MATRIX_CS4A		(1 << 4)	/* Chip Select 4 Assignment */
 #define			AT91_MATRIX_CS4A_SMC		(0 << 4)
 #define			AT91_MATRIX_CS4A_SMC_CF1	(1 << 4)
-#define		AT91_MATRIX_CS5A		(1 << 5 )	/* Chip Select 5 Assignment */
+#define		AT91_MATRIX_CS5A		(1 << 5)	/* Chip Select 5 Assignment */
 #define			AT91_MATRIX_CS5A_SMC		(0 << 5)
 #define			AT91_MATRIX_CS5A_SMC_CF2	(1 << 5)
 #define		AT91_MATRIX_DBPUC		(1 << 8)	/* Data Bus Pull-up Configuration */
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/board.h linux-2.6-stable/include/asm-arm/arch-at91/board.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/board.h	Thu May 17 12:13:17 2007
+++ linux-2.6-stable/include/asm-arm/arch-at91/board.h	Thu May 10 12:21:10 2007
@@ -124,9 +124,21 @@
 };
 extern void __init at91_add_device_ac97(struct atmel_ac97_data *data);
 
+ /* ISI */
+extern void __init at91_add_device_isi(void);
+
  /* LEDs */
 extern u8 at91_leds_cpu;
 extern u8 at91_leds_timer;
 extern void __init at91_init_leds(u8 cpu_led, u8 timer_led);
 
+struct at91_gpio_led {
+	u8		index;		/* index of LED */
+	char*		name;		/* name of LED */
+	u8		gpio;		/* AT91_PIN_xx */
+	u8		flags;		/* 1=active-high */
+	char*		trigger;	/* default trigger */
+};
+extern void __init at91_gpio_leds(struct at91_gpio_led *leds, int nr);
+
 #endif
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/ics1523.h linux-2.6-stable/include/asm-arm/arch-at91/ics1523.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/ics1523.h	Thu Jan  1 02:00:00 1970
+++ linux-2.6-stable/include/asm-arm/arch-at91/ics1523.h	Mon May 14 13:49:47 2007
@@ -0,0 +1,154 @@
+//*----------------------------------------------------------------------------
+//*         ATMEL Microcontroller Software Support  -  ROUSSET  -
+//*----------------------------------------------------------------------------
+//* The software is delivered "AS IS" without warranty or condition of any
+//* kind, either express, implied or statutory. This includes without
+//* limitation any warranty or condition with respect to merchantability or
+//* fitness for any particular purpose, or against the infringements of
+//* intellectual property rights of others.
+//*----------------------------------------------------------------------------
+//* File Name           : ics1523.h
+//* Object              : Clock Generator Prototyping File.
+//*
+//* 1.0 08/28/02 ED     : Creation
+//* 1.2 13/01/03 FB		: Update on lib V3
+//*----------------------------------------------------------------------------
+
+#ifndef ics1523_h
+#define ics1523_h
+
+/*-------------------------------------------*/
+/* ICS1523 TWI Serial Clock Definition       */
+/*-------------------------------------------*/
+
+#define		ICS_MIN_CLOCK		100		/* Min Frequency Access Clock KHz */
+#define		ICS_MAX_CLOCK		400		/* Max Frequency Access Clock KHz */
+#define		ICS_TRANSFER_RATE	ICS_MAX_CLOCK	/* Transfer speed to apply */
+
+#define		ICS_WRITE_CLK_PNB	30		/* TWCK Clock Periods required to write */
+#define		ICS_READ_CLK_PNB	40		/* TWCK Clock Periods required to read */
+
+/*-------------------------------------------*/
+/* ICS1523 Write Operation Definition        */
+/*-------------------------------------------*/
+
+#define		ICS1523_ACCESS_OK	0		/* OK */
+#define		ICS1523_ACCESS_ERROR	-1		/* NOK */
+
+/*-------------------------------------------*/
+/* ICS1523 Device Addresses Definition       */
+/*-------------------------------------------*/
+
+#define		ICS_ADDR		0x26		/* Device Address */
+
+/*--------------------------------------------------*/
+/* ICS1523 Registers Internal Addresses Definition  */
+/*--------------------------------------------------*/
+
+#define		ICS_ICR			0x0		/* Input Control Register */
+#define		ICS_LCR			0x1		/* Loop Control Register */
+#define		ICS_FD0			0x2		/* PLL FeedBack Divider LSBs */
+#define		ICS_FD1			0x3		/* PLL FeedBack Divider MSBs */
+#define		ICS_DPAO		0x4		/* Dynamic Phase Aligner Offset */
+#define		ICS_DPAC		0x5		/* Dynamic Phase Aligner Resolution */
+#define		ICS_OE			0x6		/* Output Enables Register */
+#define		ICS_OD			0x7		/* Osc Divider Register */
+#define		ICS_SWRST		0x8		/* DPA & PLL Reset Register */
+#define		ICS_VID			0x10		/* Chip Version Register */
+#define		ICS_RID			0x11		/* Chip Revision Register */
+#define		ICS_SR			0x12		/* Status Register */
+
+/*------------------------------------------------------*/
+/* ICS1523 Input Control Register Bits Definition       */
+/*------------------------------------------------------*/
+
+#define		ICS_PDEN		0x1		/* Phase Detector Enable */
+#define		ICS_PDPOL		0x2		/* Phase Detector Enable Polarity */
+#define		ICS_REFPOL		0x4		/* External Reference Polarity */
+#define		ICS_FBKPOL		0x8		/* External Feedback Polarity */
+#define		ICS_FBKSEL		0x10		/* External Feedback Select */
+#define		ICS_FUNCSEL		0x20		/* Function Out Select */
+#define		ICS_ENPLS		0x40		/* Enable PLL Lock/Ref Status Output */
+#define		ICS_ENDLS		0x80		/* Enable DPA Lock/Ref Status Output */
+
+/*-----------------------------------------------------*/
+/* ICS1523 Loop Control Register Bits Definition       */
+/*-----------------------------------------------------*/
+
+#define		ICS_PFD			0x7		/* Phase Detector Gain */
+#define		ICS_PSD			0x30		/* Post-Scaler Divider */
+
+/*----------------------------------------------------*/
+/* ICS1523 PLL FeedBack Divider LSBs Definition       */
+/*----------------------------------------------------*/
+
+#define		ICS_FBDL		0xFF		/* PLL FeedBack Divider LSBs */
+
+/*----------------------------------------------------*/
+/* ICS1523 PLL FeedBack Divider MSBs Definition       */
+/*----------------------------------------------------*/
+
+#define		ICS_FBDM		0xF		/* PLL FeedBack Divider MSBs */
+
+/*------------------------------------------------------------*/
+/* ICS1523 Dynamic Phase Aligner Offset Bits Definition       */
+/*------------------------------------------------------------*/
+
+#define		ICS_DPAOS		0x2F		/* Dynamic Phase Aligner Offset */
+#define		ICS_FILSEL		0x80		/* Loop Filter Select */
+
+/*----------------------------------------------------------------*/
+/* ICS1523 Dynamic Phase Aligner Resolution Bits Definition       */
+/*----------------------------------------------------------------*/
+
+#define		ICS_DPARES		0x3		/* Dynamic Phase Aligner Resolution */
+#define		ICS_MMREV		0xFC		/* Metal Mask Revision Number */
+
+/*-------------------------------------------------------*/
+/* ICS1523 Output Enables Register Bits Definition       */
+/*-------------------------------------------------------*/
+
+#define		ICS_OEPCK		0x1		/* Output Enable for PECL PCLK Outputs */
+#define		ICS_OETCK		0x2		/* Output Enable for STTL CLK Output */
+#define		ICS_OEP2		0x4		/* Output Enable for PECL CLK/2 Outputs */
+#define		ICS_OET2		0x8		/* Output Enable for STTL CLK/2 Output */
+#define		ICS_OEF			0x10		/* Output Enable for STTL FUNC Output */
+#define		ICS_CLK2INV		0x20		/* CLK/2 Invert */
+#define		ICS_OSCL		0xC0		/* SSTL Clock Scaler */
+
+/*----------------------------------------------------*/
+/* ICS1523 Osc Divider Register Bits Definition       */
+/*----------------------------------------------------*/
+
+#define		ICS_OSCDIV		0x7F		/* Oscillator Divider Modulus */
+#define		ICS_INSEL		0x80		/* Input Select */
+
+/*---------------------------------------------------*/
+/* ICS1523 DPA & PLL Reset Register Definition       */
+/*---------------------------------------------------*/
+
+#define		ICS_DPAR		0x0A		/* DPA Reset Command */
+#define		ICS_PLLR		0x50		/* PLL Reset Command */
+
+/*------------------------------------------------*/
+/* ICS1523 Chip Version Register Definition       */
+/*------------------------------------------------*/
+
+#define		ICS_CHIPV		0xFF		/* Chip Version */
+
+/*-------------------------------------------------*/
+/* ICS1523 Chip Revision Register Definition       */
+/*-------------------------------------------------*/
+
+#define		ICS_CHIPR		0xFF		/* Chip Revision */
+
+/*------------------------------------------*/
+/* ICS1523 Status Register Definition       */
+/*------------------------------------------*/
+
+#define		ICS_DPALOCK		0x1		/* DPA Lock Status */
+#define		ICS_PLLLOCK		0x2		/* PLL Lock Status */
+
+int at91_ics1523_init(void);
+
+#endif /* ics1523_h */
diff -urN -x CVS linux-2.6.22-rc1/include/asm-arm/arch-at91/spi.h linux-2.6-stable/include/asm-arm/arch-at91/spi.h
--- linux-2.6.22-rc1/include/asm-arm/arch-at91/spi.h	Thu Jan  1 02:00:00 1970
+++ linux-2.6-stable/include/asm-arm/arch-at91/spi.h	Mon May 14 13:49:47 2007
@@ -0,0 +1,54 @@
+/*
+ * Serial Peripheral Interface (SPI) driver for the Atmel AT91RM9200
+ *
+ * (c) SAN People (Pty) Ltd
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * as published by the Free Software Foundation; either version
+ * 2 of the License, or (at your option) any later version.
+ */
+
+#ifndef AT91_LEGACY_SPI_H
+#define AT91_LEGACY_SPI_H
+
+#define SPI_MAJOR		153	/* registered device number */
+
+#define DEFAULT_SPI_CLK		6000000
+
+
+/* Maximum number of buffers in a single SPI transfer.
+ *  DataFlash uses maximum of 2
+ *  spidev interface supports up to 8.
+ */
+#define MAX_SPI_TRANSFERS	8
+#define NR_SPI_DEVICES		4	/* number of devices on SPI bus */
+
+/*
+ * Describes the buffers for a SPI transfer.
+ * A transmit & receive buffer must be specified for each transfer
+ */
+struct spi_transfer_list {
+	void* tx[MAX_SPI_TRANSFERS];	/* transmit */
+	int txlen[MAX_SPI_TRANSFERS];
+	void* rx[MAX_SPI_TRANSFERS];	/* receive */
+	int rxlen[MAX_SPI_TRANSFERS];
+	int nr_transfers;		/* number of transfers */
+	int curr;			/* current transfer */
+};
+
+struct spi_local {
+	unsigned int pcs;		/* Peripheral Chip Select value */
+
+	struct spi_transfer_list *xfers;	/* current transfer list */
+	dma_addr_t tx, rx;		/* DMA address for current transfer */
+	dma_addr_t txnext, rxnext;	/* DMA address for next transfer */
+};
+
+
+/* Exported functions */
+extern void spi_access_bus(short device);
+extern void spi_release_bus(short device);
+extern int spi_transfer(struct spi_transfer_list* list);
+
+#endif
diff -urN -x CVS linux-2.6.22-rc1/include/linux/clk.h linux-2.6-stable/include/linux/clk.h
--- linux-2.6.22-rc1/include/linux/clk.h	Thu Apr 26 05:08:32 2007
+++ linux-2.6-stable/include/linux/clk.h	Tue May  8 12:13:31 2007
@@ -121,4 +121,24 @@
  */
 struct clk *clk_get_parent(struct clk *clk);
 
+/**
+ * clk_must_disable - report whether a clock's users must disable it
+ * @clk: one node in the clock tree
+ *
+ * This routine returns true only if the upcoming system state requires
+ * disabling the specified clock.
+ *
+ * It's common for platform power states to constrain certain clocks (and
+ * their descendants) to be unavailable, while other states allow that
+ * clock to be active.  A platform's power states often include an "all on"
+ * mode; system wide sleep states like "standby" or "suspend-to-RAM"; and
+ * operating states which sacrifice functionality for lower power usage.
+ *
+ * The constraint value is commonly tested in device driver suspend(), to
+ * leave clocks active if they are needed for features like wakeup events.
+ * On platforms that support reduced functionality operating states, the
+ * constraint may also need to be tested during resume() and probe() calls.
+ */
+int clk_must_disable(struct clk *clk);
+
 #endif
diff -urN -x CVS linux-2.6.22-rc1/include/linux/i2c-id.h linux-2.6-stable/include/linux/i2c-id.h
--- linux-2.6.22-rc1/include/linux/i2c-id.h	Thu May 17 12:13:23 2007
+++ linux-2.6-stable/include/linux/i2c-id.h	Mon May 14 10:18:35 2007
@@ -203,6 +203,7 @@
 
 /* --- PCA 9564 based algorithms */
 #define I2C_HW_A_ISA		0x1a0000 /* generic ISA Bus interface card */
+#define I2C_HW_A_PLAT		0x1a0001 /* generic platform_bus interface */
 
 /* --- ACPI Embedded controller algorithms                              */
 #define I2C_HW_ACPI_EC          0x1f0000
diff -urN -x CVS linux-2.6.22-rc1/sound/soc/at91/eti_b1_wm8731.c linux-2.6-stable/sound/soc/at91/eti_b1_wm8731.c
--- linux-2.6.22-rc1/sound/soc/at91/eti_b1_wm8731.c	Thu May 17 12:13:36 2007
+++ linux-2.6-stable/sound/soc/at91/eti_b1_wm8731.c	Mon May 14 10:19:04 2007
@@ -34,8 +34,7 @@
 #include <sound/soc.h>
 #include <sound/soc-dapm.h>
 
-#include <asm/arch/hardware.h>
-#include <asm/arch/at91_pio.h>
+#include <asm/hardware.h>
 #include <asm/arch/gpio.h>
 
 #include "../codecs/wm8731.h"
@@ -48,13 +47,6 @@
 #define	DBG(x...)
 #endif
 
-#define AT91_PIO_TF1	(1 << (AT91_PIN_PB6 - PIN_BASE) % 32)
-#define AT91_PIO_TK1	(1 << (AT91_PIN_PB7 - PIN_BASE) % 32)
-#define AT91_PIO_TD1	(1 << (AT91_PIN_PB8 - PIN_BASE) % 32)
-#define AT91_PIO_RD1	(1 << (AT91_PIN_PB9 - PIN_BASE) % 32)
-#define AT91_PIO_RK1	(1 << (AT91_PIN_PB10 - PIN_BASE) % 32)
-#define AT91_PIO_RF1	(1 << (AT91_PIN_PB11 - PIN_BASE) % 32)
-
 static struct clk *pck1_clk;
 static struct clk *pllb_clk;
 
@@ -277,7 +269,6 @@
 static int __init eti_b1_init(void)
 {
 	int ret;
-	u32 ssc_pio_lines;
 	struct at91_ssc_periph *ssc = eti_b1_dai.cpu_dai->private_data;
 
 	if (!request_mem_region(AT91RM9200_BASE_SSC1, SZ_16K, "soc-audio")) {
@@ -311,19 +302,12 @@
 		goto fail_io_unmap;
 	}
 
- 	ssc_pio_lines = AT91_PIO_TF1 | AT91_PIO_TK1 | AT91_PIO_TD1
-			| AT91_PIO_RD1 /* | AT91_PIO_RK1 */ | AT91_PIO_RF1;
-
-	/* Reset all PIO registers and assign lines to peripheral A */
- 	at91_sys_write(AT91_PIOB + PIO_PDR,  ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_ODR,  ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_IFDR, ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_CODR, ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_IDR,  ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_MDDR, ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_PUDR, ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_ASR,  ssc_pio_lines);
- 	at91_sys_write(AT91_PIOB + PIO_OWDR, ssc_pio_lines);
+ 	at91_set_A_periph(AT91_PIN_PB6, 0);	/* TF1 */
+ 	at91_set_A_periph(AT91_PIN_PB7, 0);	/* TK1 */
+ 	at91_set_A_periph(AT91_PIN_PB8, 0);	/* TD1 */
+ 	at91_set_A_periph(AT91_PIN_PB9, 0);	/* RD1 */
+/* 	at91_set_A_periph(AT91_PIN_PB10, 0);*/	/* RK1 */ 	
+ 	at91_set_A_periph(AT91_PIN_PB11, 0);	/* RF1 */
 
 	/*
 	 * Set PCK1 parent to PLLB and its rate to 12 Mhz.
diff -urN linux-2.6.22-rc5/drivers/char/at91_spi.c linux-2.6.22-rc5.new/drivers/char/at91_spi.c
--- linux-2.6.22-rc5/drivers/char/at91_spi.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/char/at91_spi.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,336 @@
+/*
+ * Serial Peripheral Interface (SPI) driver for the Atmel AT91RM9200 (Thunder)
+ *
+ *  Copyright (C) SAN People (Pty) Ltd
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * as published by the Free Software Foundation; either version
+ * 2 of the License, or (at your option) any later version.
+ */
+
+#include <linux/init.h>
+#include <linux/dma-mapping.h>
+#include <linux/module.h>
+#include <linux/sched.h>
+#include <linux/completion.h>
+#include <linux/interrupt.h>
+#include <linux/clk.h>
+#include <linux/platform_device.h>
+#include <linux/atmel_pdc.h>
+#include <asm/io.h>
+#include <asm/semaphore.h>
+
+#include <asm/arch/at91_spi.h>
+#include <asm/arch/board.h>
+#include <asm/arch/spi.h>
+
+#undef DEBUG_SPI
+
+static struct spi_local spi_dev[NR_SPI_DEVICES];	/* state of the SPI devices */
+static int spi_enabled = 0;
+static struct semaphore spi_lock;			/* protect access to SPI bus */
+static int current_device = -1;				/* currently selected SPI device */
+static struct clk *spi_clk;				/* SPI clock */
+static void __iomem *spi_base;				/* SPI peripheral base-address */
+
+DECLARE_COMPLETION(transfer_complete);
+
+
+#define at91_spi_read(reg)		__raw_readl(spi_base + (reg))
+#define at91_spi_write(reg, val)	__raw_writel((val), spi_base + (reg))
+
+
+/* ......................................................................... */
+
+/*
+ * Access and enable the SPI bus.
+ * This MUST be called before any transfers are performed.
+ */
+void spi_access_bus(short device)
+{
+	/* Ensure that requested device is valid */
+	if ((device < 0) || (device >= NR_SPI_DEVICES))
+		panic("at91_spi: spi_access_bus called with invalid device");
+
+	if (spi_enabled == 0) {
+		clk_enable(spi_clk);				/* Enable Peripheral clock */
+		at91_spi_write(AT91_SPI_CR, AT91_SPI_SPIEN);	/* Enable SPI */
+#ifdef DEBUG_SPI
+		printk("SPI on\n");
+#endif
+	}
+	spi_enabled++;
+
+	/* Lock the SPI bus */
+	down(&spi_lock);
+	current_device = device;
+
+	/* Configure SPI bus for device */
+	at91_spi_write(AT91_SPI_MR, AT91_SPI_MSTR | AT91_SPI_MODFDIS | (spi_dev[device].pcs << 16));
+}
+
+/*
+ * Relinquish control of the SPI bus.
+ */
+void spi_release_bus(short device)
+{
+	if (device != current_device)
+		panic("at91_spi: spi_release called with invalid device");
+
+	/* Release the SPI bus */
+	current_device = -1;
+	up(&spi_lock);
+
+	spi_enabled--;
+	if (spi_enabled == 0) {
+		at91_spi_write(AT91_SPI_CR, AT91_SPI_SPIDIS);	/* Disable SPI */
+		clk_disable(spi_clk);				/* Disable Peripheral clock */
+#ifdef DEBUG_SPI
+		printk("SPI off\n");
+#endif
+	}
+}
+
+/*
+ * Perform a data transfer over the SPI bus
+ */
+int spi_transfer(struct spi_transfer_list* list)
+{
+	struct spi_local *device = (struct spi_local *) &spi_dev[current_device];
+	int tx_size;
+
+	if (!list)
+		panic("at91_spi: spi_transfer called with NULL transfer list");
+	if (current_device == -1)
+		panic("at91_spi: spi_transfer called without acquiring bus");
+
+#ifdef DEBUG_SPI
+	printk("SPI transfer start [%i]\n", list->nr_transfers);
+#endif
+
+	/* If we are in 16-bit mode, we need to modify what we pass to the PDC */
+	tx_size = (at91_spi_read(AT91_SPI_CSR(current_device)) & AT91_SPI_BITS_16) ? 2 : 1;
+
+	/* Store transfer list */
+	device->xfers = list;
+	list->curr = 0;
+
+	/* Assume there must be at least one transfer */
+	device->tx = dma_map_single(NULL, list->tx[0], list->txlen[0], DMA_TO_DEVICE);
+	device->rx = dma_map_single(NULL, list->rx[0], list->rxlen[0], DMA_FROM_DEVICE);
+
+	/* Program PDC registers */
+	at91_spi_write(ATMEL_PDC_TPR, device->tx);
+	at91_spi_write(ATMEL_PDC_RPR, device->rx);
+	at91_spi_write(ATMEL_PDC_TCR, list->txlen[0] / tx_size);
+	at91_spi_write(ATMEL_PDC_RCR, list->rxlen[0] / tx_size);
+
+	/* Is there a second transfer? */
+	if (list->nr_transfers > 1) {
+		device->txnext = dma_map_single(NULL, list->tx[1], list->txlen[1], DMA_TO_DEVICE);
+		device->rxnext = dma_map_single(NULL, list->rx[1], list->rxlen[1], DMA_FROM_DEVICE);
+
+		/* Program Next PDC registers */
+		at91_spi_write(ATMEL_PDC_TNPR, device->txnext);
+		at91_spi_write(ATMEL_PDC_RNPR, device->rxnext);
+		at91_spi_write(ATMEL_PDC_TNCR, list->txlen[1] / tx_size);
+		at91_spi_write(ATMEL_PDC_RNCR, list->rxlen[1] / tx_size);
+	}
+	else {
+		device->txnext = 0;
+		device->rxnext = 0;
+		at91_spi_write(ATMEL_PDC_TNCR, 0);
+		at91_spi_write(ATMEL_PDC_RNCR, 0);
+	}
+
+	// TODO: If we are doing consecutive transfers (at high speed, or
+	//   small buffers), then it might be worth modifying the 'Delay between
+	//   Consecutive Transfers' in the CSR registers.
+	//   This is an issue if we cannot chain the next buffer fast enough
+	//   in the interrupt handler.
+
+	/* Enable transmitter and receiver */
+	at91_spi_write(ATMEL_PDC_PTCR, ATMEL_PDC_RXTEN | ATMEL_PDC_TXTEN);
+
+	at91_spi_write(AT91_SPI_IER, AT91_SPI_ENDRX);		/* enable buffer complete interrupt */
+	wait_for_completion(&transfer_complete);
+
+#ifdef DEBUG_SPI
+	printk("SPI transfer end\n");
+#endif
+
+	return 0;
+}
+
+/* ......................................................................... */
+
+/*
+ * Handle interrupts from the SPI controller.
+ */
+static irqreturn_t at91spi_interrupt(int irq, void *dev_id)
+{
+	unsigned int status;
+	struct spi_local *device = (struct spi_local *) &spi_dev[current_device];
+	struct spi_transfer_list *list = device->xfers;
+
+#ifdef DEBUG_SPI
+	printk("SPI interrupt %i\n", current_device);
+#endif
+
+	if (!list)
+		panic("at91_spi: spi_interrupt with a NULL transfer list");
+
+		status = at91_spi_read(AT91_SPI_SR) & at91_spi_read(AT91_SPI_IMR);	/* read status */
+
+	dma_unmap_single(NULL, device->tx, list->txlen[list->curr], DMA_TO_DEVICE);
+	dma_unmap_single(NULL, device->rx, list->rxlen[list->curr], DMA_FROM_DEVICE);
+
+	device->tx = device->txnext;	/* move next transfer to current transfer */
+	device->rx = device->rxnext;
+
+	list->curr = list->curr + 1;
+	if (list->curr == list->nr_transfers) {		/* all transfers complete */
+		at91_spi_write(AT91_SPI_IDR, AT91_SPI_ENDRX);		/* disable interrupt */
+
+		/* Disable transmitter and receiver */
+		at91_spi_write(ATMEL_PDC_PTCR, ATMEL_PDC_RXTDIS | ATMEL_PDC_TXTDIS);
+
+		device->xfers = NULL;
+		complete(&transfer_complete);
+	}
+	else if (list->curr+1 == list->nr_transfers) {	/* no more next transfers */
+		device->txnext = 0;
+		device->rxnext = 0;
+		at91_spi_write(ATMEL_PDC_TNCR, 0);
+		at91_spi_write(ATMEL_PDC_RNCR, 0);
+	}
+	else {
+		int i = (list->curr)+1;
+
+		/* If we are in 16-bit mode, we need to modify what we pass to the PDC */
+		int tx_size = (at91_spi_read(AT91_SPI_CSR(current_device)) & AT91_SPI_BITS_16) ? 2 : 1;
+
+		device->txnext = dma_map_single(NULL, list->tx[i], list->txlen[i], DMA_TO_DEVICE);
+		device->rxnext = dma_map_single(NULL, list->rx[i], list->rxlen[i], DMA_FROM_DEVICE);
+		at91_spi_write(ATMEL_PDC_TNPR, device->txnext);
+		at91_spi_write(ATMEL_PDC_RNPR, device->rxnext);
+		at91_spi_write(ATMEL_PDC_TNCR, list->txlen[i] / tx_size);
+		at91_spi_write(ATMEL_PDC_RNCR, list->rxlen[i] / tx_size);
+	}
+	return IRQ_HANDLED;
+}
+
+/* ......................................................................... */
+
+/*
+ * Initialize the SPI controller
+ */
+static int __init at91spi_probe(struct platform_device *pdev)
+{
+	int i;
+	unsigned long scbr;
+	struct resource *res;
+
+	init_MUTEX(&spi_lock);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res)
+		return -ENXIO;
+
+	if (!request_mem_region(res->start, res->end - res->start + 1, "at91_spi"))
+		return -EBUSY;
+
+	spi_base = ioremap(res->start, res->end - res->start + 1);
+	if (!spi_base) {
+		release_mem_region(res->start, res->end - res->start + 1);
+		return -ENOMEM;
+	}
+
+	spi_clk = clk_get(NULL, "spi_clk");
+	if (IS_ERR(spi_clk)) {
+		printk(KERN_ERR "at91_spi: no clock defined\n");
+		iounmap(spi_base);
+		release_mem_region(res->start, res->end - res->start + 1);
+		return -ENODEV;
+	}
+
+	at91_spi_write(AT91_SPI_CR, AT91_SPI_SWRST);	/* software reset of SPI controller */
+
+	/*
+	 * Calculate the correct SPI baud-rate divisor.
+	 */
+	scbr = clk_get_rate(spi_clk) / (2 * DEFAULT_SPI_CLK);
+	scbr = scbr + 1;		/* round up */
+
+	printk(KERN_INFO "at91_spi: Baud rate set to %ld\n", clk_get_rate(spi_clk) / (2 * scbr));
+
+	/* Set Chip Select registers to good defaults */
+	for (i = 0; i < 4; i++) {
+		at91_spi_write(AT91_SPI_CSR(i), AT91_SPI_CPOL | AT91_SPI_BITS_8 | (16 << 16) | (scbr << 8));
+	}
+
+	at91_spi_write(ATMEL_PDC_PTCR, ATMEL_PDC_RXTDIS | ATMEL_PDC_TXTDIS);
+
+	memset(&spi_dev, 0, sizeof(spi_dev));
+	spi_dev[0].pcs = 0xE;
+	spi_dev[1].pcs = 0xD;
+	spi_dev[2].pcs = 0xB;
+	spi_dev[3].pcs = 0x7;
+
+	if (request_irq(AT91RM9200_ID_SPI, at91spi_interrupt, 0, "spi", NULL)) {
+		clk_put(spi_clk);
+		iounmap(spi_base);
+		release_mem_region(res->start, res->end - res->start + 1);
+		return -EBUSY;
+	}
+
+	at91_spi_write(AT91_SPI_CR, AT91_SPI_SPIEN);		/* Enable SPI */
+
+	return 0;
+}
+
+static int __devexit at91spi_remove(struct platform_device *pdev)
+{
+	struct resource *res;
+
+	at91_spi_write(AT91_SPI_CR, AT91_SPI_SPIDIS);		/* Disable SPI */
+	clk_put(spi_clk);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	iounmap(spi_base);
+	release_mem_region(res->start, res->end - res->start + 1);
+
+	free_irq(AT91RM9200_ID_SPI, 0);
+	return 0;
+}
+
+static struct platform_driver at91spi_driver = {
+	.probe		= at91spi_probe,
+	.remove		= __devexit_p(at91spi_remove),
+	.driver		= {
+		.name	= "at91_spi",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static int __init at91spi_init(void)
+{
+	return platform_driver_register(&at91spi_driver);
+}
+
+static void __exit at91spi_exit(void)
+{
+	platform_driver_unregister(&at91spi_driver);
+}
+
+EXPORT_SYMBOL(spi_access_bus);
+EXPORT_SYMBOL(spi_release_bus);
+EXPORT_SYMBOL(spi_transfer);
+
+module_init(at91spi_init);
+module_exit(at91spi_exit);
+
+MODULE_LICENSE("GPL")
+MODULE_AUTHOR("Andrew Victor")
+MODULE_DESCRIPTION("SPI driver for Atmel AT91RM9200")
diff -urN linux-2.6.22-rc5/drivers/char/at91_spidev.c linux-2.6.22-rc5.new/drivers/char/at91_spidev.c
--- linux-2.6.22-rc5/drivers/char/at91_spidev.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/char/at91_spidev.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,236 @@
+/*
+ * User-space interface to the SPI bus on Atmel AT91RM9200
+ *
+ *  Copyright (C) 2003 SAN People (Pty) Ltd
+ *
+ * Based on SPI driver by Rick Bronson
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * as published by the Free Software Foundation; either version
+ * 2 of the License, or (at your option) any later version.
+ */
+
+#include <linux/module.h>
+#include <linux/init.h>
+#include <linux/slab.h>
+#include <linux/highmem.h>
+#include <linux/pagemap.h>
+#include <asm/arch/spi.h>
+
+#ifdef CONFIG_DEVFS_FS
+#include <linux/devfs_fs_kernel.h>
+#endif
+
+
+#undef DEBUG_SPIDEV
+
+/* ......................................................................... */
+
+/*
+ * Read or Write to SPI bus.
+ */
+static ssize_t spidev_rd_wr(struct file *file, char *buf, size_t count, loff_t *offset)
+{
+	unsigned int spi_device = (unsigned int) file->private_data;
+
+	struct mm_struct * mm;
+	struct page ** maplist;
+	struct spi_transfer_list* list;
+	int    pgcount;
+
+	unsigned int ofs, pagelen;
+	int res, i, err;
+
+	if (!count) {
+		return 0;
+	}
+
+	list = kmalloc(sizeof(struct spi_transfer_list), GFP_KERNEL);
+	if (!list) {
+		return -ENOMEM;
+	}
+
+	mm = current->mm;
+
+	pgcount = ((unsigned long)buf+count+PAGE_SIZE-1)/PAGE_SIZE - (unsigned long)buf/PAGE_SIZE;
+
+	if (pgcount >= MAX_SPI_TRANSFERS) {
+		kfree(list);
+		return -EFBIG;
+	}
+
+	maplist = kmalloc (pgcount * sizeof (struct page *), GFP_KERNEL);
+
+	if (!maplist) {
+		kfree(list);
+		return -ENOMEM;
+	}
+	flush_cache_all();
+	down_read(&mm->mmap_sem);
+	err= get_user_pages(current, mm, (unsigned long)buf, pgcount, 1, 0, maplist, NULL);
+	up_read(&mm->mmap_sem);
+
+	if (err < 0) {
+		kfree(list);
+		kfree(maplist);
+		return err;
+	}
+	pgcount = err;
+
+#ifdef DEBUG_SPIDEV
+	printk("spidev_rd_rw: %i %i\n", count, pgcount);
+#endif
+
+	/* Set default return value = transfer length */
+	res = count;
+
+	/*
+	 * At this point, the virtual area buf[0] .. buf[count-1] will have
+	 * corresponding pages mapped in the physical memory and locked until
+	 * we unmap the kiobuf.  The pages cannot be swapped out or moved
+	 * around.
+	 */
+	ofs = (unsigned long) buf & (PAGE_SIZE -1);
+	pagelen = PAGE_SIZE - ofs;
+	if (count < pagelen)
+		pagelen = count;
+
+	for (i = 0; i < pgcount; i++) {
+		flush_dcache_page(maplist[i]);
+
+		list->tx[i] = list->rx[i] = page_address(maplist[i]) + ofs;
+		list->txlen[i] = list->rxlen[i] = pagelen;
+
+#ifdef DEBUG_SPIDEV
+		printk("  %i: %x  (%i)\n", i, list->tx[i], list->txlen[i]);
+#endif
+
+		ofs = 0;	/* all subsequent transfers start at beginning of a page */
+		count = count - pagelen;
+		pagelen = (count < PAGE_SIZE) ? count : PAGE_SIZE;
+	}
+	list->nr_transfers = pgcount;
+
+	/* Perform transfer on SPI bus */
+	spi_access_bus(spi_device);
+	spi_transfer(list);
+	spi_release_bus(spi_device);
+
+	while (pgcount--) {
+		page_cache_release (maplist[pgcount]);
+	}
+	flush_cache_all();
+
+	kfree(maplist);
+	kfree(list);
+
+	return res;
+}
+
+static int spidev_ioctl(struct inode *inode, struct file *file, unsigned int cmd, unsigned long arg)
+{
+	int spi_device = MINOR(inode->i_rdev);
+
+	if (spi_device >= NR_SPI_DEVICES)
+		return -ENODEV;
+
+	// TODO: This interface can be used to configure the SPI bus.
+	// Configurable options could include: Speed, Clock Polarity, Clock Phase
+
+	switch(cmd) {
+		default:
+			return -ENOIOCTLCMD;
+	}
+}
+
+/*
+ * Open the SPI device
+ */
+static int spidev_open(struct inode *inode, struct file *file)
+{
+	unsigned int spi_device = MINOR(inode->i_rdev);
+
+	if (spi_device >= NR_SPI_DEVICES)
+		return -ENODEV;
+
+	/*
+	 * 'private_data' is actually a pointer, but we overload it with the
+	 * value we want to store.
+	 */
+	file->private_data = (void *)spi_device;
+
+	return 0;
+}
+
+/*
+ * Close the SPI device
+ */
+static int spidev_close(struct inode *inode, struct file *file)
+{
+	return 0;
+}
+
+/* ......................................................................... */
+
+static struct file_operations spidev_fops = {
+	.owner		= THIS_MODULE,
+	.llseek		= no_llseek,
+	.read		= spidev_rd_wr,
+	.write		= (int (*) (struct file *file, const char *buf, size_t count, loff_t *offset))spidev_rd_wr,
+	.ioctl		= spidev_ioctl,
+	.open		= spidev_open,
+	.release	= spidev_close,
+};
+
+/*
+ * Install the SPI /dev interface driver
+ */
+static int __init at91_spidev_init(void)
+{
+#ifdef CONFIG_DEVFS_FS
+	int i;
+#endif
+
+	if (register_chrdev(SPI_MAJOR, "spi", &spidev_fops)) {
+		printk(KERN_ERR "at91_spidev: Unable to get major %d for SPI bus\n", SPI_MAJOR);
+		return -EIO;
+	}
+
+#ifdef CONFIG_DEVFS_FS
+	devfs_mk_dir("spi");
+	for (i = 0; i < NR_SPI_DEVICES; i++) {
+		devfs_mk_cdev(MKDEV(SPI_MAJOR, i), S_IFCHR | S_IRUSR | S_IWUSR, "spi/%d",i);
+	}
+#endif
+	printk(KERN_INFO "AT91 SPI driver loaded\n");
+
+	return 0;
+}
+
+/*
+ * Remove the SPI /dev interface driver
+ */
+static void __exit at91_spidev_exit(void)
+{
+#ifdef CONFIG_DEVFS_FS
+	int i;
+	for (i = 0; i < NR_SPI_DEVICES; i++) {
+		devfs_remove("spi/%d", i);
+	}
+
+	devfs_remove("spi");
+#endif
+
+	if (unregister_chrdev(SPI_MAJOR, "spi")) {
+		printk(KERN_ERR "at91_spidev: Unable to release major %d for SPI bus\n", SPI_MAJOR);
+		return;
+	}
+}
+
+module_init(at91_spidev_init);
+module_exit(at91_spidev_exit);
+
+MODULE_LICENSE("GPL")
+MODULE_AUTHOR("Andrew Victor")
+MODULE_DESCRIPTION("SPI /dev interface for Atmel AT91RM9200")
diff -urN linux-2.6.22-rc5/drivers/char/Kconfig linux-2.6.22-rc5.new/drivers/char/Kconfig
--- linux-2.6.22-rc5/drivers/char/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/char/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -1083,5 +1083,21 @@
 
 source "drivers/s390/char/Kconfig"
 
+config AT91_SPI
+	bool "SPI driver (legacy) for AT91RM9200 processors"
+	depends on ARCH_AT91RM9200
+	default y
+	help
+	  The SPI driver gives access to this serial bus on the AT91RM9200
+	  processor.
+
+config AT91_SPIDEV
+	bool "SPI device interface (legacy) for AT91RM9200 processors"
+	depends on ARCH_AT91RM9200 && AT91_SPI
+	default n
+	help
+	  The SPI driver gives user mode access to this serial
+	  bus on the AT91RM9200 processor.
+
 endmenu
 
diff -urN linux-2.6.22-rc5/drivers/char/Makefile linux-2.6.22-rc5.new/drivers/char/Makefile
--- linux-2.6.22-rc5/drivers/char/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/char/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -93,6 +93,8 @@
 obj-$(CONFIG_GPIO_VR41XX)	+= vr41xx_giu.o
 obj-$(CONFIG_GPIO_TB0219)	+= tb0219.o
 obj-$(CONFIG_TELCLOCK)		+= tlclk.o
+obj-$(CONFIG_AT91_SPI)		+= at91_spi.o
+obj-$(CONFIG_AT91_SPIDEV)	+= at91_spidev.o
 
 obj-$(CONFIG_WATCHDOG)		+= watchdog/
 obj-$(CONFIG_MWAVE)		+= mwave/
diff -urN linux-2.6.22-rc5/drivers/i2c/busses/i2c-at91.c linux-2.6.22-rc5.new/drivers/i2c/busses/i2c-at91.c
--- linux-2.6.22-rc5/drivers/i2c/busses/i2c-at91.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/i2c/busses/i2c-at91.c	2007-07-29 05:55:39.000000000 +0200
@@ -31,8 +31,11 @@
 #include <asm/arch/board.h>
 #include <asm/arch/cpu.h>
 
-#define TWI_CLOCK		100000		/* Hz. max 400 Kbits/sec */
 
+/* Clockrate is configurable - max 400 Kbits/sec */
+static unsigned int clockrate = CONFIG_I2C_AT91_CLOCKRATE;
+module_param(clockrate, uint, 0);
+MODULE_PARM_DESC(clockrate, "The TWI clockrate");
 
 static struct clk *twi_clk;
 static void __iomem *twi_base;
@@ -53,7 +56,7 @@
 	at91_twi_write(AT91_TWI_CR, AT91_TWI_MSEN);	/* Set Master mode */
 
 	/* Calcuate clock dividers */
-	cdiv = (clk_get_rate(twi_clk) / (2 * TWI_CLOCK)) - 3;
+	cdiv = (clk_get_rate(twi_clk) / (2 * clockrate)) - 3;
 	cdiv = cdiv + 1;	/* round up */
 	ckdiv = 0;
 	while (cdiv > 255) {
@@ -61,11 +64,12 @@
 		cdiv = cdiv >> 1;
 	}
 
-	if (cpu_is_at91rm9200()) {			/* AT91RM9200 Errata #22 */
-		if (ckdiv > 5) {
-			printk(KERN_ERR "AT91 I2C: Invalid TWI_CLOCK value!\n");
-			ckdiv = 5;
-		}
+	if (cpu_is_at91rm9200() && (ckdiv > 5)) {	/* AT91RM9200 Errata #22 */
+		printk(KERN_ERR "AT91 I2C: Invalid TWI clockrate!\n");
+		ckdiv = 5;
+	} else if (ckdiv > 7) {
+		printk(KERN_ERR "AT91 I2C: Invalid TWI clockrate!\n");
+		ckdiv = 7;
 	}
 
 	at91_twi_write(AT91_TWI_CWGR, (ckdiv << 16) | (cdiv << 8) | cdiv);
diff -urN linux-2.6.22-rc5/drivers/i2c/busses/i2c-pca.c linux-2.6.22-rc5.new/drivers/i2c/busses/i2c-pca.c
--- linux-2.6.22-rc5/drivers/i2c/busses/i2c-pca.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/i2c/busses/i2c-pca.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,213 @@
+/*
+ *  Platform driver for PCA9564 I2C bus controller.
+ *
+ *  (C) 2006 Andrew Victor
+ *
+ *  Based on i2c-pca-isa.c driver for PCA9564 on ISA boards
+ *    Copyright (C) 2004 Arcom Control Systems
+ *
+ *  This program is free software; you can redistribute it and/or modify
+ *  it under the terms of the GNU General Public License as published by
+ *  the Free Software Foundation; either version 2 of the License, or
+ *  (at your option) any later version.
+ *
+ *  This program is distributed in the hope that it will be useful,
+ *  but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *  MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *  GNU General Public License for more details.
+ *
+ *  You should have received a copy of the GNU General Public License
+ *  along with this program; if not, write to the Free Software
+ *  Foundation, Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+
+#include <linux/kernel.h>
+#include <linux/module.h>
+#include <linux/moduleparam.h>
+#include <linux/delay.h>
+#include <linux/init.h>
+#include <linux/interrupt.h>
+#include <linux/wait.h>
+#include <linux/platform_device.h>
+
+#include <linux/i2c.h>
+#include <linux/i2c-algo-pca.h>
+
+#include <asm/io.h>
+
+#include "../algos/i2c-algo-pca.h"
+
+#define PCA_OWN_ADDRESS		0x55	/* our address for slave mode */
+#define PCA_CLOCK		I2C_PCA_CON_59kHz
+
+//#define REG_SHIFT		2
+#define REG_SHIFT		0
+
+//#define DEBUG_IO
+
+#define PCA_IO_SIZE 4
+
+static void __iomem *base_addr;
+static int irq;
+static wait_queue_head_t pca_wait;
+
+static int pca_getown(struct i2c_algo_pca_data *adap)
+{
+	return PCA_OWN_ADDRESS;
+}
+
+static int pca_getclock(struct i2c_algo_pca_data *adap)
+{
+	return PCA_CLOCK;
+}
+
+static void pca_writebyte(struct i2c_algo_pca_data *adap, int reg, int val)
+{
+#ifdef DEBUG_IO
+	static char *names[] = { "T/O", "DAT", "ADR", "CON" };
+	printk("*** write %s at %#lx <= %#04x\n", names[reg], (unsigned long) base_addr+reg, val);
+#endif
+	udelay(1);
+	outb(val, base_addr + (reg << REG_SHIFT));
+}
+
+static int pca_readbyte(struct i2c_algo_pca_data *adap, int reg)
+{
+	int res;
+
+	udelay(1);
+	res = inb(base_addr + (reg << REG_SHIFT));
+#ifdef DEBUG_IO
+	{
+		static char *names[] = { "STA", "DAT", "ADR", "CON" };
+		printk("*** read  %s => %#04x\n", names[reg], res);
+	}
+#endif
+	return res;
+}
+
+static int pca_waitforinterrupt(struct i2c_algo_pca_data *adap)
+{
+	int ret = 0;
+
+	if (irq > -1) {
+		ret = wait_event_interruptible(pca_wait,
+				pca_readbyte(adap, I2C_PCA_CON) & I2C_PCA_CON_SI);
+	} else {
+		while ((pca_readbyte(adap, I2C_PCA_CON) & I2C_PCA_CON_SI) == 0)
+			udelay(100);
+	}
+	return ret;
+}
+
+static irqreturn_t pca_handler(int this_irq, void *dev_id)
+{
+	wake_up_interruptible(&pca_wait);
+	return IRQ_HANDLED;
+}
+
+static struct i2c_algo_pca_data pca_i2c_data = {
+	.get_own		= pca_getown,
+	.get_clock		= pca_getclock,
+	.write_byte		= pca_writebyte,
+	.read_byte		= pca_readbyte,
+	.wait_for_interrupt	= pca_waitforinterrupt,
+};
+
+static struct i2c_adapter pca_i2c_ops = {
+	.owner          = THIS_MODULE,
+	.id		= I2C_HW_A_PLAT,
+	.algo_data	= &pca_i2c_data,
+	.name		= "PCA9564",
+	.class		= I2C_CLASS_HWMON,
+};
+
+static int __devinit pca_i2c_probe(struct platform_device *pdev)
+{
+	struct resource *res;
+
+	init_waitqueue_head(&pca_wait);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res)
+		return -ENODEV;
+
+	if (!request_mem_region(res->start, PCA_IO_SIZE, "PCA9564"))
+		return -ENXIO;
+
+	base_addr = ioremap(res->start, PCA_IO_SIZE);
+	if (base_addr == NULL)
+		goto out_region;
+
+	irq = platform_get_irq(pdev, 0);
+	if (irq > -1) {
+		if (request_irq(irq, pca_handler, 0, "pca9564", NULL) < 0) {
+			printk(KERN_ERR "i2c-pca: Request irq%d failed\n", irq);
+			goto out_remap;
+		}
+	}
+
+	/* set up the driverfs linkage to our parent device */
+	pca_i2c_ops.dev.parent = &pdev->dev;
+
+	if (i2c_pca_add_bus(&pca_i2c_ops) < 0) {
+		printk(KERN_ERR "i2c-pca: Failed to add i2c bus\n");
+		goto out_irq;
+	}
+
+	return 0;
+
+ out_irq:
+	if (irq > -1)
+		free_irq(irq, &pca_i2c_ops);
+
+ out_remap:
+	iounmap(base_addr);
+
+ out_region:
+	release_mem_region(res->start, PCA_IO_SIZE);
+	return -ENODEV;
+}
+
+static int __devexit pca_i2c_remove(struct platform_device *pdev)
+{
+	struct resource *res;
+
+	i2c_del_adapter(&pca_i2c_ops);
+
+	if (irq > 0)
+		free_irq(irq, NULL);
+
+	iounmap(base_addr);
+
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	release_mem_region(res->start, PCA_IO_SIZE);
+
+	return 0;
+}
+
+static struct platform_driver pca_i2c_driver = {
+	.probe		= pca_i2c_probe,
+	.remove		= __devexit_p(pca_i2c_remove),
+	.driver		= {
+		.name	= "pca9564",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static int __init pca_i2c_init(void)
+{
+	return platform_driver_register(&pca_i2c_driver);
+}
+
+static void __exit pca_i2c_exit(void)
+{
+	platform_driver_unregister(&pca_i2c_driver);
+}
+
+module_init(pca_i2c_init);
+module_exit(pca_i2c_exit);
+
+MODULE_AUTHOR("Andrew Victor");
+MODULE_DESCRIPTION("PCA9564 platform driver");
+MODULE_LICENSE("GPL");
diff -urN linux-2.6.22-rc5/drivers/i2c/busses/Kconfig linux-2.6.22-rc5.new/drivers/i2c/busses/Kconfig
--- linux-2.6.22-rc5/drivers/i2c/busses/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/i2c/busses/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -80,6 +80,14 @@
 	  This supports the use of the I2C interface on Atmel AT91
 	  processors.
 
+config I2C_AT91_CLOCKRATE
+	prompt "Atmel AT91 I2C/TWI clock-rate"
+	depends on I2C_AT91
+	int
+	default 100000
+	help
+	  Set the AT91 I2C/TWI clock-rate.
+
 config I2C_AU1550
 	tristate "Au1550/Au1200 SMBus interface"
 	depends on SOC_AU1550 || SOC_AU1200
@@ -598,6 +606,14 @@
 	  This driver can also be built as a module.  If so, the module
 	  will be called i2c-voodoo3.
 
+config I2C_PCA
+	tristate "PCA9564"
+	depends on I2C
+	select I2C_ALGOPCA
+	help
+	  This driver support the Philips PCA 9564 Parallel bus to I2C
+	  bus controller.
+
 config I2C_PCA_ISA
 	tristate "PCA9564 on an ISA bus"
 	depends on ISA
diff -urN linux-2.6.22-rc5/drivers/i2c/busses/Makefile linux-2.6.22-rc5.new/drivers/i2c/busses/Makefile
--- linux-2.6.22-rc5/drivers/i2c/busses/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/i2c/busses/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -30,6 +30,7 @@
 obj-$(CONFIG_I2C_PARPORT)	+= i2c-parport.o
 obj-$(CONFIG_I2C_PARPORT_LIGHT)	+= i2c-parport-light.o
 obj-$(CONFIG_I2C_PASEMI)	+= i2c-pasemi.o
+obj-$(CONFIG_I2C_PCA)		+= i2c-pca.o
 obj-$(CONFIG_I2C_PCA_ISA)	+= i2c-pca-isa.o
 obj-$(CONFIG_I2C_PIIX4)		+= i2c-piix4.o
 obj-$(CONFIG_I2C_PNX)		+= i2c-pnx.o
diff -urN linux-2.6.22-rc5/drivers/leds/Kconfig linux-2.6.22-rc5.new/drivers/leds/Kconfig
--- linux-2.6.22-rc5/drivers/leds/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/leds/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -77,6 +77,13 @@
 	  This option enables support for the Soekris net4801 and net4826 error
 	  LED.
 
+config LEDS_AT91
+	tristate "LED support using AT91 GPIOs"
+	depends on LEDS_CLASS && ARCH_AT91 && !LEDS
+	help
+	  This option enables support for LEDs connected to GPIO lines
+	  on AT91-based boards.
+
 config LEDS_WRAP
 	tristate "LED Support for the WRAP series LEDs"
 	depends on LEDS_CLASS && SCx200_GPIO
diff -urN linux-2.6.22-rc5/drivers/leds/leds-at91.c linux-2.6.22-rc5.new/drivers/leds/leds-at91.c
--- linux-2.6.22-rc5/drivers/leds/leds-at91.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/leds/leds-at91.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,140 @@
+/*
+ * AT91 GPIO based LED driver
+ *
+ * Copyright (C) 2006 David Brownell
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License version 2 as
+ * published by the Free Software Foundation.
+ */
+
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/leds.h>
+
+#include <asm/arch/board.h>
+#include <asm/arch/gpio.h>
+
+static LIST_HEAD(at91_led_list);	/* list of AT91 LEDs */
+
+struct at91_led {
+	struct led_classdev	cdev;
+	struct list_head	list;
+	struct at91_gpio_led	*led_data;
+};
+
+/*
+ * Change the state of the LED.
+ */
+static void at91_led_set(struct led_classdev *cdev, enum led_brightness value)
+{
+	struct at91_led	*led = container_of(cdev, struct at91_led, cdev);
+	short		active = (value == LED_OFF);
+
+	if (led->led_data->flags & 1)	/* active high/low? */
+		active = !active;
+	at91_set_gpio_value(led->led_data->gpio, active);
+}
+
+static int __devexit at91_led_remove(struct platform_device *pdev)
+{
+	struct at91_led		*led;
+
+	list_for_each_entry (led, &at91_led_list, list)
+		led_classdev_unregister(&led->cdev);
+
+#warning "Free allocated memory"
+	// TODO: Free memory.	kfree(led);
+
+	return 0;
+}
+
+static int __init at91_led_probe(struct platform_device *pdev)
+{
+	int			status = 0;
+	struct at91_gpio_led	*pdata = pdev->dev.platform_data;
+	unsigned		nr_leds;
+	struct at91_led		*led;
+
+	if (!pdata)
+		return -ENODEV;
+
+	nr_leds = pdata->index;		/* first index stores number of LEDs */
+
+	while (nr_leds--) {
+		led = kzalloc(sizeof(struct at91_led), GFP_KERNEL);
+		if (!led) {
+			dev_err(&pdev->dev, "No memory for device\n");
+			status = -ENOMEM;
+			goto cleanup;
+		}
+		led->led_data = pdata;
+		led->cdev.name = pdata->name;
+		led->cdev.brightness_set = at91_led_set,
+		led->cdev.default_trigger = pdata->trigger;
+
+		status = led_classdev_register(&pdev->dev, &led->cdev);
+		if (status < 0) {
+			dev_err(&pdev->dev, "led_classdev_register failed - %d\n", status);
+cleanup:
+			at91_led_remove(pdev);
+			break;
+		}
+		list_add(&led->list, &at91_led_list);
+		pdata++;
+	}
+	return status;
+}
+
+#ifdef CONFIG_PM
+static int at91_led_suspend(struct platform_device *dev, pm_message_t state)
+{
+	struct at91_led	*led;
+
+	list_for_each_entry (led, &at91_led_list, list)
+		led_classdev_suspend(&led->cdev);
+
+	return 0;
+}
+
+static int at91_led_resume(struct platform_device *dev)
+{
+	struct at91_led	*led;
+
+	list_for_each_entry (led, &at91_led_list, list)
+		led_classdev_resume(&led->cdev);
+
+	return 0;
+}
+#else
+#define	at91_led_suspend	NULL
+#define	at91_led_resume		NULL
+#endif
+
+static struct platform_driver at91_led_driver = {
+	.probe		= at91_led_probe,
+	.remove		= __devexit_p(at91_led_remove),
+	.suspend	= at91_led_suspend,
+	.resume		= at91_led_resume,
+	.driver		= {
+		.name	= "at91_leds",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static int __init at91_led_init(void)
+{
+	return platform_driver_register(&at91_led_driver);
+}
+module_init(at91_led_init);
+
+static void __exit at91_led_exit(void)
+{
+	platform_driver_unregister(&at91_led_driver);
+}
+module_exit(at91_led_exit);
+
+MODULE_DESCRIPTION("AT91 GPIO LED driver");
+MODULE_AUTHOR("David Brownell");
+MODULE_LICENSE("GPL");
diff -urN linux-2.6.22-rc5/drivers/leds/Makefile linux-2.6.22-rc5.new/drivers/leds/Makefile
--- linux-2.6.22-rc5/drivers/leds/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/leds/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -16,6 +16,7 @@
 obj-$(CONFIG_LEDS_WRAP)			+= leds-wrap.o
 obj-$(CONFIG_LEDS_H1940)		+= leds-h1940.o
 obj-$(CONFIG_LEDS_COBALT)		+= leds-cobalt.o
+obj-$(CONFIG_LEDS_AT91)			+= leds-at91.o
 
 # LED Triggers
 obj-$(CONFIG_LEDS_TRIGGER_TIMER)	+= ledtrig-timer.o
diff -urN linux-2.6.22-rc5/drivers/mmc/host/at91_mci.c linux-2.6.22-rc5.new/drivers/mmc/host/at91_mci.c
--- linux-2.6.22-rc5/drivers/mmc/host/at91_mci.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/mmc/host/at91_mci.c	2007-07-29 05:57:56.000000000 +0200
@@ -85,7 +85,7 @@
 
 #define AT91_MCI_ERRORS	(AT91_MCI_RINDE | AT91_MCI_RDIRE | AT91_MCI_RCRCE	\
 		| AT91_MCI_RENDE | AT91_MCI_RTOE | AT91_MCI_DCRCE		\
-		| AT91_MCI_DTOE | AT91_MCI_OVRE | AT91_MCI_UNRE)			
+		| AT91_MCI_DTOE | AT91_MCI_OVRE | AT91_MCI_UNRE)
 
 #define at91_mci_read(host, reg)	__raw_readl((host)->baseaddr + (reg))
 #define at91_mci_write(host, reg, val)	__raw_writel((val), (host)->baseaddr + (reg))
@@ -560,9 +560,7 @@
 	pr_debug("Status = %08X [%08X %08X %08X %08X]\n",
 		 status, cmd->resp[0], cmd->resp[1], cmd->resp[2], cmd->resp[3]);
 
-	if (status & (AT91_MCI_RINDE | AT91_MCI_RDIRE | AT91_MCI_RCRCE |
-			AT91_MCI_RENDE | AT91_MCI_RTOE | AT91_MCI_DCRCE |
-			AT91_MCI_DTOE | AT91_MCI_OVRE | AT91_MCI_UNRE)) {
+	if (status & AT91_MCI_ERRORS) {
 		if ((status & AT91_MCI_RCRCE) && !(mmc_resp_type(cmd) & MMC_RSP_CRC)) {
 			cmd->error = MMC_ERR_NONE;
 		}
@@ -663,15 +661,15 @@
 
 	int_status = at91_mci_read(host, AT91_MCI_SR);
 	int_mask = at91_mci_read(host, AT91_MCI_IMR);
-	
+
 	pr_debug("MCI irq: status = %08X, %08X, %08X\n", int_status, int_mask,
 		int_status & int_mask);
-	
+
 	int_status = int_status & int_mask;
 
 	if (int_status & AT91_MCI_ERRORS) {
 		completed = 1;
-		
+
 		if (int_status & AT91_MCI_UNRE)
 			pr_debug("MMC: Underrun error\n");
 		if (int_status & AT91_MCI_OVRE)
@@ -819,7 +817,7 @@
 	mmc->f_min = 375000;
 	mmc->f_max = 25000000;
 	mmc->ocr_avail = MMC_VDD_32_33 | MMC_VDD_33_34;
-	mmc->caps = MMC_CAP_BYTEBLOCK;
+	mmc->caps = MMC_CAP_BYTEBLOCK | MMC_CAP_MULTIWRITE;
 
 	mmc->max_blk_size = 4095;
 	mmc->max_blk_count = mmc->max_req_size;
@@ -893,6 +891,8 @@
 
 	mmc_add_host(mmc);
 
+	device_init_wakeup(&pdev->dev, 1);
+
 	/*
 	 * monitor card insertion/removal if we can
 	 */
@@ -922,6 +922,8 @@
 
 	host = mmc_priv(mmc);
 
+	device_init_wakeup(&pdev->dev, 0);
+
 	if (host->present != -1) {
 		free_irq(host->board->det_pin, host);
 		cancel_delayed_work(&host->mmc->detect);
@@ -949,8 +951,12 @@
 static int at91_mci_suspend(struct platform_device *pdev, pm_message_t state)
 {
 	struct mmc_host *mmc = platform_get_drvdata(pdev);
+	struct at91mci_host *host = mmc_priv(mmc);
 	int ret = 0;
 
+	if (device_may_wakeup(&pdev->dev))
+		enable_irq_wake(host->board->det_pin);
+
 	if (mmc)
 		ret = mmc_suspend_host(mmc, state);
 
@@ -960,8 +966,12 @@
 static int at91_mci_resume(struct platform_device *pdev)
 {
 	struct mmc_host *mmc = platform_get_drvdata(pdev);
+	struct at91mci_host *host = mmc_priv(mmc);
 	int ret = 0;
 
+	if (device_may_wakeup(&pdev->dev))
+		disable_irq_wake(host->board->det_pin);
+
 	if (mmc)
 		ret = mmc_resume_host(mmc);
 
diff -urN linux-2.6.22-rc5/drivers/mtd/devices/at91_dataflash.c linux-2.6.22-rc5.new/drivers/mtd/devices/at91_dataflash.c
--- linux-2.6.22-rc5/drivers/mtd/devices/at91_dataflash.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/mtd/devices/at91_dataflash.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,667 @@
+/*
+ * Atmel DataFlash driver for Atmel AT91RM9200 (Thunder)
+ *
+ *  Copyright (C) SAN People (Pty) Ltd
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License
+ * as published by the Free Software Foundation; either version
+ * 2 of the License, or (at your option) any later version.
+*/
+
+#include <linux/module.h>
+#include <linux/init.h>
+#include <linux/slab.h>
+#include <linux/pci.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+
+#include <asm/arch/spi.h>
+
+#undef DEBUG_DATAFLASH
+
+#define DATAFLASH_MAX_DEVICES	4	/* max number of dataflash devices */
+#undef	DATAFLASH_ALWAYS_ADD_DEVICE	/* always add whole device when using partitions? */
+
+#define OP_READ_CONTINUOUS	0xE8
+#define OP_READ_PAGE		0xD2
+#define OP_READ_BUFFER1		0xD4
+#define OP_READ_BUFFER2		0xD6
+#define OP_READ_STATUS		0xD7
+
+#define OP_ERASE_PAGE		0x81
+#define OP_ERASE_BLOCK		0x50
+
+#define OP_TRANSFER_BUF1	0x53
+#define OP_TRANSFER_BUF2	0x55
+#define OP_COMPARE_BUF1		0x60
+#define OP_COMPARE_BUF2		0x61
+
+#define OP_PROGRAM_VIA_BUF1	0x82
+#define OP_PROGRAM_VIA_BUF2	0x85
+
+struct dataflash_local
+{
+	int spi;			/* SPI chip-select number */
+
+	unsigned int page_size;		/* number of bytes per page */
+	unsigned short page_offset;	/* page offset in flash address */
+};
+
+
+/* Detected DataFlash devices */
+static struct mtd_info* mtd_devices[DATAFLASH_MAX_DEVICES];
+static int nr_devices = 0;
+
+/* ......................................................................... */
+
+#ifdef CONFIG_MTD_PARTITIONS
+
+static struct mtd_partition static_partitions_2M[] =
+{
+	{
+		.name		= "bootloader",
+		.offset		= 0,
+		.size		= 1 * 32 * 8 * 528,	/* 1st sector = 32 blocks * 8 pages * 528 bytes */
+		.mask_flags	= MTD_WRITEABLE,	/* read-only */
+	},
+	{
+		.name		= "kernel",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= 6 * 32 * 8 * 528,	/* 6 sectors */
+	},
+	{
+		.name		= "filesystem",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= MTDPART_SIZ_FULL,	/* rest = 9 sectors */
+	}
+};
+
+static struct mtd_partition static_partitions_4M[] =
+{
+	{
+		.name		= "bootloader",
+		.offset		= 0,
+		.size		= 1 * 64 * 8 * 528,	/* 1st sector = 64 blocks * 8 pages * 528 bytes */
+		.mask_flags	= MTD_WRITEABLE,	/* read-only */
+	},
+	{
+		.name		= "kernel",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= 4 * 64 * 8 * 528,	/* 4 sectors */
+	},
+	{
+		.name		= "filesystem",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= MTDPART_SIZ_FULL,	/* rest = 11 sectors */
+	}
+};
+
+#if defined(CONFIG_MACH_KAFA)
+static struct mtd_partition static_partitions_8M[] =
+{
+	{
+		name:		"romboot",
+		offset:		0,
+		size:		16 * 1056,	/* 160 Kb */
+		mask_flags:	MTD_WRITEABLE,		/* read-only */
+	},
+	{
+		name:		"uboot",
+		offset:		MTDPART_OFS_APPEND, /* Sperry, NXTBLK is broken */
+		size:		128 * 1056,		/* 1 MB */
+	},
+	{
+		name:		"kernel",
+		offset:		MTDPART_OFS_APPEND, /* Sperry, NXTBLK is broken */
+		size:		1024 * 1056,		/* 1 MB */
+	},
+	{
+		name:		"filesystem",
+		offset:		MTDPART_OFS_APPEND, /* Sperry, NXTBLK is broken */
+		size:		MTDPART_SIZ_FULL,
+	}
+};
+
+#elif defined(CONFIG_MACH_MULTMDP)
+
+static struct mtd_partition static_partitions_8M[] =
+{
+	{
+		.name		= "bootloader",
+		.offset		= 0,
+		.size		= 12 * 1056,		/* 1st sector = 32 blocks * 8 pages * 1056 bytes */
+		.mask_flags	= MTD_WRITEABLE,	/* read-only */
+	},
+	{
+		.name		= "configuration",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= 20 * 1056,
+	},
+	{
+		.name		= "kernel",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= 1520 * 1056,
+	},
+	{
+		.name		= "filesystem",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= MTDPART_SIZ_FULL,
+	}
+};
+
+#else
+
+static struct mtd_partition static_partitions_8M[] =
+{
+	{
+		.name		= "bootloader",
+		.offset		= 0,
+		.size		= 1 * 32 * 8 * 1056,	/* 1st sector = 32 blocks * 8 pages * 1056 bytes */
+		.mask_flags	= MTD_WRITEABLE,	/* read-only */
+	},
+	{
+		.name		= "kernel",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= 5 * 32 * 8 * 1056,	/* 5 sectors */
+	},
+	{
+		.name		= "filesystem",
+		.offset		= MTDPART_OFS_NXTBLK,
+		.size		= MTDPART_SIZ_FULL,	/* rest = 26 sectors */
+	}
+};
+#endif
+
+static const char *part_probes[] = { "cmdlinepart", NULL, };
+
+#endif
+
+/* ......................................................................... */
+
+/* Allocate a single SPI transfer descriptor.  We're assuming that if multiple
+   SPI transfers occur at the same time, spi_access_bus() will serialize them.
+   If this is not valid, then either (i) each dataflash 'priv' structure
+   needs it's own transfer descriptor, (ii) we lock this one, or (iii) use
+   another mechanism.   */
+static struct spi_transfer_list* spi_transfer_desc;
+
+/*
+ * Perform a SPI transfer to access the DataFlash device.
+ */
+static int do_spi_transfer(int nr, char* tx, int tx_len, char* rx, int rx_len,
+		char* txnext, int txnext_len, char* rxnext, int rxnext_len)
+{
+	struct spi_transfer_list* list = spi_transfer_desc;
+
+	list->tx[0] = tx;	list->txlen[0] = tx_len;
+	list->rx[0] = rx;	list->rxlen[0] = rx_len;
+
+	list->tx[1] = txnext;	list->txlen[1] = txnext_len;
+	list->rx[1] = rxnext;	list->rxlen[1] = rxnext_len;
+
+	list->nr_transfers = nr;
+
+	return spi_transfer(list);
+}
+
+/* ......................................................................... */
+
+/*
+ * Poll the DataFlash device until it is READY.
+ */
+static void at91_dataflash_waitready(void)
+{
+	char* command = kmalloc(2, GFP_KERNEL);
+
+	if (!command)
+		return;
+
+	do {
+		command[0] = OP_READ_STATUS;
+		command[1] = 0;
+
+		do_spi_transfer(1, command, 2, command, 2, NULL, 0, NULL, 0);
+	} while ((command[1] & 0x80) == 0);
+
+	kfree(command);
+}
+
+/*
+ * Return the status of the DataFlash device.
+ */
+static unsigned short at91_dataflash_status(void)
+{
+	unsigned short status;
+	char* command = kmalloc(2, GFP_KERNEL);
+
+	if (!command)
+		return 0;
+
+	command[0] = OP_READ_STATUS;
+	command[1] = 0;
+
+	do_spi_transfer(1, command, 2, command, 2, NULL, 0, NULL, 0);
+	status = command[1];
+
+	kfree(command);
+	return status;
+}
+
+/* ......................................................................... */
+
+/*
+ * Erase blocks of flash.
+ */
+static int at91_dataflash_erase(struct mtd_info *mtd, struct erase_info *instr)
+{
+	struct dataflash_local *priv = (struct dataflash_local *) mtd->priv;
+	unsigned int pageaddr;
+	char* command;
+
+#ifdef DEBUG_DATAFLASH
+	printk("dataflash_erase: addr=%i len=%i\n", instr->addr, instr->len);
+#endif
+
+	/* Sanity checks */
+	if (instr->addr + instr->len > mtd->size)
+		return -EINVAL;
+	if ((instr->len % mtd->erasesize != 0) || (instr->len % priv->page_size != 0))
+		return -EINVAL;
+	if ((instr->addr % priv->page_size) != 0)
+		return -EINVAL;
+
+	command = kmalloc(4, GFP_KERNEL);
+	if (!command)
+		return -ENOMEM;
+
+	while (instr->len > 0) {
+		/* Calculate flash page address */
+		pageaddr = (instr->addr / priv->page_size) << priv->page_offset;
+
+		command[0] = OP_ERASE_PAGE;
+		command[1] = (pageaddr & 0x00FF0000) >> 16;
+		command[2] = (pageaddr & 0x0000FF00) >> 8;
+		command[3] = 0;
+#ifdef DEBUG_DATAFLASH
+		printk("ERASE: (%x) %x %x %x [%i]\n", command[0], command[1], command[2], command[3], pageaddr);
+#endif
+
+		/* Send command to SPI device */
+		spi_access_bus(priv->spi);
+		do_spi_transfer(1, command, 4, command, 4, NULL, 0, NULL, 0);
+
+		at91_dataflash_waitready();		/* poll status until ready */
+		spi_release_bus(priv->spi);
+
+		instr->addr += priv->page_size;		/* next page */
+		instr->len -= priv->page_size;
+	}
+
+	kfree(command);
+
+	/* Inform MTD subsystem that erase is complete */
+	instr->state = MTD_ERASE_DONE;
+	if (instr->callback)
+		instr->callback(instr);
+
+	return 0;
+}
+
+/*
+ * Read from the DataFlash device.
+ *   from   : Start offset in flash device
+ *   len    : Amount to read
+ *   retlen : About of data actually read
+ *   buf    : Buffer containing the data
+ */
+static int at91_dataflash_read(struct mtd_info *mtd, loff_t from, size_t len, size_t *retlen, u_char *buf)
+{
+	struct dataflash_local *priv = (struct dataflash_local *) mtd->priv;
+	unsigned int addr;
+	char* command;
+
+#ifdef DEBUG_DATAFLASH
+	printk("dataflash_read: %lli .. %lli\n", from, from+len);
+#endif
+
+	*retlen = 0;
+
+	/* Sanity checks */
+	if (!len)
+		return 0;
+	if (from + len > mtd->size)
+		return -EINVAL;
+
+	/* Calculate flash page/byte address */
+	addr = (((unsigned)from / priv->page_size) << priv->page_offset) + ((unsigned)from % priv->page_size);
+
+	command = kmalloc(8, GFP_KERNEL);
+	if (!command)
+		return -ENOMEM;
+
+	command[0] = OP_READ_CONTINUOUS;
+	command[1] = (addr & 0x00FF0000) >> 16;
+	command[2] = (addr & 0x0000FF00) >> 8;
+	command[3] = (addr & 0x000000FF);
+#ifdef DEBUG_DATAFLASH
+	printk("READ: (%x) %x %x %x\n", command[0], command[1], command[2], command[3]);
+#endif
+
+	/* Send command to SPI device */
+	spi_access_bus(priv->spi);
+	do_spi_transfer(2, command, 8, command, 8, buf, len, buf, len);
+	spi_release_bus(priv->spi);
+
+	*retlen = len;
+	kfree(command);
+	return 0;
+}
+
+/*
+ * Write to the DataFlash device.
+ *   to     : Start offset in flash device
+ *   len    : Amount to write
+ *   retlen : Amount of data actually written
+ *   buf    : Buffer containing the data
+ */
+static int at91_dataflash_write(struct mtd_info *mtd, loff_t to, size_t len, size_t *retlen, const u_char *buf)
+{
+	struct dataflash_local *priv = (struct dataflash_local *) mtd->priv;
+	unsigned int pageaddr, addr, offset, writelen;
+	size_t remaining;
+	u_char *writebuf;
+	unsigned short status;
+	int res = 0;
+	char* command;
+	char* tmpbuf = NULL;
+
+#ifdef DEBUG_DATAFLASH
+	printk("dataflash_write: %lli .. %lli\n", to, to+len);
+#endif
+
+	*retlen = 0;
+
+	/* Sanity checks */
+	if (!len)
+		return 0;
+	if (to + len > mtd->size)
+		return -EINVAL;
+
+	command = kmalloc(4, GFP_KERNEL);
+	if (!command)
+		return -ENOMEM;
+
+	pageaddr = ((unsigned)to / priv->page_size);
+	offset = ((unsigned)to % priv->page_size);
+	if (offset + len > priv->page_size)
+		writelen = priv->page_size - offset;
+	else
+		writelen = len;
+	writebuf = (u_char *)buf;
+	remaining = len;
+
+	/* Allocate temporary buffer */
+	tmpbuf = kmalloc(priv->page_size, GFP_KERNEL);
+	if (!tmpbuf) {
+		kfree(command);
+		return -ENOMEM;
+	}
+
+	/* Gain access to the SPI bus */
+	spi_access_bus(priv->spi);
+
+	while (remaining > 0) {
+#ifdef DEBUG_DATAFLASH
+		printk("write @ %i:%i len=%i\n", pageaddr, offset, writelen);
+#endif
+
+		/* (1) Transfer to Buffer1 */
+		if (writelen != priv->page_size) {
+			addr = pageaddr << priv->page_offset;
+			command[0] = OP_TRANSFER_BUF1;
+			command[1] = (addr & 0x00FF0000) >> 16;
+			command[2] = (addr & 0x0000FF00) >> 8;
+			command[3] = 0;
+#ifdef DEBUG_DATAFLASH
+			printk("TRANSFER: (%x) %x %x %x\n", command[0], command[1], command[2], command[3]);
+#endif
+			do_spi_transfer(1, command, 4, command, 4, NULL, 0, NULL, 0);
+			at91_dataflash_waitready();
+		}
+
+		/* (2) Program via Buffer1 */
+		addr = (pageaddr << priv->page_offset) + offset;
+		command[0] = OP_PROGRAM_VIA_BUF1;
+		command[1] = (addr & 0x00FF0000) >> 16;
+		command[2] = (addr & 0x0000FF00) >> 8;
+		command[3] = (addr & 0x000000FF);
+#ifdef DEBUG_DATAFLASH
+		printk("PROGRAM: (%x) %x %x %x\n", command[0], command[1], command[2], command[3]);
+#endif
+		do_spi_transfer(2, command, 4, command, 4, writebuf, writelen, tmpbuf, writelen);
+		at91_dataflash_waitready();
+
+		/* (3) Compare to Buffer1 */
+		addr = pageaddr << priv->page_offset;
+		command[0] = OP_COMPARE_BUF1;
+		command[1] = (addr & 0x00FF0000) >> 16;
+		command[2] = (addr & 0x0000FF00) >> 8;
+		command[3] = 0;
+#ifdef DEBUG_DATAFLASH
+		printk("COMPARE: (%x) %x %x %x\n", command[0], command[1], command[2], command[3]);
+#endif
+		do_spi_transfer(1, command, 4, command, 4, NULL, 0, NULL, 0);
+		at91_dataflash_waitready();
+
+		/* Get result of the compare operation */
+		status = at91_dataflash_status();
+		if ((status & 0x40) == 1) {
+			printk("at91_dataflash: Write error on page %i\n", pageaddr);
+			remaining = 0;
+			res = -EIO;
+		}
+
+		remaining = remaining - writelen;
+		pageaddr++;
+		offset = 0;
+		writebuf += writelen;
+		*retlen += writelen;
+
+		if (remaining > priv->page_size)
+			writelen = priv->page_size;
+		else
+			writelen = remaining;
+	}
+
+	/* Release SPI bus */
+	spi_release_bus(priv->spi);
+
+	kfree(tmpbuf);
+	kfree(command);
+	return res;
+}
+
+/* ......................................................................... */
+
+/*
+ * Initialize and register DataFlash device with MTD subsystem.
+ */
+static int __init add_dataflash(int channel, char *name, int IDsize,
+		int nr_pages, int pagesize, int pageoffset)
+{
+	struct mtd_info *device;
+	struct dataflash_local *priv;
+#ifdef CONFIG_MTD_PARTITIONS
+	struct mtd_partition *mtd_parts = 0;
+	int mtd_parts_nr = 0;
+#endif
+
+	if (nr_devices >= DATAFLASH_MAX_DEVICES) {
+		printk(KERN_ERR "at91_dataflash: Too many devices detected\n");
+		return 0;
+	}
+
+	device = kmalloc(sizeof(struct mtd_info) + strlen(name) + 8, GFP_KERNEL);
+	if (!device)
+		return -ENOMEM;
+	memset(device, 0, sizeof(struct mtd_info));
+
+	device->name = (char *)&device[1];
+	sprintf(device->name, "%s.spi%d", name, channel);
+	device->size = nr_pages * pagesize;
+	device->erasesize = pagesize;
+	device->writesize = pagesize;
+	device->owner = THIS_MODULE;
+	device->type = MTD_DATAFLASH;
+	device->flags = MTD_WRITEABLE;
+	device->erase = at91_dataflash_erase;
+	device->read = at91_dataflash_read;
+	device->write = at91_dataflash_write;
+
+	priv = (struct dataflash_local *) kmalloc(sizeof(struct dataflash_local), GFP_KERNEL);
+	if (!priv) {
+		kfree(device);
+		return -ENOMEM;
+	}
+	memset(priv, 0, sizeof(struct dataflash_local));
+
+	priv->spi = channel;
+	priv->page_size = pagesize;
+	priv->page_offset = pageoffset;
+	device->priv = priv;
+
+	mtd_devices[nr_devices] = device;
+	nr_devices++;
+	printk("at91_dataflash: %s detected [spi%i] (%i bytes)\n", name, channel, device->size);
+
+#ifdef CONFIG_MTD_PARTITIONS
+#ifdef CONFIG_MTD_CMDLINE_PARTS
+	mtd_parts_nr = parse_mtd_partitions(device, part_probes, &mtd_parts, 0);
+#endif
+	if (mtd_parts_nr <= 0) {
+		switch (IDsize) {
+			case SZ_2M:
+				mtd_parts = static_partitions_2M;
+				mtd_parts_nr = ARRAY_SIZE(static_partitions_2M);
+				break;
+			case SZ_4M:
+				mtd_parts = static_partitions_4M;
+				mtd_parts_nr = ARRAY_SIZE(static_partitions_4M);
+				break;
+			case SZ_8M:
+				mtd_parts = static_partitions_8M;
+				mtd_parts_nr = ARRAY_SIZE(static_partitions_8M);
+				break;
+		}
+	}
+
+	if (mtd_parts_nr > 0) {
+#ifdef DATAFLASH_ALWAYS_ADD_DEVICE
+		add_mtd_device(device);
+#endif
+		return add_mtd_partitions(device, mtd_parts, mtd_parts_nr);
+	}
+#endif
+	return add_mtd_device(device);		/* add whole device */
+}
+
+/*
+ * Detect and initialize DataFlash device connected to specified SPI channel.
+ *
+ *   Device            Density         ID code                 Nr Pages        Page Size       Page offset
+ *   AT45DB011B        1Mbit   (128K)  xx0011xx (0x0c)         512             264             9
+ *   AT45DB021B        2Mbit   (256K)  xx0101xx (0x14)         1025            264             9
+ *   AT45DB041B        4Mbit   (512K)  xx0111xx (0x1c)         2048            264             9
+ *   AT45DB081B        8Mbit   (1M)    xx1001xx (0x24)         4096            264             9
+ *   AT45DB0161B       16Mbit  (2M)    xx1011xx (0x2c)         4096            528             10
+ *   AT45DB0321B       32Mbit  (4M)    xx1101xx (0x34)         8192            528             10
+ *   AT45DB0642        64Mbit  (8M)    xx1111xx (0x3c)         8192            1056            11
+ *   AT45DB1282        128Mbit (16M)   xx0100xx (0x10)         16384           1056            11
+ */
+static int __init at91_dataflash_detect(int channel)
+{
+	int res = 0;
+	unsigned short status;
+
+	spi_access_bus(channel);
+	status = at91_dataflash_status();
+	spi_release_bus(channel);
+	if (status != 0xff) {			/* no dataflash device there */
+		switch (status & 0x3c) {
+			case 0x0c:	/* 0 0 1 1 */
+				res = add_dataflash(channel, "AT45DB011B", SZ_128K, 512, 264, 9);
+				break;
+			case 0x14:	/* 0 1 0 1 */
+				res = add_dataflash(channel, "AT45DB021B", SZ_256K, 1025, 264, 9);
+				break;
+			case 0x1c:	/* 0 1 1 1 */
+				res = add_dataflash(channel, "AT45DB041B", SZ_512K, 2048, 264, 9);
+				break;
+			case 0x24:	/* 1 0 0 1 */
+				res = add_dataflash(channel, "AT45DB081B", SZ_1M, 4096, 264, 9);
+				break;
+			case 0x2c:	/* 1 0 1 1 */
+				res = add_dataflash(channel, "AT45DB161B", SZ_2M, 4096, 528, 10);
+				break;
+			case 0x34:	/* 1 1 0 1 */
+				res = add_dataflash(channel, "AT45DB321B", SZ_4M, 8192, 528, 10);
+				break;
+			case 0x3c:	/* 1 1 1 1 */
+				res = add_dataflash(channel, "AT45DB642", SZ_8M, 8192, 1056, 11);
+				break;
+// Currently unsupported since Atmel removed the "Main Memory Program via Buffer" commands.
+//			case 0x10:	/* 0 1 0 0 */
+//				res = add_dataflash(channel, "AT45DB1282", SZ_16M, 16384, 1056, 11);
+//				break;
+			default:
+				printk(KERN_ERR "at91_dataflash: Unknown device (%x)\n", status & 0x3c);
+		}
+	}
+
+	return res;
+}
+
+static int __init at91_dataflash_init(void)
+{
+	spi_transfer_desc = kmalloc(sizeof(struct spi_transfer_list), GFP_KERNEL);
+	if (!spi_transfer_desc)
+		return -ENOMEM;
+
+	/* DataFlash (SPI chip select 0) */
+	at91_dataflash_detect(0);
+
+#ifdef CONFIG_MTD_AT91_DATAFLASH_CARD
+	/* DataFlash card (SPI chip select 3) */
+	at91_dataflash_detect(3);
+#endif
+
+	return 0;
+}
+
+static void __exit at91_dataflash_exit(void)
+{
+	int i;
+
+	for (i = 0; i < DATAFLASH_MAX_DEVICES; i++) {
+		if (mtd_devices[i]) {
+#ifdef CONFIG_MTD_PARTITIONS
+			del_mtd_partitions(mtd_devices[i]);
+#else
+			del_mtd_device(mtd_devices[i]);
+#endif
+			kfree(mtd_devices[i]->priv);
+			kfree(mtd_devices[i]);
+		}
+	}
+	nr_devices = 0;
+	kfree(spi_transfer_desc);
+}
+
+
+module_init(at91_dataflash_init);
+module_exit(at91_dataflash_exit);
+
+MODULE_LICENSE("GPL");
+MODULE_AUTHOR("Andrew Victor");
+MODULE_DESCRIPTION("DataFlash driver for Atmel AT91RM9200");
diff -urN linux-2.6.22-rc5/drivers/mtd/devices/Kconfig linux-2.6.22-rc5.new/drivers/mtd/devices/Kconfig
--- linux-2.6.22-rc5/drivers/mtd/devices/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/mtd/devices/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -269,5 +269,11 @@
 	  LinuxBIOS or if you need to recover a DiskOnChip Millennium on which
 	  you have managed to wipe the first block.
 
-endmenu
+config MTD_AT91_DATAFLASH
+	tristate "AT91RM9200 DataFlash AT45DBxxx (legacy driver)"
+	depends on MTD && ARCH_AT91RM9200 && AT91_SPI
+	help
+	  This enables access to the DataFlash (AT45DBxxx) on the AT91RM9200.
+	  If you have such a board, say 'Y'.
 
+endmenu
diff -urN linux-2.6.22-rc5/drivers/mtd/devices/Makefile linux-2.6.22-rc5.new/drivers/mtd/devices/Makefile
--- linux-2.6.22-rc5/drivers/mtd/devices/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/mtd/devices/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -18,3 +18,4 @@
 obj-$(CONFIG_MTD_DATAFLASH)	+= mtd_dataflash.o
 obj-$(CONFIG_MTD_DATAFLASH26)	+= at91_dataflash26.o
 obj-$(CONFIG_MTD_M25P80)	+= m25p80.o
+obj-$(CONFIG_MTD_AT91_DATAFLASH)+= at91_dataflash.o
diff -urN linux-2.6.22-rc5/drivers/net/arm/at91_ether.c linux-2.6.22-rc5.new/drivers/net/arm/at91_ether.c
--- linux-2.6.22-rc5/drivers/net/arm/at91_ether.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/net/arm/at91_ether.c	2007-07-29 05:55:39.000000000 +0200
@@ -894,6 +894,7 @@
 			skb_reserve(skb, 2);
 			memcpy(skb_put(skb, pktlen), p_recv, pktlen);
 
+			skb->dev = dev;
 			skb->protocol = eth_type_trans(skb, dev);
 			dev->last_rx = jiffies;
 			lp->stats.rx_bytes += pktlen;
@@ -978,14 +979,22 @@
 	struct net_device *dev;
 	struct at91_private *lp;
 	unsigned int val;
-	int res;
+	struct resource *res;
+	int ret;
 
 	dev = alloc_etherdev(sizeof(struct at91_private));
 	if (!dev)
 		return -ENOMEM;
 
-	dev->base_addr = AT91_VA_BASE_EMAC;
-	dev->irq = AT91RM9200_ID_EMAC;
+	/* Get I/O base address and IRQ */
+	res = platform_get_resource(pdev, IORESOURCE_MEM, 0);
+	if (!res) {
+		free_netdev(dev);
+		return -ENODEV;
+	}
+	dev->base_addr = res->start;
+	dev->irq = platform_get_irq(pdev, 0);
+
 	SET_MODULE_OWNER(dev);
 
 	/* Install the interrupt handler */
@@ -1058,12 +1067,12 @@
 	lp->phy_address = phy_address;	/* MDI address of PHY */
 
 	/* Register the network interface */
-	res = register_netdev(dev);
-	if (res) {
+	ret = register_netdev(dev);
+	if (ret) {
 		free_irq(dev->irq, dev);
 		free_netdev(dev);
 		dma_free_coherent(NULL, sizeof(struct recv_desc_bufs), lp->dlist, (dma_addr_t)lp->dlist_phys);
-		return res;
+		return ret;
 	}
 
 	/* Determine current link speed */
diff -urN linux-2.6.22-rc5/drivers/serial/atmel_serial.c linux-2.6.22-rc5.new/drivers/serial/atmel_serial.c
--- linux-2.6.22-rc5/drivers/serial/atmel_serial.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/serial/atmel_serial.c	2007-07-29 05:55:39.000000000 +0200
@@ -7,6 +7,8 @@
  *  Based on drivers/char/serial_sa1100.c, by Deep Blue Solutions Ltd.
  *  Based on drivers/char/serial.c, by Linus Torvalds, Theodore Ts'o.
  *
+ *  DMA support added by Chip Coldwell.
+ *
  * This program is free software; you can redistribute it and/or modify
  * it under the terms of the GNU General Public License as published by
  * the Free Software Foundation; either version 2 of the License, or
@@ -33,6 +35,7 @@
 #include <linux/sysrq.h>
 #include <linux/tty_flip.h>
 #include <linux/platform_device.h>
+#include <linux/dma-mapping.h>
 #include <linux/atmel_pdc.h>
 
 #include <asm/io.h>
@@ -47,6 +50,11 @@
 
 #include "atmel_serial.h"
 
+#define SUPPORT_PDC
+#define PDC_BUFFER_SIZE		(L1_CACHE_BYTES << 3)
+#warning "Revisit"
+#define PDC_RX_TIMEOUT		(3 * 10)		/* 3 bytes */
+
 #if defined(CONFIG_SERIAL_ATMEL_CONSOLE) && defined(CONFIG_MAGIC_SYSRQ)
 #define SUPPORT_SYSRQ
 #endif
@@ -107,6 +115,13 @@
 static int (*atmel_open_hook)(struct uart_port *);
 static void (*atmel_close_hook)(struct uart_port *);
 
+struct atmel_dma_buffer {
+	unsigned char	*buf;
+	dma_addr_t	dma_addr;
+	size_t		dma_size;
+	unsigned int	ofs;
+};
+
 /*
  * We wrap our port structure around the generic uart_port.
  */
@@ -114,10 +129,20 @@
 	struct uart_port	uart;		/* uart */
 	struct clk		*clk;		/* uart clock */
 	unsigned short		suspended;	/* is port suspended? */
+
+	short			use_dma_rx;	/* enable PDC receiver */
+	short			pdc_rx_idx;	/* current PDC RX buffer */
+	struct atmel_dma_buffer	pdc_rx[2];	/* PDC receier */
+
+	short			use_dma_tx;	/* enable PDC transmitter */
+	struct atmel_dma_buffer	pdc_tx;		/* PDC transmitter */
 };
 
 static struct atmel_uart_port atmel_ports[ATMEL_MAX_UART];
 
+#define PDC_RX_BUF(port)	&(port)->pdc_rx[(port)->pdc_rx_idx]
+#define PDC_RX_SWITCH(port)	(port)->pdc_rx_idx = !(port)->pdc_rx_idx
+
 #ifdef SUPPORT_SYSRQ
 static struct console atmel_console;
 #endif
@@ -205,7 +230,12 @@
 {
 	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 
-	UART_PUT_IDR(port, ATMEL_US_TXRDY);
+	if (atmel_port->use_dma_tx) {
+		UART_PUT_PTCR(port, ATMEL_PDC_TXTDIS);		/* disable PDC transmit */
+		UART_PUT_IDR(port, ATMEL_US_ENDTX | ATMEL_US_TXBUFE);
+	}
+	else
+		UART_PUT_IDR(port, ATMEL_US_TXRDY);
 }
 
 /*
@@ -215,7 +245,17 @@
 {
 	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 
-	UART_PUT_IER(port, ATMEL_US_TXRDY);
+	if (atmel_port->use_dma_tx) {
+		if (UART_GET_PTSR(port) & ATMEL_PDC_TXTEN)
+			/* The transmitter is already running.  Yes, we
+			   really need this.*/
+			return;
+
+		UART_PUT_IER(port, ATMEL_US_ENDTX | ATMEL_US_TXBUFE);
+		UART_PUT_PTCR(port, ATMEL_PDC_TXTEN);		/* re-enable PDC transmit */
+	}
+	else
+		UART_PUT_IER(port, ATMEL_US_TXRDY);
 }
 
 /*
@@ -225,7 +265,12 @@
 {
 	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 
-	UART_PUT_IDR(port, ATMEL_US_RXRDY);
+	if (atmel_port->use_dma_rx) {
+		UART_PUT_PTCR(port, ATMEL_PDC_RXTDIS);		/* disable PDC receive */
+		UART_PUT_IDR(port, ATMEL_US_ENDRX | ATMEL_US_TIMEOUT);
+	}
+	else
+		UART_PUT_IDR(port, ATMEL_US_RXRDY);
 }
 
 /*
@@ -248,6 +293,134 @@
 }
 
 /*
+ * Receive data via the PDC.  A buffer has been fulled.
+ */
+static void atmel_pdc_endrx(struct uart_port *port)
+{
+	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
+	struct tty_struct *tty = port->info->tty;
+	struct atmel_dma_buffer *pdc = PDC_RX_BUF(atmel_port);
+	unsigned int count;
+
+	count = pdc->dma_size - pdc->ofs;
+	if (likely(count > 0)) {
+		dma_sync_single_for_cpu(port->dev, pdc->dma_addr, pdc->dma_size, DMA_FROM_DEVICE);
+		tty_insert_flip_string(tty, pdc->buf + pdc->ofs, count);
+		tty_flip_buffer_push(tty);
+
+		port->icount.rx += count;
+	}
+
+	/* Set this buffer as the next receive buffer */
+	pdc->ofs = 0;
+	UART_PUT_RNPR(port, pdc->dma_addr);
+	UART_PUT_RNCR(port, pdc->dma_size);
+
+	/* Switch to next buffer */
+	PDC_RX_SWITCH(atmel_port);		/* next PDC buffer */
+}
+
+/*
+ * Receive data via the PDC.  At least one byte was received, but the
+ * buffer was not full when the inter-character timeout expired.
+ */
+static void atmel_pdc_timeout(struct uart_port *port)
+{
+	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
+	struct tty_struct *tty = port->info->tty;
+	struct atmel_dma_buffer *pdc = PDC_RX_BUF(atmel_port);
+	/* unsigned */ int ofs, count;
+
+	ofs = UART_GET_RPR(port) - pdc->dma_addr;	/* current DMA adress */
+	count = ofs - pdc->ofs;
+
+	if (likely(count > 0)) {
+		dma_sync_single_for_cpu(port->dev, pdc->dma_addr, pdc->dma_size, DMA_FROM_DEVICE);
+		tty_insert_flip_string(tty, pdc->buf + pdc->ofs, count);
+		tty_flip_buffer_push(tty);
+
+		pdc->ofs = ofs;
+		port->icount.rx += count;
+	}
+
+	/* reset the UART timeout */
+	UART_PUT_CR(port, ATMEL_US_STTTO);
+}
+
+/*
+ * Deal with parity, framing and overrun errors.
+ */
+static void atmel_pdc_rxerr(struct uart_port *port, unsigned int status)
+{
+	/* clear error */
+	UART_PUT_CR(port, ATMEL_US_RSTSTA);
+
+	if (status & ATMEL_US_RXBRK) {
+		status &= ~(ATMEL_US_PARE | ATMEL_US_FRAME);	/* ignore side-effect */
+		port->icount.brk++;
+	}
+	if (status & ATMEL_US_PARE)
+		port->icount.parity++;
+	if (status & ATMEL_US_FRAME)
+		port->icount.frame++;
+	if (status & ATMEL_US_OVRE)
+		port->icount.overrun++;
+}
+
+/*
+ * A transmission via the PDC is complete.
+ */
+static void atmel_pdc_endtx(struct uart_port *port)
+{
+	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
+	struct circ_buf *xmit = &port->info->xmit;
+	struct atmel_dma_buffer *pdc = &atmel_port->pdc_tx;
+
+	xmit->tail += pdc->ofs;
+	if (xmit->tail >= SERIAL_XMIT_SIZE)
+		xmit->tail -= SERIAL_XMIT_SIZE;
+
+	port->icount.tx += pdc->ofs;
+	pdc->ofs = 0;
+
+	if (uart_circ_chars_pending(xmit) < WAKEUP_CHARS)
+		uart_write_wakeup(port);
+}
+
+/*
+ * The PDC transmitter is idle, so either start the next transfer or
+ * disable the transmitter.
+ */
+static void atmel_pdc_txbufe(struct uart_port *port)
+{
+	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
+	struct circ_buf *xmit = &port->info->xmit;
+	struct atmel_dma_buffer *pdc = &atmel_port->pdc_tx;
+	int count;
+
+	if (!uart_circ_empty(xmit)) {
+		/* more to transmit - setup next transfer */
+		UART_PUT_PTCR(port, ATMEL_PDC_TXTDIS);			/* disable PDC transmit */
+		dma_sync_single_for_device(port->dev, pdc->dma_addr, pdc->dma_size, DMA_TO_DEVICE);
+
+		if (xmit->tail < xmit->head)
+			count = xmit->head - xmit->tail;
+		else
+			count = SERIAL_XMIT_SIZE - xmit->tail;
+		pdc->ofs = count;
+
+		UART_PUT_TPR(port, pdc->dma_addr + xmit->tail);
+		UART_PUT_TCR(port, count);
+		UART_PUT_PTCR(port, ATMEL_PDC_TXTEN);			/* re-enable PDC transmit */
+	}
+	else {
+		/* nothing left to transmit - disable the transmitter */
+		UART_PUT_PTCR(port, ATMEL_PDC_TXTDIS);			/* disable PDC transmit */
+		UART_PUT_IDR(port, ATMEL_US_ENDTX | ATMEL_US_TXBUFE);
+	}
+}
+
+/*
  * Characters received (called from interrupt handler)
  */
 static void atmel_rx_chars(struct uart_port *port)
@@ -349,6 +522,14 @@
 	status = UART_GET_CSR(port);
 	pending = status & UART_GET_IMR(port);
 	while (pending) {
+		/* PDC receive */
+		if (pending & ATMEL_US_ENDRX)
+			atmel_pdc_endrx(port);
+		if (pending & ATMEL_US_TIMEOUT)
+			atmel_pdc_timeout(port);
+		if (atmel_port->use_dma_rx && pending & (ATMEL_US_RXBRK | ATMEL_US_OVRE | ATMEL_US_FRAME | ATMEL_US_PARE))
+			atmel_pdc_rxerr(port, pending);
+
 		/* Interrupt receive */
 		if (pending & ATMEL_US_RXRDY)
 			atmel_rx_chars(port);
@@ -363,6 +544,12 @@
 		if (pending & (ATMEL_US_RIIC | ATMEL_US_DSRIC | ATMEL_US_DCDIC | ATMEL_US_CTSIC))
 			wake_up_interruptible(&port->info->delta_msr_wait);
 
+		/* PDC transmit */
+		if (pending & ATMEL_US_ENDTX)
+			atmel_pdc_endtx(port);
+		if (pending & ATMEL_US_TXBUFE)
+			atmel_pdc_txbufe(port);
+
 		/* Interrupt transmit */
 		if (pending & ATMEL_US_TXRDY)
 			atmel_tx_chars(port);
@@ -401,6 +588,47 @@
 	}
 
 	/*
+	 * Initialize DMA (if necessary)
+	 */
+	if (atmel_port->use_dma_rx) {
+		int i;
+
+		for (i = 0; i < 2; i++) {
+			struct atmel_dma_buffer *pdc = &atmel_port->pdc_rx[i];
+
+			pdc->buf = kmalloc(PDC_BUFFER_SIZE, GFP_KERNEL);
+			if (pdc->buf == NULL) {
+				if (i != 0) {
+					dma_unmap_single(port->dev, atmel_port->pdc_rx[0].dma_addr, PDC_BUFFER_SIZE, DMA_FROM_DEVICE);
+					kfree(atmel_port->pdc_rx[0].buf);
+				}
+				free_irq(port->irq, port);
+				return -ENOMEM;
+			}
+			pdc->dma_addr = dma_map_single(port->dev, pdc->buf, PDC_BUFFER_SIZE, DMA_FROM_DEVICE);
+			pdc->dma_size = PDC_BUFFER_SIZE;
+			pdc->ofs = 0;
+		}
+
+		atmel_port->pdc_rx_idx = 0;
+
+		UART_PUT_RPR(port, atmel_port->pdc_rx[0].dma_addr);
+		UART_PUT_RCR(port, PDC_BUFFER_SIZE);
+
+		UART_PUT_RNPR(port, atmel_port->pdc_rx[1].dma_addr);
+		UART_PUT_RNCR(port, PDC_BUFFER_SIZE);
+	}
+	if (atmel_port->use_dma_tx) {
+		struct atmel_dma_buffer *pdc = &atmel_port->pdc_tx;
+		struct circ_buf *xmit = &port->info->xmit;
+
+		pdc->buf = xmit->buf;
+		pdc->dma_addr = dma_map_single(port->dev, pdc->buf, SERIAL_XMIT_SIZE, DMA_TO_DEVICE);
+		pdc->dma_size = SERIAL_XMIT_SIZE;
+		pdc->ofs = 0;
+	}
+
+	/*
 	 * If there is a specific "open" function (to register
 	 * control line interrupts)
 	 */
@@ -418,7 +646,15 @@
 	UART_PUT_CR(port, ATMEL_US_RSTSTA | ATMEL_US_RSTRX);
 	UART_PUT_CR(port, ATMEL_US_TXEN | ATMEL_US_RXEN);		/* enable xmit & rcvr */
 
-	UART_PUT_IER(port, ATMEL_US_RXRDY);		/* enable receive only */
+	if (atmel_port->use_dma_rx) {
+		UART_PUT_RTOR(port, PDC_RX_TIMEOUT);		/* set UART timeout */
+		UART_PUT_CR(port, ATMEL_US_STTTO);
+
+		UART_PUT_IER(port, ATMEL_US_ENDRX | ATMEL_US_TIMEOUT);
+		UART_PUT_PTCR(port, ATMEL_PDC_RXTEN);		/* enable PDC controller */
+	}
+	else
+		UART_PUT_IER(port, ATMEL_US_RXRDY);		/* enable receive only */
 
 	return 0;
 }
@@ -431,6 +667,31 @@
 	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 
 	/*
+	 * Ensure everything is stopped.
+	 */
+	atmel_stop_rx(port);
+	atmel_stop_tx(port);
+
+	/*
+	 * Shut-down the DMA.
+	 */
+	if (atmel_port->use_dma_rx) {
+		int i;
+
+		for (i = 0; i < 2; i++) {
+			struct atmel_dma_buffer *pdc = &atmel_port->pdc_rx[i];
+
+			dma_unmap_single(port->dev, pdc->dma_addr, pdc->dma_size, DMA_FROM_DEVICE);
+			kfree(pdc->buf);
+		}
+	}
+	if (atmel_port->use_dma_tx) {
+		struct atmel_dma_buffer *pdc = &atmel_port->pdc_tx;
+
+		dma_unmap_single(port->dev, pdc->dma_addr, pdc->dma_size, DMA_TO_DEVICE);
+	}
+
+	/*
 	 * Disable all interrupts, port and break condition.
 	 */
 	UART_PUT_CR(port, ATMEL_US_RSTSTA);
@@ -481,6 +742,7 @@
  */
 static void atmel_set_termios(struct uart_port *port, struct ktermios * termios, struct ktermios * old)
 {
+	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 	unsigned long flags;
 	unsigned int mode, imr, quot, baud;
 
@@ -490,7 +752,7 @@
 	baud = uart_get_baud_rate(port, termios, old, 0, port->uartclk/16);
 	quot = uart_get_divisor(port, baud);
 
-	if (quot > 65535) {		/* BRGR is 16-bit, so switch to slower clock */
+	if (quot > 65535) {	/* BRGR is 16-bit, so switch to slower clock */
 		quot /= 8;
 		mode |= ATMEL_US_USCLKS_MCK_DIV8;
 	}
@@ -539,6 +801,9 @@
 	if (termios->c_iflag & (BRKINT | PARMRK))
 		port->read_status_mask |= ATMEL_US_RXBRK;
 
+	if (atmel_port->use_dma_rx)	/* need to enable error interrupts */
+		UART_PUT_IER(port, port->read_status_mask);
+
 	/*
 	 * Characters to ignore
 	 */
@@ -717,6 +982,13 @@
 		clk_enable(atmel_port->clk);
 		port->uartclk = clk_get_rate(atmel_port->clk);
 	}
+
+#ifdef SUPPORT_PDC
+	atmel_port->use_dma_rx = data->use_dma_rx;
+	atmel_port->use_dma_tx = data->use_dma_tx;
+	if (atmel_port->use_dma_tx)
+		port->fifosize = PDC_BUFFER_SIZE;
+#endif
 }
 
 /*
@@ -893,7 +1165,8 @@
 	struct uart_port *port = platform_get_drvdata(pdev);
 	struct atmel_uart_port *atmel_port = (struct atmel_uart_port *) port;
 
-	if (device_may_wakeup(&pdev->dev) && !at91_suspend_entering_slow_clock())
+	if (device_may_wakeup(&pdev->dev)
+			&& !clk_must_disable(atmel_port->clk))
 		enable_irq_wake(port->irq);
 	else {
 		uart_suspend_port(&atmel_uart, port);
diff -urN linux-2.6.22-rc5/drivers/spi/Kconfig linux-2.6.22-rc5.new/drivers/spi/Kconfig
--- linux-2.6.22-rc5/drivers/spi/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/spi/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -55,6 +55,7 @@
 config SPI_ATMEL
 	tristate "Atmel SPI Controller"
 	depends on (ARCH_AT91 || AVR32) && SPI_MASTER
+	select SPI_AT91_MANUAL_CS if ARCH_AT91RM9200
 	help
 	  This selects a driver for the Atmel SPI Controller, present on
 	  many AT32 (AVR32) and AT91 (ARM) chips.
@@ -100,6 +101,24 @@
 	  inexpensive battery powered microcontroller evaluation board.
 	  This same cable can be used to flash new firmware.
 
+config SPI_AT91
+	tristate "AT91RM9200 Bitbang SPI Master"
+	depends on SPI_MASTER && ARCH_AT91RM9200 && !SPI_ATMEL && EXPERIMENTAL
+	select SPI_BITBANG
+	select SPI_AT91_MANUAL_CS
+	help
+	  This is dumb PIO bitbanging driver for the Atmel AT91RM9200.
+	  The SPI_ATMEL driver will be its replacement, using the native
+	  SPI hardware and its DMA controller.
+
+config SPI_AT91_MANUAL_CS
+	bool
+	depends on ARCH_AT91RM9200
+	help
+	  Works around an AT91RM9200 problem whereby the SPI chip-select
+	  will be wrongly disabled.  The workaround uses those pins as
+	  GPIOs instead of letting the SPI controller manage them.
+
 config SPI_IMX
 	tristate "Freescale iMX SPI controller"
 	depends on SPI_MASTER && ARCH_IMX && EXPERIMENTAL
diff -urN linux-2.6.22-rc5/drivers/spi/Makefile linux-2.6.22-rc5.new/drivers/spi/Makefile
--- linux-2.6.22-rc5/drivers/spi/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/spi/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -23,6 +23,7 @@
 obj-$(CONFIG_SPI_MPC83xx)		+= spi_mpc83xx.o
 obj-$(CONFIG_SPI_S3C24XX_GPIO)		+= spi_s3c24xx_gpio.o
 obj-$(CONFIG_SPI_S3C24XX)		+= spi_s3c24xx.o
+obj-$(CONFIG_SPI_AT91)			+= spi_at91_bitbang.o
 # 	... add above this line ...
 
 # SPI protocol drivers (device/link on bus)
diff -urN linux-2.6.22-rc5/drivers/spi/spi_at91_bitbang.c linux-2.6.22-rc5.new/drivers/spi/spi_at91_bitbang.c
--- linux-2.6.22-rc5/drivers/spi/spi_at91_bitbang.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/spi/spi_at91_bitbang.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,207 @@
+/*
+ * at91_spi.c - at91 SPI driver (BOOTSTRAP/BITBANG VERSION)
+ *
+ * Copyright (C) 2006 David Brownell
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+ */
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+
+#include <linux/spi/spi.h>
+#include <linux/spi/spi_bitbang.h>
+
+#include <asm/arch/gpio.h>
+
+
+/*
+ * FIXME this bitbanging version is just to help bootstrap systems until
+ * there's a native SPI+IRQ+DMA controller driver ... such a driver should
+ * be a drop-in replacement for this one, and much faster.
+ *
+ * remember:
+ *
+ *	- other at91 parts (like at91sam9) have multiple controllers
+ *	  and different pin muxing; this version is at91rm9200 specfic.
+ *
+ *	- at91sam9261 SPI0 pins are directly muxed with MMC/SD pins.
+ *
+ *	- rm9200 spi chipselects drop wrongly, so the native driver
+ *	  will need to use gpios much like this does.
+ *
+ *	- real hardware only allows 8..16 bits per word, while this
+ *	  bitbanger allows 1..32 (incompatible superset).
+ *
+ *	- this disregards clock parameters.  with inlined gpio calls,
+ *	  gcc 3.4.4 produces about 1.5 mbit/sec, more than 2x faster
+ *	  than using the subroutined veresion from txrx_word().
+ *
+ *	- suspend/resume and <linux/clk.h> support is missing ...
+ */
+
+#define	spi_miso_bit	AT91_PIN_PA0
+#define	spi_mosi_bit	AT91_PIN_PA1
+#define	spi_sck_bit	AT91_PIN_PA2
+
+struct at91_spi {
+	struct spi_bitbang	bitbang;
+	struct platform_device	*pdev;
+};
+
+/*----------------------------------------------------------------------*/
+
+static inline void setsck(struct spi_device *spi, int is_on)
+{
+	at91_set_gpio_value(spi_sck_bit, is_on);
+}
+
+static inline void setmosi(struct spi_device *spi, int is_on)
+{
+	at91_set_gpio_value(spi_mosi_bit, is_on);
+}
+
+static inline int getmiso(struct spi_device *spi)
+{
+	return at91_get_gpio_value(spi_miso_bit);
+}
+
+static void at91_spi_chipselect(struct spi_device *spi, int is_active)
+{
+	unsigned long cs = (unsigned long) spi->controller_data;
+
+	/* set default clock polarity */
+	if (is_active)
+		setsck(spi, spi->mode & SPI_CPOL);
+
+	/* only support active-low (default) */
+	at91_set_gpio_value(cs, !is_active);
+}
+
+/*
+ * NOTE:  this is "as fast as we can"; it should be a function of
+ * the device clock ...
+ */
+#define	spidelay(X)	do{} while(0)
+
+#define	EXPAND_BITBANG_TXRX
+#include <linux/spi/spi_bitbang.h>
+
+static u32 at91_spi_txrx_word_mode0(struct spi_device *spi,
+		unsigned nsecs, u32 word, u8 bits)
+{
+	return bitbang_txrx_be_cpha0(spi, nsecs, 0, word, 8);
+}
+
+static u32 at91_spi_txrx_word_mode1(struct spi_device *spi,
+		unsigned nsecs, u32 word, u8 bits)
+{
+	return bitbang_txrx_be_cpha1(spi, nsecs, 0, word, 8);
+}
+
+static u32 at91_spi_txrx_word_mode2(struct spi_device *spi,
+		unsigned nsecs, u32 word, u8 bits)
+{
+	return bitbang_txrx_be_cpha0(spi, nsecs, 1, word, 8);
+}
+
+static u32 at91_spi_txrx_word_mode3(struct spi_device *spi,
+		unsigned nsecs, u32 word, u8 bits)
+{
+	return bitbang_txrx_be_cpha1(spi, nsecs, 1, word, 8);
+}
+
+/*----------------------------------------------------------------------*/
+
+static int __init at91_spi_probe(struct platform_device *pdev)
+{
+	int			status;
+	struct spi_master	*master;
+	struct at91_spi		*at91_spi;
+
+	if (pdev->id != 0)	/* SPI0 bus */
+		return -EINVAL;
+
+	master = spi_alloc_master(&pdev->dev, sizeof *at91_spi);
+	if (!master)
+		return -ENOMEM;
+
+	at91_spi = spi_master_get_devdata(master);
+	at91_spi->pdev = pdev;
+	platform_set_drvdata(pdev, at91_spi);
+
+	/* SPI and bitbang hookup */
+	master->bus_num = 0;
+	master->num_chipselect = 4;
+
+	at91_spi->bitbang.master = spi_master_get(master);
+	at91_spi->bitbang.chipselect = at91_spi_chipselect;
+	at91_spi->bitbang.txrx_word[SPI_MODE_0] = at91_spi_txrx_word_mode0;
+	at91_spi->bitbang.txrx_word[SPI_MODE_1] = at91_spi_txrx_word_mode1;
+	at91_spi->bitbang.txrx_word[SPI_MODE_2] = at91_spi_txrx_word_mode2;
+	at91_spi->bitbang.txrx_word[SPI_MODE_3] = at91_spi_txrx_word_mode3;
+
+	status = spi_bitbang_start(&at91_spi->bitbang);
+	if (status < 0)
+		(void) spi_master_put(at91_spi->bitbang.master);
+
+	return status;
+}
+
+static int __exit at91_spi_remove(struct platform_device *pdev)
+{
+	struct at91_spi	*at91_spi = platform_get_drvdata(pdev);
+	int status;
+
+	/* stop() unregisters child devices too */
+	status = spi_bitbang_stop(&at91_spi->bitbang);
+	(void) spi_master_put(at91_spi->bitbang.master);
+
+	platform_set_drvdata(pdev, NULL);
+	return status;
+}
+
+static struct platform_driver at91_spi_driver = {
+	.probe		= at91_spi_probe,
+	.remove		= __exit_p(at91_spi_remove),
+	.driver		= {
+		.name	= "at91_spi",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static int __init at91_spi_init(void)
+{
+	at91_set_gpio_output(spi_sck_bit, 0);
+	at91_set_gpio_output(spi_mosi_bit, 0);
+	at91_set_gpio_input(spi_miso_bit, 1 /* pullup */);
+
+	/* register driver */
+	return platform_driver_register(&at91_spi_driver);
+}
+
+static void __exit at91_spi_exit(void)
+{
+	platform_driver_unregister(&at91_spi_driver);
+}
+
+device_initcall(at91_spi_init);
+module_exit(at91_spi_exit);
+
+MODULE_ALIAS("at91_spi.0");
+
+MODULE_DESCRIPTION("AT91 SPI support (BOOTSTRAP/BITBANG VERSION)");
+MODULE_AUTHOR("David Brownell");
+MODULE_LICENSE("GPL");
diff -urN linux-2.6.22-rc5/drivers/usb/gadget/at91_udc.c linux-2.6.22-rc5.new/drivers/usb/gadget/at91_udc.c
--- linux-2.6.22-rc5/drivers/usb/gadget/at91_udc.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/usb/gadget/at91_udc.c	2007-07-29 05:55:39.000000000 +0200
@@ -1803,7 +1803,7 @@
 	 */
 	if ((!udc->suspended && udc->addr)
 			|| !wake
-			|| at91_suspend_entering_slow_clock()) {
+			|| clk_must_disable(udc->fclk)) {
 		pullup(udc, 0);
 		wake = 0;
 	} else
diff -urN linux-2.6.22-rc5/drivers/usb/host/ohci-at91.c linux-2.6.22-rc5.new/drivers/usb/host/ohci-at91.c
--- linux-2.6.22-rc5/drivers/usb/host/ohci-at91.c	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/usb/host/ohci-at91.c	2007-07-29 05:55:39.000000000 +0200
@@ -299,7 +299,7 @@
 	 *
 	 * REVISIT: some boards will be able to turn VBUS off...
 	 */
-	if (at91_suspend_entering_slow_clock()) {
+	if (clk_must_disable(fclk)) {
 		ohci_usb_reset (ohci);
 		at91_stop_clock();
 	}
diff -urN linux-2.6.22-rc5/drivers/video/backlight/kb920x_bl.c linux-2.6.22-rc5.new/drivers/video/backlight/kb920x_bl.c
--- linux-2.6.22-rc5/drivers/video/backlight/kb920x_bl.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/video/backlight/kb920x_bl.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,164 @@
+/*
+ * Backlight Driver for KB9202
+ *
+ * Copyright (c) 2006 KwikByte
+ *
+ * Based on Sharp's Corgi Backlight Driver
+ *
+ * This file is subject to the terms and conditions of the GNU General Public
+ * License.  See the file "COPYING" in the main directory of this archive
+ * for more details.
+ */
+
+#include <linux/module.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/spinlock.h>
+#include <linux/fb.h>
+#include <linux/backlight.h>
+
+#include <asm/arch/gpio.h>
+
+/* The backlight is on(1)/off(0) */
+#define	KB9202_DEFAULT_INTENSITY	1
+#define	KB9202_MAX_INTENSITY		1
+
+static int kb9202bl_suspended;
+static int current_intensity = 0;
+static DEFINE_SPINLOCK(bl_lock);
+
+static int kb9202bl_set_intensity(struct backlight_device *bd)
+{
+	unsigned long flags;
+	int intensity = bd->props.brightness;
+
+	if (bd->props.power != FB_BLANK_UNBLANK)
+		intensity = 0;
+	if (bd->props.fb_blank != FB_BLANK_UNBLANK)
+		intensity = 0;
+	if (kb9202bl_suspended)
+		intensity = 0;
+
+	if ((!current_intensity) && (bd->props.power == FB_BLANK_UNBLANK))
+		intensity = 1;
+
+	spin_lock_irqsave(&bl_lock, flags);
+	if (intensity)
+		gpio_set_value(AT91_PIN_PC23, 1);
+	else
+		gpio_set_value(AT91_PIN_PC23, 0);
+	spin_unlock_irqrestore(&bl_lock, flags);
+
+	current_intensity = intensity;
+
+	return 0;
+}
+
+static int kb9202bl_get_intensity(struct backlight_device *bd)
+{
+	return current_intensity;
+}
+
+static struct backlight_ops kb9202bl_ops = {
+	.get_brightness	= kb9202bl_get_intensity,
+	.update_status	= kb9202bl_set_intensity,
+};
+
+static int __init kb9202bl_probe(struct platform_device *pdev)
+{
+	struct backlight_device *bd;
+
+	bd = backlight_device_register ("kb9202-bl", &pdev->dev, NULL, &kb9202bl_ops);
+	if (IS_ERR(bd))
+		return PTR_ERR(bd);
+
+	platform_set_drvdata(pdev, bd);
+
+	bd->props.max_brightness = KB9202_MAX_INTENSITY;
+	bd->props.brightness = KB9202_DEFAULT_INTENSITY;
+	(void) kb9202bl_set_intensity(bd);
+
+	return 0;
+}
+
+static int kb9202bl_remove(struct platform_device *pdev)
+{
+	struct backlight_device *bd = platform_get_drvdata(pdev);
+
+	bd->props.brightness = 0;
+	bd->props.power = 0;
+	(void) kb9202bl_set_intensity(bd);
+
+	backlight_device_unregister(bd);
+
+	return 0;
+}
+
+#ifdef CONFIG_PM
+static int kb9202bl_suspend(struct platform_device *dev, pm_message_t state)
+{
+	struct backlight_device *bd = platform_get_drvdata(pdev);
+
+	kb9202bl_suspended = 1;
+	(void) kb9202bl_set_intensity(bd);
+	return 0;
+}
+
+static int kb9202bl_resume(struct platform_device *dev)
+{
+	struct backlight_device *bd = platform_get_drvdata(pdev);
+
+	kb9202bl_suspended = 0;
+	(void) kb9202bl_set_intensity(bd);
+	return 0;
+}
+#else
+#define kb9202bl_suspend	NULL
+#define kb9202bl_resume		NULL
+#endif
+
+static struct platform_driver kb9202bl_driver = {
+	.probe		= kb9202bl_probe,
+	.remove		= kb9202bl_remove,
+	.suspend	= kb9202bl_suspend,
+	.resume		= kb9202bl_resume,
+	.driver		= {
+		.name	= "kb9202-bl",
+		.owner	= THIS_MODULE,
+	},
+};
+
+static struct platform_device *kb9202bl_device;
+
+static int __init kb9202bl_init(void)
+{
+	int ret;
+
+	ret = platform_driver_register(&kb9202bl_driver);
+	if (!ret) {
+		kb9202bl_device = platform_device_alloc("kb9202-bl", -1);
+		if (!kb9202bl_device)
+			return -ENOMEM;
+
+		ret = platform_device_add(kb9202bl_device);
+		if (ret) {
+			platform_device_put(kb9202bl_device);
+			platform_driver_unregister(&kb9202bl_driver);
+		}
+	}
+	return ret;
+}
+
+static void __exit kb9202bl_exit(void)
+{
+	platform_device_unregister(kb9202bl_device);
+	platform_driver_unregister(&kb9202bl_driver);
+}
+
+module_init(kb9202bl_init);
+module_exit(kb9202bl_exit);
+
+MODULE_AUTHOR("KwikByte <kb9200_dev@kwikbyte.com>");
+MODULE_DESCRIPTION("KB9202 Backlight Driver");
+MODULE_LICENSE("GPL");
diff -urN linux-2.6.22-rc5/drivers/video/backlight/Kconfig linux-2.6.22-rc5.new/drivers/video/backlight/Kconfig
--- linux-2.6.22-rc5/drivers/video/backlight/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/video/backlight/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -71,3 +71,11 @@
 	help
 	  If you have a Intel LE80578 (Carillo Ranch) say Y to enable the
 	  backlight driver.
+
+config BACKLIGHT_KB920x
+	tristate "KwikByte KB9202 Backlight Driver"
+	depends on BACKLIGHT_CLASS_DEVICE && MACH_KB9200
+	default y
+	help
+	  If you have a KwikByte KB9202 board, say Y to enable the
+	  backlight driver.
diff -urN linux-2.6.22-rc5/drivers/video/backlight/Makefile linux-2.6.22-rc5.new/drivers/video/backlight/Makefile
--- linux-2.6.22-rc5/drivers/video/backlight/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/video/backlight/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -7,3 +7,4 @@
 obj-$(CONFIG_BACKLIGHT_LOCOMO)	+= locomolcd.o
 obj-$(CONFIG_BACKLIGHT_PROGEAR) += progear_bl.o
 obj-$(CONFIG_BACKLIGHT_CARILLO_RANCH) += cr_bllcd.o
+obj-$(CONFIG_BACKLIGHT_KB920x)	+= kb920x_bl.o
diff -urN linux-2.6.22-rc5/drivers/video/Kconfig linux-2.6.22-rc5.new/drivers/video/Kconfig
--- linux-2.6.22-rc5/drivers/video/Kconfig	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/video/Kconfig	2007-07-29 05:55:39.000000000 +0200
@@ -822,6 +822,17 @@
 	  framebuffer.  Product specs at
 	  <http://www.erd.epson.com/vdc/html/products.htm>.
 
+config FB_S1D15605
+	tristate "Epson S1D15605 framebuffer support"
+	depends on FB
+	default m if MACH_KB9200
+	select FB_CFB_FILLRECT
+	select FB_CFB_COPYAREA
+	select FB_CFB_IMAGEBLIT
+	help
+	  Build in support for the S1D15605 Epson Research 128x64
+	  LCD controller as a framebuffer.
+
 config FB_S1D13XXX
 	tristate "Epson S1D13XXX framebuffer support"
 	depends on FB
@@ -835,7 +846,7 @@
 
 config FB_ATMEL
 	tristate "AT91/AT32 LCD Controller support"
-	depends on FB && (ARCH_AT91SAM9261 || ARCH_AT91SAM9263 || AVR32)
+	depends on FB && (ARCH_AT91SAM9261 || ARCH_AT91SAM9263 || ARCH_AT91SAM9RL || AVR32)
 	select FB_CFB_FILLRECT
 	select FB_CFB_COPYAREA
 	select FB_CFB_IMAGEBLIT
diff -urN linux-2.6.22-rc5/drivers/video/Makefile linux-2.6.22-rc5.new/drivers/video/Makefile
--- linux-2.6.22-rc5/drivers/video/Makefile	2007-06-17 04:09:12.000000000 +0200
+++ linux-2.6.22-rc5.new/drivers/video/Makefile	2007-07-29 05:55:39.000000000 +0200
@@ -87,7 +87,8 @@
 obj-$(CONFIG_FB_SA1100)           += sa1100fb.o
 obj-$(CONFIG_FB_HIT)              += hitfb.o
 obj-$(CONFIG_FB_EPSON1355)	  += epson1355fb.o
-obj-$(CONFIG_FB_ATMEL)		  += atmel_lcdfb.o
+obj-$(CONFIG_FB_S1D15605)	  += s1d15605fb.o
+obj-$(CONFIG_FB_ATMEL)            += atmel_lcdfb.o
 obj-$(CONFIG_FB_PVR2)             += pvr2fb.o
 obj-$(CONFIG_FB_VOODOO1)          += sstfb.o
 obj-$(CONFIG_FB_ARMCLCD)	  += amba-clcd.o
diff -urN linux-2.6.22-rc5/drivers/video/s1d15605fb.c linux-2.6.22-rc5.new/drivers/video/s1d15605fb.c
--- linux-2.6.22-rc5/drivers/video/s1d15605fb.c	1970-01-01 01:00:00.000000000 +0100
+++ linux-2.6.22-rc5.new/drivers/video/s1d15605fb.c	2007-07-29 05:55:39.000000000 +0200
@@ -0,0 +1,659 @@
+/*
+ *  drivers/video/s1d15605.c
+ *
+ * Adapted from several sources including:
+ * 1) Driver for AT91 LCD Controller
+ *    Copyright (C) 2006 Atmel
+ *
+ * 2) Copyright (C) 2005 S. Kevin Hester
+ *
+ *   This file is subject to the terms and conditions of the GNU General Public
+ *   License. See the file COPYING in the main directory of this archive for
+ *   more details.
+ *
+ *   This is a basic framebuffer driver for the Optrex F-51320 128x64 mono LCD
+ *   display.  This display uses a clone of the common Epson SED 1531 display
+ *   controller.
+ *
+ *   I've heavily borrowed code from the vfb.c driver.
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 59 Temple Place, Suite 330, Boston, MA  02111-1307  USA
+ */
+
+#ifdef DEBUG
+#define MSG(string, args...) printk("s1d15605fb:" string, ##args)
+#else
+#define MSG(string, args...)
+#endif
+
+#include <linux/kernel.h>
+#include <linux/platform_device.h>
+#include <linux/dma-mapping.h>
+#include <linux/interrupt.h>
+#include <linux/clk.h>
+#include <linux/fb.h>
+#include <linux/init.h>
+#include <linux/delay.h>
+
+#include <asm/uaccess.h>
+
+#include <asm/arch/board.h>
+#include <asm/arch/gpio.h>
+
+#ifdef CONFIG_PMAC_BACKLIGHT
+#include <asm/backlight.h>
+#endif
+
+#define VIDEOWIDTH		128
+#define VIDEOHEIGHT		64
+#define VIDEODEPTH		1	/* bits/pixel */
+#define VIDEOWIDTH_BYTES	((VIDEOWIDTH * VIDEODEPTH) / 8)
+
+/* The number of bytes that actually go to the device */
+#define ACTUALVIDEOMEMSIZE	(VIDEOWIDTH_BYTES * VIDEOHEIGHT)
+#define VIDEOMEMSIZE		PAGE_SIZE
+
+static struct fb_var_screeninfo s1d15605_default __initdata = {
+	.xres		= VIDEOWIDTH,
+	.yres		= VIDEOHEIGHT,
+	.xres_virtual	= VIDEOWIDTH,
+	.yres_virtual	= VIDEOHEIGHT,
+	.bits_per_pixel	= VIDEODEPTH,
+	.red		= { 0, 1, 0 },
+	.green		= { 0, 1, 0 },
+	.blue		= { 0, 1, 0 },
+	.activate	= FB_ACTIVATE_NOW,
+	.pixclock	= 20000,
+	.vmode		= FB_VMODE_NONINTERLACED,
+};
+
+static struct fb_fix_screeninfo s1d15605_fix __initdata = {
+	.id		= "s1d15605",
+	.type		= FB_TYPE_PACKED_PIXELS,
+	.visual		= FB_VISUAL_MONO10,
+	.xpanstep	= 0,
+	.ypanstep	= 0,
+	.ywrapstep	= 0,
+	.accel		= FB_ACCEL_NONE,
+};
+
+struct s1d15605fb_info {
+	struct fb_info		*info;
+	char			*mmio;
+	unsigned long		reset_pin;
+	struct platform_device	*pdev;
+};
+
+/*
+ * LCD device interface
+ */
+#define	RESET_DISPLAY		0xE2
+#define	LCD_BIAS_1_9		0xA2
+#define	ADC_SELECT_REVERSE	0xA1
+#define	COMMON_OUTPUT_NORMAL	0xC0
+#define	V5_RESISTOR_RATIO	0x26
+#define	ELECTRONIC_VOLUME_SET	0x81
+#define	ELECTRONIC_VOLUME_INIT	0x20
+#define	POWER_CONTROL_SET	0x28
+#define	VOLTAGE_REGULATOR	0x02
+#define	VOLTAGE_FOLLOWER	0x01
+#define	BOOSTER_CIRCUIT		0x04
+#define	DISPLAY_ON		0xAF
+#define	START_LINE_SET		0x40
+#define	PAGE_ADDRESS_SET	0xB0
+#define	COLUMN_ADDRESS_HIGH	0x10
+#define	COLUMN_ADDRESS_LOW	0x00
+#define	RESISTOR_RATIO_START	0x20
+
+#define	NUM_OF_PAGES		8
+#define	NUM_OF_COLUMNS		128
+
+#define	WRITE_COMMAND(x)	__raw_writeb((x), (sinfo)->mmio)
+#define	READ_COMMAND		__raw_readb((sinfo)->mmio)
+#define	WRITE_DATA(x)		__raw_writeb((x), (sinfo)->mmio + (0x10000))
+#define	READ_DATA		__raw_readb((sinfo)->mmio + (0x10000))
+
+
+/*
+ *	s1d15605fb_resize_framebuffer
+ *
+ *	Free allocated space if different.  Allocate on new of changed.
+ *	Returns -ENOMEM if the new framebuffer can not be allocated,
+ *	zero on success.
+ */
+static int s1d15605fb_resize_framebuffer(struct s1d15605fb_info *sinfo)
+{
+	struct fb_info			*info = sinfo->info;
+	struct fb_fix_screeninfo	*fix = &info->fix;
+	struct fb_var_screeninfo	*var = &info->var;
+	unsigned int			new_size;
+	void				*new_vaddr;
+
+	new_size = ((var->xres_virtual * var->yres_virtual * var->bits_per_pixel) / 8);
+
+	MSG("%s: x (%d) y (%d) bpp (%d): new size 0x%08x\n", __FUNCTION__,
+		var->xres_virtual, var->yres_virtual, var->bits_per_pixel, new_size);
+
+	if (new_size == fix->smem_len)
+		return 0;
+
+	if (fix->smem_len) {
+		kfree(info->screen_base);
+	}
+
+	new_vaddr = kmalloc(new_size, GFP_KERNEL);
+
+	if (!new_vaddr) {
+		fix->smem_len = 0;
+		return -ENOMEM;
+	}
+
+	info->screen_base = new_vaddr;
+	fix->smem_start = (unsigned)new_vaddr;
+	fix->smem_len = new_size;
+	fix->line_length = (var->xres_virtual * var->bits_per_pixel) / 8;
+
+	dev_info(info->device,
+		"%luKiB frame buffer at %08lx (mapped at %p)\n",
+		(unsigned long)info->fix.smem_len / 1024,
+		(unsigned long)info->fix.smem_start,
+		info->screen_base);
+
+	return 0;
+}
+
+
+/*
+ * The s1d15605 seems to be divided into eight 128 pixel wide pages (from top to
+ * bottom) each page seems to be eight pixels high, where these eight pixels are
+ * one byte
+ */
+static void s1d15605_update(struct fb_info *info)
+{
+	struct s1d15605fb_info	*sinfo = info->par;
+	int			page, i, row, colmask;
+	u8			retVal, *rowPtr;
+
+	WRITE_COMMAND(START_LINE_SET);
+	for (page = 0; page < NUM_OF_PAGES; ++page) {
+		WRITE_COMMAND(PAGE_ADDRESS_SET + page);
+		WRITE_COMMAND(COLUMN_ADDRESS_HIGH);
+		WRITE_COMMAND(COLUMN_ADDRESS_LOW);
+
+		for (i = 0; i < NUM_OF_COLUMNS; ++i)
+		{
+			/* point of opportunity: optimization */
+			colmask = (1 << (i & 0x7));
+			rowPtr = (u8*)(info->screen_base);
+			rowPtr += (VIDEOWIDTH_BYTES * 8 * page);
+			rowPtr += (i >> 3);
+			retVal = 0;
+			for (row = 0; row < 8; ++row)
+			{
+				retVal = (retVal >> 1) | (((*rowPtr) & colmask) ? 0x80 : 0);
+				rowPtr += VIDEOWIDTH_BYTES;
+			}
+			WRITE_DATA(retVal);
+		}
+	}
+
+	WRITE_COMMAND(DISPLAY_ON);
+}
+
+
+/*
+ * Setting the video mode has been split into two parts.
+ * First part, xxxfb_check_var, must not write anything
+ * to hardware, it should only verify and adjust var.
+ * This means it doesn't alter par but it does use hardware
+ * data from it to check this var.
+ */
+static int s1d15605_check_var(struct fb_var_screeninfo *var, struct fb_info *info)
+{
+	/*
+	 * Some very basic checks
+	 */
+	if (!var->xres)
+		var->xres = 1;
+	if (!var->yres)
+		var->yres = 1;
+	if (var->xres > var->xres_virtual)
+		var->xres_virtual = var->xres;
+	if (var->yres > var->yres_virtual)
+		var->yres_virtual = var->yres;
+
+	if(var->bits_per_pixel > VIDEODEPTH)
+		return -EINVAL;
+
+	/*
+	 * Memory limit
+	 */
+	if (((var->yres_virtual * var->bits_per_pixel * var->yres_virtual) >> 3) >
+			ACTUALVIDEOMEMSIZE)
+		return -ENOMEM;
+
+	/*
+	 * Now that we checked it we alter var. The reason being is that the video
+	 * mode passed in might not work but slight changes to it might make it
+	 * work. This way we let the user know what is acceptable.
+	 */
+	switch (var->bits_per_pixel) {
+	case 1:
+		var->red.offset = var->green.offset = var->blue.offset = 0;
+		var->red.length = var->green.length = var->blue.length
+			= var->bits_per_pixel;
+		break;
+	default:
+		return -EINVAL;
+	}
+
+	var->xoffset = var->yoffset = 0;
+	var->red.msb_right = var->green.msb_right = var->blue.msb_right =
+		var->transp.msb_right = 0;
+
+	return 0;
+}
+
+
+/*
+ * This routine actually sets the video mode. It's in here where we
+ * the hardware state info->par and fix which can be affected by the
+ * change in par. For this driver it doesn't do much.
+ */
+static int s1d15605_set_par(struct fb_info *info)
+{
+	int	ret;
+
+	MSG("%s:\n", __func__);
+	MSG("  * resolution: %ux%u (%ux%u virtual)\n",
+		 info->var.xres, info->var.yres,
+		 info->var.xres_virtual, info->var.yres_virtual);
+
+	ret = s1d15605fb_resize_framebuffer(info->par);
+
+	info->fix.visual = FB_VISUAL_MONO10;
+	return ret;
+}
+
+
+/*
+ * Set a single color register. The values supplied are already
+ * rounded down to the hardware's capabilities (according to the
+ * entries in the var structure). Return != 0 for invalid regno.
+ */
+static int s1d15605_setcolreg(u_int regno, u_int red, u_int green, u_int blue,
+			u_int transp, struct fb_info *info)
+{
+	if (regno > 1)	/* no. of hw registers - we only do mono now */
+		return 1;
+
+	return 0;
+}
+
+
+/*
+ * Currently, the routine will simply shut-off the backlight and prevent
+ * updates/refreshes.  Modify according to application.
+ *
+ * 0 unblank, 1 blank, 2 no vsync, 3 no hsync, 4 off
+ */
+static int s1d15605_blank(int blank, struct fb_info *info)
+{
+#ifdef CONFIG_PMAC_BACKLIGHT
+	if (blank)
+		pmac_backlight->props.power = FB_BLANK_POWERDOWN;
+	else
+		pmac_backlight->props.power = FB_BLANK_UNBLANK;
+	backlight_update_status(pmac_backlight);
+#endif
+	return 1;
+}
+
+
+/*
+ * Pan or Wrap the Display
+ *
+ * This call looks only at xoffset, yoffset and the FB_VMODE_YWRAP flag
+ */
+/*
+static int s1d15605_pan_display(struct fb_var_screeninfo *var,
+			struct fb_info *info)
+{
+	if (var->vmode & FB_VMODE_YWRAP) {
+		if (var->yoffset < 0
+		    || var->yoffset >= info->var.yres_virtual
+		    || var->xoffset)
+			return -EINVAL;
+	} else {
+		if (var->xoffset + var->xres > info->var.xres_virtual ||
+		    var->yoffset + var->yres > info->var.yres_virtual)
+			return -EINVAL;
+	}
+	info->var.xoffset = var->xoffset;
+	info->var.yoffset = var->yoffset;
+	if (var->vmode & FB_VMODE_YWRAP)
+		info->var.vmode |= FB_VMODE_YWRAP;
+	else
+		info->var.vmode &= ~FB_VMODE_YWRAP;
+	return 0;
+}
+*/
+
+
+static void s1d15605_copyarea(struct fb_info *info, const struct fb_copyarea *region)
+{
+	cfb_copyarea(info, region);
+	s1d15605_update(info);
+}
+
+
+static void s1d15605_fillrect (struct fb_info *info, const struct fb_fillrect *rect)
+{
+	cfb_fillrect(info, rect);
+	s1d15605_update(info);
+}
+
+
+static void s1d15605_imageblit(struct fb_info *p, const struct fb_image *image)
+{
+	cfb_imageblit(p, image);
+	s1d15605_update(p);
+}
+
+
+/*
+ * Write the users data to our framebuffer, and then trigger a psuedo DMA
+ */
+static ssize_t s1d15605_write(struct file *file, const char *buf,
+			size_t count, loff_t *ppos)
+{
+	unsigned long p = *ppos;
+	struct inode *inode = file->f_dentry->d_inode;
+	int fbidx = iminor(inode);
+	struct fb_info *info = registered_fb[fbidx];
+	int err;
+
+	if (p > info->fix.smem_len)
+		return -ENOSPC;
+	if (count >= info->fix.smem_len)
+		count = info->fix.smem_len;
+	err = 0;
+	if (count + p > info->fix.smem_len) {
+		count = info->fix.smem_len - p;
+		err = -ENOSPC;
+	}
+	if (count) {
+		char *base_addr;
+
+		base_addr = info->screen_base;
+		count -= copy_from_user(base_addr+p, buf, count);
+		*ppos += count;
+		err = -EFAULT;
+	}
+
+	s1d15605_update(info);
+
+	if (count)
+		return count;
+
+	return err;
+}
+
+#ifdef	USE_PRIVATE_VMA_FXS
+static void s1d15605_vma_open(struct vm_area_struct *vma)
+{
+	// FIXME - store stats in the device data via vm_private_data
+}
+
+
+static void s1d15605_vma_close(struct vm_area_struct *vma)
+{
+	// FIXME - store stats in the device data via vm_private_data
+}
+
+
+static struct page *s1d15605_vma_nopage(struct vm_area_struct *vma,
+				unsigned long address, int *type)
+{
+	struct page *page;
+	struct fb_info *info = vma->vm_private_data;
+
+	page = virt_to_page(info->screen_base);
+	get_page(page);
+
+	// FIXME - now someone has a link to our page, start periodically blitting
+	// latest updates to the actual device.
+
+	return page;
+}
+
+
+static struct vm_operations_struct s1d15605_vm_ops = {
+	.open	= s1d15605_vma_open,
+	.close	= s1d15605_vma_close,
+	.nopage	= s1d15605_vma_nopage
+};
+
+
+/* We don't do much here - because we have special vm_ops */
+static int s1d15605_mmap(struct fb_info *info, struct vm_area_struct *vma)
+{
+	vma->vm_ops = &s1d15605_vm_ops;
+	vma->vm_flags |= VM_RESERVED;
+	vma->vm_private_data = info;
+	s1d15605_vma_open(vma);
+
+	return 0;
+}
+#endif /* USE_PRIVATE_VMA_FXS */
+
+
+static struct fb_ops s1d15605fb_ops = {
+	.owner		= THIS_MODULE,
+	.fb_check_var	= s1d15605_check_var,
+	.fb_set_par	= s1d15605_set_par,
+	.fb_setcolreg	= s1d15605_setcolreg,
+	.fb_blank	= s1d15605_blank,
+//	.fb_pan_display	= s1d15605_pan_display,
+	.fb_fillrect	= s1d15605_fillrect,
+	.fb_copyarea	= s1d15605_copyarea,
+	.fb_imageblit	= s1d15605_imageblit,
+	.fb_write	= s1d15605_write,
+#ifdef	USE_PRIVATE_VMA_FXS
+	.fb_mmap	= s1d15605_mmap,
+#endif
+};
+
+
+static void s1d15605_device_init(struct s1d15605fb_info *sinfo) {
+
+	char	value;
+
+	/* release the reset line by reading the device - proto hardware */
+	value = READ_COMMAND;
+	value = READ_COMMAND;
+
+#ifdef CONFIG_MACH_KB9200
+	/* new boards have dedicated reset line */
+	gpio_set_value(sinfo->reset_pin, 1);
+#endif
+
+	/* initialize the device within 5ms */
+	WRITE_COMMAND(RESET_DISPLAY);
+	WRITE_COMMAND(LCD_BIAS_1_9);
+	WRITE_COMMAND(ADC_SELECT_REVERSE);
+	WRITE_COMMAND(COMMON_OUTPUT_NORMAL);
+	WRITE_COMMAND(V5_RESISTOR_RATIO);
+	WRITE_COMMAND(ELECTRONIC_VOLUME_SET);
+	WRITE_COMMAND(ELECTRONIC_VOLUME_INIT);
+	WRITE_COMMAND(POWER_CONTROL_SET | VOLTAGE_REGULATOR | VOLTAGE_FOLLOWER | BOOSTER_CIRCUIT);
+	WRITE_COMMAND(DISPLAY_ON);
+
+	WRITE_COMMAND(RESISTOR_RATIO_START + 4);
+	WRITE_COMMAND(ELECTRONIC_VOLUME_SET);
+	WRITE_COMMAND(0x33);
+}
+
+
+static int s1d15605fb_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct fb_info *info;
+	struct s1d15605fb_info *sinfo;
+	int ret;
+
+	MSG("%s\n", __func__);
+
+	if (!(info = framebuffer_alloc(sizeof(struct s1d15605fb_info), dev))) {
+		dev_err(dev, "Cannot allocate framebuffer struct\n");
+		return -ENOMEM;
+	}
+
+	sinfo = info->par;
+	sinfo->info = info;
+	sinfo->pdev = pdev;
+
+	if (pdev->num_resources < 2) {
+		dev_err(dev, "Resources unusable\n");
+		ret = -ENODEV;
+		goto free_info;
+	}
+
+	info->fbops = &s1d15605fb_ops;
+	strcpy(info->fix.id, pdev->name);
+
+	info->fix.mmio_start = pdev->resource[0].start;
+	info->fix.mmio_len = pdev->resource[0].end - pdev->resource[0].start + 1;
+	sinfo->reset_pin = pdev->resource[1].start;
+
+	ret = s1d15605fb_resize_framebuffer(sinfo);
+	if (ret < 0) {
+		dev_err(dev, "Cannot resize framebuffer: %d\n", ret);
+		goto free_fb;
+	}
+
+	if (!request_mem_region(info->fix.mmio_start,
+				info->fix.mmio_len, pdev->name)) {
+		ret = -EBUSY;
+		goto free_fb;
+	}
+
+	sinfo->mmio = ioremap(info->fix.mmio_start, info->fix.mmio_len);
+	if (!sinfo->mmio) {
+		dev_err(dev, "Cannot map LCD memory region\n");
+		goto release_mem;
+	}
+
+	s1d15605_device_init(sinfo);
+
+	ret = fb_find_mode(&info->var, info, NULL, NULL, 0, NULL, 1);
+
+	if (!ret || (ret == 4))
+		info->var = s1d15605_default;
+
+	info->fix = s1d15605_fix;
+	info->flags = FBINFO_FLAG_DEFAULT |
+/*		FBINFO_HWACCEL_YPAN | */
+		FBINFO_HWACCEL_FILLRECT | FBINFO_HWACCEL_COPYAREA;
+
+	ret = register_framebuffer(info);
+	if (ret < 0) {
+		dev_err(dev, "Failed to register framebuffer device: %d\n", ret);
+		goto unmap_mmio;
+	}
+
+	dev_set_drvdata(dev, info);
+
+	memset(info->screen_base, 0, info->fix.smem_len);
+	info->var.activate |= FB_ACTIVATE_NOW;
+	ret = fb_set_var(info, &info->var);
+	if (ret) {
+		dev_warn(dev, "Unable to set display parameters\n");
+	}
+
+	info->var.activate &= ~(FB_ACTIVATE_FORCE | FB_ACTIVATE_NOW);
+
+	dev_dbg(dev, "%s SUCCESS\n", __func__);
+
+	dev_info(dev, "Driver $Revision: 1.1 $\n");
+
+	return 0;
+
+unmap_mmio:
+	iounmap(sinfo->mmio);
+release_mem:
+	release_mem_region(info->fix.mmio_start, info->fix.mmio_len);
+free_fb:
+	kfree(info->screen_base);
+
+free_info:
+	framebuffer_release(info);
+
+	dev_dbg(dev, "%s FAILED\n", __func__);
+	return ret;
+}
+
+
+static int s1d15605fb_remove(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct fb_info *info = dev_get_drvdata(dev);
+	struct s1d15605fb_info *sinfo = info->par;
+
+	if (!sinfo)
+		return 0;
+
+	unregister_framebuffer(info);
+
+	iounmap(sinfo->mmio);
+	release_mem_region(info->fix.mmio_start, info->fix.mmio_len);
+
+	kfree(info->screen_base);
+
+	dev_set_drvdata(dev, NULL);
+	framebuffer_release(info);
+	return 0;
+}
+
+
+static struct platform_driver s1d15605fb_driver = {
+	.probe		= s1d15605fb_probe,
+	.remove		= s1d15605fb_remove,
+	.driver		= {
+		.name	= "s1d15605fb",
+		.owner	= THIS_MODULE,
+	},
+};
+
+
+static int __init s1d15605fb_init(void)
+{
+	return platform_driver_register(&s1d15605fb_driver);
+}
+
+
+static void __exit s1d15605fb_exit(void)
+{
+	platform_driver_unregister(&s1d15605fb_driver);
+}
+
+
+module_init(s1d15605fb_init);
+module_exit(s1d15605fb_exit);
+
+
+MODULE_AUTHOR("KwikByte");
+MODULE_DESCRIPTION("Epson S1D15605 LCD Controller framebuffer driver");
+MODULE_LICENSE("GPL");
