diff -ruN rt61-cvs-2007060307-old/Module/rt_config.h rt61-cvs-2007060307-new/Module/rt_config.h
--- rt61-cvs-2007060307-old/Module/rt_config.h	2007-06-03 14:35:29.000000000 +0200
+++ rt61-cvs-2007060307-new/Module/rt_config.h	2007-08-25 20:45:36.000000000 +0200
@@ -162,7 +162,6 @@
 #endif
 
 #ifdef __BIG_ENDIAN
-#warning Compiling for big endian machine.
 #define BIG_ENDIAN TRUE
 #endif				/* __BIG_ENDIAN */
 
diff -ruN rt61-cvs-2007060307-old/Module/rtmp.h rt61-cvs-2007060307-new/Module/rtmp.h
--- rt61-cvs-2007060307-old/Module/rtmp.h	2007-05-19 19:19:17.000000000 +0200
+++ rt61-cvs-2007060307-new/Module/rtmp.h	2007-08-25 20:44:27.000000000 +0200
@@ -1617,14 +1617,8 @@
 VOID RTMPFreeDMAMemory(IN PRTMP_ADAPTER pAdapter);
 // Enable & Disable NIC interrupt via writing interrupt mask register
 // Since it use ADAPTER structure, it have to be put after structure definition.
-#ifdef BIG_ENDIAN
-inline
-#endif
- VOID NICDisableInterrupt(IN PRTMP_ADAPTER pAdapter);
-#ifdef BIG_ENDIAN
-inline
-#endif
- VOID NICEnableInterrupt(IN PRTMP_ADAPTER pAdapter);
+VOID NICDisableInterrupt(IN PRTMP_ADAPTER pAdapter);
+VOID NICEnableInterrupt(IN PRTMP_ADAPTER pAdapter);
 VOID NICInitTxRxRingAndBacklogQueue(IN PRTMP_ADAPTER pAdapter);
 VOID NICReadEEPROMParameters(IN PRTMP_ADAPTER pAd);
 VOID NICInitAsicFromEEPROM(IN PRTMP_ADAPTER pAd);
diff -ruN rt61-cvs-2007060307-old/Module/rtmp_init.c rt61-cvs-2007060307-new/Module/rtmp_init.c
--- rt61-cvs-2007060307-old/Module/rtmp_init.c	2007-05-23 14:14:23.000000000 +0200
+++ rt61-cvs-2007060307-new/Module/rtmp_init.c	2007-08-25 20:43:51.000000000 +0200
@@ -549,24 +549,14 @@
 
 // By removing 'inline' directive from the function definitions.
 // Then Driverloader is compiled and runs smooth after kernel 2.6.9
-#ifdef BIG_ENDIAN
-inline VOID
-#else
-VOID
-#endif
-NICDisableInterrupt(IN PRTMP_ADAPTER pAdapter)
+VOID NICDisableInterrupt(IN PRTMP_ADAPTER pAdapter)
 {
 	RTMP_IO_WRITE32(pAdapter, INT_MASK_CSR, 0xffffff7f);	// 0xffffff7f
 	RTMP_IO_WRITE32(pAdapter, MCU_INT_MASK_CSR, 0xffffffff);
 	RTMP_CLEAR_FLAG(pAdapter, fRTMP_ADAPTER_INTERRUPT_ACTIVE);
 }
 
-#ifdef BIG_ENDIAN
-inline VOID
-#else
-VOID
-#endif
-NICEnableInterrupt(IN PRTMP_ADAPTER pAdapter)
+VOID NICEnableInterrupt(IN PRTMP_ADAPTER pAdapter)
 {
 	//
 	// Flag "fOP_STATUS_DOZE" On, means ASIC put to sleep, else means ASIC WakeUp
