diff -Nru 1/acx_struct.h 2/acx_struct.h
--- 1/acx_struct.h	2007-10-03 23:42:39.000000000 +0800
+++ 2/acx_struct.h	2007-10-06 01:15:32.000000000 +0800
@@ -1425,7 +1425,13 @@
 
 	const u16	*io;		/* points to ACX100 or ACX111 PCI I/O register address set */
 
+#ifdef CONFIG_PCI
 	struct pci_dev	*pdev;
+#endif
+#ifdef CONFIG_VLYNQ
+	struct vlynq_device	*vdev;
+#endif
+	struct device *bus_dev;
 
 	unsigned long	membase;
 	unsigned long	membase2;
diff -Nru 1/pci.c 2/pci.c
--- 1/pci.c	2007-10-03 23:42:39.000000000 +0800
+++ 2/pci.c	2007-10-06 01:15:32.000000000 +0800
@@ -33,11 +33,15 @@
 #include <linux/ethtool.h>
 #include <linux/dma-mapping.h>
 #include <linux/workqueue.h>
+#ifdef CONFIG_VLYNQ
+#include <linux/vlynq.h>
+#endif
 
 #include "acx.h"
 
 /***********************************************************************
 */
+#ifdef CONFIG_PCI
 #define PCI_TYPE		(PCI_USES_MEM | PCI_ADDR0 | PCI_NO_ACPI_WAKE)
 #define PCI_ACX100_REGION1		0x01
 #define PCI_ACX100_REGION1_SIZE		0x1000	/* Memory size - 4K bytes */
@@ -74,7 +78,7 @@
 #define PCI_UNKNOWN	5
 #define PCI_POWER_ERROR	-1
 #endif
-
+#endif /* CONFIG_PCI */
 /***********************************************************************
 */
 
@@ -87,12 +91,6 @@
 static void acxpci_s_up(struct ieee80211_hw *hw);
 static void acxpci_s_down(struct ieee80211_hw *hw);
 
-void acxpci_put_devname(acx_device_t *adev, struct ethtool_drvinfo *info)
-{
-
-        strncpy(info->bus_info,pci_name(adev->pdev), ETHTOOL_BUSINFO_LEN);
-}
-
 /***********************************************************************
 ** Register access
 **
@@ -605,12 +603,12 @@
 	snprintf(filename, sizeof(filename), "tiacx1%02dc%02X",
 		 IS_ACX111(adev) * 11, adev->radio_type);
 
-	fw_image = acx_s_read_fw(&adev->pdev->dev, filename, &file_size);
+	fw_image = acx_s_read_fw(adev->bus_dev, filename, &file_size);
 	if (!fw_image) {
 		adev->need_radio_fw = 1;
 		filename[sizeof("tiacx1NN") - 1] = '\0';
 		fw_image =
-		    acx_s_read_fw(&adev->pdev->dev, filename, &file_size);
+		    acx_s_read_fw(adev->bus_dev, filename, &file_size);
 		if (!fw_image) {
 			FN_EXIT1(NOT_OK);
 			return NOT_OK;
@@ -670,7 +668,7 @@
 
 	snprintf(filename, sizeof(filename), "tiacx1%02dr%02X",
 		 IS_ACX111(adev) * 11, adev->radio_type);
-	radio_image = acx_s_read_fw(&adev->pdev->dev, filename, &size);
+	radio_image = acx_s_read_fw(adev->bus_dev, filename, &size);
 	if (!radio_image) {
 		printk("acx: can't load radio module '%s'\n", filename);
 		goto fail;
@@ -886,7 +884,9 @@
 
 	acx_lock(adev, flags);
 
+#ifdef CONFIG_PCI
 	acxpci_l_reset_mac(adev);
+#endif
 
 	ecpu_ctrl = read_reg16(adev, IO_ACX_ECPU_CTRL) & 1;
 	if (!ecpu_ctrl) {
@@ -1426,6 +1426,7 @@
 };
 
 
+#ifdef CONFIG_PCI
 static int __devinit
 acxpci_e_probe(struct pci_dev *pdev, const struct pci_device_id *id)
 {
@@ -1477,6 +1478,7 @@
 	/* acx_sem_lock(adev); */
 	adev->ieee = ieee;
 	adev->pdev = pdev;
+	adev->bus_dev = &pdev->dev;
 	adev->dev_type = DEVTYPE_PCI;
 
 /** Finished with private interface **/
@@ -1916,7 +1918,7 @@
 	return OK;
 }
 #endif /* CONFIG_PM */
-
+#endif /* CONFIG_PCI */
 
 /***********************************************************************
 ** acxpci_s_up
@@ -1998,7 +2000,7 @@
 	/* then wait until interrupts have finished executing on other CPUs */
 	acx_lock(adev, flags);
 	disable_acx_irq(adev);
-        synchronize_irq(adev->pdev->irq);
+        synchronize_irq(adev->irq);
 	acx_unlock(adev, flags);
 
 	/* we really don't want to have an asynchronous tasklet disturb us
@@ -3449,8 +3451,7 @@
 {
 	void *ptr;
 
-	ptr = dma_alloc_coherent(adev->pdev ? &adev->pdev->dev : NULL,
-				 size, phy, GFP_KERNEL);
+	ptr = dma_alloc_coherent(adev->bus_dev, size, phy, GFP_KERNEL);
 
 	if (ptr) {
 		log(L_DEBUG, "%s sz=%d adr=0x%p phy=0x%08llx\n",
@@ -4016,10 +4017,370 @@
 	return OK;
 }
 
+#ifdef CONFIG_VLYNQ
+struct vlynq_reg_config {
+	u32 offset;
+	u32 value;
+};
+
+struct vlynq_known {
+	u32 chip_id;
+	char name[32];
+	struct vlynq_mapping rx_mapping[4];
+	int irq;
+	int irq_type;
+	int num_regs;
+	struct vlynq_reg_config regs[10];
+};
+
+#define CHIP_TNETW1130 0x00000009
+#define CHIP_TNETW1350 0x00000029
+
+static struct vlynq_known known_devices[] = {
+	{
+		.chip_id = CHIP_TNETW1130, .name = "TI TNETW1130",
+		.rx_mapping = {
+			{ .size = 0x22000, .offset = 0xf0000000 },
+			{ .size = 0x40000, .offset = 0xc0000000 },
+			{ .size = 0x0, .offset = 0x0 },
+			{ .size = 0x0, .offset = 0x0 },
+		},
+		.irq = 0,
+		.irq_type = IRQ_TYPE_EDGE_RISING,
+		.num_regs = 5,
+		.regs = {
+			{
+				.offset = 0x790,
+				.value = (0xd0000000 - PHYS_OFFSET)
+			},
+			{
+				.offset = 0x794,
+				.value = (0xd0000000 - PHYS_OFFSET)
+			},
+			{ .offset = 0x740, .value = 0 },
+			{ .offset = 0x744, .value = 0x00010000 },
+			{ .offset = 0x764, .value = 0x00010000 },
+		},
+	},
+	{
+		.chip_id = CHIP_TNETW1350, .name = "TI TNETW1350",
+		.rx_mapping = {
+			{ .size = 0x100000, .offset = 0x00300000 },
+			{ .size = 0x80000, .offset = 0x00000000 },
+			{ .size = 0x0, .offset = 0x0 },
+			{ .size = 0x0, .offset = 0x0 },
+		},
+		.irq = 0,
+		.irq_type = IRQ_TYPE_EDGE_RISING,
+		.num_regs = 5,
+		.regs = {
+			{
+				.offset = 0x790,
+				.value = (0x60000000 - PHYS_OFFSET)
+			},
+			{
+				.offset = 0x794,
+				.value = (0x60000000 - PHYS_OFFSET)
+			},
+			{ .offset = 0x740, .value = 0 },
+			{ .offset = 0x744, .value = 0x00010000 },
+			{ .offset = 0x764, .value = 0x00010000 },
+		},
+	},
+};
+
+static struct vlynq_device_id acx_vlynq_id[] = {
+	{ CHIP_TNETW1130, vlynq_div_auto, 0 },
+	{ CHIP_TNETW1350, vlynq_div_auto, 1 },
+	{ 0, 0, 0 },
+};
+
+static __devinit int vlynq_probe(struct vlynq_device *vdev,
+				 struct vlynq_device_id *id)
+{
+	int result = -EIO, i;
+	u32 addr;
+	struct ieee80211_hw *ieee;
+	acx_device_t *adev = NULL;
+	acx111_ie_configoption_t co;
+	struct vlynq_mapping mapping[4] = { { 0, }, };
+	struct vlynq_known *match = NULL;
+
+	FN_ENTER;
+	result = vlynq_enable_device(vdev);
+	if (result)
+		return result;
+
+	match = &known_devices[id->driver_data];
+
+	if (!match) {
+		result = -ENODEV;
+		goto fail;
+	}
+
+	mapping[0].offset = ARCH_PFN_OFFSET << PAGE_SHIFT;
+	mapping[0].size = 0x02000000;
+	vlynq_set_local_mapping(vdev, vdev->mem_start, mapping);
+	vlynq_set_remote_mapping(vdev, 0, match->rx_mapping);
+
+	set_irq_type(vlynq_virq_to_irq(vdev, match->irq), match->irq_type);
+
+	addr = (u32)ioremap(vdev->mem_start, 0x1000);
+	if (!addr) {
+		printk(KERN_ERR "%s: failed to remap io memory\n",
+		       vdev->dev.bus_id);
+		result = -ENXIO;
+		goto fail;
+	}
+
+	for (i = 0; i < match->num_regs; i++)
+		iowrite32(match->regs[i].value,
+			  (u32 *)(addr + match->regs[i].offset));
+
+	iounmap((void *)addr);
+
+	ieee = ieee80211_alloc_hw(sizeof(struct acx_device), &acxpci_hw_ops);
+	if (!ieee) {
+		printk("acx: could not allocate ieee80211 structure %s\n",
+		       vdev->dev.bus_id);
+		goto fail_alloc_netdev;
+	}
+	ieee->flags &=	 (~IEEE80211_HW_RX_INCLUDES_FCS &
+			  ~IEEE80211_HW_MONITOR_DURING_OPER) |
+			 IEEE80211_HW_WEP_INCLUDE_IV;
+	ieee->queues = 1;
+
+	adev = ieee2adev(ieee);
+
+	memset(adev, 0, sizeof(*adev));
+	/** Set up our private interface **/
+	spin_lock_init(&adev->lock);	/* initial state: unlocked */
+	/* We do not start with downed sem: we want PARANOID_LOCKING to work */
+	mutex_init(&adev->mutex);
+	/* since nobody can see new netdev yet, we can as well
+	 ** just _presume_ that we're under sem (instead of actually taking it): */
+	/* acx_sem_lock(adev); */
+	adev->ieee = ieee;
+	adev->vdev = vdev;
+	adev->bus_dev = &vdev->dev;
+	adev->dev_type = DEVTYPE_PCI;
+
+/** Finished with private interface **/
+
+	vlynq_set_drvdata(vdev, ieee);
+	if (!request_mem_region(vdev->mem_start, vdev->mem_end - vdev->mem_start, "acx")) {
+		printk("acx: cannot reserve VLYNQ memory region\n");
+		goto fail_request_mem_region;
+	}
+	adev->iobase = ioremap(vdev->mem_start, vdev->mem_end - vdev->mem_start);
+	if (!adev->iobase) {
+		printk("acx: ioremap() FAILED\n");
+		goto fail_ioremap;
+	}
+	adev->iobase2 = adev->iobase + match->rx_mapping[0].size;
+	adev->chip_type = CHIPTYPE_ACX111;
+	adev->chip_name = match->name;
+	adev->io = IO_ACX111;
+	adev->irq = vlynq_virq_to_irq(vdev, match->irq);
+
+	printk("acx: found %s-based wireless network card at %s, irq:%d, "
+	       "phymem:0x%x, mem:0x%p\n",
+	       match->name, vdev->dev.bus_id, adev->irq,
+	       vdev->mem_start, adev->iobase);
+	log(L_ANY, "initial debug setting is 0x%04X\n", acx_debug);
+
+	if (0 == adev->irq) {
+		printk("acx: can't use IRQ 0\n");
+		goto fail_irq;
+	}
+	SET_IEEE80211_DEV(ieee, &vdev->dev);
+
+
+	/* to find crashes due to weird driver access
+	 * to unconfigured interface (ifup) */
+	adev->mgmt_timer.function = (void (*)(unsigned long))0x0000dead;
+
+
+	/* ok, pci setup is finished, now start initializing the card */
+
+	/* NB: read_reg() reads may return bogus data before reset_dev(),
+	 * since the firmware which directly controls large parts of the I/O
+	 * registers isn't initialized yet.
+	 * acx100 seems to be more affected than acx111 */
+	if (OK != acxpci_s_reset_dev(adev))
+		goto fail_reset;
+
+	if (OK != acx_s_init_mac(adev))
+		goto fail_init_mac;
+
+	acx_s_interrogate(adev, &co, ACX111_IE_CONFIG_OPTIONS);
+/* TODO: merge them into one function, they are called just once and are the same for pci & usb */
+	if (OK != acxpci_read_eeprom_byte(adev, 0x05, &adev->eeprom_version))
+		goto fail_read_eeprom_version;
+
+	acx_s_parse_configoption(adev, &co);
+	acx_s_set_defaults(adev);
+	acx_s_get_firmware_version(adev);	/* needs to be after acx_s_init_mac() */
+	acx_display_hardware_details(adev);
+
+	/* Register the card, AFTER everything else has been set up,
+	 * since otherwise an ioctl could step on our feet due to
+	 * firmware operations happening in parallel or uninitialized data */
+
+
+	acx_proc_register_entries(ieee);
+
+	/* Now we have our device, so make sure the kernel doesn't try
+	 * to send packets even though we're not associated to a network yet */
+
+	/* after register_netdev() userspace may start working with dev
+	 * (in particular, on other CPUs), we only need to up the sem */
+	/* acx_sem_unlock(adev); */
+
+	printk("acx " ACX_RELEASE ": net device %s, driver compiled "
+	       "against wireless extensions %d and Linux %s\n",
+	       wiphy_name(adev->ieee->wiphy), WIRELESS_EXT, UTS_RELEASE);
+
+	MAC_COPY(adev->ieee->wiphy->perm_addr, adev->dev_addr);
+
+	log(L_IRQ | L_INIT, "using IRQ %d\n", adev->irq);
+
+/** done with board specific setup **/
+
+	acx_init_task_scheduler(adev);
+	result = ieee80211_register_hw(adev->ieee);
+	if (OK != result) {
+		printk("acx: ieee80211_register_hw() FAILED: %d\n", result);
+		goto fail_register_netdev;
+	}
+#if CMD_DISCOVERY
+	great_inquisitor(adev);
+#endif
+
+	result = OK;
+	goto done;
+
+	/* error paths: undo everything in reverse order... */
+
+
+	acxpci_s_delete_dma_regions(adev);
+
+      fail_init_mac:
+      fail_read_eeprom_version:
+      fail_reset:
+
+      fail_alloc_netdev:
+      fail_irq:
+
+	iounmap(adev->iobase);
+      fail_ioremap:
+
+	release_mem_region(vdev->mem_start, vdev->mem_end - vdev->mem_start);
+      fail_request_mem_region:
+      fail_register_netdev:
+	ieee80211_free_hw(ieee);
+      fail:
+	vlynq_disable_device(vdev);
+      done:
+	FN_EXIT1(result);
+	return result;
+}
+
+static void vlynq_remove(struct vlynq_device *vdev)
+{
+	struct ieee80211_hw *hw = vlynq_get_drvdata(vdev);
+	acx_device_t *adev = ieee2adev(hw);
+	unsigned long flags;
+	FN_ENTER;
+
+	if (!hw) {
+		log(L_DEBUG, "%s: card is unused. Skipping any release code\n",
+		    __func__);
+		goto end;
+	}
+
+
+	acx_lock(adev, flags);
+	acx_unlock(adev, flags);
+	adev->initialized = 0;
+
+	/* If device wasn't hot unplugged... */
+	if (adev_present(adev)) {
+
+		acx_sem_lock(adev);
+
+		/* disable both Tx and Rx to shut radio down properly */
+		if (adev->initialized) {
+			acx_s_issue_cmd(adev, ACX1xx_CMD_DISABLE_TX, NULL, 0);
+			acx_s_issue_cmd(adev, ACX1xx_CMD_DISABLE_RX, NULL, 0);
+		}
+		acx_lock(adev, flags);
+		/* disable power LED to save power :-) */
+		log(L_INIT, "switching off power LED to save power\n");
+		acxpci_l_power_led(adev, 0);
+		/* stop our eCPU */
+		acx_unlock(adev, flags);
+
+		acx_sem_unlock(adev);
+	}
+
+	/* unregister the device to not let the kernel
+	 * (e.g. ioctls) access a half-deconfigured device
+	 * NB: this will cause acxpci_e_close() to be called,
+	 * thus we shouldn't call it under sem!
+	 * Well, netdev did, but ieee80211 stack does not, so we
+	 * have to do so manually...
+	 */
+	acxpci_e_close(hw);
+	log(L_INIT, "removing device %s\n", wiphy_name(adev->ieee->wiphy));
+	ieee80211_unregister_hw(adev->ieee);
+
+	/* unregister_netdev ensures that no references to us left.
+	 * For paranoid reasons we continue to follow the rules */
+	acx_sem_lock(adev);
+
+	if (adev->dev_state_mask & ACX_STATE_IFACE_UP) {
+		acxpci_s_down(hw);
+		CLEAR_BIT(adev->dev_state_mask, ACX_STATE_IFACE_UP);
+	}
+
+	acx_proc_unregister_entries(adev->ieee);
+
+	/* finally, clean up PCI bus state */
+	acxpci_s_delete_dma_regions(adev);
+	if (adev->iobase)
+		iounmap(adev->iobase);
+	if (adev->iobase2)
+		iounmap(adev->iobase2);
+	release_mem_region(vdev->mem_start, vdev->mem_end - vdev->mem_start);
+
+	/* remove dev registration */
+
+	acx_sem_unlock(adev);
+	vlynq_disable_device(vdev);
+
+	/* Free netdev (quite late,
+	 * since otherwise we might get caught off-guard
+	 * by a netdev timeout handler execution
+	 * expecting to see a working dev...) */
+	ieee80211_free_hw(adev->ieee);
+
+      end:
+	FN_EXIT0;
+}
+
+static struct vlynq_driver vlynq_acx = {
+	.name = "acx_vlynq",
+	.id_table = acx_vlynq_id,
+	.probe = vlynq_probe,
+	.remove = __devexit_p(vlynq_remove),
+};
+#endif
 
 /***********************************************************************
 ** Data for init_module/cleanup_module
 */
+#ifdef CONFIG_PCI
 static const struct pci_device_id acxpci_id_tbl[] __devinitdata = {
 	{
 	 .vendor = PCI_VENDOR_ID_TI,
@@ -4071,7 +4432,7 @@
 	.resume = acxpci_e_resume
 #endif /* CONFIG_PM */
 };
-
+#endif /* CONFIG_PCI */
 
 /***********************************************************************
 ** acxpci_e_init_module
@@ -4080,7 +4441,7 @@
 */
 int __init acxpci_e_init_module(void)
 {
-	int res;
+	int res = 0;
 
 	FN_ENTER;
 
@@ -4100,10 +4461,15 @@
 #endif
 	log(L_INIT,
 	    "acx: " ENDIANNESS_STRING
-	    "acx: PCI module " ACX_RELEASE " initialized, "
+	    "acx: PCI/VLYNQ module " ACX_RELEASE " initialized, "
 	    "waiting for cards to probe...\n");
 
+#ifdef CONFIG_PCI
 	res = pci_register_driver(&acxpci_drv_id);
+#endif
+#ifdef CONFIG_VLYNQ
+	res = vlynq_register_driver(&vlynq_acx);
+#endif
 	FN_EXIT1(res);
 	return res;
 }
@@ -4119,7 +4485,12 @@
 {
 	FN_ENTER;
 
+#ifdef CONFIG_VLYNQ
+	vlynq_unregister_driver(&vlynq_acx);
+#endif
+#ifdef CONFIG_PCI
 	pci_unregister_driver(&acxpci_drv_id);
+#endif
 
 	FN_EXIT0;
 }
