From 68690045f8e220826517c0d6f9388ffc1faa57ea Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Alexis=20Lothor=C3=A9?= <alexis.lothore@bootlin.com>
Date: Mon, 29 May 2023 10:02:45 +0200
Subject: [PATCH 897/898] net: dsa: mv88e6xxx: pass mv88e6xxx_chip structure to
 port_max_speed_mode
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Some switches families have minor differences on supported link speed for
ports. Instead of redefining a new port_max_speed_mode for each different
configuration, allow to pass mv88e6xxx_chip structure to allow
differentiating those chips by known chip id

Signed-off-by: Alexis Lothoré <alexis.lothore@bootlin.com>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
Update one more instance of port_max_speed_mode that 5.15 has.
[Robert Marko]
Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 drivers/net/dsa/mv88e6xxx/chip.c |  2 +-
 drivers/net/dsa/mv88e6xxx/chip.h |  3 ++-
 drivers/net/dsa/mv88e6xxx/port.c | 12 ++++++++----
 drivers/net/dsa/mv88e6xxx/port.h | 12 ++++++++----
 4 files changed, 19 insertions(+), 10 deletions(-)

--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -443,7 +443,7 @@ static int mv88e6xxx_port_setup_mac(stru
 	}
 
 	if (speed == SPEED_MAX && chip->info->ops->port_max_speed_mode)
-		mode = chip->info->ops->port_max_speed_mode(port);
+		mode = chip->info->ops->port_max_speed_mode(chip, port);
 
 	if (chip->info->ops->port_set_pause) {
 		err = chip->info->ops->port_set_pause(chip, port, pause);
--- a/drivers/net/dsa/mv88e6xxx/chip.h
+++ b/drivers/net/dsa/mv88e6xxx/chip.h
@@ -485,7 +485,8 @@ struct mv88e6xxx_ops {
 				     int speed, int duplex);
 
 	/* What interface mode should be used for maximum speed? */
-	phy_interface_t (*port_max_speed_mode)(int port);
+	phy_interface_t (*port_max_speed_mode)(struct mv88e6xxx_chip *chip,
+					       int port);
 
 	int (*port_tag_remap)(struct mv88e6xxx_chip *chip, int port);
 
--- a/drivers/net/dsa/mv88e6xxx/port.c
+++ b/drivers/net/dsa/mv88e6xxx/port.c
@@ -357,7 +357,8 @@ int mv88e6341_port_set_speed_duplex(stru
 					       duplex);
 }
 
-phy_interface_t mv88e6341_port_max_speed_mode(int port)
+phy_interface_t mv88e6341_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					      int port)
 {
 	if (port == 5)
 		return PHY_INTERFACE_MODE_2500BASEX;
@@ -402,7 +403,8 @@ int mv88e6390_port_set_speed_duplex(stru
 					       duplex);
 }
 
-phy_interface_t mv88e6390_port_max_speed_mode(int port)
+phy_interface_t mv88e6390_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					      int port)
 {
 	if (port == 9 || port == 10)
 		return PHY_INTERFACE_MODE_2500BASEX;
@@ -427,7 +429,8 @@ int mv88e6390x_port_set_speed_duplex(str
 					       duplex);
 }
 
-phy_interface_t mv88e6390x_port_max_speed_mode(int port)
+phy_interface_t mv88e6390x_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					       int port)
 {
 	if (port == 9 || port == 10)
 		return PHY_INTERFACE_MODE_XAUI;
@@ -527,7 +530,8 @@ int mv88e6393x_port_set_speed_duplex(str
 	return 0;
 }
 
-phy_interface_t mv88e6393x_port_max_speed_mode(int port)
+phy_interface_t mv88e6393x_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					       int port)
 {
 	if (port == 0 || port == 9 || port == 10)
 		return PHY_INTERFACE_MODE_10GBASER;
--- a/drivers/net/dsa/mv88e6xxx/port.h
+++ b/drivers/net/dsa/mv88e6xxx/port.h
@@ -350,10 +350,14 @@ int mv88e6390x_port_set_speed_duplex(str
 int mv88e6393x_port_set_speed_duplex(struct mv88e6xxx_chip *chip, int port,
 				     int speed, int duplex);
 
-phy_interface_t mv88e6341_port_max_speed_mode(int port);
-phy_interface_t mv88e6390_port_max_speed_mode(int port);
-phy_interface_t mv88e6390x_port_max_speed_mode(int port);
-phy_interface_t mv88e6393x_port_max_speed_mode(int port);
+phy_interface_t mv88e6341_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					      int port);
+phy_interface_t mv88e6390_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					      int port);
+phy_interface_t mv88e6390x_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					       int port);
+phy_interface_t mv88e6393x_port_max_speed_mode(struct mv88e6xxx_chip *chip,
+					       int port);
 
 int mv88e6xxx_port_set_state(struct mv88e6xxx_chip *chip, int port, u8 state);
 
