From bfaa98808955e8f1984a1fee7bdc31add1ea72a7 Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Mon, 24 Oct 2022 13:57:23 +0100
Subject: [PATCH] media: bcm2835-unicam: Fix up start/stop api change

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -2524,7 +2524,7 @@ static int unicam_start_streaming(struct
 		goto err_streaming;
 	}
 
-	ret = media_pipeline_start(&node->video_dev.entity, &node->pipe);
+	ret = media_pipeline_start(node->video_dev.entity.pads, &node->pipe);
 	if (ret < 0) {
 		unicam_err(dev, "Failed to start media pipeline: %d\n", ret);
 		goto err_pm_put;
@@ -2618,7 +2618,7 @@ err_vpu_clock:
 		unicam_err(dev, "failed to reset the VPU clock\n");
 	clk_disable_unprepare(dev->vpu_clock);
 error_pipeline:
-	media_pipeline_stop(&node->video_dev.entity);
+	media_pipeline_stop(node->video_dev.entity.pads);
 err_pm_put:
 	unicam_runtime_put(dev);
 err_streaming:
@@ -2646,7 +2646,7 @@ static void unicam_stop_streaming(struct
 
 		unicam_disable(dev);
 
-		media_pipeline_stop(&node->video_dev.entity);
+		media_pipeline_stop(node->video_dev.entity.pads);
 
 		if (dev->clocks_enabled) {
 			if (clk_set_min_rate(dev->vpu_clock, 0))
