From f463515fa1c3d34eeff708d3c015d357049b4df1 Mon Sep 17 00:00:00 2001
From: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Date: Mon, 16 Jan 2023 15:44:52 +0100
Subject: [PATCH] media: i2c: imx290: Configure data lanes at start
 time

Upstream commit 7d399658f7c6

There's no need to configure the data lanes in the runtime PM resume
handler. Do so in imx290_start_streaming() instead.

Signed-off-by: Laurent Pinchart <laurent.pinchart@ideasonboard.com>
Reviewed-by: Alexander Stein <alexander.stein@ew.tq-group.com>
Signed-off-by: Sakari Ailus <sakari.ailus@linux.intel.com>
Signed-off-by: Mauro Carvalho Chehab <mchehab@kernel.org>
---
 drivers/media/i2c/imx290.c | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/drivers/media/i2c/imx290.c
+++ b/drivers/media/i2c/imx290.c
@@ -762,6 +762,9 @@ static int imx290_start_streaming(struct
 		return ret;
 	}
 
+	/* Set data lane count */
+	imx290_set_data_lanes(imx290);
+
 	/* Apply the register values related to current frame format */
 	format = v4l2_subdev_get_pad_format(&imx290->sd, state, 0);
 	ret = imx290_setup_format(imx290, format);
@@ -1069,9 +1072,6 @@ static int imx290_power_on(struct imx290
 	gpiod_set_value_cansleep(imx290->rst_gpio, 0);
 	usleep_range(30000, 31000);
 
-	/* Set data lane count */
-	imx290_set_data_lanes(imx290);
-
 	return 0;
 }
 
