From 674fa25b207e4bef6c27af2acfbca3a0d765a45b Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <kernel@esmil.dk>
Date: Sat, 1 Apr 2023 19:19:18 +0800
Subject: [PATCH 006/122] clk: starfive: Rename "jh7100" to "jh71x0" for the
 common code

Rename some variables from "jh7100" or "JH7100" to "jh71x0"
or "JH71X0".

Tested-by: Tommaso Merciai <tomm.merciai@gmail.com>
Reviewed-by: Conor Dooley <conor.dooley@microchip.com>
Reviewed-by: Emil Renner Berthing <emil.renner.berthing@canonical.com>
Signed-off-by: Emil Renner Berthing <kernel@esmil.dk>
Signed-off-by: Hal Feng <hal.feng@starfivetech.com>
Signed-off-by: Conor Dooley <conor.dooley@microchip.com>
---
 .../clk/starfive/clk-starfive-jh7100-audio.c  |  72 ++--
 drivers/clk/starfive/clk-starfive-jh7100.c    | 389 +++++++++---------
 drivers/clk/starfive/clk-starfive-jh71x0.c    | 282 ++++++-------
 drivers/clk/starfive/clk-starfive-jh71x0.h    |  81 ++--
 4 files changed, 418 insertions(+), 406 deletions(-)

--- a/drivers/clk/starfive/clk-starfive-jh7100-audio.c
+++ b/drivers/clk/starfive/clk-starfive-jh7100-audio.c
@@ -28,66 +28,66 @@
 #define JH7100_AUDCLK_I2SDAC_LRCLK_IOPAD	(JH7100_AUDCLK_END + 6)
 #define JH7100_AUDCLK_VAD_INTMEM                (JH7100_AUDCLK_END + 7)
 
-static const struct jh7100_clk_data jh7100_audclk_data[] = {
-	JH7100__GMD(JH7100_AUDCLK_ADC_MCLK, "adc_mclk", 0, 15, 2,
+static const struct jh71x0_clk_data jh7100_audclk_data[] = {
+	JH71X0__GMD(JH7100_AUDCLK_ADC_MCLK, "adc_mclk", 0, 15, 2,
 		    JH7100_AUDCLK_AUDIO_SRC,
 		    JH7100_AUDCLK_AUDIO_12288),
-	JH7100__GMD(JH7100_AUDCLK_I2S1_MCLK, "i2s1_mclk", 0, 15, 2,
+	JH71X0__GMD(JH7100_AUDCLK_I2S1_MCLK, "i2s1_mclk", 0, 15, 2,
 		    JH7100_AUDCLK_AUDIO_SRC,
 		    JH7100_AUDCLK_AUDIO_12288),
-	JH7100_GATE(JH7100_AUDCLK_I2SADC_APB, "i2sadc_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100_MDIV(JH7100_AUDCLK_I2SADC_BCLK, "i2sadc_bclk", 31, 2,
+	JH71X0_GATE(JH7100_AUDCLK_I2SADC_APB, "i2sadc_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0_MDIV(JH7100_AUDCLK_I2SADC_BCLK, "i2sadc_bclk", 31, 2,
 		    JH7100_AUDCLK_ADC_MCLK,
 		    JH7100_AUDCLK_I2SADC_BCLK_IOPAD),
-	JH7100__INV(JH7100_AUDCLK_I2SADC_BCLK_N, "i2sadc_bclk_n", JH7100_AUDCLK_I2SADC_BCLK),
-	JH7100_MDIV(JH7100_AUDCLK_I2SADC_LRCLK, "i2sadc_lrclk", 63, 3,
+	JH71X0__INV(JH7100_AUDCLK_I2SADC_BCLK_N, "i2sadc_bclk_n", JH7100_AUDCLK_I2SADC_BCLK),
+	JH71X0_MDIV(JH7100_AUDCLK_I2SADC_LRCLK, "i2sadc_lrclk", 63, 3,
 		    JH7100_AUDCLK_I2SADC_BCLK_N,
 		    JH7100_AUDCLK_I2SADC_LRCLK_IOPAD,
 		    JH7100_AUDCLK_I2SADC_BCLK),
-	JH7100_GATE(JH7100_AUDCLK_PDM_APB, "pdm_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100__GMD(JH7100_AUDCLK_PDM_MCLK, "pdm_mclk", 0, 15, 2,
+	JH71X0_GATE(JH7100_AUDCLK_PDM_APB, "pdm_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0__GMD(JH7100_AUDCLK_PDM_MCLK, "pdm_mclk", 0, 15, 2,
 		    JH7100_AUDCLK_AUDIO_SRC,
 		    JH7100_AUDCLK_AUDIO_12288),
-	JH7100_GATE(JH7100_AUDCLK_I2SVAD_APB, "i2svad_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100__GMD(JH7100_AUDCLK_SPDIF, "spdif", 0, 15, 2,
+	JH71X0_GATE(JH7100_AUDCLK_I2SVAD_APB, "i2svad_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0__GMD(JH7100_AUDCLK_SPDIF, "spdif", 0, 15, 2,
 		    JH7100_AUDCLK_AUDIO_SRC,
 		    JH7100_AUDCLK_AUDIO_12288),
-	JH7100_GATE(JH7100_AUDCLK_SPDIF_APB, "spdif_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100_GATE(JH7100_AUDCLK_PWMDAC_APB, "pwmdac_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100__GMD(JH7100_AUDCLK_DAC_MCLK, "dac_mclk", 0, 15, 2,
+	JH71X0_GATE(JH7100_AUDCLK_SPDIF_APB, "spdif_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0_GATE(JH7100_AUDCLK_PWMDAC_APB, "pwmdac_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0__GMD(JH7100_AUDCLK_DAC_MCLK, "dac_mclk", 0, 15, 2,
 		    JH7100_AUDCLK_AUDIO_SRC,
 		    JH7100_AUDCLK_AUDIO_12288),
-	JH7100_GATE(JH7100_AUDCLK_I2SDAC_APB, "i2sdac_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100_MDIV(JH7100_AUDCLK_I2SDAC_BCLK, "i2sdac_bclk", 31, 2,
+	JH71X0_GATE(JH7100_AUDCLK_I2SDAC_APB, "i2sdac_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0_MDIV(JH7100_AUDCLK_I2SDAC_BCLK, "i2sdac_bclk", 31, 2,
 		    JH7100_AUDCLK_DAC_MCLK,
 		    JH7100_AUDCLK_I2SDAC_BCLK_IOPAD),
-	JH7100__INV(JH7100_AUDCLK_I2SDAC_BCLK_N, "i2sdac_bclk_n", JH7100_AUDCLK_I2SDAC_BCLK),
-	JH7100_MDIV(JH7100_AUDCLK_I2SDAC_LRCLK, "i2sdac_lrclk", 31, 2,
+	JH71X0__INV(JH7100_AUDCLK_I2SDAC_BCLK_N, "i2sdac_bclk_n", JH7100_AUDCLK_I2SDAC_BCLK),
+	JH71X0_MDIV(JH7100_AUDCLK_I2SDAC_LRCLK, "i2sdac_lrclk", 31, 2,
 		    JH7100_AUDCLK_I2S1_MCLK,
 		    JH7100_AUDCLK_I2SDAC_BCLK_IOPAD),
-	JH7100_GATE(JH7100_AUDCLK_I2S1_APB, "i2s1_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100_MDIV(JH7100_AUDCLK_I2S1_BCLK, "i2s1_bclk", 31, 2,
+	JH71X0_GATE(JH7100_AUDCLK_I2S1_APB, "i2s1_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0_MDIV(JH7100_AUDCLK_I2S1_BCLK, "i2s1_bclk", 31, 2,
 		    JH7100_AUDCLK_I2S1_MCLK,
 		    JH7100_AUDCLK_I2SDAC_BCLK_IOPAD),
-	JH7100__INV(JH7100_AUDCLK_I2S1_BCLK_N, "i2s1_bclk_n", JH7100_AUDCLK_I2S1_BCLK),
-	JH7100_MDIV(JH7100_AUDCLK_I2S1_LRCLK, "i2s1_lrclk", 63, 3,
+	JH71X0__INV(JH7100_AUDCLK_I2S1_BCLK_N, "i2s1_bclk_n", JH7100_AUDCLK_I2S1_BCLK),
+	JH71X0_MDIV(JH7100_AUDCLK_I2S1_LRCLK, "i2s1_lrclk", 63, 3,
 		    JH7100_AUDCLK_I2S1_BCLK_N,
 		    JH7100_AUDCLK_I2SDAC_LRCLK_IOPAD),
-	JH7100_GATE(JH7100_AUDCLK_I2SDAC16K_APB, "i2s1dac16k_apb", 0, JH7100_AUDCLK_APB0_BUS),
-	JH7100__DIV(JH7100_AUDCLK_APB0_BUS, "apb0_bus", 8, JH7100_AUDCLK_DOM7AHB_BUS),
-	JH7100_GATE(JH7100_AUDCLK_DMA1P_AHB, "dma1p_ahb", 0, JH7100_AUDCLK_DOM7AHB_BUS),
-	JH7100_GATE(JH7100_AUDCLK_USB_APB, "usb_apb", CLK_IGNORE_UNUSED, JH7100_AUDCLK_APB_EN),
-	JH7100_GDIV(JH7100_AUDCLK_USB_LPM, "usb_lpm", CLK_IGNORE_UNUSED, 4, JH7100_AUDCLK_USB_APB),
-	JH7100_GDIV(JH7100_AUDCLK_USB_STB, "usb_stb", CLK_IGNORE_UNUSED, 3, JH7100_AUDCLK_USB_APB),
-	JH7100__DIV(JH7100_AUDCLK_APB_EN, "apb_en", 8, JH7100_AUDCLK_DOM7AHB_BUS),
-	JH7100__MUX(JH7100_AUDCLK_VAD_MEM, "vad_mem", 2,
+	JH71X0_GATE(JH7100_AUDCLK_I2SDAC16K_APB, "i2s1dac16k_apb", 0, JH7100_AUDCLK_APB0_BUS),
+	JH71X0__DIV(JH7100_AUDCLK_APB0_BUS, "apb0_bus", 8, JH7100_AUDCLK_DOM7AHB_BUS),
+	JH71X0_GATE(JH7100_AUDCLK_DMA1P_AHB, "dma1p_ahb", 0, JH7100_AUDCLK_DOM7AHB_BUS),
+	JH71X0_GATE(JH7100_AUDCLK_USB_APB, "usb_apb", CLK_IGNORE_UNUSED, JH7100_AUDCLK_APB_EN),
+	JH71X0_GDIV(JH7100_AUDCLK_USB_LPM, "usb_lpm", CLK_IGNORE_UNUSED, 4, JH7100_AUDCLK_USB_APB),
+	JH71X0_GDIV(JH7100_AUDCLK_USB_STB, "usb_stb", CLK_IGNORE_UNUSED, 3, JH7100_AUDCLK_USB_APB),
+	JH71X0__DIV(JH7100_AUDCLK_APB_EN, "apb_en", 8, JH7100_AUDCLK_DOM7AHB_BUS),
+	JH71X0__MUX(JH7100_AUDCLK_VAD_MEM, "vad_mem", 2,
 		    JH7100_AUDCLK_VAD_INTMEM,
 		    JH7100_AUDCLK_AUDIO_12288),
 };
 
 static struct clk_hw *jh7100_audclk_get(struct of_phandle_args *clkspec, void *data)
 {
-	struct jh7100_clk_priv *priv = data;
+	struct jh71x0_clk_priv *priv = data;
 	unsigned int idx = clkspec->args[0];
 
 	if (idx < JH7100_AUDCLK_END)
@@ -98,7 +98,7 @@ static struct clk_hw *jh7100_audclk_get(
 
 static int jh7100_audclk_probe(struct platform_device *pdev)
 {
-	struct jh7100_clk_priv *priv;
+	struct jh71x0_clk_priv *priv;
 	unsigned int idx;
 	int ret;
 
@@ -117,12 +117,12 @@ static int jh7100_audclk_probe(struct pl
 		struct clk_parent_data parents[4] = {};
 		struct clk_init_data init = {
 			.name = jh7100_audclk_data[idx].name,
-			.ops = starfive_jh7100_clk_ops(max),
+			.ops = starfive_jh71x0_clk_ops(max),
 			.parent_data = parents,
-			.num_parents = ((max & JH7100_CLK_MUX_MASK) >> JH7100_CLK_MUX_SHIFT) + 1,
+			.num_parents = ((max & JH71X0_CLK_MUX_MASK) >> JH71X0_CLK_MUX_SHIFT) + 1,
 			.flags = jh7100_audclk_data[idx].flags,
 		};
-		struct jh7100_clk *clk = &priv->reg[idx];
+		struct jh71x0_clk *clk = &priv->reg[idx];
 		unsigned int i;
 
 		for (i = 0; i < init.num_parents; i++) {
@@ -140,7 +140,7 @@ static int jh7100_audclk_probe(struct pl
 
 		clk->hw.init = &init;
 		clk->idx = idx;
-		clk->max_div = max & JH7100_CLK_DIV_MASK;
+		clk->max_div = max & JH71X0_CLK_DIV_MASK;
 
 		ret = devm_clk_hw_register(priv->dev, &clk->hw);
 		if (ret)
--- a/drivers/clk/starfive/clk-starfive-jh7100.c
+++ b/drivers/clk/starfive/clk-starfive-jh7100.c
@@ -23,250 +23,253 @@
 #define JH7100_CLK_GMAC_RMII_REF	(JH7100_CLK_END + 2)
 #define JH7100_CLK_GMAC_GR_MII_RX	(JH7100_CLK_END + 3)
 
-static const struct jh7100_clk_data jh7100_clk_data[] __initconst = {
-	JH7100__MUX(JH7100_CLK_CPUNDBUS_ROOT, "cpundbus_root", 4,
+static const struct jh71x0_clk_data jh7100_clk_data[] __initconst = {
+	JH71X0__MUX(JH7100_CLK_CPUNDBUS_ROOT, "cpundbus_root", 4,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL1_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_DLA_ROOT, "dla_root", 3,
+	JH71X0__MUX(JH7100_CLK_DLA_ROOT, "dla_root", 3,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL1_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_DSP_ROOT, "dsp_root", 4,
+	JH71X0__MUX(JH7100_CLK_DSP_ROOT, "dsp_root", 4,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL1_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_GMACUSB_ROOT, "gmacusb_root", 3,
+	JH71X0__MUX(JH7100_CLK_GMACUSB_ROOT, "gmacusb_root", 3,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_PERH0_ROOT, "perh0_root", 2,
+	JH71X0__MUX(JH7100_CLK_PERH0_ROOT, "perh0_root", 2,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL0_OUT),
-	JH7100__MUX(JH7100_CLK_PERH1_ROOT, "perh1_root", 2,
+	JH71X0__MUX(JH7100_CLK_PERH1_ROOT, "perh1_root", 2,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_VIN_ROOT, "vin_root", 3,
+	JH71X0__MUX(JH7100_CLK_VIN_ROOT, "vin_root", 3,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL1_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_VOUT_ROOT, "vout_root", 3,
+	JH71X0__MUX(JH7100_CLK_VOUT_ROOT, "vout_root", 3,
 		    JH7100_CLK_OSC_AUD,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100_GDIV(JH7100_CLK_AUDIO_ROOT, "audio_root", 0, 8, JH7100_CLK_PLL0_OUT),
-	JH7100__MUX(JH7100_CLK_CDECHIFI4_ROOT, "cdechifi4_root", 3,
+	JH71X0_GDIV(JH7100_CLK_AUDIO_ROOT, "audio_root", 0, 8, JH7100_CLK_PLL0_OUT),
+	JH71X0__MUX(JH7100_CLK_CDECHIFI4_ROOT, "cdechifi4_root", 3,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL1_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__MUX(JH7100_CLK_CDEC_ROOT, "cdec_root", 3,
+	JH71X0__MUX(JH7100_CLK_CDEC_ROOT, "cdec_root", 3,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL1_OUT),
-	JH7100__MUX(JH7100_CLK_VOUTBUS_ROOT, "voutbus_root", 3,
+	JH71X0__MUX(JH7100_CLK_VOUTBUS_ROOT, "voutbus_root", 3,
 		    JH7100_CLK_OSC_AUD,
 		    JH7100_CLK_PLL0_OUT,
 		    JH7100_CLK_PLL2_OUT),
-	JH7100__DIV(JH7100_CLK_CPUNBUS_ROOT_DIV, "cpunbus_root_div", 2, JH7100_CLK_CPUNDBUS_ROOT),
-	JH7100__DIV(JH7100_CLK_DSP_ROOT_DIV, "dsp_root_div", 4, JH7100_CLK_DSP_ROOT),
-	JH7100__DIV(JH7100_CLK_PERH0_SRC, "perh0_src", 4, JH7100_CLK_PERH0_ROOT),
-	JH7100__DIV(JH7100_CLK_PERH1_SRC, "perh1_src", 4, JH7100_CLK_PERH1_ROOT),
-	JH7100_GDIV(JH7100_CLK_PLL0_TESTOUT, "pll0_testout", 0, 31, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_PLL1_TESTOUT, "pll1_testout", 0, 31, JH7100_CLK_DLA_ROOT),
-	JH7100_GDIV(JH7100_CLK_PLL2_TESTOUT, "pll2_testout", 0, 31, JH7100_CLK_PERH1_SRC),
-	JH7100__MUX(JH7100_CLK_PLL2_REF, "pll2_refclk", 2,
+	JH71X0__DIV(JH7100_CLK_CPUNBUS_ROOT_DIV, "cpunbus_root_div", 2, JH7100_CLK_CPUNDBUS_ROOT),
+	JH71X0__DIV(JH7100_CLK_DSP_ROOT_DIV, "dsp_root_div", 4, JH7100_CLK_DSP_ROOT),
+	JH71X0__DIV(JH7100_CLK_PERH0_SRC, "perh0_src", 4, JH7100_CLK_PERH0_ROOT),
+	JH71X0__DIV(JH7100_CLK_PERH1_SRC, "perh1_src", 4, JH7100_CLK_PERH1_ROOT),
+	JH71X0_GDIV(JH7100_CLK_PLL0_TESTOUT, "pll0_testout", 0, 31, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_PLL1_TESTOUT, "pll1_testout", 0, 31, JH7100_CLK_DLA_ROOT),
+	JH71X0_GDIV(JH7100_CLK_PLL2_TESTOUT, "pll2_testout", 0, 31, JH7100_CLK_PERH1_SRC),
+	JH71X0__MUX(JH7100_CLK_PLL2_REF, "pll2_refclk", 2,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_OSC_AUD),
-	JH7100__DIV(JH7100_CLK_CPU_CORE, "cpu_core", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100__DIV(JH7100_CLK_CPU_AXI, "cpu_axi", 8, JH7100_CLK_CPU_CORE),
-	JH7100__DIV(JH7100_CLK_AHB_BUS, "ahb_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100__DIV(JH7100_CLK_APB1_BUS, "apb1_bus", 8, JH7100_CLK_AHB_BUS),
-	JH7100__DIV(JH7100_CLK_APB2_BUS, "apb2_bus", 8, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_DOM3AHB_BUS, "dom3ahb_bus", CLK_IS_CRITICAL, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_DOM7AHB_BUS, "dom7ahb_bus", CLK_IS_CRITICAL, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_U74_CORE0, "u74_core0", CLK_IS_CRITICAL, JH7100_CLK_CPU_CORE),
-	JH7100_GDIV(JH7100_CLK_U74_CORE1, "u74_core1", CLK_IS_CRITICAL, 8, JH7100_CLK_CPU_CORE),
-	JH7100_GATE(JH7100_CLK_U74_AXI, "u74_axi", CLK_IS_CRITICAL, JH7100_CLK_CPU_AXI),
-	JH7100_GATE(JH7100_CLK_U74RTC_TOGGLE, "u74rtc_toggle", CLK_IS_CRITICAL, JH7100_CLK_OSC_SYS),
-	JH7100_GATE(JH7100_CLK_SGDMA2P_AXI, "sgdma2p_axi", 0, JH7100_CLK_CPU_AXI),
-	JH7100_GATE(JH7100_CLK_DMA2PNOC_AXI, "dma2pnoc_axi", 0, JH7100_CLK_CPU_AXI),
-	JH7100_GATE(JH7100_CLK_SGDMA2P_AHB, "sgdma2p_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100__DIV(JH7100_CLK_DLA_BUS, "dla_bus", 4, JH7100_CLK_DLA_ROOT),
-	JH7100_GATE(JH7100_CLK_DLA_AXI, "dla_axi", 0, JH7100_CLK_DLA_BUS),
-	JH7100_GATE(JH7100_CLK_DLANOC_AXI, "dlanoc_axi", 0, JH7100_CLK_DLA_BUS),
-	JH7100_GATE(JH7100_CLK_DLA_APB, "dla_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_VP6_CORE, "vp6_core", 0, 4, JH7100_CLK_DSP_ROOT_DIV),
-	JH7100__DIV(JH7100_CLK_VP6BUS_SRC, "vp6bus_src", 4, JH7100_CLK_DSP_ROOT),
-	JH7100_GDIV(JH7100_CLK_VP6_AXI, "vp6_axi", 0, 4, JH7100_CLK_VP6BUS_SRC),
-	JH7100__DIV(JH7100_CLK_VCDECBUS_SRC, "vcdecbus_src", 4, JH7100_CLK_CDECHIFI4_ROOT),
-	JH7100__DIV(JH7100_CLK_VDEC_BUS, "vdec_bus", 8, JH7100_CLK_VCDECBUS_SRC),
-	JH7100_GATE(JH7100_CLK_VDEC_AXI, "vdec_axi", 0, JH7100_CLK_VDEC_BUS),
-	JH7100_GATE(JH7100_CLK_VDECBRG_MAIN, "vdecbrg_mainclk", 0, JH7100_CLK_VDEC_BUS),
-	JH7100_GDIV(JH7100_CLK_VDEC_BCLK, "vdec_bclk", 0, 8, JH7100_CLK_VCDECBUS_SRC),
-	JH7100_GDIV(JH7100_CLK_VDEC_CCLK, "vdec_cclk", 0, 8, JH7100_CLK_CDEC_ROOT),
-	JH7100_GATE(JH7100_CLK_VDEC_APB, "vdec_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_JPEG_AXI, "jpeg_axi", 0, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100_GDIV(JH7100_CLK_JPEG_CCLK, "jpeg_cclk", 0, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100_GATE(JH7100_CLK_JPEG_APB, "jpeg_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_GC300_2X, "gc300_2x", 0, 8, JH7100_CLK_CDECHIFI4_ROOT),
-	JH7100_GATE(JH7100_CLK_GC300_AHB, "gc300_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100__DIV(JH7100_CLK_JPCGC300_AXIBUS, "jpcgc300_axibus", 8, JH7100_CLK_VCDECBUS_SRC),
-	JH7100_GATE(JH7100_CLK_GC300_AXI, "gc300_axi", 0, JH7100_CLK_JPCGC300_AXIBUS),
-	JH7100_GATE(JH7100_CLK_JPCGC300_MAIN, "jpcgc300_mainclk", 0, JH7100_CLK_JPCGC300_AXIBUS),
-	JH7100__DIV(JH7100_CLK_VENC_BUS, "venc_bus", 8, JH7100_CLK_VCDECBUS_SRC),
-	JH7100_GATE(JH7100_CLK_VENC_AXI, "venc_axi", 0, JH7100_CLK_VENC_BUS),
-	JH7100_GATE(JH7100_CLK_VENCBRG_MAIN, "vencbrg_mainclk", 0, JH7100_CLK_VENC_BUS),
-	JH7100_GDIV(JH7100_CLK_VENC_BCLK, "venc_bclk", 0, 8, JH7100_CLK_VCDECBUS_SRC),
-	JH7100_GDIV(JH7100_CLK_VENC_CCLK, "venc_cclk", 0, 8, JH7100_CLK_CDEC_ROOT),
-	JH7100_GATE(JH7100_CLK_VENC_APB, "venc_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_DDRPLL_DIV2, "ddrpll_div2", CLK_IS_CRITICAL, 2, JH7100_CLK_PLL1_OUT),
-	JH7100_GDIV(JH7100_CLK_DDRPLL_DIV4, "ddrpll_div4", CLK_IS_CRITICAL, 2, JH7100_CLK_DDRPLL_DIV2),
-	JH7100_GDIV(JH7100_CLK_DDRPLL_DIV8, "ddrpll_div8", CLK_IS_CRITICAL, 2, JH7100_CLK_DDRPLL_DIV4),
-	JH7100_GDIV(JH7100_CLK_DDROSC_DIV2, "ddrosc_div2", CLK_IS_CRITICAL, 2, JH7100_CLK_OSC_SYS),
-	JH7100_GMUX(JH7100_CLK_DDRC0, "ddrc0", CLK_IS_CRITICAL, 4,
+	JH71X0__DIV(JH7100_CLK_CPU_CORE, "cpu_core", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0__DIV(JH7100_CLK_CPU_AXI, "cpu_axi", 8, JH7100_CLK_CPU_CORE),
+	JH71X0__DIV(JH7100_CLK_AHB_BUS, "ahb_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0__DIV(JH7100_CLK_APB1_BUS, "apb1_bus", 8, JH7100_CLK_AHB_BUS),
+	JH71X0__DIV(JH7100_CLK_APB2_BUS, "apb2_bus", 8, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_DOM3AHB_BUS, "dom3ahb_bus", CLK_IS_CRITICAL, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_DOM7AHB_BUS, "dom7ahb_bus", CLK_IS_CRITICAL, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_U74_CORE0, "u74_core0", CLK_IS_CRITICAL, JH7100_CLK_CPU_CORE),
+	JH71X0_GDIV(JH7100_CLK_U74_CORE1, "u74_core1", CLK_IS_CRITICAL, 8, JH7100_CLK_CPU_CORE),
+	JH71X0_GATE(JH7100_CLK_U74_AXI, "u74_axi", CLK_IS_CRITICAL, JH7100_CLK_CPU_AXI),
+	JH71X0_GATE(JH7100_CLK_U74RTC_TOGGLE, "u74rtc_toggle", CLK_IS_CRITICAL, JH7100_CLK_OSC_SYS),
+	JH71X0_GATE(JH7100_CLK_SGDMA2P_AXI, "sgdma2p_axi", 0, JH7100_CLK_CPU_AXI),
+	JH71X0_GATE(JH7100_CLK_DMA2PNOC_AXI, "dma2pnoc_axi", 0, JH7100_CLK_CPU_AXI),
+	JH71X0_GATE(JH7100_CLK_SGDMA2P_AHB, "sgdma2p_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0__DIV(JH7100_CLK_DLA_BUS, "dla_bus", 4, JH7100_CLK_DLA_ROOT),
+	JH71X0_GATE(JH7100_CLK_DLA_AXI, "dla_axi", 0, JH7100_CLK_DLA_BUS),
+	JH71X0_GATE(JH7100_CLK_DLANOC_AXI, "dlanoc_axi", 0, JH7100_CLK_DLA_BUS),
+	JH71X0_GATE(JH7100_CLK_DLA_APB, "dla_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_VP6_CORE, "vp6_core", 0, 4, JH7100_CLK_DSP_ROOT_DIV),
+	JH71X0__DIV(JH7100_CLK_VP6BUS_SRC, "vp6bus_src", 4, JH7100_CLK_DSP_ROOT),
+	JH71X0_GDIV(JH7100_CLK_VP6_AXI, "vp6_axi", 0, 4, JH7100_CLK_VP6BUS_SRC),
+	JH71X0__DIV(JH7100_CLK_VCDECBUS_SRC, "vcdecbus_src", 4, JH7100_CLK_CDECHIFI4_ROOT),
+	JH71X0__DIV(JH7100_CLK_VDEC_BUS, "vdec_bus", 8, JH7100_CLK_VCDECBUS_SRC),
+	JH71X0_GATE(JH7100_CLK_VDEC_AXI, "vdec_axi", 0, JH7100_CLK_VDEC_BUS),
+	JH71X0_GATE(JH7100_CLK_VDECBRG_MAIN, "vdecbrg_mainclk", 0, JH7100_CLK_VDEC_BUS),
+	JH71X0_GDIV(JH7100_CLK_VDEC_BCLK, "vdec_bclk", 0, 8, JH7100_CLK_VCDECBUS_SRC),
+	JH71X0_GDIV(JH7100_CLK_VDEC_CCLK, "vdec_cclk", 0, 8, JH7100_CLK_CDEC_ROOT),
+	JH71X0_GATE(JH7100_CLK_VDEC_APB, "vdec_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_JPEG_AXI, "jpeg_axi", 0, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0_GDIV(JH7100_CLK_JPEG_CCLK, "jpeg_cclk", 0, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0_GATE(JH7100_CLK_JPEG_APB, "jpeg_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_GC300_2X, "gc300_2x", 0, 8, JH7100_CLK_CDECHIFI4_ROOT),
+	JH71X0_GATE(JH7100_CLK_GC300_AHB, "gc300_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0__DIV(JH7100_CLK_JPCGC300_AXIBUS, "jpcgc300_axibus", 8, JH7100_CLK_VCDECBUS_SRC),
+	JH71X0_GATE(JH7100_CLK_GC300_AXI, "gc300_axi", 0, JH7100_CLK_JPCGC300_AXIBUS),
+	JH71X0_GATE(JH7100_CLK_JPCGC300_MAIN, "jpcgc300_mainclk", 0, JH7100_CLK_JPCGC300_AXIBUS),
+	JH71X0__DIV(JH7100_CLK_VENC_BUS, "venc_bus", 8, JH7100_CLK_VCDECBUS_SRC),
+	JH71X0_GATE(JH7100_CLK_VENC_AXI, "venc_axi", 0, JH7100_CLK_VENC_BUS),
+	JH71X0_GATE(JH7100_CLK_VENCBRG_MAIN, "vencbrg_mainclk", 0, JH7100_CLK_VENC_BUS),
+	JH71X0_GDIV(JH7100_CLK_VENC_BCLK, "venc_bclk", 0, 8, JH7100_CLK_VCDECBUS_SRC),
+	JH71X0_GDIV(JH7100_CLK_VENC_CCLK, "venc_cclk", 0, 8, JH7100_CLK_CDEC_ROOT),
+	JH71X0_GATE(JH7100_CLK_VENC_APB, "venc_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_DDRPLL_DIV2, "ddrpll_div2", CLK_IS_CRITICAL, 2, JH7100_CLK_PLL1_OUT),
+	JH71X0_GDIV(JH7100_CLK_DDRPLL_DIV4, "ddrpll_div4", CLK_IS_CRITICAL, 2,
+		    JH7100_CLK_DDRPLL_DIV2),
+	JH71X0_GDIV(JH7100_CLK_DDRPLL_DIV8, "ddrpll_div8", CLK_IS_CRITICAL, 2,
+		    JH7100_CLK_DDRPLL_DIV4),
+	JH71X0_GDIV(JH7100_CLK_DDROSC_DIV2, "ddrosc_div2", CLK_IS_CRITICAL, 2, JH7100_CLK_OSC_SYS),
+	JH71X0_GMUX(JH7100_CLK_DDRC0, "ddrc0", CLK_IS_CRITICAL, 4,
 		    JH7100_CLK_DDROSC_DIV2,
 		    JH7100_CLK_DDRPLL_DIV2,
 		    JH7100_CLK_DDRPLL_DIV4,
 		    JH7100_CLK_DDRPLL_DIV8),
-	JH7100_GMUX(JH7100_CLK_DDRC1, "ddrc1", CLK_IS_CRITICAL, 4,
+	JH71X0_GMUX(JH7100_CLK_DDRC1, "ddrc1", CLK_IS_CRITICAL, 4,
 		    JH7100_CLK_DDROSC_DIV2,
 		    JH7100_CLK_DDRPLL_DIV2,
 		    JH7100_CLK_DDRPLL_DIV4,
 		    JH7100_CLK_DDRPLL_DIV8),
-	JH7100_GATE(JH7100_CLK_DDRPHY_APB, "ddrphy_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100__DIV(JH7100_CLK_NOC_ROB, "noc_rob", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100__DIV(JH7100_CLK_NOC_COG, "noc_cog", 8, JH7100_CLK_DLA_ROOT),
-	JH7100_GATE(JH7100_CLK_NNE_AHB, "nne_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100__DIV(JH7100_CLK_NNEBUS_SRC1, "nnebus_src1", 4, JH7100_CLK_DSP_ROOT),
-	JH7100__MUX(JH7100_CLK_NNE_BUS, "nne_bus", 2,
+	JH71X0_GATE(JH7100_CLK_DDRPHY_APB, "ddrphy_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0__DIV(JH7100_CLK_NOC_ROB, "noc_rob", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0__DIV(JH7100_CLK_NOC_COG, "noc_cog", 8, JH7100_CLK_DLA_ROOT),
+	JH71X0_GATE(JH7100_CLK_NNE_AHB, "nne_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0__DIV(JH7100_CLK_NNEBUS_SRC1, "nnebus_src1", 4, JH7100_CLK_DSP_ROOT),
+	JH71X0__MUX(JH7100_CLK_NNE_BUS, "nne_bus", 2,
 		    JH7100_CLK_CPU_AXI,
 		    JH7100_CLK_NNEBUS_SRC1),
-	JH7100_GATE(JH7100_CLK_NNE_AXI, "nne_axi", 0, JH7100_CLK_NNE_BUS),
-	JH7100_GATE(JH7100_CLK_NNENOC_AXI, "nnenoc_axi", 0, JH7100_CLK_NNE_BUS),
-	JH7100_GATE(JH7100_CLK_DLASLV_AXI, "dlaslv_axi", 0, JH7100_CLK_NNE_BUS),
-	JH7100_GATE(JH7100_CLK_DSPX2C_AXI, "dspx2c_axi", CLK_IS_CRITICAL, JH7100_CLK_NNE_BUS),
-	JH7100__DIV(JH7100_CLK_HIFI4_SRC, "hifi4_src", 4, JH7100_CLK_CDECHIFI4_ROOT),
-	JH7100__DIV(JH7100_CLK_HIFI4_COREFREE, "hifi4_corefree", 8, JH7100_CLK_HIFI4_SRC),
-	JH7100_GATE(JH7100_CLK_HIFI4_CORE, "hifi4_core", 0, JH7100_CLK_HIFI4_COREFREE),
-	JH7100__DIV(JH7100_CLK_HIFI4_BUS, "hifi4_bus", 8, JH7100_CLK_HIFI4_COREFREE),
-	JH7100_GATE(JH7100_CLK_HIFI4_AXI, "hifi4_axi", 0, JH7100_CLK_HIFI4_BUS),
-	JH7100_GATE(JH7100_CLK_HIFI4NOC_AXI, "hifi4noc_axi", 0, JH7100_CLK_HIFI4_BUS),
-	JH7100__DIV(JH7100_CLK_SGDMA1P_BUS, "sgdma1p_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100_GATE(JH7100_CLK_SGDMA1P_AXI, "sgdma1p_axi", 0, JH7100_CLK_SGDMA1P_BUS),
-	JH7100_GATE(JH7100_CLK_DMA1P_AXI, "dma1p_axi", 0, JH7100_CLK_SGDMA1P_BUS),
-	JH7100_GDIV(JH7100_CLK_X2C_AXI, "x2c_axi", CLK_IS_CRITICAL, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100__DIV(JH7100_CLK_USB_BUS, "usb_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
-	JH7100_GATE(JH7100_CLK_USB_AXI, "usb_axi", 0, JH7100_CLK_USB_BUS),
-	JH7100_GATE(JH7100_CLK_USBNOC_AXI, "usbnoc_axi", 0, JH7100_CLK_USB_BUS),
-	JH7100__DIV(JH7100_CLK_USBPHY_ROOTDIV, "usbphy_rootdiv", 4, JH7100_CLK_GMACUSB_ROOT),
-	JH7100_GDIV(JH7100_CLK_USBPHY_125M, "usbphy_125m", 0, 8, JH7100_CLK_USBPHY_ROOTDIV),
-	JH7100_GDIV(JH7100_CLK_USBPHY_PLLDIV25M, "usbphy_plldiv25m", 0, 32, JH7100_CLK_USBPHY_ROOTDIV),
-	JH7100__MUX(JH7100_CLK_USBPHY_25M, "usbphy_25m", 2,
+	JH71X0_GATE(JH7100_CLK_NNE_AXI, "nne_axi", 0, JH7100_CLK_NNE_BUS),
+	JH71X0_GATE(JH7100_CLK_NNENOC_AXI, "nnenoc_axi", 0, JH7100_CLK_NNE_BUS),
+	JH71X0_GATE(JH7100_CLK_DLASLV_AXI, "dlaslv_axi", 0, JH7100_CLK_NNE_BUS),
+	JH71X0_GATE(JH7100_CLK_DSPX2C_AXI, "dspx2c_axi", CLK_IS_CRITICAL, JH7100_CLK_NNE_BUS),
+	JH71X0__DIV(JH7100_CLK_HIFI4_SRC, "hifi4_src", 4, JH7100_CLK_CDECHIFI4_ROOT),
+	JH71X0__DIV(JH7100_CLK_HIFI4_COREFREE, "hifi4_corefree", 8, JH7100_CLK_HIFI4_SRC),
+	JH71X0_GATE(JH7100_CLK_HIFI4_CORE, "hifi4_core", 0, JH7100_CLK_HIFI4_COREFREE),
+	JH71X0__DIV(JH7100_CLK_HIFI4_BUS, "hifi4_bus", 8, JH7100_CLK_HIFI4_COREFREE),
+	JH71X0_GATE(JH7100_CLK_HIFI4_AXI, "hifi4_axi", 0, JH7100_CLK_HIFI4_BUS),
+	JH71X0_GATE(JH7100_CLK_HIFI4NOC_AXI, "hifi4noc_axi", 0, JH7100_CLK_HIFI4_BUS),
+	JH71X0__DIV(JH7100_CLK_SGDMA1P_BUS, "sgdma1p_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0_GATE(JH7100_CLK_SGDMA1P_AXI, "sgdma1p_axi", 0, JH7100_CLK_SGDMA1P_BUS),
+	JH71X0_GATE(JH7100_CLK_DMA1P_AXI, "dma1p_axi", 0, JH7100_CLK_SGDMA1P_BUS),
+	JH71X0_GDIV(JH7100_CLK_X2C_AXI, "x2c_axi", CLK_IS_CRITICAL, 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0__DIV(JH7100_CLK_USB_BUS, "usb_bus", 8, JH7100_CLK_CPUNBUS_ROOT_DIV),
+	JH71X0_GATE(JH7100_CLK_USB_AXI, "usb_axi", 0, JH7100_CLK_USB_BUS),
+	JH71X0_GATE(JH7100_CLK_USBNOC_AXI, "usbnoc_axi", 0, JH7100_CLK_USB_BUS),
+	JH71X0__DIV(JH7100_CLK_USBPHY_ROOTDIV, "usbphy_rootdiv", 4, JH7100_CLK_GMACUSB_ROOT),
+	JH71X0_GDIV(JH7100_CLK_USBPHY_125M, "usbphy_125m", 0, 8, JH7100_CLK_USBPHY_ROOTDIV),
+	JH71X0_GDIV(JH7100_CLK_USBPHY_PLLDIV25M, "usbphy_plldiv25m", 0, 32,
+		    JH7100_CLK_USBPHY_ROOTDIV),
+	JH71X0__MUX(JH7100_CLK_USBPHY_25M, "usbphy_25m", 2,
 		    JH7100_CLK_OSC_SYS,
 		    JH7100_CLK_USBPHY_PLLDIV25M),
-	JH7100_FDIV(JH7100_CLK_AUDIO_DIV, "audio_div", JH7100_CLK_AUDIO_ROOT),
-	JH7100_GATE(JH7100_CLK_AUDIO_SRC, "audio_src", 0, JH7100_CLK_AUDIO_DIV),
-	JH7100_GATE(JH7100_CLK_AUDIO_12288, "audio_12288", 0, JH7100_CLK_OSC_AUD),
-	JH7100_GDIV(JH7100_CLK_VIN_SRC, "vin_src", 0, 4, JH7100_CLK_VIN_ROOT),
-	JH7100__DIV(JH7100_CLK_ISP0_BUS, "isp0_bus", 8, JH7100_CLK_VIN_SRC),
-	JH7100_GATE(JH7100_CLK_ISP0_AXI, "isp0_axi", 0, JH7100_CLK_ISP0_BUS),
-	JH7100_GATE(JH7100_CLK_ISP0NOC_AXI, "isp0noc_axi", 0, JH7100_CLK_ISP0_BUS),
-	JH7100_GATE(JH7100_CLK_ISPSLV_AXI, "ispslv_axi", 0, JH7100_CLK_ISP0_BUS),
-	JH7100__DIV(JH7100_CLK_ISP1_BUS, "isp1_bus", 8, JH7100_CLK_VIN_SRC),
-	JH7100_GATE(JH7100_CLK_ISP1_AXI, "isp1_axi", 0, JH7100_CLK_ISP1_BUS),
-	JH7100_GATE(JH7100_CLK_ISP1NOC_AXI, "isp1noc_axi", 0, JH7100_CLK_ISP1_BUS),
-	JH7100__DIV(JH7100_CLK_VIN_BUS, "vin_bus", 8, JH7100_CLK_VIN_SRC),
-	JH7100_GATE(JH7100_CLK_VIN_AXI, "vin_axi", 0, JH7100_CLK_VIN_BUS),
-	JH7100_GATE(JH7100_CLK_VINNOC_AXI, "vinnoc_axi", 0, JH7100_CLK_VIN_BUS),
-	JH7100_GDIV(JH7100_CLK_VOUT_SRC, "vout_src", 0, 4, JH7100_CLK_VOUT_ROOT),
-	JH7100__DIV(JH7100_CLK_DISPBUS_SRC, "dispbus_src", 4, JH7100_CLK_VOUTBUS_ROOT),
-	JH7100__DIV(JH7100_CLK_DISP_BUS, "disp_bus", 4, JH7100_CLK_DISPBUS_SRC),
-	JH7100_GATE(JH7100_CLK_DISP_AXI, "disp_axi", 0, JH7100_CLK_DISP_BUS),
-	JH7100_GATE(JH7100_CLK_DISPNOC_AXI, "dispnoc_axi", 0, JH7100_CLK_DISP_BUS),
-	JH7100_GATE(JH7100_CLK_SDIO0_AHB, "sdio0_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GDIV(JH7100_CLK_SDIO0_CCLKINT, "sdio0_cclkint", 0, 24, JH7100_CLK_PERH0_SRC),
-	JH7100__INV(JH7100_CLK_SDIO0_CCLKINT_INV, "sdio0_cclkint_inv", JH7100_CLK_SDIO0_CCLKINT),
-	JH7100_GATE(JH7100_CLK_SDIO1_AHB, "sdio1_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GDIV(JH7100_CLK_SDIO1_CCLKINT, "sdio1_cclkint", 0, 24, JH7100_CLK_PERH1_SRC),
-	JH7100__INV(JH7100_CLK_SDIO1_CCLKINT_INV, "sdio1_cclkint_inv", JH7100_CLK_SDIO1_CCLKINT),
-	JH7100_GATE(JH7100_CLK_GMAC_AHB, "gmac_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100__DIV(JH7100_CLK_GMAC_ROOT_DIV, "gmac_root_div", 8, JH7100_CLK_GMACUSB_ROOT),
-	JH7100_GDIV(JH7100_CLK_GMAC_PTP_REF, "gmac_ptp_refclk", 0, 31, JH7100_CLK_GMAC_ROOT_DIV),
-	JH7100_GDIV(JH7100_CLK_GMAC_GTX, "gmac_gtxclk", 0, 255, JH7100_CLK_GMAC_ROOT_DIV),
-	JH7100_GDIV(JH7100_CLK_GMAC_RMII_TX, "gmac_rmii_txclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
-	JH7100_GDIV(JH7100_CLK_GMAC_RMII_RX, "gmac_rmii_rxclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
-	JH7100__MUX(JH7100_CLK_GMAC_TX, "gmac_tx", 3,
+	JH71X0_FDIV(JH7100_CLK_AUDIO_DIV, "audio_div", JH7100_CLK_AUDIO_ROOT),
+	JH71X0_GATE(JH7100_CLK_AUDIO_SRC, "audio_src", 0, JH7100_CLK_AUDIO_DIV),
+	JH71X0_GATE(JH7100_CLK_AUDIO_12288, "audio_12288", 0, JH7100_CLK_OSC_AUD),
+	JH71X0_GDIV(JH7100_CLK_VIN_SRC, "vin_src", 0, 4, JH7100_CLK_VIN_ROOT),
+	JH71X0__DIV(JH7100_CLK_ISP0_BUS, "isp0_bus", 8, JH7100_CLK_VIN_SRC),
+	JH71X0_GATE(JH7100_CLK_ISP0_AXI, "isp0_axi", 0, JH7100_CLK_ISP0_BUS),
+	JH71X0_GATE(JH7100_CLK_ISP0NOC_AXI, "isp0noc_axi", 0, JH7100_CLK_ISP0_BUS),
+	JH71X0_GATE(JH7100_CLK_ISPSLV_AXI, "ispslv_axi", 0, JH7100_CLK_ISP0_BUS),
+	JH71X0__DIV(JH7100_CLK_ISP1_BUS, "isp1_bus", 8, JH7100_CLK_VIN_SRC),
+	JH71X0_GATE(JH7100_CLK_ISP1_AXI, "isp1_axi", 0, JH7100_CLK_ISP1_BUS),
+	JH71X0_GATE(JH7100_CLK_ISP1NOC_AXI, "isp1noc_axi", 0, JH7100_CLK_ISP1_BUS),
+	JH71X0__DIV(JH7100_CLK_VIN_BUS, "vin_bus", 8, JH7100_CLK_VIN_SRC),
+	JH71X0_GATE(JH7100_CLK_VIN_AXI, "vin_axi", 0, JH7100_CLK_VIN_BUS),
+	JH71X0_GATE(JH7100_CLK_VINNOC_AXI, "vinnoc_axi", 0, JH7100_CLK_VIN_BUS),
+	JH71X0_GDIV(JH7100_CLK_VOUT_SRC, "vout_src", 0, 4, JH7100_CLK_VOUT_ROOT),
+	JH71X0__DIV(JH7100_CLK_DISPBUS_SRC, "dispbus_src", 4, JH7100_CLK_VOUTBUS_ROOT),
+	JH71X0__DIV(JH7100_CLK_DISP_BUS, "disp_bus", 4, JH7100_CLK_DISPBUS_SRC),
+	JH71X0_GATE(JH7100_CLK_DISP_AXI, "disp_axi", 0, JH7100_CLK_DISP_BUS),
+	JH71X0_GATE(JH7100_CLK_DISPNOC_AXI, "dispnoc_axi", 0, JH7100_CLK_DISP_BUS),
+	JH71X0_GATE(JH7100_CLK_SDIO0_AHB, "sdio0_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GDIV(JH7100_CLK_SDIO0_CCLKINT, "sdio0_cclkint", 0, 24, JH7100_CLK_PERH0_SRC),
+	JH71X0__INV(JH7100_CLK_SDIO0_CCLKINT_INV, "sdio0_cclkint_inv", JH7100_CLK_SDIO0_CCLKINT),
+	JH71X0_GATE(JH7100_CLK_SDIO1_AHB, "sdio1_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GDIV(JH7100_CLK_SDIO1_CCLKINT, "sdio1_cclkint", 0, 24, JH7100_CLK_PERH1_SRC),
+	JH71X0__INV(JH7100_CLK_SDIO1_CCLKINT_INV, "sdio1_cclkint_inv", JH7100_CLK_SDIO1_CCLKINT),
+	JH71X0_GATE(JH7100_CLK_GMAC_AHB, "gmac_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0__DIV(JH7100_CLK_GMAC_ROOT_DIV, "gmac_root_div", 8, JH7100_CLK_GMACUSB_ROOT),
+	JH71X0_GDIV(JH7100_CLK_GMAC_PTP_REF, "gmac_ptp_refclk", 0, 31, JH7100_CLK_GMAC_ROOT_DIV),
+	JH71X0_GDIV(JH7100_CLK_GMAC_GTX, "gmac_gtxclk", 0, 255, JH7100_CLK_GMAC_ROOT_DIV),
+	JH71X0_GDIV(JH7100_CLK_GMAC_RMII_TX, "gmac_rmii_txclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
+	JH71X0_GDIV(JH7100_CLK_GMAC_RMII_RX, "gmac_rmii_rxclk", 0, 8, JH7100_CLK_GMAC_RMII_REF),
+	JH71X0__MUX(JH7100_CLK_GMAC_TX, "gmac_tx", 3,
 		    JH7100_CLK_GMAC_GTX,
 		    JH7100_CLK_GMAC_TX_INV,
 		    JH7100_CLK_GMAC_RMII_TX),
-	JH7100__INV(JH7100_CLK_GMAC_TX_INV, "gmac_tx_inv", JH7100_CLK_GMAC_TX),
-	JH7100__MUX(JH7100_CLK_GMAC_RX_PRE, "gmac_rx_pre", 2,
+	JH71X0__INV(JH7100_CLK_GMAC_TX_INV, "gmac_tx_inv", JH7100_CLK_GMAC_TX),
+	JH71X0__MUX(JH7100_CLK_GMAC_RX_PRE, "gmac_rx_pre", 2,
 		    JH7100_CLK_GMAC_GR_MII_RX,
 		    JH7100_CLK_GMAC_RMII_RX),
-	JH7100__INV(JH7100_CLK_GMAC_RX_INV, "gmac_rx_inv", JH7100_CLK_GMAC_RX_PRE),
-	JH7100_GATE(JH7100_CLK_GMAC_RMII, "gmac_rmii", 0, JH7100_CLK_GMAC_RMII_REF),
-	JH7100_GDIV(JH7100_CLK_GMAC_TOPHYREF, "gmac_tophyref", 0, 127, JH7100_CLK_GMAC_ROOT_DIV),
-	JH7100_GATE(JH7100_CLK_SPI2AHB_AHB, "spi2ahb_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GDIV(JH7100_CLK_SPI2AHB_CORE, "spi2ahb_core", 0, 31, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_EZMASTER_AHB, "ezmaster_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_E24_AHB, "e24_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_E24RTC_TOGGLE, "e24rtc_toggle", 0, JH7100_CLK_OSC_SYS),
-	JH7100_GATE(JH7100_CLK_QSPI_AHB, "qspi_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_QSPI_APB, "qspi_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_QSPI_REF, "qspi_refclk", 0, 31, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_SEC_AHB, "sec_ahb", 0, JH7100_CLK_AHB_BUS),
-	JH7100_GATE(JH7100_CLK_AES, "aes_clk", 0, JH7100_CLK_SEC_AHB),
-	JH7100_GATE(JH7100_CLK_SHA, "sha_clk", 0, JH7100_CLK_SEC_AHB),
-	JH7100_GATE(JH7100_CLK_PKA, "pka_clk", 0, JH7100_CLK_SEC_AHB),
-	JH7100_GATE(JH7100_CLK_TRNG_APB, "trng_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GATE(JH7100_CLK_OTP_APB, "otp_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GATE(JH7100_CLK_UART0_APB, "uart0_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_UART0_CORE, "uart0_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_UART1_APB, "uart1_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_UART1_CORE, "uart1_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_SPI0_APB, "spi0_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_SPI0_CORE, "spi0_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_SPI1_APB, "spi1_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_SPI1_CORE, "spi1_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_I2C0_APB, "i2c0_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_I2C0_CORE, "i2c0_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_I2C1_APB, "i2c1_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GDIV(JH7100_CLK_I2C1_CORE, "i2c1_core", 0, 63, JH7100_CLK_PERH1_SRC),
-	JH7100_GATE(JH7100_CLK_GPIO_APB, "gpio_apb", 0, JH7100_CLK_APB1_BUS),
-	JH7100_GATE(JH7100_CLK_UART2_APB, "uart2_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_UART2_CORE, "uart2_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_UART3_APB, "uart3_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_UART3_CORE, "uart3_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_SPI2_APB, "spi2_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_SPI2_CORE, "spi2_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_SPI3_APB, "spi3_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_SPI3_CORE, "spi3_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_I2C2_APB, "i2c2_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_I2C2_CORE, "i2c2_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_I2C3_APB, "i2c3_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_I2C3_CORE, "i2c3_core", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_WDTIMER_APB, "wdtimer_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_WDT_CORE, "wdt_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER0_CORE, "timer0_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER1_CORE, "timer1_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER2_CORE, "timer2_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER3_CORE, "timer3_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER4_CORE, "timer4_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER5_CORE, "timer5_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GDIV(JH7100_CLK_TIMER6_CORE, "timer6_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
-	JH7100_GATE(JH7100_CLK_VP6INTC_APB, "vp6intc_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GATE(JH7100_CLK_PWM_APB, "pwm_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GATE(JH7100_CLK_MSI_APB, "msi_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GATE(JH7100_CLK_TEMP_APB, "temp_apb", 0, JH7100_CLK_APB2_BUS),
-	JH7100_GDIV(JH7100_CLK_TEMP_SENSE, "temp_sense", 0, 31, JH7100_CLK_OSC_SYS),
-	JH7100_GATE(JH7100_CLK_SYSERR_APB, "syserr_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0__INV(JH7100_CLK_GMAC_RX_INV, "gmac_rx_inv", JH7100_CLK_GMAC_RX_PRE),
+	JH71X0_GATE(JH7100_CLK_GMAC_RMII, "gmac_rmii", 0, JH7100_CLK_GMAC_RMII_REF),
+	JH71X0_GDIV(JH7100_CLK_GMAC_TOPHYREF, "gmac_tophyref", 0, 127, JH7100_CLK_GMAC_ROOT_DIV),
+	JH71X0_GATE(JH7100_CLK_SPI2AHB_AHB, "spi2ahb_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GDIV(JH7100_CLK_SPI2AHB_CORE, "spi2ahb_core", 0, 31, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_EZMASTER_AHB, "ezmaster_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_E24_AHB, "e24_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_E24RTC_TOGGLE, "e24rtc_toggle", 0, JH7100_CLK_OSC_SYS),
+	JH71X0_GATE(JH7100_CLK_QSPI_AHB, "qspi_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_QSPI_APB, "qspi_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_QSPI_REF, "qspi_refclk", 0, 31, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_SEC_AHB, "sec_ahb", 0, JH7100_CLK_AHB_BUS),
+	JH71X0_GATE(JH7100_CLK_AES, "aes_clk", 0, JH7100_CLK_SEC_AHB),
+	JH71X0_GATE(JH7100_CLK_SHA, "sha_clk", 0, JH7100_CLK_SEC_AHB),
+	JH71X0_GATE(JH7100_CLK_PKA, "pka_clk", 0, JH7100_CLK_SEC_AHB),
+	JH71X0_GATE(JH7100_CLK_TRNG_APB, "trng_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GATE(JH7100_CLK_OTP_APB, "otp_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GATE(JH7100_CLK_UART0_APB, "uart0_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_UART0_CORE, "uart0_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_UART1_APB, "uart1_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_UART1_CORE, "uart1_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_SPI0_APB, "spi0_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_SPI0_CORE, "spi0_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_SPI1_APB, "spi1_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_SPI1_CORE, "spi1_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_I2C0_APB, "i2c0_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_I2C0_CORE, "i2c0_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_I2C1_APB, "i2c1_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GDIV(JH7100_CLK_I2C1_CORE, "i2c1_core", 0, 63, JH7100_CLK_PERH1_SRC),
+	JH71X0_GATE(JH7100_CLK_GPIO_APB, "gpio_apb", 0, JH7100_CLK_APB1_BUS),
+	JH71X0_GATE(JH7100_CLK_UART2_APB, "uart2_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_UART2_CORE, "uart2_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_UART3_APB, "uart3_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_UART3_CORE, "uart3_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_SPI2_APB, "spi2_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_SPI2_CORE, "spi2_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_SPI3_APB, "spi3_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_SPI3_CORE, "spi3_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_I2C2_APB, "i2c2_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_I2C2_CORE, "i2c2_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_I2C3_APB, "i2c3_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_I2C3_CORE, "i2c3_core", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_WDTIMER_APB, "wdtimer_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_WDT_CORE, "wdt_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER0_CORE, "timer0_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER1_CORE, "timer1_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER2_CORE, "timer2_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER3_CORE, "timer3_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER4_CORE, "timer4_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER5_CORE, "timer5_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GDIV(JH7100_CLK_TIMER6_CORE, "timer6_coreclk", 0, 63, JH7100_CLK_PERH0_SRC),
+	JH71X0_GATE(JH7100_CLK_VP6INTC_APB, "vp6intc_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GATE(JH7100_CLK_PWM_APB, "pwm_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GATE(JH7100_CLK_MSI_APB, "msi_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GATE(JH7100_CLK_TEMP_APB, "temp_apb", 0, JH7100_CLK_APB2_BUS),
+	JH71X0_GDIV(JH7100_CLK_TEMP_SENSE, "temp_sense", 0, 31, JH7100_CLK_OSC_SYS),
+	JH71X0_GATE(JH7100_CLK_SYSERR_APB, "syserr_apb", 0, JH7100_CLK_APB2_BUS),
 };
 
 static struct clk_hw *jh7100_clk_get(struct of_phandle_args *clkspec, void *data)
 {
-	struct jh7100_clk_priv *priv = data;
+	struct jh71x0_clk_priv *priv = data;
 	unsigned int idx = clkspec->args[0];
 
 	if (idx < JH7100_CLK_PLL0_OUT)
@@ -280,7 +283,7 @@ static struct clk_hw *jh7100_clk_get(str
 
 static int __init clk_starfive_jh7100_probe(struct platform_device *pdev)
 {
-	struct jh7100_clk_priv *priv;
+	struct jh71x0_clk_priv *priv;
 	unsigned int idx;
 	int ret;
 
@@ -314,12 +317,12 @@ static int __init clk_starfive_jh7100_pr
 		struct clk_parent_data parents[4] = {};
 		struct clk_init_data init = {
 			.name = jh7100_clk_data[idx].name,
-			.ops = starfive_jh7100_clk_ops(max),
+			.ops = starfive_jh71x0_clk_ops(max),
 			.parent_data = parents,
-			.num_parents = ((max & JH7100_CLK_MUX_MASK) >> JH7100_CLK_MUX_SHIFT) + 1,
+			.num_parents = ((max & JH71X0_CLK_MUX_MASK) >> JH71X0_CLK_MUX_SHIFT) + 1,
 			.flags = jh7100_clk_data[idx].flags,
 		};
-		struct jh7100_clk *clk = &priv->reg[idx];
+		struct jh71x0_clk *clk = &priv->reg[idx];
 		unsigned int i;
 
 		for (i = 0; i < init.num_parents; i++) {
@@ -341,7 +344,7 @@ static int __init clk_starfive_jh7100_pr
 
 		clk->hw.init = &init;
 		clk->idx = idx;
-		clk->max_div = max & JH7100_CLK_DIV_MASK;
+		clk->max_div = max & JH71X0_CLK_DIV_MASK;
 
 		ret = devm_clk_hw_register(priv->dev, &clk->hw);
 		if (ret)
--- a/drivers/clk/starfive/clk-starfive-jh71x0.c
+++ b/drivers/clk/starfive/clk-starfive-jh71x0.c
@@ -1,6 +1,6 @@
 // SPDX-License-Identifier: GPL-2.0
 /*
- * StarFive JH7100 Clock Generator Driver
+ * StarFive JH71X0 Clock Generator Driver
  *
  * Copyright (C) 2021-2022 Emil Renner Berthing <kernel@esmil.dk>
  */
@@ -12,27 +12,27 @@
 
 #include "clk-starfive-jh71x0.h"
 
-static struct jh7100_clk *jh7100_clk_from(struct clk_hw *hw)
+static struct jh71x0_clk *jh71x0_clk_from(struct clk_hw *hw)
 {
-	return container_of(hw, struct jh7100_clk, hw);
+	return container_of(hw, struct jh71x0_clk, hw);
 }
 
-static struct jh7100_clk_priv *jh7100_priv_from(struct jh7100_clk *clk)
+static struct jh71x0_clk_priv *jh71x0_priv_from(struct jh71x0_clk *clk)
 {
-	return container_of(clk, struct jh7100_clk_priv, reg[clk->idx]);
+	return container_of(clk, struct jh71x0_clk_priv, reg[clk->idx]);
 }
 
-static u32 jh7100_clk_reg_get(struct jh7100_clk *clk)
+static u32 jh71x0_clk_reg_get(struct jh71x0_clk *clk)
 {
-	struct jh7100_clk_priv *priv = jh7100_priv_from(clk);
+	struct jh71x0_clk_priv *priv = jh71x0_priv_from(clk);
 	void __iomem *reg = priv->base + 4 * clk->idx;
 
 	return readl_relaxed(reg);
 }
 
-static void jh7100_clk_reg_rmw(struct jh7100_clk *clk, u32 mask, u32 value)
+static void jh71x0_clk_reg_rmw(struct jh71x0_clk *clk, u32 mask, u32 value)
 {
-	struct jh7100_clk_priv *priv = jh7100_priv_from(clk);
+	struct jh71x0_clk_priv *priv = jh71x0_priv_from(clk);
 	void __iomem *reg = priv->base + 4 * clk->idx;
 	unsigned long flags;
 
@@ -42,41 +42,41 @@ static void jh7100_clk_reg_rmw(struct jh
 	spin_unlock_irqrestore(&priv->rmw_lock, flags);
 }
 
-static int jh7100_clk_enable(struct clk_hw *hw)
+static int jh71x0_clk_enable(struct clk_hw *hw)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_ENABLE, JH7100_CLK_ENABLE);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_ENABLE, JH71X0_CLK_ENABLE);
 	return 0;
 }
 
-static void jh7100_clk_disable(struct clk_hw *hw)
+static void jh71x0_clk_disable(struct clk_hw *hw)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_ENABLE, 0);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_ENABLE, 0);
 }
 
-static int jh7100_clk_is_enabled(struct clk_hw *hw)
+static int jh71x0_clk_is_enabled(struct clk_hw *hw)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 
-	return !!(jh7100_clk_reg_get(clk) & JH7100_CLK_ENABLE);
+	return !!(jh71x0_clk_reg_get(clk) & JH71X0_CLK_ENABLE);
 }
 
-static unsigned long jh7100_clk_recalc_rate(struct clk_hw *hw,
+static unsigned long jh71x0_clk_recalc_rate(struct clk_hw *hw,
 					    unsigned long parent_rate)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	u32 div = jh7100_clk_reg_get(clk) & JH7100_CLK_DIV_MASK;
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	u32 div = jh71x0_clk_reg_get(clk) & JH71X0_CLK_DIV_MASK;
 
 	return div ? parent_rate / div : 0;
 }
 
-static int jh7100_clk_determine_rate(struct clk_hw *hw,
+static int jh71x0_clk_determine_rate(struct clk_hw *hw,
 				     struct clk_rate_request *req)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 	unsigned long parent = req->best_parent_rate;
 	unsigned long rate = clamp(req->rate, req->min_rate, req->max_rate);
 	unsigned long div = min_t(unsigned long, DIV_ROUND_UP(parent, rate), clk->max_div);
@@ -102,232 +102,232 @@ static int jh7100_clk_determine_rate(str
 	return 0;
 }
 
-static int jh7100_clk_set_rate(struct clk_hw *hw,
+static int jh71x0_clk_set_rate(struct clk_hw *hw,
 			       unsigned long rate,
 			       unsigned long parent_rate)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 	unsigned long div = clamp(DIV_ROUND_CLOSEST(parent_rate, rate),
 				  1UL, (unsigned long)clk->max_div);
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_DIV_MASK, div);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_DIV_MASK, div);
 	return 0;
 }
 
-static unsigned long jh7100_clk_frac_recalc_rate(struct clk_hw *hw,
+static unsigned long jh71x0_clk_frac_recalc_rate(struct clk_hw *hw,
 						 unsigned long parent_rate)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	u32 reg = jh7100_clk_reg_get(clk);
-	unsigned long div100 = 100 * (reg & JH7100_CLK_INT_MASK) +
-			       ((reg & JH7100_CLK_FRAC_MASK) >> JH7100_CLK_FRAC_SHIFT);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	u32 reg = jh71x0_clk_reg_get(clk);
+	unsigned long div100 = 100 * (reg & JH71X0_CLK_INT_MASK) +
+			       ((reg & JH71X0_CLK_FRAC_MASK) >> JH71X0_CLK_FRAC_SHIFT);
 
-	return (div100 >= JH7100_CLK_FRAC_MIN) ? 100 * parent_rate / div100 : 0;
+	return (div100 >= JH71X0_CLK_FRAC_MIN) ? 100 * parent_rate / div100 : 0;
 }
 
-static int jh7100_clk_frac_determine_rate(struct clk_hw *hw,
+static int jh71x0_clk_frac_determine_rate(struct clk_hw *hw,
 					  struct clk_rate_request *req)
 {
 	unsigned long parent100 = 100 * req->best_parent_rate;
 	unsigned long rate = clamp(req->rate, req->min_rate, req->max_rate);
 	unsigned long div100 = clamp(DIV_ROUND_CLOSEST(parent100, rate),
-				     JH7100_CLK_FRAC_MIN, JH7100_CLK_FRAC_MAX);
+				     JH71X0_CLK_FRAC_MIN, JH71X0_CLK_FRAC_MAX);
 	unsigned long result = parent100 / div100;
 
-	/* clamp the result as in jh7100_clk_determine_rate() above */
-	if (result > req->max_rate && div100 < JH7100_CLK_FRAC_MAX)
+	/* clamp the result as in jh71x0_clk_determine_rate() above */
+	if (result > req->max_rate && div100 < JH71X0_CLK_FRAC_MAX)
 		result = parent100 / (div100 + 1);
-	if (result < req->min_rate && div100 > JH7100_CLK_FRAC_MIN)
+	if (result < req->min_rate && div100 > JH71X0_CLK_FRAC_MIN)
 		result = parent100 / (div100 - 1);
 
 	req->rate = result;
 	return 0;
 }
 
-static int jh7100_clk_frac_set_rate(struct clk_hw *hw,
+static int jh71x0_clk_frac_set_rate(struct clk_hw *hw,
 				    unsigned long rate,
 				    unsigned long parent_rate)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 	unsigned long div100 = clamp(DIV_ROUND_CLOSEST(100 * parent_rate, rate),
-				     JH7100_CLK_FRAC_MIN, JH7100_CLK_FRAC_MAX);
-	u32 value = ((div100 % 100) << JH7100_CLK_FRAC_SHIFT) | (div100 / 100);
+				     JH71X0_CLK_FRAC_MIN, JH71X0_CLK_FRAC_MAX);
+	u32 value = ((div100 % 100) << JH71X0_CLK_FRAC_SHIFT) | (div100 / 100);
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_DIV_MASK, value);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_DIV_MASK, value);
 	return 0;
 }
 
-static u8 jh7100_clk_get_parent(struct clk_hw *hw)
+static u8 jh71x0_clk_get_parent(struct clk_hw *hw)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	u32 value = jh7100_clk_reg_get(clk);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	u32 value = jh71x0_clk_reg_get(clk);
 
-	return (value & JH7100_CLK_MUX_MASK) >> JH7100_CLK_MUX_SHIFT;
+	return (value & JH71X0_CLK_MUX_MASK) >> JH71X0_CLK_MUX_SHIFT;
 }
 
-static int jh7100_clk_set_parent(struct clk_hw *hw, u8 index)
+static int jh71x0_clk_set_parent(struct clk_hw *hw, u8 index)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	u32 value = (u32)index << JH7100_CLK_MUX_SHIFT;
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	u32 value = (u32)index << JH71X0_CLK_MUX_SHIFT;
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_MUX_MASK, value);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_MUX_MASK, value);
 	return 0;
 }
 
-static int jh7100_clk_mux_determine_rate(struct clk_hw *hw,
+static int jh71x0_clk_mux_determine_rate(struct clk_hw *hw,
 					 struct clk_rate_request *req)
 {
 	return clk_mux_determine_rate_flags(hw, req, 0);
 }
 
-static int jh7100_clk_get_phase(struct clk_hw *hw)
+static int jh71x0_clk_get_phase(struct clk_hw *hw)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	u32 value = jh7100_clk_reg_get(clk);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	u32 value = jh71x0_clk_reg_get(clk);
 
-	return (value & JH7100_CLK_INVERT) ? 180 : 0;
+	return (value & JH71X0_CLK_INVERT) ? 180 : 0;
 }
 
-static int jh7100_clk_set_phase(struct clk_hw *hw, int degrees)
+static int jh71x0_clk_set_phase(struct clk_hw *hw, int degrees)
 {
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
 	u32 value;
 
 	if (degrees == 0)
 		value = 0;
 	else if (degrees == 180)
-		value = JH7100_CLK_INVERT;
+		value = JH71X0_CLK_INVERT;
 	else
 		return -EINVAL;
 
-	jh7100_clk_reg_rmw(clk, JH7100_CLK_INVERT, value);
+	jh71x0_clk_reg_rmw(clk, JH71X0_CLK_INVERT, value);
 	return 0;
 }
 
 #ifdef CONFIG_DEBUG_FS
-static void jh7100_clk_debug_init(struct clk_hw *hw, struct dentry *dentry)
+static void jh71x0_clk_debug_init(struct clk_hw *hw, struct dentry *dentry)
 {
-	static const struct debugfs_reg32 jh7100_clk_reg = {
+	static const struct debugfs_reg32 jh71x0_clk_reg = {
 		.name = "CTRL",
 		.offset = 0,
 	};
-	struct jh7100_clk *clk = jh7100_clk_from(hw);
-	struct jh7100_clk_priv *priv = jh7100_priv_from(clk);
+	struct jh71x0_clk *clk = jh71x0_clk_from(hw);
+	struct jh71x0_clk_priv *priv = jh71x0_priv_from(clk);
 	struct debugfs_regset32 *regset;
 
 	regset = devm_kzalloc(priv->dev, sizeof(*regset), GFP_KERNEL);
 	if (!regset)
 		return;
 
-	regset->regs = &jh7100_clk_reg;
+	regset->regs = &jh71x0_clk_reg;
 	regset->nregs = 1;
 	regset->base = priv->base + 4 * clk->idx;
 
 	debugfs_create_regset32("registers", 0400, dentry, regset);
 }
 #else
-#define jh7100_clk_debug_init NULL
+#define jh71x0_clk_debug_init NULL
 #endif
 
-static const struct clk_ops jh7100_clk_gate_ops = {
-	.enable = jh7100_clk_enable,
-	.disable = jh7100_clk_disable,
-	.is_enabled = jh7100_clk_is_enabled,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_gate_ops = {
+	.enable = jh71x0_clk_enable,
+	.disable = jh71x0_clk_disable,
+	.is_enabled = jh71x0_clk_is_enabled,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_div_ops = {
-	.recalc_rate = jh7100_clk_recalc_rate,
-	.determine_rate = jh7100_clk_determine_rate,
-	.set_rate = jh7100_clk_set_rate,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_div_ops = {
+	.recalc_rate = jh71x0_clk_recalc_rate,
+	.determine_rate = jh71x0_clk_determine_rate,
+	.set_rate = jh71x0_clk_set_rate,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_fdiv_ops = {
-	.recalc_rate = jh7100_clk_frac_recalc_rate,
-	.determine_rate = jh7100_clk_frac_determine_rate,
-	.set_rate = jh7100_clk_frac_set_rate,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_fdiv_ops = {
+	.recalc_rate = jh71x0_clk_frac_recalc_rate,
+	.determine_rate = jh71x0_clk_frac_determine_rate,
+	.set_rate = jh71x0_clk_frac_set_rate,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_gdiv_ops = {
-	.enable = jh7100_clk_enable,
-	.disable = jh7100_clk_disable,
-	.is_enabled = jh7100_clk_is_enabled,
-	.recalc_rate = jh7100_clk_recalc_rate,
-	.determine_rate = jh7100_clk_determine_rate,
-	.set_rate = jh7100_clk_set_rate,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_gdiv_ops = {
+	.enable = jh71x0_clk_enable,
+	.disable = jh71x0_clk_disable,
+	.is_enabled = jh71x0_clk_is_enabled,
+	.recalc_rate = jh71x0_clk_recalc_rate,
+	.determine_rate = jh71x0_clk_determine_rate,
+	.set_rate = jh71x0_clk_set_rate,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_mux_ops = {
-	.determine_rate = jh7100_clk_mux_determine_rate,
-	.set_parent = jh7100_clk_set_parent,
-	.get_parent = jh7100_clk_get_parent,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_mux_ops = {
+	.determine_rate = jh71x0_clk_mux_determine_rate,
+	.set_parent = jh71x0_clk_set_parent,
+	.get_parent = jh71x0_clk_get_parent,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_gmux_ops = {
-	.enable = jh7100_clk_enable,
-	.disable = jh7100_clk_disable,
-	.is_enabled = jh7100_clk_is_enabled,
-	.determine_rate = jh7100_clk_mux_determine_rate,
-	.set_parent = jh7100_clk_set_parent,
-	.get_parent = jh7100_clk_get_parent,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_gmux_ops = {
+	.enable = jh71x0_clk_enable,
+	.disable = jh71x0_clk_disable,
+	.is_enabled = jh71x0_clk_is_enabled,
+	.determine_rate = jh71x0_clk_mux_determine_rate,
+	.set_parent = jh71x0_clk_set_parent,
+	.get_parent = jh71x0_clk_get_parent,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_mdiv_ops = {
-	.recalc_rate = jh7100_clk_recalc_rate,
-	.determine_rate = jh7100_clk_determine_rate,
-	.get_parent = jh7100_clk_get_parent,
-	.set_parent = jh7100_clk_set_parent,
-	.set_rate = jh7100_clk_set_rate,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_mdiv_ops = {
+	.recalc_rate = jh71x0_clk_recalc_rate,
+	.determine_rate = jh71x0_clk_determine_rate,
+	.get_parent = jh71x0_clk_get_parent,
+	.set_parent = jh71x0_clk_set_parent,
+	.set_rate = jh71x0_clk_set_rate,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_gmd_ops = {
-	.enable = jh7100_clk_enable,
-	.disable = jh7100_clk_disable,
-	.is_enabled = jh7100_clk_is_enabled,
-	.recalc_rate = jh7100_clk_recalc_rate,
-	.determine_rate = jh7100_clk_determine_rate,
-	.get_parent = jh7100_clk_get_parent,
-	.set_parent = jh7100_clk_set_parent,
-	.set_rate = jh7100_clk_set_rate,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_gmd_ops = {
+	.enable = jh71x0_clk_enable,
+	.disable = jh71x0_clk_disable,
+	.is_enabled = jh71x0_clk_is_enabled,
+	.recalc_rate = jh71x0_clk_recalc_rate,
+	.determine_rate = jh71x0_clk_determine_rate,
+	.get_parent = jh71x0_clk_get_parent,
+	.set_parent = jh71x0_clk_set_parent,
+	.set_rate = jh71x0_clk_set_rate,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-static const struct clk_ops jh7100_clk_inv_ops = {
-	.get_phase = jh7100_clk_get_phase,
-	.set_phase = jh7100_clk_set_phase,
-	.debug_init = jh7100_clk_debug_init,
+static const struct clk_ops jh71x0_clk_inv_ops = {
+	.get_phase = jh71x0_clk_get_phase,
+	.set_phase = jh71x0_clk_set_phase,
+	.debug_init = jh71x0_clk_debug_init,
 };
 
-const struct clk_ops *starfive_jh7100_clk_ops(u32 max)
+const struct clk_ops *starfive_jh71x0_clk_ops(u32 max)
 {
-	if (max & JH7100_CLK_DIV_MASK) {
-		if (max & JH7100_CLK_MUX_MASK) {
-			if (max & JH7100_CLK_ENABLE)
-				return &jh7100_clk_gmd_ops;
-			return &jh7100_clk_mdiv_ops;
+	if (max & JH71X0_CLK_DIV_MASK) {
+		if (max & JH71X0_CLK_MUX_MASK) {
+			if (max & JH71X0_CLK_ENABLE)
+				return &jh71x0_clk_gmd_ops;
+			return &jh71x0_clk_mdiv_ops;
 		}
-		if (max & JH7100_CLK_ENABLE)
-			return &jh7100_clk_gdiv_ops;
-		if (max == JH7100_CLK_FRAC_MAX)
-			return &jh7100_clk_fdiv_ops;
-		return &jh7100_clk_div_ops;
+		if (max & JH71X0_CLK_ENABLE)
+			return &jh71x0_clk_gdiv_ops;
+		if (max == JH71X0_CLK_FRAC_MAX)
+			return &jh71x0_clk_fdiv_ops;
+		return &jh71x0_clk_div_ops;
 	}
 
-	if (max & JH7100_CLK_MUX_MASK) {
-		if (max & JH7100_CLK_ENABLE)
-			return &jh7100_clk_gmux_ops;
-		return &jh7100_clk_mux_ops;
+	if (max & JH71X0_CLK_MUX_MASK) {
+		if (max & JH71X0_CLK_ENABLE)
+			return &jh71x0_clk_gmux_ops;
+		return &jh71x0_clk_mux_ops;
 	}
 
-	if (max & JH7100_CLK_ENABLE)
-		return &jh7100_clk_gate_ops;
+	if (max & JH71X0_CLK_ENABLE)
+		return &jh71x0_clk_gate_ops;
 
-	return &jh7100_clk_inv_ops;
+	return &jh71x0_clk_inv_ops;
 }
-EXPORT_SYMBOL_GPL(starfive_jh7100_clk_ops);
+EXPORT_SYMBOL_GPL(starfive_jh71x0_clk_ops);
--- a/drivers/clk/starfive/clk-starfive-jh71x0.h
+++ b/drivers/clk/starfive/clk-starfive-jh71x0.h
@@ -1,6 +1,6 @@
 /* SPDX-License-Identifier: GPL-2.0 */
-#ifndef __CLK_STARFIVE_JH7100_H
-#define __CLK_STARFIVE_JH7100_H
+#ifndef __CLK_STARFIVE_JH71X0_H
+#define __CLK_STARFIVE_JH71X0_H
 
 #include <linux/bits.h>
 #include <linux/clk-provider.h>
@@ -8,107 +8,116 @@
 #include <linux/spinlock.h>
 
 /* register fields */
-#define JH7100_CLK_ENABLE	BIT(31)
-#define JH7100_CLK_INVERT	BIT(30)
-#define JH7100_CLK_MUX_MASK	GENMASK(27, 24)
-#define JH7100_CLK_MUX_SHIFT	24
-#define JH7100_CLK_DIV_MASK	GENMASK(23, 0)
-#define JH7100_CLK_FRAC_MASK	GENMASK(15, 8)
-#define JH7100_CLK_FRAC_SHIFT	8
-#define JH7100_CLK_INT_MASK	GENMASK(7, 0)
+#define JH71X0_CLK_ENABLE	BIT(31)
+#define JH71X0_CLK_INVERT	BIT(30)
+#define JH71X0_CLK_MUX_MASK	GENMASK(27, 24)
+#define JH71X0_CLK_MUX_SHIFT	24
+#define JH71X0_CLK_DIV_MASK	GENMASK(23, 0)
+#define JH71X0_CLK_FRAC_MASK	GENMASK(15, 8)
+#define JH71X0_CLK_FRAC_SHIFT	8
+#define JH71X0_CLK_INT_MASK	GENMASK(7, 0)
 
 /* fractional divider min/max */
-#define JH7100_CLK_FRAC_MIN	100UL
-#define JH7100_CLK_FRAC_MAX	25599UL
+#define JH71X0_CLK_FRAC_MIN	100UL
+#define JH71X0_CLK_FRAC_MAX	25599UL
 
 /* clock data */
-struct jh7100_clk_data {
+struct jh71x0_clk_data {
 	const char *name;
 	unsigned long flags;
 	u32 max;
 	u8 parents[4];
 };
 
-#define JH7100_GATE(_idx, _name, _flags, _parent) [_idx] = {			\
+#define JH71X0_GATE(_idx, _name, _flags, _parent)				\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = CLK_SET_RATE_PARENT | (_flags),				\
-	.max = JH7100_CLK_ENABLE,						\
+	.max = JH71X0_CLK_ENABLE,						\
 	.parents = { [0] = _parent },						\
 }
 
-#define JH7100__DIV(_idx, _name, _max, _parent) [_idx] = {			\
+#define JH71X0__DIV(_idx, _name, _max, _parent)					\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = 0,								\
 	.max = _max,								\
 	.parents = { [0] = _parent },						\
 }
 
-#define JH7100_GDIV(_idx, _name, _flags, _max, _parent) [_idx] = {		\
+#define JH71X0_GDIV(_idx, _name, _flags, _max, _parent)				\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = _flags,							\
-	.max = JH7100_CLK_ENABLE | (_max),					\
+	.max = JH71X0_CLK_ENABLE | (_max),					\
 	.parents = { [0] = _parent },						\
 }
 
-#define JH7100_FDIV(_idx, _name, _parent) [_idx] = {				\
+#define JH71X0_FDIV(_idx, _name, _parent)					\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = 0,								\
-	.max = JH7100_CLK_FRAC_MAX,						\
+	.max = JH71X0_CLK_FRAC_MAX,						\
 	.parents = { [0] = _parent },						\
 }
 
-#define JH7100__MUX(_idx, _name, _nparents, ...) [_idx] = {			\
+#define JH71X0__MUX(_idx, _name, _nparents, ...)				\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = 0,								\
-	.max = ((_nparents) - 1) << JH7100_CLK_MUX_SHIFT,			\
+	.max = ((_nparents) - 1) << JH71X0_CLK_MUX_SHIFT,			\
 	.parents = { __VA_ARGS__ },						\
 }
 
-#define JH7100_GMUX(_idx, _name, _flags, _nparents, ...) [_idx] = {		\
+#define JH71X0_GMUX(_idx, _name, _flags, _nparents, ...)			\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = _flags,							\
-	.max = JH7100_CLK_ENABLE |						\
-		(((_nparents) - 1) << JH7100_CLK_MUX_SHIFT),			\
+	.max = JH71X0_CLK_ENABLE |						\
+		(((_nparents) - 1) << JH71X0_CLK_MUX_SHIFT),			\
 	.parents = { __VA_ARGS__ },						\
 }
 
-#define JH7100_MDIV(_idx, _name, _max, _nparents, ...) [_idx] = {		\
+#define JH71X0_MDIV(_idx, _name, _max, _nparents, ...)				\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = 0,								\
-	.max = (((_nparents) - 1) << JH7100_CLK_MUX_SHIFT) | (_max),		\
+	.max = (((_nparents) - 1) << JH71X0_CLK_MUX_SHIFT) | (_max),		\
 	.parents = { __VA_ARGS__ },						\
 }
 
-#define JH7100__GMD(_idx, _name, _flags, _max, _nparents, ...) [_idx] = {	\
+#define JH71X0__GMD(_idx, _name, _flags, _max, _nparents, ...)			\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = _flags,							\
-	.max = JH7100_CLK_ENABLE |						\
-		(((_nparents) - 1) << JH7100_CLK_MUX_SHIFT) | (_max),		\
+	.max = JH71X0_CLK_ENABLE |						\
+		(((_nparents) - 1) << JH71X0_CLK_MUX_SHIFT) | (_max),		\
 	.parents = { __VA_ARGS__ },						\
 }
 
-#define JH7100__INV(_idx, _name, _parent) [_idx] = {				\
+#define JH71X0__INV(_idx, _name, _parent)					\
+[_idx] = {									\
 	.name = _name,								\
 	.flags = CLK_SET_RATE_PARENT,						\
-	.max = JH7100_CLK_INVERT,						\
+	.max = JH71X0_CLK_INVERT,						\
 	.parents = { [0] = _parent },						\
 }
 
-struct jh7100_clk {
+struct jh71x0_clk {
 	struct clk_hw hw;
 	unsigned int idx;
 	unsigned int max_div;
 };
 
-struct jh7100_clk_priv {
+struct jh71x0_clk_priv {
 	/* protect clk enable and set rate/parent from happening at the same time */
 	spinlock_t rmw_lock;
 	struct device *dev;
 	void __iomem *base;
 	struct clk_hw *pll[3];
-	struct jh7100_clk reg[];
+	struct jh71x0_clk reg[];
 };
 
-const struct clk_ops *starfive_jh7100_clk_ops(u32 max);
+const struct clk_ops *starfive_jh71x0_clk_ops(u32 max);
 
 #endif
