From 10ff8ba24c68f704ecf5a58878617dfe149a14c6 Mon Sep 17 00:00:00 2001
From: John Cox <jc@kynesim.co.uk>
Date: Mon, 2 Oct 2023 15:15:13 +0100
Subject: [PATCH] dts/bcm2712: Add iommu to rpivid

Add iommu to rpivid so it can cope with scatter/gather

Signed-off-by: John Cox <jc@kynesim.co.uk>
---
 arch/arm/boot/dts/bcm2712.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/bcm2712.dtsi
+++ b/arch/arm/boot/dts/bcm2712.dtsi
@@ -1158,6 +1158,7 @@
 			clocks = <&firmware_clocks 11>;
 			clock-names = "hevc";
 			status = "disabled";
+			iommus = <&iommu2>;
 		};
 
 		sdio1: mmc@fff000 {
