From 89bd4e64da3345c2764a42875b99c96fa8931967 Mon Sep 17 00:00:00 2001
From: Joerg Schambacher <joerg@hifiberry.com>
Date: Thu, 1 Feb 2024 17:32:44 +0100
Subject: [PATCH 1265/1295] ASoC: DACplus - fix 16bit sample support in clock
 consumer mode

The former code did not adjust the physical sample width when
in clock consumer mode and has taken the fixed 32 bit default.
This has caused the audio to be played at half its frequency due to
the fixed bclk_ratio of 64.

Signed-off-by: Joerg Schambacher <joerg@hifiberry.com>
---
 sound/soc/bcm/hifiberry_dacplus.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

--- a/sound/soc/bcm/hifiberry_dacplus.c
+++ b/sound/soc/bcm/hifiberry_dacplus.c
@@ -279,13 +279,11 @@ static int snd_rpi_hifiberry_dacplus_hw_
 	int ret = 0;
 	struct snd_soc_pcm_runtime *rtd = substream->private_data;
 	int channels = params_channels(params);
-	int width = 32;
+	int width = snd_pcm_format_physical_width(params_format(params));
 
 	if (snd_rpi_hifiberry_is_dacpro) {
 		struct snd_soc_component *component = asoc_rtd_to_codec(rtd, 0)->component;
 
-		width = snd_pcm_format_physical_width(params_format(params));
-
 		snd_rpi_hifiberry_dacplus_set_sclk(component,
 			params_rate(params));
 
