// SPDX-License-Identifier: (GPL-2.0 OR MIT)

/dts-v1/;
#include <dt-bindings/input/input.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/leds/common.h>

#include "mt7986a.dtsi"

/ {
	model = "Acer Predator W6";
	compatible = "acer,predator-w6", "mediatek,mt7986a";

	aliases {
		serial0 = &uart0;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	chosen {
		stdout-path = "serial0:115200n8";
		bootargs = "dm-mod.create=\"dm-verity,,,ro,0 31544 verity 1 PARTLABEL=rootfs PARTLABEL=rootfs 4096 4096 3943 3944 sha256 2f969fa9e9e4e20b37746f22633e85b178f5db7c143e11f92733a704299cc933 2dd56e34b15c6c84573cf26c4392028421061d2c808975217b45e9a5b49d2087\" rootfstype=squashfs,ext4 rootwait root=/dev/mmcblk0p6 fstools_ignore_partname=1";
	};

	memory {
		reg = <0 0x40000000 0 0x20000000>;
	};

	reg_1p8v: regulator-1p8v {
		compatible = "regulator-fixed";
		regulator-name = "fixed-1.8V";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-boot-on;
		regulator-always-on;
	};

	reg_3p3v: regulator-3p3v {
		compatible = "regulator-fixed";
		regulator-name = "fixed-3.3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
	};

	reg_5v: regulator-5v {
		compatible = "regulator-fixed";
		regulator-name = "fixed-5V";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
		regulator-always-on;
	};

	gpio-keys {
		compatible = "gpio-keys";

		factory {
			label = "factory";
			linux,code = <KEY_RESTART>;
			gpios = <&pio 9 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&pio 10 GPIO_ACTIVE_LOW>;
		};
	};


	leds {
		compatible = "gpio-leds";

		led_status: led@0 {
			label = "ant0:red";
			gpios = <&pio 1 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@1 {
			label = "ant0:green";
			gpios = <&pio 2 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@2 {
			label = "ant0:blue";
			gpios = <&pio 36 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@3 {
			label = "ant1:red";
			gpios = <&pio 35 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@4 {
			label = "ant1:green";
			gpios = <&pio 34 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@5 {
			label = "ant1:blue";
			gpios = <&pio 33 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@6 {
			label = "ant2:red";
			gpios = <&pio 38 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@7 {
			label = "ant2:green";
			gpios = <&pio 37 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@8 {
			label = "ant2:blue";
			gpios = <&pio 26 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@9 {
			label = "ant3:red";
			gpios = <&pio 25 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@10 {
			label = "ant3:green";
			gpios = <&pio 24 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@11 {
			label = "ant3:blue";
			gpios = <&pio 23 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@12 {
			label = "ant4:red";
			gpios = <&pio 28 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@13 {
			label = "ant4:green";
			gpios = <&pio 27 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@14 {
			label = "ant4:blue";
			gpios = <&pio 32 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@15 {
			label = "ant5:red";
			gpios = <&pio 45 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@16 {
			label = "ant5:green";
			gpios = <&pio 44 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led@17 {
			label = "ant5:blue";
			gpios = <&pio 43 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};
	};

};

&eth {
	status = "okay";

	gmac0: mac@0 {
		/* LAN */
		compatible = "mediatek,eth-mac";
		reg = <0>;
		phy-mode = "2500base-x";

		fixed-link {
			speed = <2500>;
			full-duplex;
			pause;
		};
	};

	gmac1: mac@1 {
		/* WAN */
		compatible = "mediatek,eth-mac";
		reg = <1>;
		phy-mode = "2500base-x";
		phy-handle = <&phy6>;
	};

	mdio: mdio-bus {
		#address-cells = <1>;
		#size-cells = <0>;
	};
};

&mdio {
	phy6: phy@6 {
		compatible = "ethernet-phy-ieee802.3-c45";
		reg = <6>;

		reset-gpios = <&pio 6 GPIO_ACTIVE_LOW>;
		reset-assert-us = <10000>;
		reset-deassert-us = <10000>;

		/* LED0: nc ; LED1: nc ; LED2: Amber ; LED3: Green */
		mxl,led-config = <0x0 0x0 0x370 0x80>;
	};

	switch: switch@1f {
		compatible = "mediatek,mt7531";
		reg = <31>;

		reset-gpios = <&pio 5 GPIO_ACTIVE_HIGH>;
		reset-assert-us = <10000>;
		reset-deassert-us = <10000>;
	};
};

&pio {
	mmc0_pins_default: mmc0-pins {
		mux {
			function = "emmc";
			groups = "emmc_51";
		};
		conf-cmd-dat {
			pins = "EMMC_DATA_0", "EMMC_DATA_1", "EMMC_DATA_2",
			       "EMMC_DATA_3", "EMMC_DATA_4", "EMMC_DATA_5",
			       "EMMC_DATA_6", "EMMC_DATA_7", "EMMC_CMD";
			input-enable;
			drive-strength = <4>;
			mediatek,pull-up-adv = <1>;	/* pull-up 10K */
		};
		conf-clk {
			pins = "EMMC_CK";
			drive-strength = <6>;
			mediatek,pull-down-adv = <2>;	/* pull-down 50K */
		};
		conf-ds {
			pins = "EMMC_DSL";
			mediatek,pull-down-adv = <2>;	/* pull-down 50K */
		};
		conf-rst {
			pins = "EMMC_RSTB";
			drive-strength = <4>;
			mediatek,pull-up-adv = <1>;	/* pull-up 10K */
		};
	};

	mmc0_pins_uhs: mmc0-uhs-pins {
		mux {
			function = "emmc";
			groups = "emmc_51";
		};
		conf-cmd-dat {
			pins = "EMMC_DATA_0", "EMMC_DATA_1", "EMMC_DATA_2",
			       "EMMC_DATA_3", "EMMC_DATA_4", "EMMC_DATA_5",
			       "EMMC_DATA_6", "EMMC_DATA_7", "EMMC_CMD";
			input-enable;
			drive-strength = <4>;
			mediatek,pull-up-adv = <1>;	/* pull-up 10K */
		};
		conf-clk {
			pins = "EMMC_CK";
			drive-strength = <6>;
			mediatek,pull-down-adv = <2>;	/* pull-down 50K */
		};
		conf-ds {
			pins = "EMMC_DSL";
			mediatek,pull-down-adv = <2>;	/* pull-down 50K */
		};
		conf-rst {
			pins = "EMMC_RSTB";
			drive-strength = <4>;
			mediatek,pull-up-adv = <1>;	/* pull-up 10K */
		};
	};

	pcie_pins: pcie-pins {
		mux {
			function = "pcie";
			groups = "pcie_pereset";
		};
	};

	wf_2g_5g_pins: wf_2g_5g-pins {
		mux {
			function = "wifi";
			groups = "wf_2g", "wf_5g";
		};
		conf {
			pins = "WF0_HB1", "WF0_HB2", "WF0_HB3", "WF0_HB4",
			       "WF0_HB0", "WF0_HB0_B", "WF0_HB5", "WF0_HB6",
			       "WF0_HB7", "WF0_HB8", "WF0_HB9", "WF0_HB10",
			       "WF0_TOP_CLK", "WF0_TOP_DATA", "WF1_HB1",
			       "WF1_HB2", "WF1_HB3", "WF1_HB4", "WF1_HB0",
			       "WF1_HB5", "WF1_HB6", "WF1_HB7", "WF1_HB8",
			       "WF1_TOP_CLK", "WF1_TOP_DATA";
			drive-strength = <4>;
		};
	};

	wf_dbdc_pins: wf-dbdc-pins {
		mux {
			function = "wifi";
			groups = "wf_dbdc";
		};
		conf {
			pins = "WF0_HB1", "WF0_HB2", "WF0_HB3", "WF0_HB4",
				"WF0_HB0", "WF0_HB0_B", "WF0_HB5", "WF0_HB6",
				"WF0_HB7", "WF0_HB8", "WF0_HB9", "WF0_HB10",
				"WF0_TOP_CLK", "WF0_TOP_DATA", "WF1_HB1",
				"WF1_HB2", "WF1_HB3", "WF1_HB4", "WF1_HB0",
				"WF1_HB5", "WF1_HB6", "WF1_HB7", "WF1_HB8",
				"WF1_TOP_CLK", "WF1_TOP_DATA";
			drive-strength = <4>;
		};
	};
};

&switch {
	ports {
		#address-cells = <1>;
		#size-cells = <0>;

		port@0 {
			reg = <0>;
			label = "game";
			phy-handle = <&swphy0>;
		};

		port@1 {
			reg = <1>;
			label = "lan1";
			phy-handle = <&swphy1>;
		};

		port@2 {
			reg = <2>;
			label = "lan2";
			phy-handle = <&swphy2>;
		};

		port@3 {
			reg = <3>;
			label = "lan3";
			phy-handle = <&swphy3>;
		};

		port@6 {
			reg = <6>;
			label = "cpu";
			ethernet = <&gmac0>;
			phy-mode = "2500base-x";

			fixed-link {
				speed = <2500>;
				full-duplex;
				pause;
			};
		};
	};

	mdio {
		#address-cells = <1>;
		#size-cells = <0>;

		swphy0: phy@0 {
			reg = <0>;

			mediatek,led-config = <
				0x21 0x8009 /* BASIC_CTRL */
				0x22 0x0c00 /* ON_DURATION */
				0x23 0x1400 /* BLINK_DURATION */
				0x24 0xc001 /* LED0_ON_CTRL */
				0x25 0x0000 /* LED0_BLINK_CTRL */
				0x26 0xc007 /* LED1_ON_CTRL */
				0x27 0x003f /* LED1_BLINK_CTRL */
			>;
		};

		swphy1: phy@1 {
			reg = <1>;

			mediatek,led-config = <
				0x21 0x8009 /* BASIC_CTRL */
				0x22 0x0c00 /* ON_DURATION */
				0x23 0x1400 /* BLINK_DURATION */
				0x24 0xc001 /* LED0_ON_CTRL */
				0x25 0x0000 /* LED0_BLINK_CTRL */
				0x26 0xc007 /* LED1_ON_CTRL */
				0x27 0x003f /* LED1_BLINK_CTRL */
			>;
		};

		swphy2: phy@2 {
			reg = <2>;

			mediatek,led-config = <
				0x21 0x8009 /* BASIC_CTRL */
				0x22 0x0c00 /* ON_DURATION */
				0x23 0x1400 /* BLINK_DURATION */
				0x24 0xc001 /* LED0_ON_CTRL */
				0x25 0x0000 /* LED0_BLINK_CTRL */
				0x26 0xc007 /* LED1_ON_CTRL */
				0x27 0x003f /* LED1_BLINK_CTRL */
			>;
		};

		swphy3: phy@3 {
			reg = <3>;

			mediatek,led-config = <
				0x21 0x8009 /* BASIC_CTRL */
				0x22 0x0c00 /* ON_DURATION */
				0x23 0x1400 /* BLINK_DURATION */
				0x24 0xc001 /* LED0_ON_CTRL */
				0x25 0x0000 /* LED0_BLINK_CTRL */
				0x26 0xc007 /* LED1_ON_CTRL */
				0x27 0x003f /* LED1_BLINK_CTRL */
			>;
		};
	};
};

&wifi {
	status = "okay";
	pinctrl-names = "default", "dbdc";
	pinctrl-0 = <&wf_2g_5g_pins>;
	pinctrl-1 = <&wf_dbdc_pins>;
};

&trng {
	status = "okay";
};

&watchdog {
	status = "okay";
};

&crypto {
	status = "okay";
};

&uart0 {
	status = "okay";
};

&ssusb {
	vusb33-supply = <&reg_3p3v>;
	vbus-supply = <&reg_5v>;
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&mmc0 {
	status = "okay";
	pinctrl-names = "default", "state_uhs";
	pinctrl-0 = <&mmc0_pins_default>;
	pinctrl-1 = <&mmc0_pins_uhs>;
	bus-width = <0x08>;
	max-frequency = <200000000>;
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
	mmc-hs400-1_8v;
	hs400-ds-delay = <0x14014>;
	vmmc-supply = <&reg_3p3v>;
	vqmmc-supply = <&reg_1p8v>;
	non-removable;
	no-sd;
	no-sdio;
};

&pcie {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie_pins>;
	status = "okay";
};

&pcie_phy {
	status = "okay";
};
