From 011e40a166fdaa65fb9946b7cd91efec85b70dbb Mon Sep 17 00:00:00 2001
From: Michael Walle <michael@walle.cc>
Date: Tue, 4 Apr 2023 18:21:27 +0100
Subject: [PATCH] nvmem: cell: drop global cell_post_process

There are no users anymore for the global cell_post_process callback
anymore. New users should use proper nvmem layouts.

Signed-off-by: Michael Walle <michael@walle.cc>
Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20230404172148.82422-20-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/core.c           | 9 ---------
 include/linux/nvmem-provider.h | 2 --
 2 files changed, 11 deletions(-)

--- a/drivers/nvmem/core.c
+++ b/drivers/nvmem/core.c
@@ -39,7 +39,6 @@ struct nvmem_device {
 	unsigned int		nkeepout;
 	nvmem_reg_read_t	reg_read;
 	nvmem_reg_write_t	reg_write;
-	nvmem_cell_post_process_t cell_post_process;
 	struct gpio_desc	*wp_gpio;
 	struct nvmem_layout	*layout;
 	void *priv;
@@ -903,7 +902,6 @@ struct nvmem_device *nvmem_register(cons
 	nvmem->type = config->type;
 	nvmem->reg_read = config->reg_read;
 	nvmem->reg_write = config->reg_write;
-	nvmem->cell_post_process = config->cell_post_process;
 	nvmem->keepout = config->keepout;
 	nvmem->nkeepout = config->nkeepout;
 	if (config->of_node)
@@ -1575,13 +1573,6 @@ static int __nvmem_cell_read(struct nvme
 		if (rc)
 			return rc;
 	}
-
-	if (nvmem->cell_post_process) {
-		rc = nvmem->cell_post_process(nvmem->priv, id, index,
-					      cell->offset, buf, cell->bytes);
-		if (rc)
-			return rc;
-	}
 
 	if (len)
 		*len = cell->bytes;
--- a/include/linux/nvmem-provider.h
+++ b/include/linux/nvmem-provider.h
@@ -85,7 +85,6 @@ struct nvmem_cell_info {
  * @no_of_node:	Device should not use the parent's of_node even if it's !NULL.
  * @reg_read:	Callback to read data.
  * @reg_write:	Callback to write data.
- * @cell_post_process:	Callback for vendor specific post processing of cell data
  * @size:	Device size.
  * @word_size:	Minimum read/write access granularity.
  * @stride:	Minimum read/write access stride.
@@ -118,7 +117,6 @@ struct nvmem_config {
 	bool			no_of_node;
 	nvmem_reg_read_t	reg_read;
 	nvmem_reg_write_t	reg_write;
-	nvmem_cell_post_process_t cell_post_process;
 	int	size;
 	int	word_size;
 	int	stride;
