// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

/dts-v1/;

#include "ipq8074.dtsi"
#include "ipq8074-hk-cpu.dtsi"
#include "ipq8074-ess.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "Zbtlink ZBT-Z800AX";
	compatible = "zbtlink,zbt-z800ax", "qcom,ipq8074";

	aliases {
		led-boot = &led_net;
		led-failsafe = &led_net;
		led-upgrade = &led_net;
		serial0 = &blsp1_uart5;
		/*
		 * Aliases as required by u-boot
		 * to patch MAC addresses
		 */
		ethernet0 = &dp1;
		ethernet1 = &dp2;
		ethernet2 = &dp3;
		ethernet3 = &dp4;
		ethernet4 = &dp5;
		label-mac-device = &dp1;
	};

	chosen {
		stdout-path = "serial0:115200n8";
		bootargs-append = " root=/dev/ubiblock0_1";
	};

	gpio-export {
		compatible = "gpio-export";

		lte-power {
			gpio-export,name = "lte_power";
			gpio-export,output = <1>;
			gpios = <&tlmm 55 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-0 = <&button_pins>;
		pinctrl-names = "default";

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&tlmm 34 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "wps";
			linux,code = <KEY_WPS_BUTTON>;
			gpios = <&tlmm 46 GPIO_ACTIVE_LOW>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_net: net {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WAN_ONLINE;
			gpios = <&tlmm 22 GPIO_ACTIVE_HIGH>;
		};

		module {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_MOBILE;
			gpios = <&tlmm 30 GPIO_ACTIVE_HIGH>;
		};

		wlan2g {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN_2GHZ;
			gpios = <&tlmm 42 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1radio";
		};

		wlan5g {
			color = <LED_COLOR_ID_GREEN>;
			function =  LED_FUNCTION_WLAN_5GHZ;
			gpios = <&tlmm 43 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0radio";
		};
	};
};

&tlmm {
	button_pins: button-pins {
		mux {
			pins = "gpio34", "gpio46";
			function = "gpio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};

	mdio_pins: mdio-pins {
		mdc {
			pins = "gpio68";
			function = "mdc";
			drive-strength = <8>;
			bias-pull-up;
		};

		mdio {
			pins = "gpio69";
			function = "mdio";
			drive-strength = <8>;
			bias-pull-up;
		};
	};
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	cs-select = <0>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		#address-cells = <1>;
		#size-cells = <1>;
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "0:sbl1";
				reg = <0x0 0x50000>;
				read-only;
			};

			partition@50000 {
				label = "0:mibib";
				reg = <0x50000 0x10000>;
				read-only;
			};

			partition@60000 {
				label = "0:bootconfig";
				reg = <0x60000 0x20000>;
				read-only;
			};

			partition@80000 {
				label = "0:bootconfig1";
				reg = <0x80000 0x20000>;
				read-only;
			};

			partition@a0000 {
				label = "0:qsee";
				reg = <0xa0000 0x180000>;
				read-only;
			};

			partition@220000 {
				label = "0:qsee_1";
				reg = <0x220000 0x180000>;
				read-only;
			};

			partition@3a0000 {
				label = "0:devcfg";
				reg = <0x3a0000 0x10000>;
				read-only;
			};

			partition@3b0000 {
				label = "0:devcfg_1";
				reg = <0x3b0000 0x10000>;
				read-only;
			};

			partition@3c0000 {
				label = "0:apdp";
				reg = <0x3c0000 0x10000>;
				read-only;
			};

			partition@3d0000 {
				label = "0:apdp_1";
				reg = <0x3d0000 0x10000>;
				read-only;
			};

			partition@3e0000 {
				label = "0:rpm";
				reg = <0x3e0000 0x40000>;
				read-only;
			};

			partition@420000 {
				label = "0:rpm_1";
				reg = <0x420000 0x40000>;
				read-only;
			};

			partition@460000 {
				label = "0:cdt";
				reg = <0x460000 0x10000>;
				read-only;
			};

			partition@470000 {
				label = "0:cdt_1";
				reg = <0x470000 0x10000>;
				read-only;
			};

			partition@480000 {
				label = "0:appsblenv";
				reg = <0x480000 0x10000>;
			};

			partition@490000 {
				label = "0:appsbl";
				reg = <0x490000 0xa0000>;
				read-only;
			};

			partition@530000 {
				label = "0:appsbl_1";
				reg = <0x530000 0xa0000>;
				read-only;
			};

			partition@5d0000 {
				label = "0:art";
				reg = <0x5d0000 0x40000>;
				read-only;
			};

			partition@610000 {
				label = "0:ethphyfw";
				reg = <0x610000 0x80000>;
				read-only;
			};
		};
	};
};

&blsp1_uart5 {
	status = "okay";
};

&cryptobam {
	status = "okay";
};

&crypto {
	status = "okay";
};

&prng {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&qpic_nand {
	status = "okay";

	partitions {
		status = "disabled";
	};

	nand@0 {
		reg = <0>;
		nand-ecc-strength = <8>;
		nand-ecc-step-size = <512>;
		nand-bus-width = <8>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "rootfs";
				reg = <0x0000000 0x3400000>;
			};

			partition@3400000 {
				label = "0:wififw";
				reg = <0x3400000 0x0800000>;
				read-only;
			};

			partition@3c00000 {
				label = "rootfs_1";
				reg = <0x3c00000 0x3400000>;
			};

			partition@7000000 {
				label = "0:wififw_1";
				reg = <0x7000000 0x0800000>;
				read-only;
			};
		};
	};
};

&qusb_phy_0 {
	status = "okay";
};

&qusb_phy_1 {
	status = "okay";
};

&ssphy_0 {
	status = "okay";
};

&ssphy_1 {
	status = "okay";
};

&usb_0 {
	status = "okay";
};

&usb_1 {
	status = "okay";
};

&mdio {
	status = "okay";

	pinctrl-0 = <&mdio_pins>;
	pinctrl-names = "default";
	reset-gpios = <&tlmm 37 GPIO_ACTIVE_LOW>;

	ethernet-phy-package@0 {
		compatible = "qcom,qca8075-package";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;

		qca8075_0: ethernet-phy@0 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <0>;
		};

		qca8075_1: ethernet-phy@1 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <1>;
		};

		qca8075_2: ethernet-phy@2 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <2>;
		};

		qca8075_3: ethernet-phy@3 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <3>;
		};

		qca8075_4: ethernet-phy@4 {
			compatible = "ethernet-phy-ieee802.3-c22";
			reg = <4>;
		};
	};
};

&switch {
	status = "okay";

	switch_lan_bmp = <(ESS_PORT1 | ESS_PORT2 | ESS_PORT3 | ESS_PORT4)>;
	switch_wan_bmp = <ESS_PORT5>;
	switch_mac_mode = <MAC_MODE_PSGMII>;

	qcom,port_phyinfo {
		port@1 {
			port_id = <1>;
			phy_address = <0>;
		};
		port@2 {
			port_id = <2>;
			phy_address = <1>;
		};
		port@3 {
			port_id = <3>;
			phy_address = <2>;
		};
		port@4 {
			port_id = <4>;
			phy_address = <3>;
		};
		port@5 {
			port_id = <5>;
			phy_address = <4>;
		};
	};
};

&edma {
	status = "okay";
};

&dp1 {
	status = "okay";
	phy-handle = <&qca8075_0>;
	label = "lan1";
};

&dp2 {
	status = "okay";
	phy-handle = <&qca8075_1>;
	label = "lan2";
};

&dp3 {
	status = "okay";
	phy-handle = <&qca8075_2>;
	label = "lan3";
};

&dp4 {
	status = "okay";
	phy-handle = <&qca8075_3>;
	label = "lan4";
};

&dp5 {
	status = "okay";
	phy-handle = <&qca8075_4>;
	label = "wan";
};

&wifi {
	status = "okay";

	qcom,ath11k-calibration-variant = "ZBT-Z800AX";
};
