From cdbefcc4fdaa9623f6bed4beef692e6d4453a17d Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.com>
Date: Mon, 6 Mar 2023 17:15:36 +0000
Subject: [PATCH] overlays: pca953x: Fix a typos in the pcal variants

Signed-off-by: Phil Elwell <phil@raspberrypi.com>
---
 arch/arm/boot/dts/overlays/README              |  6 +++---
 arch/arm/boot/dts/overlays/pca953x-overlay.dts | 12 ++++++------
 2 files changed, 9 insertions(+), 9 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -3045,9 +3045,9 @@ Params: addr                    I2C addr
         pca9574                 Select the NXP PCA9574 (8 bit)
         pca9575                 Select the NXP PCA9575 (16 bit)
         pca9698                 Select the NXP PCA9698 (40 bit)
-        pca16416                Select the NXP PCA16416 (16 bit)
-        pca16524                Select the NXP PCA16524 (24 bit)
-        pca19555a               Select the NXP PCA19555A (16 bit)
+        pcal6416                Select the NXP PCAL6416 (16 bit)
+        pcal6524                Select the NXP PCAL6524 (24 bit)
+        pcal9555a               Select the NXP PCAL9555A (16 bit)
         max7310                 Select the Maxim MAX7310 (8 bit)
         max7312                 Select the Maxim MAX7312 (16 bit)
         max7313                 Select the Maxim MAX7313 (16 bit)
--- a/arch/arm/boot/dts/overlays/pca953x-overlay.dts
+++ b/arch/arm/boot/dts/overlays/pca953x-overlay.dts
@@ -110,19 +110,19 @@
 	fragment@15 {
 		target = <&pca>;
 		__dormant__ {
-			compatible = "nxp,pca16416";
+			compatible = "nxp,pcal6416";
 		};
 	};
 	fragment@16 {
 		target = <&pca>;
 		__dormant__ {
-			compatible = "nxp,pca16524";
+			compatible = "nxp,pcal6524";
 		};
 	};
 	fragment@17 {
 		target = <&pca>;
 		__dormant__ {
-			compatible = "nxp,pca19555a";
+			compatible = "nxp,pcal9555a";
 		};
 	};
 	fragment@18 {
@@ -220,9 +220,9 @@
 		pca9574 = <0>, "+12";
 		pca9575 = <0>, "+13";
 		pca9698 = <0>, "+14";
-		pca16416 = <0>, "+15";
-		pca16524 = <0>, "+16";
-		pca19555a = <0>, "+17";
+		pcal6416 = <0>, "+15";
+		pcal6524 = <0>, "+16";
+		pcal9555a = <0>, "+17";
 		max7310 = <0>, "+18";
 		max7312 = <0>, "+19";
 		max7313 = <0>, "+20";
