From 1d81e51d6d79d9098013b2e8cdd677bae998c5d8 Mon Sep 17 00:00:00 2001
From: David Bauer <mail@david-bauer.net>
Date: Fri, 28 Apr 2023 02:22:59 +0200
Subject: [PATCH 1/2] mt7530: register OF node for internal MDIO bus

The MT753x switches provide a switch-internal MDIO bus for the embedded
PHYs.

Register a OF sub-node on the switch OF-node for this internal MDIO bus.
This allows to configure the embedded PHYs using device-tree.

Signed-off-by: David Bauer <mail@david-bauer.net>
---
 drivers/net/dsa/mt7530.c | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -2356,10 +2356,13 @@ mt7530_setup_mdio(struct mt7530_priv *pr
 {
 	struct dsa_switch *ds = priv->ds;
 	struct device *dev = priv->dev;
+	struct device_node *np, *mnp;
 	struct mii_bus *bus;
 	static int idx;
 	int ret;
 
+	np = priv->dev->of_node;
+
 	bus = devm_mdiobus_alloc(dev);
 	if (!bus)
 		return -ENOMEM;
@@ -2376,7 +2379,9 @@ mt7530_setup_mdio(struct mt7530_priv *pr
 	if (priv->irq)
 		mt7530_setup_mdio_irq(priv);
 
-	ret = devm_mdiobus_register(dev, bus);
+	mnp = of_get_child_by_name(np, "mdio");
+	ret = devm_of_mdiobus_register(dev, bus, mnp);
+	of_node_put(mnp);
 	if (ret) {
 		dev_err(dev, "failed to register MDIO bus: %d\n", ret);
 		if (priv->irq)
