From 10b0a19d62d932a6eb01ceb8749190aaf0ff063e Mon Sep 17 00:00:00 2001
From: Shaohui Xie <Shaohui.Xie@freescale.com>
Date: Mon, 11 Jul 2016 10:47:20 +0800
Subject: [PATCH 12/70] dts: ls1043a: add fman/bman/qman/ethernet nodes

commit ecb0901ba0a6558a05054d21ad9e70999a6f7ca1
[context adjustment]

Signed-off-by: Shaohui Xie <Shaohui.Xie@freescale.com>
Signed-off-by: Zhao Qiang <qiang.zhao@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi     |  461 ++++++++++++++++++++
 .../boot/dts/freescale/qoriq-bman1-portals.dtsi    |  104 +++++
 .../boot/dts/freescale/qoriq-qman1-portals.dtsi    |  136 ++++++
 3 files changed, 701 insertions(+)
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-bman1-portals.dtsi
 create mode 100644 arch/arm64/boot/dts/freescale/qoriq-qman1-portals.dtsi

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -50,6 +50,16 @@
 	#address-cells = <2>;
 	#size-cells = <2>;
 
+	aliases {
+		ethernet0 = &fm1mac1;
+		ethernet1 = &fm1mac2;
+		ethernet2 = &fm1mac3;
+		ethernet3 = &fm1mac4;
+		ethernet4 = &fm1mac5;
+		ethernet5 = &fm1mac6;
+		ethernet6 = &fm1mac9;
+	};
+
 	cpus {
 		#address-cells = <1>;
 		#size-cells = <0>;
@@ -174,6 +184,323 @@
 			bus-width = <4>;
 		};
 
+		qman: qman@1880000 {
+			compatible = "fsl,qman";
+			reg = <0x00 0x1880000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+		};
+
+		bman: bman@1890000 {
+			compatible = "fsl,bman";
+			reg = <0x00 0x1890000 0x0 0x10000>;
+			interrupts = <0 45 0x4>;
+		};
+
+		fman0: fman@1a00000 {
+			#address-cells = <1>;
+			#size-cells = <1>;
+			cell-index = <0>;
+			compatible = "fsl,fman", "simple-bus";
+			ranges = <0x0 0x00 0x1a00000 0x100000>;
+			reg = <0x00 0x1a00000 0x0 0x100000>;
+			clock-frequency = <0>;
+			interrupts = <0 44 0x4>,
+				     <0 45 0x4>;
+
+			cc {
+				compatible = "fsl,fman-cc";
+			};
+
+			muram@0 {
+				compatible = "fsl,fman-muram";
+				reg = <0x0 0x60000>;
+			};
+
+			bmi@80000 {
+				compatible = "fsl,fman-bmi";
+				reg = <0x80000 0x400>;
+			};
+
+			qmi@80400 {
+				compatible = "fsl,fman-qmi";
+				reg = <0x80400 0x400>;
+			};
+
+			fman0_oh1: port@82000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x82000 0x1000>;
+			};
+
+			fman0_oh2: port@83000 {
+				cell-index = <1>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x83000 0x1000>;
+			};
+
+			fman0_oh3: port@84000 {
+				cell-index = <2>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x84000 0x1000>;
+			};
+
+			fman0_oh4: port@85000 {
+				cell-index = <3>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x85000 0x1000>;
+			};
+
+			fman0_oh5: port@86000 {
+				cell-index = <4>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x86000 0x1000>;
+			};
+
+			fman0_oh6: port@87000 {
+				cell-index = <5>;
+				compatible = "fsl,fman-port-oh";
+				reg = <0x87000 0x1000>;
+			};
+
+			policer@c0000 {
+				compatible = "fsl,fman-policer";
+				reg = <0xc0000 0x1000>;
+			};
+
+			keygen@c1000 {
+				compatible = "fsl,fman-keygen";
+				reg = <0xc1000 0x1000>;
+			};
+
+			dma@c2000 {
+				compatible = "fsl,fman-dma";
+				reg = <0xc2000 0x1000>;
+			};
+
+			fpm@c3000 {
+				compatible = "fsl,fman-fpm";
+				reg = <0xc3000 0x1000>;
+			};
+
+			parser@c7000 {
+				compatible = "fsl,fman-parser";
+				reg = <0xc7000 0x1000>;
+			};
+
+			vsps@dc000 {
+				compatible = "fsl,fman-vsps";
+				reg = <0xdc000 0x1000>;
+			};
+
+			mdio0: mdio@fc000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xfc000 0x1000>;
+			};
+
+			xmdio0: mdio@fd000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xfd000 0x1000>;
+			};
+
+			fman0_rx0: port@88000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x88000 0x1000>;
+			};
+
+			fman0_tx0: port@a8000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xa8000 0x1000>;
+			};
+
+			fm1mac1: ethernet@e0000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-memac";
+				reg = <0xe0000 0x1000>;
+				fsl,port-handles = <&fman0_rx0 &fman0_tx0>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@e1000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xe1000 0x1000>;
+			};
+
+			fman0_rx1: port@89000 {
+				cell-index = <1>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x89000 0x1000>;
+			};
+
+			fman0_tx1: port@a9000 {
+				cell-index = <1>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xa9000 0x1000>;
+			};
+
+			fm1mac2: ethernet@e2000 {
+				cell-index = <1>;
+				compatible = "fsl,fman-memac";
+				reg = <0xe2000 0x1000>;
+				fsl,port-handles = <&fman0_rx1 &fman0_tx1>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@e3000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xe3000 0x1000>;
+			};
+
+			fman0_rx2: port@8a000 {
+				cell-index = <2>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x8a000 0x1000>;
+			};
+
+			fman0_tx2: port@aa000 {
+				cell-index = <2>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xaa000 0x1000>;
+			};
+
+			fm1mac3: ethernet@e4000 {
+				cell-index = <2>;
+				compatible = "fsl,fman-memac";
+				reg = <0xe4000 0x1000>;
+				fsl,port-handles = <&fman0_rx2 &fman0_tx2>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@e5000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xe5000 0x1000>;
+			};
+
+			fman0_rx3: port@8b000 {
+				cell-index = <3>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x8b000 0x1000>;
+			};
+
+			fman0_tx3: port@ab000 {
+				cell-index = <3>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xab000 0x1000>;
+			};
+
+			fm1mac4: ethernet@e6000 {
+				cell-index = <3>;
+				compatible = "fsl,fman-memac";
+				reg = <0xe6000 0x1000>;
+				fsl,port-handles = <&fman0_rx3 &fman0_tx3>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@e7000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xe7000 0x1000>;
+			};
+
+			fman0_rx4: port@8c000 {
+				cell-index = <4>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x8c000 0x1000>;
+			};
+
+			fman0_tx4: port@ac000 {
+				cell-index = <4>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xac000 0x1000>;
+			};
+
+			fm1mac5: ethernet@e8000 {
+				cell-index = <4>;
+				compatible = "fsl,fman-memac";
+				reg = <0xe8000 0x1000>;
+				fsl,port-handles = <&fman0_rx4 &fman0_tx4>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@e9000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xe9000 0x1000>;
+			};
+
+			fman0_rx5: port@8d000 {
+				cell-index = <5>;
+				compatible = "fsl,fman-port-1g-rx";
+				reg = <0x8d000 0x1000>;
+			};
+
+			fman0_tx5: port@ad000 {
+				cell-index = <5>;
+				compatible = "fsl,fman-port-1g-tx";
+				reg = <0xad000 0x1000>;
+			};
+
+			fm1mac6: ethernet@ea000 {
+				cell-index = <5>;
+				compatible = "fsl,fman-memac";
+				reg = <0xea000 0x1000>;
+				fsl,port-handles = <&fman0_rx5 &fman0_tx5>;
+				ptimer-handle = <&ptp_timer0>;
+			};
+
+			mdio@eb000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xeb000 0x1000>;
+			};
+
+			fman0_10g_rx0: port@90000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-port-10g-rx";
+				reg = <0x90000 0x1000>;
+			};
+
+			fman0_10g_tx0: port@b0000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-port-10g-tx";
+				reg = <0xb0000 0x1000>;
+				fsl,qman-channel-id = <0x800>;
+			};
+
+			fm1mac9: ethernet@f0000 {
+				cell-index = <0>;
+				compatible = "fsl,fman-memac";
+				reg = <0xf0000 0x1000>;
+				fsl,port-handles = <&fman0_10g_rx0 &fman0_10g_tx0>;
+			};
+
+			mdio@f1000 {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				compatible = "fsl,fman-memac-mdio";
+				reg = <0xf1000 0x1000>;
+			};
+
+			ptp_timer0: rtc@fe000 {
+				compatible = "fsl,fman-rtc";
+				reg = <0xfe000 0x1000>;
+			};
+		};
+
 		dspi0: dspi@2100000 {
 			compatible = "fsl,ls1043a-dspi", "fsl,ls1021a-v1.0-dspi";
 			#address-cells = <1>;
@@ -522,4 +849,138 @@
 		};
 	};
 
+	fsl,dpaa {
+		compatible = "fsl,ls1043a-dpaa", "simple-bus", "fsl,dpaa";
+		ethernet@0 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac1>;
+		};
+		ethernet@1 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac2>;
+		};
+		ethernet@2 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac3>;
+		};
+		ethernet@3 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac4>;
+		};
+		ethernet@4 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac5>;
+		};
+		ethernet@5 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac6>;
+		};
+		ethernet@8 {
+			compatible = "fsl,dpa-ethernet";
+			fsl,fman-mac = <&fm1mac9>;
+		};
+	};
+
+	qportals: qman-portals@500000000 {
+		   ranges = <0x0 0x5 0x00000000 0x8000000>;
+        };
+	bportals: bman-portals@508000000 {
+		   ranges = <0x0 0x5 0x08000000 0x8000000>;
+        };
+	reserved-memory {
+		#address-cells = <2>;
+		#size-cells = <2>;
+		ranges;
+
+		bman_fbpr: bman-fbpr {
+			size = <0 0x1000000>;
+			alignment = <0 0x1000000>;
+		};
+		qman_fqd: qman-fqd {
+			size = <0 0x400000>;
+			alignment = <0 0x400000>;
+		};
+		qman_pfdr: qman-pfdr {
+			size = <0 0x2000000>;
+			alignment = <0 0x2000000>;
+		};
+	};
+};
+
+&fman0 {
+	/* offline - 1 */
+	port@82000 {
+		fsl,qman-channel-id = <0x809>;
+	};
+
+	/* tx - 10g - 2 */
+	port@a8000 {
+		fsl,qman-channel-id = <0x802>;
+	};
+	/* tx - 10g - 3 */
+	port@a9000 {
+		fsl,qman-channel-id = <0x803>;
+	};
+	/* tx - 1g - 2 */
+	port@aa000 {
+		fsl,qman-channel-id = <0x804>;
+	};
+	/* tx - 1g - 3 */
+	port@ab000 {
+		fsl,qman-channel-id = <0x805>;
+	};
+	/* tx - 1g - 4 */
+	port@ac000 {
+		fsl,qman-channel-id = <0x806>;
+	};
+	/* tx - 1g - 5 */
+	port@ad000 {
+		fsl,qman-channel-id = <0x807>;
+	};
+	/* tx - 10g - 0 */
+	port@b0000 {
+		fsl,qman-channel-id = <0x800>;
+	};
+	/* tx - 10g - 1 */
+	port@b1000 {
+		fsl,qman-channel-id = <0x801>;
+	};
+	/* offline - 2 */
+	port@83000 {
+		fsl,qman-channel-id = <0x80a>;
+	};
+	/* offline - 3 */
+	port@84000 {
+		fsl,qman-channel-id = <0x80b>;
+	};
+	/* offline - 4 */
+	port@85000 {
+		fsl,qman-channel-id = <0x80c>;
+	};
+	/* offline - 5 */
+	port@86000 {
+		fsl,qman-channel-id = <0x80d>;
+	};
+	/* offline - 6 */
+	port@87000 {
+		fsl,qman-channel-id = <0x80e>;
+	};
+};
+
+&bman_fbpr {
+	compatible = "fsl,bman-fbpr";
+	alloc-ranges = <0 0 0x10000 0>;
 };
+
+&qman_fqd {
+	compatible = "fsl,qman-fqd";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+&qman_pfdr {
+	compatible = "fsl,qman-pfdr";
+	alloc-ranges = <0 0 0x10000 0>;
+};
+
+/include/ "qoriq-qman1-portals.dtsi"
+/include/ "qoriq-bman1-portals.dtsi"
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-bman1-portals.dtsi
@@ -0,0 +1,104 @@
+/*
+ * QorIQ BMan Portal device tree stub for 10 portals
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions are met:
+ *     * Redistributions of source code must retain the above copyright
+ *	 notice, this list of conditions and the following disclaimer.
+ *     * Redistributions in binary form must reproduce the above copyright
+ *	 notice, this list of conditions and the following disclaimer in the
+ *	 documentation and/or other materials provided with the distribution.
+ *     * Neither the name of Freescale Semiconductor nor the
+ *	 names of its contributors may be used to endorse or promote products
+ *	 derived from this software without specific prior written permission.
+ *
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") as published by the Free Software
+ * Foundation, either version 2 of that License or (at your option) any
+ * later version.
+ *
+ * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
+ * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
+ * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
+ * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
+ * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
+ * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
+ * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
+ * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+
+&bportals {
+	  #address-cells = <1>;
+	  #size-cells = <1>;
+	  compatible = "simple-bus";
+	  bportal0: bman-portal@0 {
+		cell-index = <0>;
+		compatible = "fsl,bman-portal";
+		reg = <0x0 0x4000 0x4000000 0x4000>;
+		interrupts = <0 173 0x4>;
+	};
+	bportal1: bman-portal@10000 {
+		cell-index = <1>;
+		compatible = "fsl,bman-portal";
+		reg = <0x10000 0x4000 0x4010000 0x4000>;
+		interrupts = <0 175 0x4>;
+	};
+	bportal2: bman-portal@20000 {
+		cell-index = <2>;
+		compatible = "fsl,bman-portal";
+		reg = <0x20000 0x4000 0x4020000 0x4000>;
+		interrupts = <0 177 0x4>;
+	};
+	bportal3: bman-portal@30000 {
+		cell-index = <3>;
+		compatible = "fsl,bman-portal";
+		reg = <0x30000 0x4000 0x4030000 0x4000>;
+		interrupts = <0 179 0x4>;
+	};
+	bportal4: bman-portal@40000 {
+		cell-index = <4>;
+		compatible = "fsl,bman-portal";
+		reg = <0x40000 0x4000 0x4040000 0x4000>;
+		interrupts = <0 181 0x4>;
+		};
+	bportal5: bman-portal@50000 {
+		cell-index = <5>;
+		compatible = "fsl,bman-portal";
+		reg = <0x50000 0x4000 0x4050000 0x4000>;
+		interrupts = <0 183 0x4>;
+	};
+	bportal6: bman-portal@60000 {
+		cell-index = <6>;
+		compatible = "fsl,bman-portal";
+		reg = <0x60000 0x4000 0x4060000 0x4000>;
+		interrupts = <0 185 0x4>;
+	};
+	bportal7: bman-portal@70000 {
+		cell-index = <7>;
+		compatible = "fsl,bman-portal";
+		reg = <0x70000 0x4000 0x4070000 0x4000>;
+		interrupts = <0 187 0x4>;
+	};
+	bportal8: bman-portal@80000 {
+		cell-index = <8>;
+		compatible = "fsl,bman-portal";
+		reg = <0x80000 0x4000 0x4080000 0x4000>;
+		interrupts = <0 189 0x4>;
+	};
+/*	bportal9: bman-portal@90000 {
+		cell-index = <9>;
+		compatible = "fsl,bman-portal";
+		reg = <0x90000 0x4000 0x4090000 0x4000>;
+		interrupts = <0 191 0x4>;
+	}; */
+	 bman-bpids@0 {
+                compatible = "fsl,bpid-range";
+                fsl,bpid-range = <32 32>;
+        };
+
+};
--- /dev/null
+++ b/arch/arm64/boot/dts/freescale/qoriq-qman1-portals.dtsi
@@ -0,0 +1,136 @@
+/*
+ * QorIQ QMan Portal device tree stub for 10 portals & 15 pool channels
+ *
+ * Copyright 2011-2016 Freescale Semiconductor Inc.
+ *
+ * Redistribution and use in source and binary forms, with or without
+ * modification, are permitted provided that the following conditions are met:
+ *     * Redistributions of source code must retain the above copyright
+ *	 notice, this list of conditions and the following disclaimer.
+ *     * Redistributions in binary form must reproduce the above copyright
+ *	 notice, this list of conditions and the following disclaimer in the
+ *	 documentation and/or other materials provided with the distribution.
+ *     * Neither the name of Freescale Semiconductor nor the
+ *	 names of its contributors may be used to endorse or promote products
+ *	 derived from this software without specific prior written permission.
+ *
+ *
+ * ALTERNATIVELY, this software may be distributed under the terms of the
+ * GNU General Public License ("GPL") as published by the Free Software
+ * Foundation, either version 2 of that License or (at your option) any
+ * later version.
+ *
+ * THIS SOFTWARE IS PROVIDED BY Freescale Semiconductor ``AS IS'' AND ANY
+ * EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
+ * WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
+ * DISCLAIMED. IN NO EVENT SHALL Freescale Semiconductor BE LIABLE FOR ANY
+ * DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES
+ * (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
+ * LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND
+ * ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT
+ * (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
+ * SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
+ */
+&qportals {
+
+	  #address-cells = <1>;
+	  #size-cells = <1>;
+	  compatible = "simple-bus";
+	  qportal0: qman-portal@0 {
+		cell-index = <0>;
+		compatible = "fsl,qman-portal";
+		reg = <0x0 0x4000 0x4000000 0x4000>;
+		interrupts = <0 172 0x4>;
+		fsl,qman-channel-id = <0x0>;
+	};
+
+	qportal1: qman-portal@10000 {
+		  cell-index = <1>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x10000 0x4000 0x4010000 0x4000>;
+		  interrupts = <0 174 0x4>;
+		  fsl,qman-channel-id = <1>;
+	};
+
+	qportal2: qman-portal@20000 {
+		  cell-index = <2>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x20000 0x4000 0x4020000 0x4000>;
+		  interrupts = <0 176 0x4>;
+		  fsl,qman-channel-id = <2>;
+	};
+
+	qportal3: qman-portal@30000 {
+		  cell-index = <3>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x30000 0x4000 0x4030000 0x4000>;
+		  interrupts = <0 178 0x4>;
+		  fsl,qman-channel-id = <3>;
+	};
+
+	qportal4: qman-portal@40000 {
+		  cell-index = <4>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x40000 0x4000 0x4040000 0x4000>;
+		  interrupts = <0 180 0x4>;
+		  fsl,qman-channel-id = <4>;
+	};
+
+	qportal5: qman-portal@50000 {
+		  cell-index = <5>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x50000 0x4000 0x4050000 0x4000>;
+		  interrupts = <0 182 0x4>;
+		  fsl,qman-channel-id = <5>;
+	};
+
+	qportal6: qman-portal@60000 {
+		  cell-index = <6>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x60000 0x4000 0x4060000 0x4000>;
+		  interrupts = <0 184 0x4>;
+		  fsl,qman-channel-id = <6>;
+	};
+
+	qportal7: qman-portal@70000 {
+		  cell-index = <7>;
+		  compatible = "fsl,qman-portal";
+		  reg = <0x70000 0x4000 0x4070000 0x4000>;
+		  interrupts = <0 186 0x4>;
+		  fsl,qman-channel-id = <7>;
+	};
+
+	qportal8: qman-portal@80000 {
+		cell-index = <8>;
+		compatible = "fsl,qman-portal";
+		reg = <0x80000 0x4000 0x4080000 0x4000>;
+		interrupts = <0 188 0x4>;
+		fsl,qman-channel-id = <8>;
+	};
+
+/*	qportal9: qman-portal@90000 {
+		cell-index = <9>;
+		compatible = "fsl,qman-portal";
+		reg = <0x90000 0x4000 0x4090000 0x4000>;
+		interrupts = <0 190 0x4>;
+		fsl,qman-channel-id = <9>;
+	}; */
+
+	qman-fqids@0 {
+                compatible = "fsl,fqid-range";
+                fsl,fqid-range = <256 256>;
+        };
+        qman-fqids@1 {
+                compatible = "fsl,fqid-range";
+                fsl,fqid-range = <32768 32768>;
+        };
+        qman-pools@0 {
+                compatible = "fsl,pool-channel-range";
+                fsl,pool-channel-range = <0x401 0xf>;
+        };
+        qman-cgrids@0 {
+                compatible = "fsl,cgrid-range";
+                fsl,cgrid-range = <0 256>;
+        };
+
+};
\ No newline at end of file
