From 9cd8b4a2ee9d0e6a5b91845bdd6f4b7e114fc8c4 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jogo@openwrt.org>
Date: Sat, 7 Dec 2013 14:22:41 +0100
Subject: [PATCH 41/53] MIPS: BCM63XX: define variant id field

---
 arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h | 2 ++
 1 file changed, 2 insertions(+)

--- a/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
+++ b/arch/mips/include/asm/mach-bcm63xx/bcm63xx_regs.h
@@ -9,6 +9,8 @@
 #define PERF_REV_REG			0x0
 #define REV_CHIPID_SHIFT		16
 #define REV_CHIPID_MASK			(0xffff << REV_CHIPID_SHIFT)
+#define REV_VARID_SHIFT			8
+#define REV_VARID_MASK			(0xf << REV_VARID_SHIFT)
 #define REV_REVID_SHIFT			0
 #define REV_REVID_MASK			(0xff << REV_REVID_SHIFT)
 
