From: Felix Fietkau <nbd@nbd.name>
Date: Tue, 23 Apr 2024 12:35:21 +0200
Subject: [PATCH] net: enable fraglist GRO by default

This can significantly improve performance for packet forwarding/bridging

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/include/linux/netdev_features.h
+++ b/include/linux/netdev_features.h
@@ -242,10 +242,10 @@ static inline int find_next_netdev_featu
 #define NETIF_F_UPPER_DISABLES	NETIF_F_LRO
 
 /* changeable features with no special hardware requirements */
-#define NETIF_F_SOFT_FEATURES	(NETIF_F_GSO | NETIF_F_GRO)
+#define NETIF_F_SOFT_FEATURES	(NETIF_F_GSO | NETIF_F_GRO | NETIF_F_GRO_FRAGLIST)
 
 /* Changeable features with no special hardware requirements that defaults to off. */
-#define NETIF_F_SOFT_FEATURES_OFF	(NETIF_F_GRO_FRAGLIST | NETIF_F_GRO_UDP_FWD)
+#define NETIF_F_SOFT_FEATURES_OFF	(NETIF_F_GRO_UDP_FWD)
 
 #define NETIF_F_VLAN_FEATURES	(NETIF_F_HW_VLAN_CTAG_FILTER | \
 				 NETIF_F_HW_VLAN_CTAG_RX | \
