From: Felix Fietkau <nbd@nbd.name>
Date: Sat, 27 Apr 2024 18:54:25 +0200
Subject: [PATCH] net: bridge: fix multicast-to-unicast with fraglist GSO

Calling skb_copy on a SKB_GSO_FRAGLIST skb is not valid, since it returns
an invalid linearized skb. This code only needs to change the ethernet
header, so pskb_copy is the right function to call here.

Fixes: 6db6f0eae605 ("bridge: multicast to unicast")
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/net/bridge/br_forward.c
+++ b/net/bridge/br_forward.c
@@ -266,7 +266,7 @@ static void maybe_deliver_addr(struct ne
 	if (skb->dev == p->dev && ether_addr_equal(src, addr))
 		return;
 
-	skb = skb_copy(skb, GFP_ATOMIC);
+	skb = pskb_copy(skb, GFP_ATOMIC);
 	if (!skb) {
 		DEV_STATS_INC(dev, tx_dropped);
 		return;
