From ebd924d773223593142d417c41d4ee6fa16f1805 Mon Sep 17 00:00:00 2001
From: OpenWrt community <openwrt-devel@lists.openwrt.org>
Date: Wed, 13 Jul 2022 13:45:56 +0200
Subject: [PATCH] net/dsa/mv88e6xxx: disable ATU violation

---
 drivers/net/dsa/mv88e6xxx/chip.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -3500,6 +3500,9 @@ static int mv88e6xxx_setup_port(struct m
 	else
 		reg = 1 << port;
 
+	/* Disable ATU member violation interrupt */
+	reg |= MV88E6XXX_PORT_ASSOC_VECTOR_IGNORE_WRONG;
+
 	err = mv88e6xxx_port_write(chip, port, MV88E6XXX_PORT_ASSOC_VECTOR,
 				   reg);
 	if (err)
